Skip to main content

## Magazine Buttons

Each magazine has a button that provides an easy way to unlock a magazine.

(see front panel)

Each magazine can be configured to have a portion designated as an I/O station. To unlock the I/O station, press the magazine button for less than 3 seconds.

To unlock the entire magazine, press the magazine button for more than 3 seconds.

|  | The user will need to pull out the magazine, as the magazine does not eject.

After a magazine has been open and closed, an library inventory will be performed. The button LED provides an indicator of the current state of that magazine.

Magazine State | LED state | Description
Closed | Steady ON | I/O station is enabled
Closed | Slow Flash | Magazine unlock is in progress
Closed | Fast Flash | Magazine is unlocked
Closed | OFF | I/O station is not enabled
Opened | OFF | Magazine is opened

| NOTE |

1. If an magazine unlock is in process, no other magazines or I/O station s can be unlocked.
2. If an unlocked magazine is not opened within 30 seconds, the magazine will be locked.