Skip to main content

## Drive Tests

After selecting the drive on which the test should be executed, one of the following drive tests can be selected:

- Power On Self Test (POST)
- Normal Read/Write Test
- Head Test
- Media Test
- Wrap Test
- SKLM for z/OS Basic Path Check (only visible if SKLM for z/OS is configured)
- SKLM for z/OS Full Path Check (only visible if SKLM for z/OS is configured)

In case the Power On Self Test was selected, no additional parameter needs to be configured and you can press Run to start the test.
In case selecting Normal Read/Write, Head or Media Test, it is necessary to select the Module of the I/O Station where the diagnostic cartridge, which is required for the test, should be inserted. The diagnostic cartridge must be inserted in the top most slot of the selected I/O Station. Be aware that at least one I/O Station must be enabled to execute the tests.

In case selecting the Wrap Test, it is necessary to select the SAS or FC port you are going to test. In this port, you need to insert the WrapTest connector.