Skip to main content

## Reset

The Configuration > Reset page provides the following submenus:

- Full Factory Reset
- Reset Internal IP Range

From the Configuration > Reset > Full Factory Reset page you can start a full factory reset of the library. This action clears all the configuration data of the library.

From the Configuration > Reset > Reset Internal IP Range page you can start the process for resetting the internal IP range.

For internal communication between modules, the tape library uses an Ethernet connection with an internal IP address range. To prevent any conflict between the internal IP address range and the external IP addresses it is required to select the internal IP range before the tape library gets connected to the external Ethernet port.

If the already configured internal IP range has a conflict with the network environment the library is connected to, the internal IP range must be reconfigured.

1. After the Reset Internal IP Range menu is entered, this screen appears.
2. Press Enter to start the process to reset the internal IP range. The library will reset and the screen to select the internal IP range appears on the Operator Panel. After a new range is selected, the library finishes the reset and access to the Web GUI is possible again.