Skip to main content

## Move Cartridges

With this action, you can move a cartridge that is located in a source element to an available destination element within the same logical library. A movement

between logical libraries must be confirmed.

- Source Elements - Tape drives, enabled I/O station, and storage slots that contain a tape cartridge
- Destination Elements - Tape drives, enabled I/O station, and storage slots that do not contain a tape cartridge

Tape drives are listed at the top of each element list and listed in the order of their drive numbers. Tape drives are numbered from the physical top of the library starting with Drive (1).
Slots are listed in the order of the slot numbers. Slots are numbered m.s, where m is the module number and s is the slot within the module.

Filtering based on barcode

To see a subset of the cartridges in the library, enter some or all of the barcode label characters in the search area and click Search. The Source Element list updates to display only the cartridges with labels that include the characters in the search box.

To perform a different search or display all of the available cartridges, click Barcode Filter Off.

Moving a cartridge

1. Select the cartridge from Source Elements .
2. Select the destination location from Destination Elements .
3. Click Move.