Skip to main content

## Graphical View

This action shows a graphical representation of the elements, such as slots and tape drives, with information about the cartridge stored in the element.
Unused slots, which are not available for move operations, are greyed out and marked with a cross. Cartridges stored in these slots are displayed in the same way like regular slots.

Warning state and error state for a specific drive or cartridge are indicated with icons.
Expand the module section to see the inventory for that module. Elements containing media are designated with a barcode label. Hover over a cartridge to see information about that cartridge.

Cartridge in Slot:

Cartridge in Drive:

Moving the mouse over drive or cartridge will display additional information:

- Drive - LTO generation of drive and format (Full Height or Half Height)
- Drive # - The drive number
- Serial # - Serial number of the drive
- Slot # - The slot number in the form <module>.<slot>, where module is the module number and slot is the slot number
- Barcode - Barcode data on label
- Generation - LTO generation of cartridge
- Logical Library - The logical library number
- SCSI Element Address - SCSI Address reported to the SCSI Host
- Media Loads - The number of media loads
- Encryption - Indicates whether data on this media is encrypted or not encrypted
- Media Type - Indicates whether this media is a data or a cleaning cartridge