Skip to main content

## Graphical View

To view the elements organized by logical libraries, use the Graphical View action.

The graphical view of the logical library map displays the logical library number for every magazine. Magazine #8, which can be configured as I/O station magazine, displays single slots. When they are configured as I/O station, the slot number gets a leading ‘I/O’.

Moving the mouse over a logical library layer will display additional information:

- Name - Logical library name
- Barcode - Barcode orientation
- Media Removal - Indicates whether media removal is allowed or prevented by the host
- Encryption - Encryption type
- Logical Library S/N - Serial number of the logical library
- Sequential Mode - Indicates whether Sequential Mode is enabled or disabled
- Drive Count - Number of drives in this logical library
- Slot Count - Number of slots in this logical library
- Cartridge Count - Number of cartridges in this logical library
- I/O Station Count - Number of I/O station in this logical library

Moving the mouse over a drive will display additional information such as:

- Drive - LTO generation of drive and format (Full Height or Half Height)
- Drive # - The drive number
- Serial # - Serial number of the drive
- Logical Library - The logical library number

- SCSI Element Address - SCSI Address which is reported to a SCSI Host

If a cartridge is loaded in this drive additional information about the cartridge is displayed such as:

- Barcode - Barcode data on label
- Generation - LTO generation of cartridge
- Logical Library - The logical library number
- Cartridge Loads - Number of loads
- Encryption - Encryption status
- Cartridge Type - Data cartridge, Cleaning Cartridge