Skip to main content

## Modify Port Settings

Use this action to modify the port configuration. This is only available for fibre channel drives.

- Speed — The currently selected speed. The default is Automatic.
- Port Type

- Automatic
- Loop(L) — Enables selection of the Addressing Mode.
- Fabric(N/F)

- Addressing Mode — When Port Type is set to Loop, Addressing Mode can be set to Soft or Hard.
- Loop ID / ALPA — When Addressing Mode is set to Hard, you can choose an ALPA address from the drop-down list.