Skip to main content

## Drive

From the Status > Drive screen you can see the configuration and status of each drive that is installed in the library. Use Up and Down to select a drive from the drive list The drive list already provides the powered status of the drives (On, Off).

The Status > Drive > Drive x screen provides the following status information:

- Vendor
- Personality
- Firmware
- Generation
- Form Factor - HH, FH
- Interface Type - Fibre Channel (FC), SAS
- Manufacturer S/N
- Powered - On, Off
- WWNN
- Temperature
- Logical Library
- Encryption
- Cartridge - Barcode label, N/A if no cartridge loaded
- Module Location
- Cooling Fan Status - Active, Not Active

Fibre Channel Drive: Status for Port 0 and Port 1 (if present)

- WWPN
- Speed
- Port Type
- Port ID or Loop ID / ALPA
- Interface

SAS Drive: Status for Port 0 and Port 1

- WWPN
- Interface
- Speed