Skip to main content

## Move Media

Navigate to Operation > Move Media page.

1. Pressing the Enter button opens the screen for selecting the source type (Cartridge by Barcode, Drives, Slots, I/O Slots).
   The number in brackets provides the amount of full elements for each type.
   After the source type is selected, using Next to navigate to the screen for selecting the source cartridge.
2. Depending on the selected source type, the available cartridges to move are offered in a drop down box.
   After the cartridge is selected, using Next to navigate to the screen for selecting the destination type.

1. On the destination type screen, it is possible to define the type of the destination for the cartridge move.
   Possible options are Empty Drives, Empty Slots or Empty I/O Slots.
   The number in brackets provides the amount of free elements for each type.
   After the source type is selected, using Next to navigate to the screen for selecting the destination.
2. Depending on the selected destination type, the available free elements are offered in a drop down box.
   After the destination is selected, using Submit start the move operation.
3. In case the source and destination are located in two different logical libraries, the move operation need to be confirmed.
4. Once the move operation is started, the source and destination will be shown in a screen until the move is completed.