Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### DBCWK

Prolog

Control Block Contents
DBCWK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### DBCWK Prolog

     NAME       : HCPDBCWK
     DESCRIPTION: DASD Block I/O work block
     DSECT      : DBCWK
     FUNCTION   : Contains information specific to DASD block
                  I/O requests.  It is basically a work area
                  for HCPDBC and it is also now used as the control
                  block to represent the current state of a
                  particular Diagnose 250 or *BLOCKIO (request).
                  (The SNDBK and BRQBK used to fulfill these
                  roles, any fields in those control blocks
                  now reside here).
                  Since a number fields are specific to the particular
                  i/o request, there is an overlay portion of this control
                  block at label DBCSPECL.  The overlays are defined in
                  here and there is an overlay for each type of i/o.
     LOCATED BY : This is pointed to by R13 in all of the
                  block i/o handlers (HCPBIM, HCPBIR, HCPDGB
                  HCPBID, HCPDGD, HCPDBC and HCPDBD).
     CREATED BY : HCPDGB (Diag A4 handling)
                  HCPBIM (*BLOCKIO handling)
                  HCPBID (Diag 250 handling)
                  HCPDGD (Diag 18  handling)
     DELETED BY : HCPDGB (Diag A4 handling)
                  HCPBIM (*BLOCKIO handling)
                  HCPBID or HCPBIR (Diag 250 handling)
                  HCPDGD (Diag 18  handling)
     COMMENTS   : The DBCWK area contains one BPLBK (DBCSINGL) and one
                  IPARML Reply (DBCPARML).  If the size of either of
                  these control blocks changes, then DBCSINGL and
                  DBCPARML should be updated accordingly.

#### DBCWK Control Block Content

#### DBCWK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      DBCWK          DASD Block I/O work block
    0000    0 Dbl-Word     8 DBCIASIT       I-ASIT for the
                                            SBIOP/SBILIST/BPLBK and guest
                                            buffers.
         Work area can be used as a temporary save area by any routine that
         needs to save something temporarily. The general rule of thumb is that
         a value stored in DBCWORK is only used within the subroutine that
         stored it there, any exceptions to this rule are noted in the code.
    0008    8 Dbl-Word     8 DBCWORK (0)    Temporary work area
    0008    8 Signed       4 DBCWORK1       Work word 1
    000C   12 Signed       4 DBCWORK2       Work word 2
    0010   16 Signed       4 DBCWORK3       Work word 3
    0014   20 Signed       4 DBCWORK4       Work word 4
         The following 4 bytes (1 word) are used to hold various processing bits
         common to all types of block i/o.
    0018   24 Bitstring    1 DBCSWTCH       Flags for processing control
              1... ....      DBCGOOD        X'80' At least one good i/o
              .1.. ....      DBCNSTD        X'40' Nonstandard block size
              ..1. ....      DBCNOCAR       X'20' No caching requested
              ...1 ....      DBCWRITE       X'10' Type of I/O 1 for read, 0
                                            for write
              .... 1...      DBCCACC        X'08' Cache access held
              .... .1..      DBCINCAC       X'04' This I/O operation is no
                                            longer eligible for caching
              .... ..1.      DBCARMOD       X'02' In AR Mode
              .... ...1      DBCPRIM        X'01' Parameter list in primary
    0019   25 Bitstring    1 DBCSWTC2       More flags for processing
              1... ....      DBCNOTEL       X'80' Not eligible for cache
              .1.. ....      DBCBLKER       X'40' Found block in error
              ..1. ....      DBCREPLP       X'20' Must replace Parm List
              ...1 ....      DBCCOPYP       X'10' Made copy of Parm list
              .... 1...      DBCASYNC       X'08' Asynchronous blockio
              .... .1..      DBCDG250       X'04' DIAG 250 i/o
              .... ..1.      DBCBLKIO       X'02' *BLOCKIO i/o
              .... ...1      DBCDGA4        X'01' DIAGA4 i/o
         DBCGKEY has key for storage protection checks
    001A   26 Bitstring    1 DBCGKEY        Storage key
    001B   27 Bitstring    1 DBCSWTC4       More processing bits
              1... ....      DBCGLDEL       X'80' All track deletion req.
              .1.. ....      DBCNOREL       X'40' Don't release on read
              ..1. ....      DBCRDCPY       X'20' Read access must copy data
              ...1 ....      DBCARGST       X'10' Guest in AR mode
              .... 1...      DBCSAWWR       X'08' At least 1 write in req.
              .... .1..      DBCWFAIL       X'04' At least 1 write failed
              .... ..1.      DBCXSTOR       X'02' Cache block on XSTOR
              .... ...1      DBCDIDIO       X'01' Did I/O for this request
    001C   28 Signed       4 DBCSAV         original SAVBK address
         The DBCHALET is used for the block list control block for the
         particular type of block i/o request.
    0020   32 Signed       4 DBCHALET       ALET for guest space (CP)
    0024   36 Signed       4 DBCEALET       Guest version of ALET.
    0028   40 Signed       4 DBCERET        Return address save
    002C   44 Signed       4 DBCERET2       2'nd level return address save
    0030   48 Signed       4 DBCDPSBK       DPSBK Address
    0034   52 Signed       4 DBCANCHR       BIOPG page list anchor
         The following fields used to be in a separate control block called a
         DVCPL. They are now placed here to avoid having to load up its address
         all the time.
    0038   56 Signed       4 DBCHFRST       Beginning of DVIENTRY linked list
    003C   60 Signed       4 DBCHLAST       End of DVIENTRY linked list
    0040   64 Address      4 DBCOPPTR       Beginning of DVIOP linked list
    0044   68 Signed       4 DBCTFRST       DVTRK (tracks accessed) list
    0048   72 Address      4 DBCLCKAD       Address of lock word
    004C   76 Signed       4 DBCMAXCH       Max channel program size
    0050   80 Signed       4 DBCKEY         Key save area
    0054   84 Signed       4 DBCBKNUM       Block number save area
    0058   88 Signed       4 DBCDVC         DBC/DBE - ptr to DVIENTRY DGB/DGD
                                            - ptr to DVIOP
    005C   92 Signed       4 DBCTKPTR       Pointer to previous DVTRK
    0060   96 Signed       4 DBCRTRAK       Relative track save area
    0064  100 Signed       4 DBCTCHBK       Last Read TCHBK Addr
    0068  104 Signed       4 DBCMXENT       Max entry count
    006C  108 Signed       4 DBCERRAD       Address where a host storage
                                            error occurred on parameter list.
         The following fields are the CDATA word and the DPSBK information from
         the currently-in-use track, by that we mean that it is the one we will
         next try to copy data to/from.
    0070  112 Signed       4 DBCTKDAT (0)   Data for current track
    0070  112 Signed       4 DBCCDATA (0)   TCHBK save
    0070  112 Signed       2 DBCVCYL        Virtual cylinder
    0072  114 Bitstring    1 DBCFSTRN       First record number
    0073  115 Bitstring    1 DBCLOWRN       Low record number
    0074  116 Signed       4 * (0)
    0074  116 Bitstring    1 *              Reserved for IBM use
    0075  117 Bitstring    3 DBCDPSTF (0)   DPSBK stuff we care about
    0075  117 Bitstring    1 DBCHIRN        Highest record number
    0076  118 Signed       2 DBCTKSIZ       Blocksize of track
              00000002       DBCTKLEN       (*-DBCTKDAT+3)/4 Size in words of
                                            track data
         The following field is the read copy of the data. We only have 1 read
         track accessed at any given time, yet for *BLOCKIO and DIAG 250 we may
         have mixed reads and writes. So if we get write access to a track, then
         we copy the read data to this temporary save area. Then, if we later
         read from the current read track, then we can just copy the data back
         instead of going through a re-access of the track.
    0078  120 Signed       4 DBCRDSAV (2)   Read save area
    0080  128 Signed       4 DBCBLKCT       Remember block count
    0084  132 Signed       4 DBCRC          Return code save area
    0088  136 Signed       2 DBCBLKSZ       Block size
    008A  138 Signed       2 DBCHSID        Hash id for cache
    008C  140 Signed       2 DBCOFSET       OFFSET into track
    008E  142 Signed       2 DBCDBICT       Count of DBIRQ blocks sent to
                                            HCPIOS
    0090  144 Signed       4 DBCDVIAD       Pointer to next DVIOP to schedule
                                            for these i/o oper.
    0094  148 Address      4 DBCNEXT        Pointer to next DBCWK for this
                                            virtual device
    0098  152 Signed       4 DBCRELRT       Release return address
    009C  156 Signed       4 DBCMALET       ALET FOR MDC address space for
                                            last track accessed
    00A0  160 Signed       4 * (0)
    00A0  160 Bitstring    1 DBCSWTC5       More processing bits
              1... ....      DBCDG18        X'80' Processing a Diag X'18'
    00A1  161 Bitstring    1 *              Reserved for IBM use
    00A2  162 Signed       2 *              Reserved for IBM use
    00A4  164 Signed       4 *              Reserved for IBM use
    00A8  168 Dbl-Word     8 DBCSPECL (0)
    00A8  168 Dbl-Word     8 * (10)         Overlay area, note that this
                                            leaves room for service.
              0000001F       DBCWKLEN       (*-DBCWK+7)/8 Size in double
                                            words
         DIAGNOSE 18 Specific fields Are overlayed at label DBCSPECL.
    00A8  168 Dbl-Word     8 DBCSVCCW       Host copy of CCW
         DBCARGSV has BBCCHH of first SEEK in CCW program and the relocated CC
         address for the minidisk.
    00B0  176 Dbl-Word     8 DBCARGSV (0)   First SEEK arguments
    00B0  176 Signed       2 DBCARGBB       BB portion of seek
    00B2  178 Signed       2 DBCARGCC       CC portion of seek
    00B4  180 Signed       2 DBCARGHH       HH portion of seek
    00B6  182 Signed       2 DBCCYLSV       Relocated CC of seek
         DBCNXTSV has BBCCHH of latest SEEK in CCW program
    00B8  184 Dbl-Word     8 DBCNXTSV (0)   Latest SEEK arguments
    00B8  184 Signed       2 DBCNXTBB       BB portion of seek
    00BA  186 Signed       2 DBCNXTCC       CC portion of seek
    00BC  188 Signed       2 DBCNXTHH       HH portion of seek
    00BE  190 Signed       2 *              Reserved for IBM use
         DBCORIEN has the latest record orientation information in it. It has
         the CCHHR of the last record that we read from the cache.
    00C0  192 Bitstring    5 DBCORIEN (0)   Latest SIDE arguments
    00C0  192 Signed       2 DBCORICC       CC of SIDE
    00C2  194 Signed       2 DBCORIHH       HH of SIDE
    00C4  196 Bitstring    1 DBCORIR        R of SIDE
    00C5  197 Bitstring    1 DBC18SWT       More flags
              1... ....      DBCFIRST       X'80' Working on first CCW
              .1.. ....      DBCBUSYV       X'40' Made the VDEV busy
              ..1. ....      DBCSILI        X'20' SILI bit on
              ...1 ....      DBCMIXED       X'10' Mixed blocksizes found
              .... 1...      DBCREMOV       X'08' Can remove DVIENTRYs
              .... .1..      DBCSTD         X'04' Track is standard
              .... ..1.      DBCEOT         X'02' Reached End of Track
    00C6  198 Signed       2 DBCMAXSZ       Max block size found
    00C8  200 Signed       4 DBCIORAD       IORBK save address
    00CC  204 Signed       4 DBCGCCW        Guest CCW Address
    00D0  208 Signed       4 DBCCCWCT       CCW count
    00D4  212 Signed       4 DBCCYLTK       Relative track for cyl
    00D8  216 Signed       4 DBCSEKPT       Last SearchID DVIENTRY
    00DC  220 Signed       4 DBCCPSPT       Last C.P.S. Pointer
    00E0  224 Signed       4 DBCTKHED       Track pointer
    00E4  228 Signed       4 DBC18RC        Diag 18 return code
    00E8  232 Signed       4 * (4)          Reserved for IBM use
         DIAGNOSE A4 Specific fields Are overlayed at label DBCSPECL.
    00A8  168 Bitstring    1 DBCA4SWT       More flags
              1... ....      DBCVDEV        X'80' Got the VDEV lock to be
                                            copied back to guest storage.
              .1.. ....      DBCBUSY        X'40' We turned on VDEVBUSY
              ..1. ....      DBCREPS        X'20' SBIOP must be replaced on
                                            exit
              .... 1...      DBCINIOR       X'08' Initialized IORBK
              .... .1..      DBCCOPYS       X'04' SBIOP was copied to host
                                            stor
              .... ..1.      DBCQDSK        X'02' Have Vdisk I/O lock
              .... ...1      DBCBKOUT       X'01' End-user breakout enabled
    00A9  169 Bitstring    1 DBCARNUM       ARx access register
    00AA  170 Bitstring    1 DBCLPM         Guest LPM
    00AB  171 Bitstring    1 *              Reserved for IBM use
    00AC  172 Signed       4 DBCAR9         Save for current ALET
    00B0  176 Signed       4 DBCPROG        Prog check operand
    00B4  180 Signed       4 DBCIORBK       IORBK save address
    00B8  184 Signed       4 DBCBLKPR       Blocks processed
    00BC  188 Signed       4 DBCSBIOP       Address of SBIOP
    00C0  192 Signed       4 DBCGADDR       Guest addr of SBIOP
    00C4  196 Signed       4 *              Reserved for IBM use
    00C8  200 Signed       4 DBCGLIST       SBILIST guest address
    00CC  204 Signed       4 * (11)         Reserved for IBM use
         DIAGNOSE 250 Specific fields are overlayed at label DBCSPECL.
         The following is an address space buffer. It holds the latest address
         space info on a guest buffer specified in the BELBK entry. I.E. It
         holds the latest BELBALET and the associated things that we care about.
         A non-zero entry indicates that we have access to the data space
         containing the buffer. A zero entry means that there is no address
         space attached for a given BELBK entry.
    00A8  168 Dbl-Word     8 DBCBASIT       BELBK I-asit Address
    00B0  176 Signed       4 DBCBKIBK       BKIBK address
    00B4  180 Address      4 DBCHALBK       Address of the host-ART
                                            .lookaside block .containing the
                                            ALET/i-ASIT .pairs associated
                                            with .the data buffers in the
                                            .BELBK entries.
    00B8  184 Bitstring    1 DBCDOPER       Operation field for the DIAG
                                            X'250' request
              1... ....      DBCABSET       X'80' Abort exit was established
              .1.. ....      DBCABORT       X'40' Abort exit was driven
              ..1. ....      DBCASYRQ       X'20' Guest requested
                                            asynchronous processing.
              ...1 ....      DBCBYPAS       X'10' Guest requested that we
                                            bypass minidisk cache
              .... 1...      DBCBELST       X'08' The BELBK could not be
                                            stored for the completion of an
                                            asynchronous request.
    00B9  185 Bitstring    1 DBCFLAGS       More processing flags
              1... ....      DBCBELGT       X'80' Used GETST to get BELBK
              .1.. ....      DBCGTHAL       X'40' Used GETST to get HALBK
    00BA  186 Bitstring    1 DBC250RC       Return code for request
                                            processing
              .... ....      DBCRC00        X'00' A synchronous request was
                                            successful (either scheduled and
                                            completed, or from cache) or an
                                            asynchronous request was
                                            successfully satisfied from
                                            cache.
              .... 1...      DBCRC08        X'08' An asynchronous request was
                                            initiated (all or part of the I/O
                                            was scheduled).
              .... 11..      DBCRC12        X'0C' A request was partially
                                            successful. If asynchronous, part
                                            of the request was satisfied from
                                            cache, but an error occurred
                                            preventing the entire request
                                            from completing successfully.
              ..1. 1...      DBCRC40        X'28' All of the BELBK entries
                                            were in error, or all DVIOPs were
                                            in error.
              ..1. 11..      DBCRC44        X'2C' Remove or reset terminated
                                            a synchronous request.
              ..11 ....      DBCRC48        X'30' A synchronous request was
                                            terminated by the user (the abort
                                            exit was driven).
              1111 1111      DBCRC255       X'FF' A catastrophic error (abend
                                            condition) occurred. Some I/O may
                                            have been scheduled or done.
    00BB  187 Bitstring    1 *              Reserved for IBM use
    00BC  188 Signed       2 DBCBELCT       Number of entries in the block
                                            .I/O entry list
    00BE  190 Signed       2 *              Reserved for IBM use
    00C0  192 Address      4 DBCBELBK       Address of the block I/O .entry
                                            list in host .storage.
    00C4  196 Address      4 DBCGBELA       Address of the block I/O .entry
                                            list in guest .storage.
    00C8  200 Signed       4 DBCIPARM       Interruption parameter, if this
                                            .is an asynchronous request.
    00CC  204 Signed       4 DBCOFFCP       Offset for block number - .this
                                            is a copy of BKIOFFCP
    00D0  208 Signed       4 * (10)         Reserved for IBM use
         **BLOCKIO Specific fields are overlayed at label DBCSPECL.
         DBCSINGL contains a BPLBK, so any changes to the BPLBK size affect this
         field. NOTES : Currently the BPLBK is 4F, but the last 1F is unused, so
         using 3F for DBCSINGL works (and is all we can fit in DBCSPECL at this
         time).
    00A8  168 Signed       4 DBCSINGL (3)   Storage for a single block I/O
                                            version of the multiple block I/O
                                            parameter list Mapped by HCPBPLBK
    00B4  180 Signed       4 DBCBLKAD       BLKIO address
    00B8  184 Bitstring    1 DBCBOPER       Operation field for SEND Request
              1... ....      DBCMONO        X'80' Indicate Single BLK SEND
                                            REQ Protocol
              .1.. ....      DBCMULTI       X'40' Indicate Multi BLK SEND REQ
                                            Protocol
              ..1. ....      DBCIWAIT       X'20' Indicate waiting for I/O
                                            interrupts
              ...1 ....      DBCSYNC        X'10' Guest request is
                                            synchronous
              .... 1...      DBCGOTBL       X'08' got storage for blockio
                                            list
              .... .1..      DBCSEXIT       X'04' Exitted to caller already
                                            DBCBLKRC codes are defined in
                                            HCPBIM
    00B9  185 Bitstring    1 DBCBLKRC       IUCV Reply Return Code
    00BA  186 Signed       2 DBCSSHCT       Number of real SSCH issued to
                                            handle this send request.
    00BC  188 Signed       4 DBCMSGID       IUCV message id
    00C0  192 Signed       4 DBCTRGCL (0)   IUCV target class
    00C0  192 Bitstring    3 *              ...IUCV target class
    00C3  195 Bitstring    1 DBCBLKRQ       Blockio service request
              1... ....      DBCBLKNC       X'80' Bypass MDC processing
              .... ..11      DBCBLKMB       X'03' Multi-block request
              .... ..1.      DBCBLKRD       X'02' Single block read
              .... ...1      DBCBLKWR       X'01' Single block write
    00C4  196 Address      4 DBCPLADR       Address of the multiple block
                                            parameter list in host real
                                            storage
    00C8  200 Signed       4 DBCGPLST       Guest address of the multiple
                                            block
         DBCPARML houses an IPARML, so any changes to the IPARML size affect
         this field.
    00CC  204 Bitstring   40 DBCPARML       IUCV reply parameter list
              00FFFF7C       DBCTCMSK       X'FFFFFFFF'-(DBCBLKNC+DBCBLKMB)
                                            Mask to validate DBCTRGCL (IUCV
                                            target class)
    00F4  244 Signed       2 DBCPLCNT       Count of elements in the multiple
                                            block parameter list
    00F6  246 Signed       2 DBCPLSIZ       Size of the multiple block
                                            parameter list in bytes

#### DBCWK Storage Layout

    *** DBCWK - DASD Block I/O work block
    *
    *     +-------------------------------------------------------+
    *   0 |                       DBCIASIT                        |
    *     +---------------------------+---------------------------+
    *   8 |         DBCWORK1          |         DBCWORK2          |
    *     +---------------------------+---------------------------+
    *  10 |         DBCWORK3          |         DBCWORK4          |
    *     +------+------+------+------+---------------------------+
    *  18 |:SWTCH|:SWTC2|:GKEY |:SWTC4|          DBCSAV           |
    *     +------+------+------+------+---------------------------+
    *  20 |         DBCHALET          |         DBCEALET          |
    *     +---------------------------+---------------------------+
    *  28 |         DBCERET           |         DBCERET2          |
    *     +---------------------------+---------------------------+
    *  30 |         DBCDPSBK          |         DBCANCHR          |
    *     +---------------------------+---------------------------+
    *  38 |         DBCHFRST          |         DBCHLAST          |
    *     +---------------------------+---------------------------+
    *  40 |         DBCOPPTR          |         DBCTFRST          |
    *     +---------------------------+---------------------------+
    *  48 |         DBCLCKAD          |         DBCMAXCH          |
    *     +---------------------------+---------------------------+
    *  50 |          DBCKEY           |         DBCBKNUM          |
    *     +---------------------------+---------------------------+
    *  58 |          DBCDVC           |         DBCTKPTR          |
    *     +---------------------------+---------------------------+
    *  60 |         DBCRTRAK          |         DBCTCHBK          |
    *     +---------------------------+---------------------------+
    *  68 |         DBCMXENT          |         DBCERRAD          |
    *     +-------------+------+------+------+------+-------------+
    *  70 |  DBCVCYL    |:FSTRN|:LOWRN|//////|:HIRN |  DBCTKSIZ   |
    *     +-------------+------+------+------+------+-------------+
    *  78 |                       DBCRDSAV                        |
    *     +---------------------------+---------------------------+
    *  80 |         DBCBLKCT          |          DBCRC            |
    *     +-------------+-------------+-------------+-------------+
    *  88 |  DBCBLKSZ   |  DBCHSID    |  DBCOFSET   |  DBCDBICT   |
    *     +-------------+-------------+-------------+-------------+
    *  90 |         DBCDVIAD          |         DBCNEXT           |
    *     +---------------------------+---------------------------+
    *  98 |         DBCRELRT          |         DBCMALET          |
    *     +------+------+-------------+---------------------------+
    *  A0 |:SWTC5|//////|/////////////|///////////////////////////|
    *     +------+------+-------------+---------------------------+
    *  A8 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  F8
    *
    *** DBCWK - DASD Block I/O work block

    *** Overlay for DBCSPECL in DBCWK
    *
    *     +-------------------------------------------------------+
    *  A8 |                       DBCSVCCW                        |
    *     +-------------+-------------+-------------+-------------+
    *  B0 |  DBCARGBB   |  DBCARGCC   |  DBCARGHH   |  DBCCYLSV   |
    *     +-------------+-------------+-------------+-------------+
    *  B8 |  DBCNXTBB   |  DBCNXTCC   |  DBCNXTHH   |/////////////|
    *     +-------------+-------------+------+------+-------------+
    *  C0 |  DBCORICC   |  DBCORIHH   |:ORIR |:18SWT|  DBCMAXSZ   |
    *     +-------------+-------------+------+------+-------------+
    *  C8 |         DBCIORAD          |         DBCGCCW           |
    *     +---------------------------+---------------------------+
    *  D0 |         DBCCCWCT          |         DBCCYLTK          |
    *     +---------------------------+---------------------------+
    *  D8 |         DBCSEKPT          |         DBCCPSPT          |
    *     +---------------------------+---------------------------+
    *  E0 |         DBCTKHED          |         DBC18RC           |
    *     +---------------------------+---------------------------+
    *  E8 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  F8
    *
    *** Overlay for DBCSPECL in DBCWK

    *** Overlay for DBCSPECL in DBCWK
    *
    *     +------+------+------+------+---------------------------+
    *  A8 |:A4SWT|:ARNUM|DBCLPM|//////|          DBCAR9           |
    *     +------+------+------+------+---------------------------+
    *  B0 |         DBCPROG           |         DBCIORBK          |
    *     +---------------------------+---------------------------+
    *  B8 |         DBCBLKPR          |         DBCSBIOP          |
    *     +---------------------------+---------------------------+
    *  C0 |         DBCGADDR          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  C8 |         DBCGLIST          |///////////////////////////|
    *     +---------------------------+///////////////////////////|
    *  D0 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  F8
    *
    *** Overlay for DBCSPECL in DBCWK

    *** Overlay for DBCSPECL in DBCWK
    *
    *     +-------------------------------------------------------+
    *  A8 |                       DBCBASIT                        |
    *     +---------------------------+---------------------------+
    *  B0 |         DBCBKIBK          |         DBCHALBK          |
    *     +------+------+------+------+-------------+-------------+
    *  B8 |:DOPER|:FLAGS|:250RC|//////|  DBCBELCT   |/////////////|
    *     +------+------+------+------+-------------+-------------+
    *  C0 |         DBCBELBK          |         DBCGBELA          |
    *     +---------------------------+---------------------------+
    *  C8 |         DBCIPARM          |         DBCOFFCP          |
    *     +---------------------------+---------------------------+
    *  D0 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  F8
    *
    *** Overlay for DBCSPECL in DBCWK

    *** Overlay for DBCSPECL in DBCWK
    *
    *     +-------------------------------------------------------+
    *  A8 |                       DBCSINGL                        |
    *     |                           +---------------------------+
    *  B0 |                           |         DBCBLKAD          |
    *     +------+------+-------------+---------------------------+
    *  B8 |:BOPER|:BLKRC|  DBCSSHCT   |         DBCMSGID          |
    *     +------+------+------+------+---------------------------+
    *  C0 |////////////////////|:BLKRQ|         DBCPLADR          |
    *     +--------------------+------+---------------------------+
    *  C8 |         DBCGPLST          |                           |
    *     +---------------------------+                           |
    *  D0 |                                                       |
    *     =                       DBCPARML                        =
    *     |                           +-------------+-------------+
    *  F0 |                           |  DBCPLCNT   |  DBCPLSIZ   |
    *     +---------------------------+-------------+-------------+
    *  F8
    *
    *** Overlay for DBCSPECL in DBCWK

#### DBCWK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    DBCABORT       00B8 40
    DBCABSET       00B8 80
    DBCANCHR       0034
    DBCARGBB       00B0
    DBCARGCC       00B2
    DBCARGHH       00B4
    DBCARGST       001B 10
    DBCARGSV       00B0
    DBCARMOD       0018 02
    DBCARNUM       00A9
    DBCAR9         00AC
    DBCASYNC       0019 08
    DBCASYRQ       00B8 20
    DBCA4SWT       00A8
    DBCBASIT       00A8
    DBCBELBK       00C0
    DBCBELCT       00BC
    DBCBELGT       00B9 80
    DBCBELST       00B8 08
    DBCBKIBK       00B0
    DBCBKNUM       0054
    DBCBKOUT       00A8 01
    DBCBLKAD       00B4
    DBCBLKCT       0080
    DBCBLKER       0019 40
    DBCBLKIO       0019 02
    DBCBLKMB       00C3 03
    DBCBLKNC       00C3 80
    DBCBLKPR       00B8
    DBCBLKRC       00B9
    DBCBLKRD       00C3 02
    DBCBLKRQ       00C3
    DBCBLKSZ       0088
    DBCBLKWR       00C3 01
    DBCBOPER       00B8
    DBCBUSY        00A8 40
    DBCBUSYV       00C5 40
    DBCBYPAS       00B8 10
    DBCCACC        0018 08
    DBCCCWCT       00D0
    DBCCDATA       0070
    DBCCOPYP       0019 10
    DBCCOPYS       00A8 04
    DBCCPSPT       00DC
    DBCCYLSV       00B6
    DBCCYLTK       00D4
    DBCDBICT       008E
    DBCDGA4        0019 01
    DBCDG18        00A0 80
    DBCDG250       0019 04
    DBCDIDIO       001B 01
    DBCDOPER       00B8
    DBCDPSBK       0030
    DBCDPSTF       0075
    DBCDVC         0058
    DBCDVIAD       0090
    DBCEALET       0024
    DBCEOT         00C5 02
    DBCERET        0028
    DBCERET2       002C
    DBCERRAD       006C
    DBCFIRST       00C5 80
    DBCFLAGS       00B9
    DBCFSTRN       0072
    DBCGADDR       00C0
    DBCGBELA       00C4
    DBCGCCW        00CC
    DBCGKEY        001A
    DBCGLDEL       001B 80
    DBCGLIST       00C8
    DBCGOOD        0018 80
    DBCGOTBL       00B8 08
    DBCGPLST       00C8
    DBCGTHAL       00B9 40
    DBCHALBK       00B4
    DBCHALET       0020
    DBCHFRST       0038
    DBCHIRN        0075
    DBCHLAST       003C
    DBCHSID        008A
    DBCIASIT       0000
    DBCINCAC       0018 04
    DBCINIOR       00A8 08
    DBCIORAD       00C8
    DBCIORBK       00B4
    DBCIPARM       00C8
    DBCIWAIT       00B8 20
    DBCKEY         0050
    DBCLCKAD       0048
    DBCLOWRN       0073
    DBCLPM         00AA
    DBCMALET       009C
    DBCMAXCH       004C
    DBCMAXSZ       00C6
    DBCMIXED       00C5 10
    DBCMONO        00B8 80
    DBCMSGID       00BC
    DBCMULTI       00B8 40
    DBCMXENT       0068
    DBCNEXT        0094
    DBCNOCAR       0018 20
    DBCNOREL       001B 40
    DBCNOTEL       0019 80
    DBCNSTD        0018 40
    DBCNXTBB       00B8
    DBCNXTCC       00BA
    DBCNXTHH       00BC
    DBCNXTSV       00B8
    DBCOFFCP       00CC
    DBCOFSET       008C
    DBCOPPTR       0040
    DBCORICC       00C0
    DBCORIEN       00C0
    DBCORIHH       00C2
    DBCORIR        00C4
    DBCPARML       00CC
    DBCPLADR       00C4
    DBCPLCNT       00F4
    DBCPLSIZ       00F6
    DBCPRIM        0018 01
    DBCPROG        00B0
    DBCQDSK        00A8 02
    DBCRC          0084
    DBCRC00        00BA 00
    DBCRC08        00BA 08
    DBCRC12        00BA 0C
    DBCRC255       00BA FF
    DBCRC40        00BA 28
    DBCRC44        00BA 2C
    DBCRC48        00BA 30
    DBCRDCPY       001B 20
    DBCRDSAV       0078
    DBCRELRT       0098
    DBCREMOV       00C5 08
    DBCREPLP       0019 20
    DBCREPS        00A8 20
    DBCRTRAK       0060
    DBCSAV         001C
    DBCSAWWR       001B 08
    DBCSBIOP       00BC
    DBCSEKPT       00D8
    DBCSEXIT       00B8 04
    DBCSILI        00C5 20
    DBCSINGL       00A8
    DBCSPECL       00A8
    DBCSSHCT       00BA
    DBCSTD         00C5 04
    DBCSVCCW       00A8
    DBCSWTCH       0018
    DBCSWTC2       0019
    DBCSWTC4       001B
    DBCSWTC5       00A0
    DBCSYNC        00B8 10
    DBCTCHBK       0064
    DBCTCMSK       00CC 00FFFF7C
    DBCTFRST       0044
    DBCTKDAT       0070
    DBCTKHED       00E0
    DBCTKLEN       0076 00000002
    DBCTKPTR       005C
    DBCTKSIZ       0076
    DBCTRGCL       00C0
    DBCVCYL        0070
    DBCVDEV        00A8 80
    DBCWFAIL       001B 04
    DBCWKLEN       00A8 0000001F
    DBCWORK        0008
    DBCWORK1       0008
    DBCWORK2       000C
    DBCWORK3       0010
    DBCWORK4       0014
    DBCWRITE       0018 10
    DBCXSTOR       001B 02
    DBC18RC        00E4
    DBC18SWT       00C5
    DBC250RC       00BA

This information is based on z/VM V4R3.0. Last updated on 30 Apr 2002 at 16:00:33 EDT.
Copyright IBM Corporation, 1990, 2002