Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### XCRBK

Prolog

Control Block Contents
XCRBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### XCRBK Prolog

     Name       : HCPXCRBK
     Description: CP Exit Call Request Block
     DSECT      : XCRBK
     COPYRIGHT -
                  THIS MODULE IS "RESTRICTED MATERIALS OF IBM"
                  5654-A17 (C) COPYRIGHT IBM CORP. - 1995, 2001
                  LICENSED MATERIALS - PROPERTY OF IBM
     Function   : This control block contains information used to
                  authorize user exit routines to find their entry
                  points.
     Located by : XITBK.XITXCRBK
                  XCRBK.XCRFWD
     Created by : HCPZIX
     Deleted by : HCPZIX
     References : HCPICRBK - Indirect Call Request Block

#### XCRBK Control Block Content

#### XCRBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      XCRBK          CP Exit Call Request Block
         These fields map the Indirect Call Request Block. These fields must
         match the analogous fields in the ICRBK. The fields are defined
         explicitly here in order that BLOCKDEF can correctly describe them.
         CKMAINT is used in the hope that an assembly error will alert one to
         any possible inconsistencies between the definitions here and the ICRBK
         definitions.
    0000    0 Dbl-Word     8 XCRICRBK (0)   ICRBK fields
    0000    0 Character    8 XCREPNAM       Name of exit routine ep
    0008    8 Address      4 XCRADDRL       Address of the ICLBK, or 0.
    000C   12 Bitstring    1 XCRATTR        Attributes for call
              .1.. ....      ICRRLONG       X'40' Caller is LONGREG
              ..1. ....      ICRELONG       X'20' Callee is LONGREG
              ...1 ....      ICRESTA        X'10' callee uses static savearea
              .... 1...      ICRRMP         X'08' caller MP capable
              .... .1..      ICRERES        X'04' callee Resident
              .... ..1.      ICREMP         X'02' callee MP capable
              .... ...1      ICRTRC         X'01' issue TRACE instruction
    000D   13 Bitstring    1 *              Reserved
    000E   14 Bitstring    1 *              Reserved
    000F   15 Bitstring    1 *              Reserved
         Thus ends the Indirect Call Request Block fields
    0010   16 Dbl-Word     8 XCRUSRD1       Reserved for non-IBM use
    0018   24 Dbl-Word     8 XCRUSRD2       Reserved for non-IBM use
    0020   32 Signed       4 XCRUSRF1       Reserved for non-IBM use
    0024   36 Signed       4 XCRUSRF2       Reserved for non-IBM use
    0028   40 Signed       2 XCRUSRH1       Reserved for non-IBM use
    002A   42 Signed       2 XCRUSRH2       Reserved for non-IBM use
    002C   44 Bitstring    1 XCRUSRX1       Reserved for non-IBM use
    002D   45 Bitstring    1 XCRUSRX2       Reserved for non-IBM use
    002E   46 Bitstring    1 XCRUSRX3       Reserved for non-IBM use
    002F   47 Bitstring    1 XCRUSRX4       Reserved for non-IBM use
    0030   48 Address      4 XCRFWD         Address of next XCRBK
    0034   52 Signed       4 XCRATMPT       Count of attempts to call this
                                            routine
    0038   56 Signed       4 XCRCALLS       Count of calls to this exit
    003C   60 Signed       4 *              Reserved
    0040   64 Dbl-Word     8 XCRMSACT       Time (in micro-seconds) that .
                                            this routine was active.
    0048   72 Dbl-Word     8 XCR$END (0)    The end

#### XCRBK Storage Layout

    *** XCRBK - CP Exit Call Request Block
    *
    *     +-------------------------------------------------------+
    *   0 |                       XCREPNAM                        |
    *     +---------------------------+------+------+------+------+
    *   8 |         XCRADDRL          |:ATTR |//////|//////|//////|
    *     +---------------------------+------+------+------+------+
    *  10 |                       XCRUSRD1                        |
    *     +-------------------------------------------------------+
    *  18 |                       XCRUSRD2                        |
    *     +---------------------------+---------------------------+
    *  20 |         XCRUSRF1          |         XCRUSRF2          |
    *     +-------------+-------------+------+------+------+------+
    *  28 |  XCRUSRH1   |  XCRUSRH2   |:USRX1|:USRX2|:USRX3|:USRX4|
    *     +-------------+-------------+------+------+------+------+
    *  30 |          XCRFWD           |         XCRATMPT          |
    *     +---------------------------+---------------------------+
    *  38 |         XCRCALLS          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  40 |                       XCRMSACT                        |
    *     +-------------------------------------------------------+
    *
    *** XCRBK - CP Exit Call Request Block

#### XCRBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    ICRELONG       000C 20
    ICREMP         000C 02
    ICRERES        000C 04
    ICRESTA        000C 10
    ICRRLONG       000C 40
    ICRRMP         000C 08
    ICRTRC         000C 01
    XCR$END        0048
    XCRADDRL       0008
    XCRATMPT       0034
    XCRATTR        000C
    XCRCALLS       0038
    XCREPNAM       0000
    XCRFWD         0030
    XCRICRBK       0000
    XCRMSACT       0040
    XCRUSRD1       0010
    XCRUSRD2       0018
    XCRUSRF1       0020
    XCRUSRF2       0024
    XCRUSRH1       0028
    XCRUSRH2       002A
    XCRUSRX1       002C
    XCRUSRX2       002D
    XCRUSRX3       002E
    XCRUSRX4       002F

This information is based on z/VM V4R3.0. Last updated on 30 Apr 2002 at 18:33:11 EDT.
Copyright IBM Corporation, 1990, 2002