Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### T64LB

Prolog

Control Block Contents
T64LB DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### T64LB Prolog

     NAME       : HCPFCWDS
     DESCRIPTION: TLB64 Entry (64 bit addresses)
     DSECT      : T64LB

#### T64LB Control Block Content

#### T64LB DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      T64LB          TLB64 Entry (64 bit addresses)
    0000    0 Address      4 T64LBNXT       Address of next TLB entry
    0004    4 Address      4 T64LBHST       Host frame address
    0008    8 Bitstring    8 T64GSTAD (0)   64 bit address
    0008    8 Address      4 T64LBGHI       High order word for 64 bit guest
                                            .address
    000C   12 Address      4 T64LBGLO       Low order word guest addr
              00000010       T64LBSZE       *-T64LB

#### T64LB Storage Layout

    *** T64LB - TLB64 Entry (64 bit addresses)
    *
    *     +---------------------------+---------------------------+
    *   0 |         T64LBNXT          |         T64LBHST          |
    *     +---------------------------+---------------------------+
    *   8 |         T64LBGHI          |         T64LBGLO          |
    *     +---------------------------+---------------------------+
    *  10
    *
    *** T64LB - TLB64 Entry (64 bit addresses)

#### T64LB Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    T64GSTAD       0008
    T64LBGHI       0008
    T64LBGLO       000C
    T64LBHST       0004
    T64LBNXT       0000
    T64LBSZE       000C 00000010

This information is based on z/VM V4R3.0. Last updated on 1 May 2002 at 08:41:01 EDT.
Copyright IBM Corporation, 1990, 2002