Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### TRPBK

Prolog

Control Block Contents
TRPBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### TRPBK Prolog

     NAME       : HCPTRPBK
     DESCRIPTION: TRACE TRAP BLOCK
     DSECT      : TRPBK
     FUNCTION   : HCPTRPBK CONTAINS ALL DESCRIPTIVE INFORMATION ABOUT A
                  PARTICULAR TRACE TRAP CURRENTLY DEFINED BY THE TRACE
                  COMMAND.
     LOCATED BY : TRPNEXT   CHAINED
                  TRSANCHR  FIELD OF HCPTRSBK
     CREATED BY : HCPTRIP
     DELETED BY : HCPTRICL, HCPTRITD, HCPTRIX
     SERIALIZED : CREATED AND DELETED UNDER CONSOLE FUNCTION MODE,
                  READ UNDER VMDBK DISPATCH LOCK.

#### TRPBK Control Block Content

#### TRPBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      TRPBK          TRACE TRAP BLOCK
    0000    0 Address      4 TRPNEXT        POINTER TO NEXT TRAP BLOCK IN
                                            LIST
    0004    4 Signed       4 TRPIDENT       FOUR CHARACTER TRAP IDENTIFIER
    0008    8 Signed       2 TRPSKIP        COUNT REMAINING IN CURRENT SKIP
                                            COUNT
    000A   10 Signed       2 TRPSTOP        DISPLAYS REMAINING UNTIL CONSOLE
                                            STOP
    000C   12 Signed       2 TRPPASS        PASS COUNT (REFRESHES TRPPASS IF
                                            PRESENT)
    000E   14 Signed       2 TRPSTEP        STEP COUNT
    0010   16 Address      4 TRPCPNXT       POINTER TO NEXT CP COMMAND IN
                                            CHAIN
    0014   20 Address      4 TRPCPCMD       POINTER TO THIS CP COMMAND
         Notes : HCPTRR and HCPTGR contain DSECTS for TRPINEXT followed by
         TRPIRNG. TRPINEXT and TRPIRNG must be on doubleword boundaries for the
         code to work correctly.
    0018   24 Address      4 TRPINEXT       POINTER TO NEXT RANGE AFTER THIS
                                            IRANGE.
    001C   28 Signed       4 *              Reserved
    0020   32 Dbl-Word     8 TRPIRNG (2)    Instruction fetch (ifetch) range
         NOTES : The following 3 fields must remain in this order so they can be
         passed as input to the PUTADSP or FMTADSP subroutines in HCPCQE via one
         register as follows: GPR 7 = 31-BIT POINTER to address space info: R7
         -> DOUBLEWORD ASCE (TRPIASCE) FULLWORD STO (TRPISTO ) HALFWORD ASN
         (TRPIASN )
    0030   48 Dbl-Word     8 TRPIASCE       ASCE for address space of ifetch
                                            addr
    0038   56 Signed       4 TRPISTO        SEGMENT TABLE ORIGN FOR ADDRESS
                                            SPACE OF IFETCH ADDRESS
                                            'FFFFFFFE': INDICATE LOGICAL
                                            ADDRESS
    003C   60 Signed       2 TRPIASN        Address Space Number for address
                                            space of IFETCH range. This field
                                            is only valid when the TRPIASNF
                                            bit is on.
    003E   62 Bitstring    1 * (2)          Reserved
    0040   64 Signed       2 TRPDBW         NUMBER OF DOUBLEWORDS IN THIS
                                            BLOCK
    0042   66 Bitstring    1 TRPCNTRL       TRACING SCREENING/OUTPUT CONTROL
              1... ....      TRPPROB        X'80' RESTRICT TO PROBLEM MODE
                                            ONLY
              .1.. ....      TRPSUPV        X'40' RESTRICT TO SUPERVISOR MODE
                                            ONLY
              ..1. ....      TRPDAT         X'20' RESTRICT TO D.A.T. MODE
                                            ONLY
              ...1 ....      TRPNODAT       X'10' RESTRICT TO NON-D.A.T. MODE
                                            ONLY
              .... 1...      TRPPRINT       X'08' SEND DISPLAY (IF ANY) TO
                                            PRINTER
              .... .1..      TRPTERM        X'04' SEND DISPLAY (IF ANY) TO
                                            TERMINAL
              .... ..1.      TRPNOSIM       X'02' DELETE INSTRUCTION
                                            SIMULATION
              .... ...1      TRPHIT         X'01' TRAP HAS DEFERRED
                                            PROCESSING
    0043   67 Bitstring    1 TRPCTL2
              1... ....      TRPIDSET       X'80' TRAP ID WAS SET VIA 'ID'
                                            OPTION
              .1.. ....      TRPIDATP       X'40' INSTRUCTION DATA PRESENT.
              ..1. ....      TRPIASNF       X'20' TRPIASN contains the ASN of
                                            an address space.
              ...1 ....      TRPASNF        X'10' TRPBASN or TRPSASN contains
                                            the ASN of an address space.
              .... 1...      TRP370         X'08' Trap is restricted to 370
                                            mode addr sp
              .... .1..      TRPESA         X'04' Trap is restricted to ESA
                                            mode addr sp
              .... ..1.      TRPXC          X'02' Trap is restricted to XC
                                            mode addr sp
              .... ...1      TRPESAME       X'01' Trap is restricted to ESAME
                                            addr sp Note regarding TRPTYPE
                                            values: TRPTYPE bits 0-3 are
                                            commonly referenced as bits
                                            (based on the HCPEQUAT values for
                                            CR9B0). These bits are: CR9SUBR
                                            X'80' Monitor Successful Branches
                                            CR9IFET X'40' Monitor Instruction
                                            Fetch CR9SALT X'20' Monitor
                                            Storage Alterations CR9GPRS X'10'
                                            Monitor Register Alterations
                                            TRPTYPE bits 4-7 must be
                                            referenced as CODES (defined
                                            below).
    0044   68 Bitstring    1 TRPTYPE        TRACE TRAP TYPE DEFINITION
              00000001       TRPINTCP       1 TRACE OF INSTRUCTION BY
                                            MNEMONIC
              00000002       TRPSVC         2 SVC INSTRUCTION EVENT TRAP
              00000003       TRPDIAG        3 DIAG INSTRUCTION EVENT TRAP
              00000004       TRPMCALL       4 SUCCESSFUL MONITOR CALL TRAP
              00000005       TRPPGM         5 PROGRAM INTERRUPTION EVENT TRAP
              00000006       TRPEXT         6 EXTERNAL INTERRUPTION EVENT
                                            TRAP
              00000007       TRPMCH         7 MACHINE CHECK INTERRUPTION
                                            EVENT TRAP
              00000008       TRPIOACT       8 I/O Activity Trap
              00000009       TRPAIF         9 Adapter Interruption Facility
                                            Trap
    0045   69 Bitstring    1 TRPTYPE1       TRACE TRAP TYPE DEFINITION
              1... ....      TRPBAC         X'80' Branch-address-control
              .... 1...      TRPAR          X'08' ACCESS REGISTER ALTERATION
                                            TRAP
              .... .1..      TRPGG          X'04' GG REGISTER ALTERATION TRAP
              .... ..1.      TRPGGDEF       X'02' GG trap with no MASK or
                                            DATA specified
              .... 1...      TRPIOINS       X'08' I/O Instructions
              .... .1..      TRPIOINT       X'04' I/O Interruptions (PSW
                                            FLIPS)
              .... ..1.      TRPIOCCW       X'02' CCW CHAINS FOR GIVEN
                                            DEVICE(S)
    0046   70 Bitstring    1 TRPSFLAG       STORAGE ALTERATION TRAP FLAG
              1... ....      TRPSPDAT       X'80' STORAGE ALTERATION DATA
                                            PRESENT
              .1.. ....      TRPS1ST        X'40' FIRST DATA SECTION EQUAL
                                            LAST INT.
              ..1. ....      TRPS2ND        X'20' SECOND DATA SECTION EQUAL
                                            LAST INT
              ...1 ....      TRPSLAST       X'10' BOTH SECTIONS EQUAL LAST
                                            INTERRUPT
              .... 1...      TRPSDISP       X'08' DISPLAY THIS DATA TRAP
              .... .1..      TRPSPMAS       X'04' STORAGE ALTERATION MASK
                                            PRESENT (REFRESHES TRPSTOP IF
                                            PRESENT) (ZERO IF NONE)
    0047   71 Bitstring    1 TRPFLAG        TRPBK flag byte
              1... ....      TRPIADSP       X'80' Trap is restricted to
                                            instructions... . fetched from a
                                            specific addr space
              .1.. ....      TRPBADSP       X'40' Trap is restricted to
                                            branch events... . into a
                                            specific address space
              ..1. ....      TRPSADSP       X'20' Trap is restricted to
                                            storage ... .alterations in a
                                            specific addr space
              111. ....      TRPADSP        TRPIADSP+TRPSADSP+TRPBADSP
              ...1 ....      TRPIODDX       X'10' IODATA was specified on
                                            TRACE cmd
    0048   72 Dbl-Word     8 TRPOVRLY (11)  OVERLAY REGION
         For Instruction traps and Storage alteration traps, if the DATA option
         is specified, the data will be stored in the control block after the
         fields in the overlay region. So, this control block could have up to
         256 extra bytes which contain data.
         Overlay region for STANDARD (code range format) trap information
         TRPCLOWR/TRPCUPPR contain information that is relative to the type of
         trace trap.
         Trap type Information in TRPCLOWR/TRPCUPPR ---------
         ******************************-- mnemonic opcode SVC SVC number range
         DIAG Diagnose code range MC Monitor call code range EXT External
         interruption code range PROG Program interruption code range I/O Device
         range
    0048   72 Bitstring    2 TRPCLOWR (0)   range lower bound
    0048   72 Bitstring    1 TRPCLWR0       TRPCLOWR byte 0
    0049   73 Bitstring    1 TRPCLWR1       TRPCLOWR byte 1
    004A   74 Bitstring    2 TRPCUPPR (0)   range upper bound
    004A   74 Bitstring    1 TRPCUPR0       TRPCUPPR byte 0
    004B   75 Bitstring    1 TRPCUPR1       TRPCUPPR byte 1
    004C   76 Signed       2 TRPDLOWR       DEVICE LOWER BOUND
    004E   78 Signed       2 TRPDUPPR       DEVICE UPPER BOUND
    0050   80 Signed       2 TRPIODNN       IODATA byte limit for each CCW
              0000000B       TRPCDDBW       (*-TRPBK+7)/8 NUMBER OF
                                            DOUBLEWORDS
         Here is the 'TRACE INSTRUCTION DATA' data area.
    0052   82 Signed       2 TRPDATAL       LENGTH OF 'TRACE INSTRUCTION'
                                            DATA
              00000054       TRPINLEN       *-TRPBK FIXED PORTION OF
                                            INSTRUCTION TRAP
    0054   84 Character  256 TRPIDATA (0)   'TRACE INSTRUCTION' DATA
         Overlay region for GPR and GG alteration trap information
         NOTES : The GPR and GG overlay listed below MUST match the AR overlay
         EXACTLY in the use of the fields and overlay displacements. In HCPCQE,
         the GPR/GG overlay is used for ALL register traps (including ARs).
         NOTES : The range fields (TRPGGPRL and TRPGGPRU) must remain adjacent
         to each other in this exact way to they can be passed as input to the
         FMTRANGE, or FMRANG8 subroutines in HCPCQE via one register.
    0048   72 Dbl-Word     8 TRPGGPRM (0)   TR G/GG MASK value (64-bit)
    0048   72 Signed       4 *              ...
    004C   76 Signed       4 TRPGPRM        TR G/GG MASK value (32-bit)
    0050   80 Dbl-Word     8 TRPGGPRL (0)   Lower data bound (64-bit)
    0050   80 Signed       4 *              ...
    0054   84 Signed       4 TRPGPRL        Lower DATA bound (32-bit)
    0058   88 Dbl-Word     8 TRPGGPRU (0)   Upper data bound (64-bit)
    0058   88 Signed       4 *              ...
    005C   92 Signed       4 TRPGPRU        Upper DATA bound (32-bit)
    0060   96 Signed       2 TRPGGPRS (0)   GPR alteration bit mask
    0060   96 Signed       2 TRPGPRS        GPR alteration bit mask
              0000000D       TRPGRDBW       (*-TRPBK+7)/8 NUMBER OF
                                            DOUBLEWORDS
         Overlay region for AR alteration trap information
         NOTES : The AR overlay listed below MUST match the GPR and GG overlay
         EXACTLY in the use of the fields and overlay displacements. In HCPCQE,
         the GPR/GG overlay is used for ALL register traps (including ARs).
    0048   72 Signed       4 *              Reserved
    004C   76 Signed       4 TRPARM         MASK FOR ACCESS REGISTER DATA
                                            COMPARE
    0050   80 Signed       4 *              Reserved...MUST BE 0 FOR HCPCQE
    0054   84 Signed       4 TRPARL         LOWER DATA BOUND FOR AR
                                            ALTERATION
    0058   88 Signed       4 *              Reserved...MUST BE 0 FOR HCPCQE
    005C   92 Signed       4 TRPARU         UPPER BOUND FOR AR ALTERATION
    0060   96 Signed       2 TRPARS         MASK FOR ACCESS REGISTER
                                            ALTERATION
              0000000D       TRPARDBW       (*-TRPBK+7)/8 NUMBER OF
                                            DOUBLEWORDS
         Overlay region for BRANCH trap information
         Notes : The TRPBSTO and TRPSSTO fields must always have the same offset
         because HCPTRR refers to both fields using TRPSSTO.
         Notes : HCPTRR and HCPTGR contain DSECTS for TRPBNEXT followed by
         TRPBRNG. TRPBNEXT and TRPBRNG must be on doubleword boundaries for the
         code to work correctly.
    0048   72 Address      4 TRPBNEXT       Link ptr for branch target range
    004C   76 Signed       4 *              Reserved
    0050   80 Dbl-Word     8 TRPBRNG (2)    BRANCH TRAP TARGET range
         NOTES : The following 3 fields must remain in this order so they can be
         passed as input to the PUTADSP or FMTADSP subroutines in HCPCQE via one
         register as follows: GPR 7 = 31-BIT POINTER to address space info: R7
         -> DOUBLEWORD ASCE (TRPBASCE) FULLWORD STO (TRPBSTO ) HALFWORD ASN
         (TRPBASN )
    0060   96 Dbl-Word     8 TRPBASCE       ASCE for address space of branch
                                            range
    0068  104 Signed       4 TRPBSTO        SEGMENT TABLE ORIGN FOR ADDRESS
                                            SPACE OF BRANCH TARGET RANGE
                                            'FFFFFFFE': INDICATE LOGICAL
                                            ADDRESS
    006C  108 Signed       2 TRPBASN        Address Space Number for the
                                            subspace of BRANCH INTO range.
                                            This field is only valid when the
                                            TRPASNF bit is on.
              0000000E       TRPBRDBW       (*-TRPBK+7)/8 NUMBER OF
                                            DOUBLEWORDS
         Overlay region for STORE (storage alteration) trap information
         Notes : HCPTRR and HCPTGR contain DSECTS for TRPSNEXT followed by
         TRPSRNG. TRPSNEXT and TRPSRNG must be on doubleword boundaries for the
         code to work correctly.
    0048   72 Address      4 TRPSNEXT       LINK PTR FOR STORAGE RANGE
    004C   76 Signed       4 *              Reserved
    0050   80 Dbl-Word     8 TRPSRNG (2)    Store trap target range
         NOTES : The following 3 fields must remain in this order so they can be
         passed as input to the PUTADSP or FMTADSP subroutines in HCPCQE via one
         register as follows: GPR 7 = 31-BIT POINTER to address space info: R7
         -> DOUBLEWORD ASCE (TRPSASCE) FULLWORD STO (TRPSSTO ) HALFWORD ASN
         (TRPSASN )
    0060   96 Dbl-Word     8 TRPSASCE       ASCE for address space of store
                                            range
    0068  104 Signed       4 TRPSSTO        SEGMENT TABLE ORIGN FOR ADDRESS
                                            SPACE OF STORE RANGES 'FFFFFFFE':
                                            INDICATE LOGICAL ADDRESS
    006C  108 Signed       2 TRPSASN        Address Space Number for the
                                            subspace of STORE INTO range.
                                            This field is only valid when the
                                            TRPASNF bit is on
    006E  110 Signed       2 *              Reserved
         TRPSASIT, TRPSPCID, and TRPXCFLG are used only for traps set by an
         ESA/XC mode guest.
    0070  112 Dbl-Word     8 TRPSASIT       i-ASIT for STORE INTO range
    0078  120 Character   33 TRPSPCID       Spaceid for STORE INTO range of
    0099  153 Bitstring    1 TRPXCFLG       XC mode flag byte
              1... ....      TRPXCPRI       X'80' This trap is restricted to
                                            primary
              .... 1...      TRPXCCFY       X'08' Used in HCPTRY to indicate
                                            that this trap's i-ASIT has been
                                            recertified
    009A  154 Character  256 TRPSDATA (0)   STORAGE ALTERATION DATA
              0000009A       TRPSTLEN       *-TRPBK BASE LENGTH FOR STORE
                                            TRAPS
         Overlay for TRPIRNG TRPIRANG and TRPIRANH will be used when CP is
         running in ESA/390 mode. TRPGIRANG and TRPGIRANH will be used when CP
         is running in ESAME mode.
         NOTES : The range fields must remain adjacent to each other so they can
         be passed as input to the FMTRANGE, FMTRANG4, or FMRANG8 subroutines in
         HCPCQE via one register.
    0020   32 Signed       4 TRPIRANG       LOWER IFETCH ADDRESS BOUNDS
    0024   36 Signed       4 TRPIRANH       UPPER IFETCH ADDRESS BOUNDS
    0028   40 Signed       4 * (2)          reserved
    0020   32 Dbl-Word     8 TRPGIRANG      LOWER IFETCH ADDRESS BOUNDS
    0028   40 Dbl-Word     8 TRPGIRANH      UPPER IFETCH ADDRESS BOUNDS
         Overlay for TRPBRNG TRPBRANG and TRPBRANH will be used when CP is
         running in ESA/390 mode. TRPGBRANG and TRPGBRANH will be used when CP
         is running in ESAME mode.
         NOTES : The range fields must remain adjacent to each other so they can
         be passed as input to the FMTRANGE, FMTRANG4, or FMRANG8 subroutines in
         HCPCQE via one register.
    0050   80 Signed       4 TRPBRANG       BRANCH TRAP TARGET LOWER RANGE
    0054   84 Signed       4 TRPBRANH       BRANCH TRAP TARGET UPPER RANGE
    0058   88 Signed       4 * (2)          reserved
    0050   80 Dbl-Word     8 TRPGBRANG      BRANCH TRAP TARGET LOWER RANGE
    0058   88 Dbl-Word     8 TRPGBRANH      BRANCH TRAP TARGET UPPER RANGE
         Overlay for TRPSRNG TRPSRANG and TRPSRANH will be used when CP is
         running in ESA/390 mode. TRPGSRANG and TRPGSRANH will be used when CP
         is running in ESAME mode.
         NOTES : The range fields must remain adjacent to each other so they can
         be passed as input to the FMTRANGE, FMTRANG4, or FMRANG8 subroutines in
         HCPCQE via one register.
    0050   80 Signed       4 TRPSRANG       LOWER STORE ADDRESS BOUNDS
    0054   84 Signed       4 TRPSRANH       UPPER STORE ADDRESS BOUNDS
    0058   88 Signed       4 * (2)          reserved
    0050   80 Dbl-Word     8 TRPGSRANG      STORE TRAP TARGET LOWER RANGE
    0058   88 Dbl-Word     8 TRPGSRANH      STORE TRAP TARGET UPPER RANGE

#### TRPBK Storage Layout

    *** TRPBK - TRACE TRAP BLOCK
    *
    *     +---------------------------+---------------------------+
    *   0 |         TRPNEXT           |         TRPIDENT          |
    *     +-------------+-------------+-------------+-------------+
    *   8 |  TRPSKIP    |  TRPSTOP    |  TRPPASS    |  TRPSTEP    |
    *     +-------------+-------------+-------------+-------------+
    *  10 |         TRPCPNXT          |         TRPCPCMD          |
    *     +---------------------------+---------------------------+
    *  18 |         TRPINEXT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  20 |                       TRPIRNG                         |
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  30 |                       TRPIASCE                        |
    *     +---------------------------+-------------+-------------+
    *  38 |         TRPISTO           |  TRPIASN    |/////////////|
    *     +-------------+------+------+------+------+------+------+
    *  40 |   TRPDBW    |:CNTRL|:CTL2 |:TYPE |:TYPE1|:SFLAG|:FLAG |
    *     +-------------+------+------+------+------+------+------+
    *  48 |                                                       |
    *     =                       TRPOVRLY                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  A0
    *
    *** TRPBK - TRACE TRAP BLOCK

    *** Overlay for TRPOVRLY in TRPBK
    *
    *     +------+------+------+------+-------------+-------------+
    *  48 |:CLWR0|:CLWR1|:CUPR0|:CUPR1|  TRPDLOWR   |  TRPDUPPR   |
    *     +------+------+------+------+-------------+-------------+
    *  50 |  TRPIODNN   |  TRPDATAL   |
    *     +-------------+-------------+
    *
    *** Overlay for TRPOVRLY in TRPBK

    *** Overlay for TRPOVRLY in TRPBK
    *
    *     +---------------------------+---------------------------+
    *  48 |///////////////////////////|         TRPGPRM           |
    *     +---------------------------+---------------------------+
    *  50 |///////////////////////////|         TRPGPRL           |
    *     +---------------------------+---------------------------+
    *  58 |///////////////////////////|         TRPGPRU           |
    *     +-------------+-------------+---------------------------+
    *  60 |  TRPGPRS    | 62
    *     +-------------+
    *
    *** Overlay for TRPOVRLY in TRPBK

    *** Overlay for TRPOVRLY in TRPBK
    *
    *     +---------------------------+---------------------------+
    *  48 |///////////////////////////|          TRPARM           |
    *     +---------------------------+---------------------------+
    *  50 |///////////////////////////|          TRPARL           |
    *     +---------------------------+---------------------------+
    *  58 |///////////////////////////|          TRPARU           |
    *     +-------------+-------------+---------------------------+
    *  60 |   TRPARS    | 62
    *     +-------------+
    *
    *** Overlay for TRPOVRLY in TRPBK

    *** Overlay for TRPOVRLY in TRPBK
    *
    *     +---------------------------+---------------------------+
    *  48 |         TRPBNEXT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  50 |                       TRPBRNG                         |
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  60 |                       TRPBASCE                        |
    *     +---------------------------+-------------+-------------+
    *  68 |         TRPBSTO           |  TRPBASN    | 6E
    *     +---------------------------+-------------+
    *
    *** Overlay for TRPOVRLY in TRPBK

    *** Overlay for TRPOVRLY in TRPBK
    *
    *     +---------------------------+---------------------------+
    *  48 |         TRPSNEXT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  50 |                       TRPSRNG                         |
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  60 |                       TRPSASCE                        |
    *     +---------------------------+-------------+-------------+
    *  68 |         TRPSSTO           |  TRPSASN    |/////////////|
    *     +---------------------------+-------------+-------------+
    *  70 |                       TRPSASIT                        |
    *     +-------------------------------------------------------+
    *  78 |                                                       |
    *     =                       TRPSPCID                        =
    *     |      +------+-----------------------------------------+
    *  98 |      |:XCFLG|
    *     +------+------+
    *
    *** Overlay for TRPOVRLY in TRPBK

    *** Overlay for TRPIRNG in TRPBK
    *
    *     +---------------------------+---------------------------+
    *  20 |         TRPIRANG          |         TRPIRANH          |
    *     +---------------------------+---------------------------+
    *  28 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  30
    *
    *** Overlay for TRPIRNG in TRPBK

    *** Overlay for TRPIRNG in TRPBK
    *
    *     +-------------------------------------------------------+
    *  20 |                      TRPGIRANG                        |
    *     +-------------------------------------------------------+
    *  28 |                      TRPGIRANH                        |
    *     +-------------------------------------------------------+
    *  30
    *
    *** Overlay for TRPIRNG in TRPBK

    *** Overlay for TRPBRNG in TRPBK
    *
    *     +---------------------------+---------------------------+
    *  50 |         TRPBRANG          |         TRPBRANH          |
    *     +---------------------------+---------------------------+
    *  58 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  60
    *
    *** Overlay for TRPBRNG in TRPBK

    *** Overlay for TRPBRNG in TRPBK
    *
    *     +-------------------------------------------------------+
    *  50 |                      TRPGBRANG                        |
    *     +-------------------------------------------------------+
    *  58 |                      TRPGBRANH                        |
    *     +-------------------------------------------------------+
    *  60
    *
    *** Overlay for TRPBRNG in TRPBK

    *** Overlay for TRPSRNG in TRPBK
    *
    *     +---------------------------+---------------------------+
    *  50 |         TRPSRANG          |         TRPSRANH          |
    *     +---------------------------+---------------------------+
    *  58 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  60
    *
    *** Overlay for TRPSRNG in TRPBK

    *** Overlay for TRPSRNG in TRPBK
    *
    *     +-------------------------------------------------------+
    *  50 |                      TRPGSRANG                        |
    *     +-------------------------------------------------------+
    *  58 |                      TRPGSRANH                        |
    *     +-------------------------------------------------------+
    *  60
    *
    *** Overlay for TRPSRNG in TRPBK

#### TRPBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    TRPADSP        0047 E0
    TRPAIF         0044 00000009
    TRPAR          0045 08
    TRPARDBW       0060 0000000D
    TRPARL         0054
    TRPARM         004C
    TRPARS         0060
    TRPARU         005C
    TRPASNF        0043 10
    TRPBAC         0045 80
    TRPBADSP       0047 40
    TRPBASCE       0060
    TRPBASN        006C
    TRPBNEXT       0048
    TRPBRANG       0050
    TRPBRANH       0054
    TRPBRDBW       006C 0000000E
    TRPBRNG        0050
    TRPBSTO        0068
    TRPCDDBW       0050 0000000B
    TRPCLOWR       0048
    TRPCLWR0       0048
    TRPCLWR1       0049
    TRPCNTRL       0042
    TRPCPCMD       0014
    TRPCPNXT       0010
    TRPCTL2        0043
    TRPCUPPR       004A
    TRPCUPR0       004A
    TRPCUPR1       004B
    TRPDAT         0042 20
    TRPDATAL       0052
    TRPDBW         0040
    TRPDIAG        0044 00000003
    TRPDLOWR       004C
    TRPDUPPR       004E
    TRPESA         0043 04
    TRPESAME       0043 01
    TRPEXT         0044 00000006
    TRPFLAG        0047
    TRPGBRANG      0050
    TRPGBRANH      0058
    TRPGG          0045 04
    TRPGGDEF       0045 02
    TRPGGPRL       0050
    TRPGGPRM       0048
    TRPGGPRS       0060
    TRPGGPRU       0058
    TRPGIRANG      0020
    TRPGIRANH      0028
    TRPGPRL        0054
    TRPGPRM        004C
    TRPGPRS        0060
    TRPGPRU        005C
    TRPGRDBW       0060 0000000D
    TRPGSRANG      0050
    TRPGSRANH      0058
    TRPHIT         0042 01
    TRPIADSP       0047 80
    TRPIASCE       0030
    TRPIASN        003C
    TRPIASNF       0043 20
    TRPIDATA       0054
    TRPIDATP       0043 40
    TRPIDENT       0004
    TRPIDSET       0043 80
    TRPINEXT       0018
    TRPINLEN       0052 00000054
    TRPINTCP       0044 00000001
    TRPIOACT       0044 00000008
    TRPIOCCW       0045 02
    TRPIODDX       0047 10
    TRPIODNN       0050
    TRPIOINS       0045 08
    TRPIOINT       0045 04
    TRPIRANG       0020
    TRPIRANH       0024
    TRPIRNG        0020
    TRPISTO        0038
    TRPMCALL       0044 00000004
    TRPMCH         0044 00000007
    TRPNEXT        0000
    TRPNODAT       0042 10
    TRPNOSIM       0042 02
    TRPOVRLY       0048
    TRPPASS        000C
    TRPPGM         0044 00000005
    TRPPRINT       0042 08
    TRPPROB        0042 80
    TRPSADSP       0047 20
    TRPSASCE       0060
    TRPSASIT       0070
    TRPSASN        006C
    TRPSDATA       009A
    TRPSDISP       0046 08
    TRPSFLAG       0046
    TRPSKIP        0008
    TRPSLAST       0046 10
    TRPSNEXT       0048
    TRPSPCID       0078
    TRPSPDAT       0046 80
    TRPSPMAS       0046 04
    TRPSRANG       0050
    TRPSRANH       0054
    TRPSRNG        0050
    TRPSSTO        0068
    TRPSTEP        000E
    TRPSTLEN       009A 0000009A
    TRPSTOP        000A
    TRPSUPV        0042 40
    TRPSVC         0044 00000002
    TRPS1ST        0046 40
    TRPS2ND        0046 20
    TRPTERM        0042 04
    TRPTYPE        0044
    TRPTYPE1       0045
    TRPXC          0043 02
    TRPXCCFY       0099 08
    TRPXCFLG       0099
    TRPXCPRI       0099 80
    TRP370         0043 08

This information is based on z/VM V4R3.0. Last updated on 1 May 2002 at 10:42:51 EDT.
Copyright IBM Corporation, 1990, 2002