Programming Interface Information: This page documents intended Programming Interfaces that allow the customer to write programs to obtain the services of z/VM.

#### LRDD

Prolog

Control Block Contents
LRDD DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### LRDD Prolog

     Name       : LRDD
     Description: LINERD Data Descriptor
     DSECT      : LRDD
     Function   : LRDD is used to map an area of storage that
                  contains information on multple reads resulting
                  from the invocation of the LINERD Macro with
                  FORM=MULTIPLE.  This descriptor DSECT has two
                  formats.  It describes either the cursor position
                  and the key pressed or it describes the data
                  input that is being returned.

#### LRDD Control Block Content

#### LRDD DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      LRDD           LINERD Data Descriptor
    0000    0 Address      4 LRDDNEXT       Pointer to next linerd descriptor
                                            (LRDD)
    0004    4 Character    8 *              Reserved
    000C   12 Signed       4 LRDDLINE       Line number
    0010   16 Signed       4 LRDDCOL        Column number
    0014   20 Address      4 LRDDTXTA       Text address - for input LRDD
    0018   24 Signed       4 LRDDTXTL       Length of text following this
                                            LRDD - for input LRDD
    001C   28 Character    4 *              Reserved
    0020   32 Bitstring    1 LRDDFLG1       Flag byte #1 - for input LRDD
              .... ...1      LRDDRESI       X'01' .... ...X Reserved area of
                                            vscreen
    0021   33 Bitstring    1 LRDDOUTL       field outlining value
    0022   34 Bitstring    1 LRDDCSET       mixed or sbcs field attribute
    0023   35 Character    6 *              Reserved
    0029   41 Bitstring    1 LRDDATTR       Attribute byte - for input LRDD
    002A   42 Bitstring    1 LRDDCOLR       Color byte - for input LRDD
    002B   43 Bitstring    1 LRDDEXHI       Extended highlighting byte -for
                                            input LRDD
    002C   44 Bitstring    1 LRDDPSS        PSS byte - for input LRDD
    002D   45 Bitstring    1 LRDDFLG2       Flag byte #2 - for cursor LRDD
              .... ...1      LRDDRESC       X'01' .... ...X Reserved area of
                                            vscreen
    002E   46 Bitstring    1 *              Reserved
    002F   47 Bitstring    1 LRDDKEY        Holds key pressed - for cursor
                                            LRDD
              00000030       LRDDLEN        *-LRDD Length of LRDD in bytes
              00000006       LRDDDBSZ       ((LRDDLEN+7)/8) Length of LRDD in
                                            doublewords

#### LRDD Storage Layout

    *** LRDD - LINERD Data Descriptor
    *
    *     +---------------------------+---------------------------+
    *   0 |         LRDDNEXT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *   8 |///////////////////////////|         LRDDLINE          |
    *     +---------------------------+---------------------------+
    *  10 |         LRDDCOL           |         LRDDTXTA          |
    *     +---------------------------+---------------------------+
    *  18 |         LRDDTXTL          |///////////////////////////|
    *     +------+------+------+------+---------------------------+
    *  20 |:DFLG1|:DOUTL|:DCSET|//////////////////////////////////|
    *     +------+------+------+------+------+------+------+------+
    *  28 |//////|:DATTR|:DCOLR|:DEXHI|:DPSS |:DFLG2|//////|:DKEY |
    *     +------+------+------+------+------+------+------+------+
    *  30
    *
    *** LRDD - LINERD Data Descriptor

#### LRDD Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    LRDDATTR       0029
    LRDDCOL        0010
    LRDDCOLR       002A
    LRDDCSET       0022
    LRDDDBSZ       002F 00000006
    LRDDEXHI       002B
    LRDDFLG1       0020
    LRDDFLG2       002D
    LRDDKEY        002F
    LRDDLEN        002F 00000030
    LRDDLINE       000C
    LRDDNEXT       0000
    LRDDOUTL       0021
    LRDDPSS        002C
    LRDDRESC       002D 01
    LRDDRESI       0020 01
    LRDDTXTA       0014
    LRDDTXTL       0018

This information is based on z/VM V4R3.0.
Last updated on 1 May 2002 at 14:23:14 EDT.
Copyright IBM Corporation, 1990, 2002