Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### LDRST

Prolog

Control Block Contents
LDRST DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### LDRST Prolog

     Name       : LDRST
     Description: Loader Storage Area
     DSECT      : LDRST
     Function   : Mapping macro that maps the CMS LOAD
                  and INCLUDE command work area. LDRST describes
                  the fields of the work area used by the loader.
                  The work area is obtained and built dynamically
                  by DMSLDR from CMS free storage. LDRST is
                  called by the LDRST macro.

#### LDRST Control Block Content

#### LDRST DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      LDRST          Loader Storage Area
    0000    0 Signed       4 GPRSAV (3)     REGISTERS 9-12
    000C   12 Signed       4 LOCSAV         BASE REGISTER A(DMSLDRA)
    0010   16 Signed       4 NATSAV         NATIVE LANG. PLIST PTR.
    0014   20 Signed       4 ENGSAV         ENGLISH PLIST POINTER
    0018   24 Character    8 NAMORIG        "ORIGIN" NAME VALUE
    0020   32 Signed       4 RETT           RETURN REGISTER FOR DMSLSB
    0024   36 Signed       4 LOCCT          (LOCCNT) NEXT LOAD LOCATION
    0028   40 Signed       4 BRAD           (STRTADDR) START EXECUTION
                                            ADDRESS
    002C   44 Signed       4 TBLREF         (ALDRTBL) TOP OF LOADER TABLE
    0030   48 Bitstring    1 FLAG1          LOADER SWITCHES (PERMANENT)
              1... ....      ABSOLUTE       X'80' ABSOLUTE LOADING
              .1.. ....      FSTXTADR       X'40' FIRST TEXT ADDRESS SAVED
              ..1. ....      COMMONEX       X'20' COMMON ENTRIES EXIST IN
                                            LOADER TABLE
              ...1 ....      PREXIST        X'10' PR ENTRIES EXEIST IN LOADER
                                            TABLE
              .... 1...      ENDCDADR       X'08' ALLOW END CARD ADDRESS
              .... .1..      NOERASE        X'04' DON'T ERASE THE LOAD MAP
              .... ..1.      WORKFILE       X'02' WORK FILE EXISTS
              .... ...1      NODUP          X'01' DO NOT TYPE MSG 202W
    0031   49 Bitstring    1 FLAG2          LOADER SWITCHES (PERMANENT)
              1... ....      STRINITC       X'80' CALL STRINIT ON LOADMOD
              .1.. ....      NOMAP          X'40' DO NOT CREATE A LOAD MAP
              ..1. ....      APRILB         X'20' REP CARD PROCESSING CONTROL
              ...1 ....      NOAUTO         X'10' NO AUTOMATIC TEXT DECK
                                            CHECKING
              .... 1...      TYPE           X'08' TYPE LOAD MAP AT TERMINAL
              .... .1..      NOREP          X'04' NO REP CARD PRINTING
              .... ..1.      NOINV          X'02' NO INVALID CARD TYPEOUT
              .... ...1      NOLIBE         X'01' NO AUTOMATIC TXT LIBRARY
                                            SEARCHING
    0032   50 Bitstring    1 FLAG3          MORE FLAGS
              1... ....      CMD            X'80' PROCESSING NAMES FROM CMD
                                            LI
              .1.. ....      RLDSAVE        X'40' Save RLD data when loading
                                            text files. This RLD information
                                            is for use in subsequent GENMOD
                                            commands.
              ..1. ....      HISTORY        X'20' HIST option of LOAD or
                                            INCLUDE specified. Save the
                                            comments when loading text files
                                            for subsequent GENMOD.
              ...1 ....      SLCBIT         X'10' SLC card was encoutered
              .... 11..      LOCCTSET       X'0C' ORIGIN HIGH specified on
                                            the
              .... 1...      HIGH           X'08' ORIGIN HIGH specified on
                                            the LOAD command
              .... .1..      LOW            X'04' ORIGIN LOW specified on the
                                            LOAD command
              .... ..11      STRTAMOD       X'03' 01=AMODE 24 10=AMODE 31
                                            11=AMODE ANY Used to determine
                                            AMODE when control is passed to
                                            loaded routine
    0033   51 Bitstring    1 FLAG4          LOADER SWITCHES
              1... ....      ORGFLG         X'80' INDICATE ORIGIN SPECIFIED
              .1.. ....      RMODEFLG       X'40' INDICATE RMODE SPECIFIED
              ..1. ....      PRESFLAG       X'20' INDICATE PRES SPECIFIED
              ...1 ....      RELOADFL       X'10' INDICATE "RELOADING"
              .... 1...      FTFLAG         X'08' INDICATE FILETYPE SPECIFIED
              .... .1..      NOVER          X'04' NO VERIFY CARD PRINTING
              .... ..1.      NOUNDEF        X'02' NO MESSAGE FOR UNDEFINED
              .... ...1      PREALLOC       X'01' PREALLOC STORAGE AVAILABLE
    0034   52 Signed       2 TBLCT          NUMBER OF ENTRIES IN LOADER TABLE
    0036   54 Signed       2 *              UNUSED
    0038   56 Signed       4 PRIMINFO       Address of program info blk (in
                                            bytes)
    003C   60 Signed       4 RLDCONST       RELOCATION CONSTANT
    0040   64 Signed       4 PARMLIST       UPDATED PARAMETER LIST POINTER
    0044   68 Signed       4 RETREG         RETURN REGISTER
    0048   72 Signed       4 APSV (16)      REGISTER SAVE AREA FOR SUBROUTINE
                                            CALLS
    0088  136 Signed       4 TEMPST         TEMPORARY RLD ROUTINE STORAGE
    008C  140 Signed       4 TMPLOC         TEMPORARY STORAGE
    0090  144 Signed       4 CRDPTR         INPUT CARD POINTER
    0098  152 Dbl-Word     8 FILE           SAVE LOCATION FOR DMSLIB
    00A0  160 Character   60 LDRREAD (0)    PARAMETER LIST FOR READING CARDS
    00A0  160 Signed       4 * (0)          Align to fullword boundary
    00A0  160 Character   60 READFSCB (0)   Extended FSCB, 60 bytes
    00A0  160 Character    8 *              File system command
    00A8  168 Character    8 *              File name
    00B0  176 Character    8 *              File type
    00B8  184 Character    2 *              File mode letter and number
    00BA  186 Address      2 *              Reserved
    00BC  188 Address      4 *              Buffer address
    00C0  192 Address      4 *              Number of bytes to read or write
    00C4  196 Character    1 *              Record format - F or V
    00C5  197 Bitstring    1 *              First flag byte
    00C6  198 Bitstring    1 *              Second flag byte
    00C7  199 Address      1 *              OPENTYP value
    00C8  200 Address      4 *              Number of bytes actually read or
                                            address of FST copy
    00CC  204 Address      4 *              Relative record number
    00D0  208 Address      4 *              Number of records to access
    00D4  212 Address      4 *              Extended write pointer
    00D8  216 Address      4 *              Extended read pointer
              000000A0       READBUF        READFSCB
              000000A8       LDRFILE        (FSCBFN-FSCBCOMM)+READFSCB,18 FN,
                                            FT, FM FIELDS
              000000A8       FNAME          (FSCBFN-FSCBCOMM)+READFSCB FILE
                                            NAME
              000000B0       FTYPE          (FSCBFT-FSCBCOMM)+READFSCB FILE
                                            TYPE
              000000B8       FMODE          (FSCBFM-FSCBCOMM)+READFSCB FILE
                                            MODE
              000000BA       CURRCSID       (FSCBITNO-FSCBCOMM)+READFSCB
                                            CURRENT CSECT ID
              000000BC       RADD           (FSCBBUFF-FSCBCOMM)+READFSCB
                                            BUFFER ADDRESS
              000000C0       RLENG          (FSCBSIZE-FSCBCOMM)+READFSCB
                                            BUFFER LENGTH
              000000C4       RFIX           (FSCBFV-FSCBCOMM)+READFSCB,1
                                            FIXED/VARIABLE
              000000C5       REPL           (FSCBFLG-FSCBCOMM)+READFSCB
                                            EXTENDED PLIST
              000000C8       NUMBYTE        (FSCBNORD-FSCBCOMM)+READFSCB #
                                            BYTES READ
              000000CC       RITEM          (FSCBAITN-FSCBCOMM)+READFSCB
                                            EXTENDED RECORD #
              000000D0       RNUM           (FSCBANIT-FSCBCOMM)+READFSCB
                                            EXTENDED # OF RECS
              000000D4       RWRPT          (FSCBWPTR-FSCBCOMM)+READFSCB
                                            EXTENDED WRITE PTR
              000000D8       RRDPT          (FSCBRPTR-FSCBCOMM)+READFSCB
                                            EXTENDED READ PTR
    00DC  220 Character   26 LDRFINIS (0)   ENTIRE FINIS PARAMETER LIST
    00DC  220 Character    8 FINIS          FINIS PARAMETER LIST START
    00E4  228 Character    8 LDRFINFN       FILENAME FOR FINIS PARAMETER LIST
    00EC  236 Character    8 LDRFINFT       FILETYPE FOR FINIS PARAMETER LIST
    00F4  244 Character    2 LDRFINFM       FILEMODE FOR FINIS PARAMETER LIST
    00F6  246 Character    1 *              UNUSED
    00F7  247 Character    1 LDRFLAG4       FLAGS (NON-PERMANENT)
              1... ....      ESD1STN        X'80' ESD1ST NOT PREVIOUSLY ON
                                            FOR PC
              .1.. ....      LDRCRLD        X'40' DMSLDRC RETURNS TO RLD
              ...1 ....      LDRESIDX       X'10' ON MEANS ESID TABLE
                                            EXTENDED
              .... 1...      LDRPR          X'08' ON MEANS PR TYPE CALLING
                                            SRCH
              .... .1..      PBKNFND        X'04' Indicates we have the PRGBK
                                            name from a TXTLIB member, don't
                                            overlay it with another member
              .... ..1.      LDRINIT        X'02' Indicates message constant
                                            areas used by LIO have been
                                            initialized
              .... ...1      DATAFND        X'01' INDICATES RECORDS WERE
                                            FOUND IN THE DECK BEING PROCESSED
    00F8  248 Bitstring    1 FLAGS          LOADER SWITCHES (NON PERMANENT)
              1... ....      START          X'80' START EXECUTION REQUESTED
              .1.. ....      ONEDYNA        X'40' ONE CALL TO DYNALOAD PER
                                            TEXT FILE
              ..1. ....      ESD1ST         X'20' FIRST ESD DATA ITEM THIS
                                            CARD
              .... 1...      SETLIB         X'08' SET UP FOR LIBRARY
                                            SEARCHING
              .... .1..      CLOSELIB       X'04' CLEAR TXT LIB SEARCHING
              .... ..1.      LUNDEF         X'02' UNDEFINED ENTRIES EXIST IN
                                            LOADER TABLE
              .... ...1      RESET          X'01' RESET 'ENTRY' SPECIFIED
    00F9  249 Bitstring    1 LDRFREE (3)    LIBRARY SEARCH WORK AREA POINTER
    00FC  252 Signed       4 LDRRLD         RLD DATA STACK POINTER
    0100  256 Signed       4 TYPLIN (2)     TYPLIN PARAMETER LIST
    0108  264 Signed       4 TYPEAD (2)     TYPLIN BUFFER ADDRESS
    0110  272 Signed       4 * (0)          Align to fullword boundary
    0110  272 Character   60 DSKLIN (0)     Extended FSCB, 60 bytes
    0110  272 Character    8 *              File system command
    0118  280 Character    8 *              File name
    0120  288 Character    8 *              File type
    0128  296 Character    2 *              File mode letter and number
    012A  298 Address      2 *              Reserved
    012C  300 Address      4 *              Buffer address
    0130  304 Address      4 *              Number of bytes to read or write
    0134  308 Character    1 *              Record format - F or V
    0135  309 Bitstring    1 *              First flag byte
    0136  310 Bitstring    1 *              Second flag byte
    0137  311 Address      1 *              OPENTYP value
    0138  312 Address      4 *              Number of bytes actually read or
                                            address of FST copy
    013C  316 Address      4 *              Relative record number
    0140  320 Address      4 *              Number of records to access
    0144  324 Address      4 *              Extended write pointer
    0148  328 Address      4 *              Extended read pointer
              00000118       DSKLINFN       (FSCBFN-FSCBCOMM)+DSKLIN FILE
                                            NAME
              00000120       DSKLINFT       (FSCBFT-FSCBCOMM)+DSKLIN FILE
                                            TYPE
              0000012C       DSKAD          (FSCBBUFF-FSCBCOMM)+DSKLIN,13
                                            BUFFER ADDRESS
              00000134       DSKFV          (FSCBFV-FSCBCOMM)+DSKLIN,1 REC
                                            FORMAT
    014C  332 Bitstring    1 HEXCON (15)
              00HEXCON       PACK           HEXCON
              00HEXCON       UNPACK         HEXCON+5
    015B  347 Character    3 *              PADDING
    015E  350 Bitstring    1 OUTPUT
    015F  351 Address      1 OUTBUFL        LENGTH OF OUTBUFL
    0160  352 Bitstring    1 OUTBUF (100)   OUTPUT BUFFER FOR LOAD MAP AND
                                            TERMINAL PRIN
    01C4  452 Signed       2 PRVCNT         ADDRESS OF NEXT PR 'LOAD ADDRESS'
    01C8  456 Signed       4 SAV67 (2)      TEMPORARY SAVE OF REGS 6 AND 7
    01D0  464 Character    8 ENTNAME        ENTRY NAME (RESET 'ENTRY' OR
                                            ENTRY CONTROL CARD)
    01D8  472 Signed       4 ENTADR         ENTRY NAME'S LOADER TABLE
                                            LOCATION
    01DC  476 Signed       4 MEMBOUND       LOW EXTEND OF FREE STORAGE
                                            (FREELOWE)
    01E0  480 Dbl-Word     8 PLISTSAV (64)  LOAD (INCLUDE) PARAMETER LIST
                                            SAVED
    03E0  992 Signed       4 REG13SAV       SAVE AREA FOR STARTED PROGRAM
    03E4  996 Signed       4 FRSTSDID       PLIST POINTER
    03E8 1000 Signed       4 LDRRLDAT       RLD DATA FIELD
    03EC 1004 Signed       4 LDR14A         R14 SAVE AREA FOR FIRST LEVEL
                                            SUBR
    03F0 1008 Address      4 LDRESIDA       ADDRESS OF ESID TABLE
    03F4 1012 Signed       4 LDRESIDL       LENGTH OF ESID TABLE IN BYTES
    03F8 1016 Bitstring 2048 LDRESID        ESID TABLE INITIAL LOCATION
              0LDRESID       LDRESIDD       L'LDRESID/8 INITIAL ESID TABLE
                                            SIZE IN DWORDS
    0BF8 3064 Signed       4 * (0)          FOR LM
    0BF8 3064 Address      1 PRMESSL        LENGTH OF FIRST LINE
    0BF9 3065 Character   50 PRMESS         FIRST LINE
    0C2B 3115 Address      1 PRMESSL2       LENGTH OF SECOND LINE
    0C2C 3116 Character   80 PRMESS2        SECOND LINE
    0C7C 3196 Address      1 CMMESSL        LENGTH OF FIRST LINE
    0C7D 3197 Character   50 CMMESS         FIRST LINE
    0CAF 3247 Address      1 CMMESSL2       LENGTH OF SECOND LINE
    0CB0 3248 Character   80 CMMESS2        SECOND LINE
    0D00 3328 Address      1 CXDMESS
    0D01 3329 Character   50 CXDTXT
    0D33 3379 Address      1 INVCRD
    0D34 3380 Character   50 INVTXT
    0D66 3430 Address      1 PTERR
    0D67 3431 Character   50 PTTXT
    0D99 3481 Address      1 CTLCRD
    0D9A 3482 Character   50 CTLTXT
    0DCC 3532 Bitstring  160 SPEC           CARD INPUT BUFFER
    0E6C 3692 Signed       4 LDRBUFS        START OF OBTAINED BUFFER
    0E70 3696 Signed       4 LDRBUFE        END OF OBTAINED BUFFER
    0E74 3700 Address      4 LDRLICMD       Current LOAD/INCLUDE block
    0E78 3704 Signed       4 OTXTAREA       Save area of OS load area of TEXT
                                            WHEN PROCESSING OS LOAD
    0E7C 3708 Signed       4 CTXTAREA       Save area of CMS load area of
                                            TEXT when processing CMS
                                            LOAD/INCLUDE
    0E80 3712 Signed       4 OBRADENT       Save area for loader table entry
                                            associated with BRAD transfer adr
                                            for OS LOAD support.
    0E84 3716 Signed       4 CBRADENT       Save area for loader table entry
                                            associated with BRAD transfer adr
                                            for CMS LOAD/INCLUDE support
    0E88 3720 Signed       4 ESDPCSA        Save area for ESD 0 or 4 entry to
                                            which an LD (ESD 1) is related
    0E8C 3724 Signed       4 READSIZE       Max read size for reading in TEXT
                                            files or TXTLIB members, setup by
                                            DMSLSBI
    0E90 3728 Character    8 FSTTNAME       Name of 1st TEXT file or TXTLIB
                                            member from LOAD command or OS
                                            type LOAD. Used in determining
                                            the correct start address of a
                                            load. Setup by LSBI.
    0E98 3736 Character    8 MEMBNAME       NAME OF MEMBER FROM TXTLIB SEARCH
                                            THAT WAS FOUND TO SATISFY THE
                                            UNDEFINED LOADER TABLE REFERENCE.
                                            USED BY END CARD PROCESS TO
                                            DETERMINE ENTRY POINT. SETUP BY
                                            DMSLIB.
    0EA0 3744 Signed       4 APSV2 (16)     Reg savearea, used by LSBL, LSBV
                                            subroutines
    0EE0 3808 Signed       4 APSV3 (6)      Reg savearea, used by LSBS
                                            subroutine
    0EF8 3832 Bitstring    1 NLFLAG1        Setup from NUCLDPF field
              1... ....      RAOVRRID       X'80' Indicate RMODE/ORIGIN or
                                            AMODE override was specified on
                                            call to LOAD
              .1.. ....      A24INLD        X'40' Indicates that there is at
                                            least one AMODE 24 CSECT in the
                                            load
              ..1. ....      R24INLD        X'20' Indicates that there is at
                                            least one RMODE 24 CSECT in the
                                            load
              ...1 ....      RMANYOVR       X'10' Indicates that there was an
                                            RMODE ANY override specified on
                                            the LOAD command. Valid with
                                            RMODEFLG or ORGFLG. If off,
                                            indicates RMODE 24 specified.
              .... 1...      NCHIST         X'08' REMOVE HISTORY RECORDS WITH
                                            AN * IN COL ONE OF THE RECORD
              .... .1..      FULLMAP        X'04' for map type,on=fullmap,
                                            off=map
              .... ..1.      PRVMAP         X'02' if on , don't flip FULLMAP
                                            bit
              .... ...1      SAMEOPT        X'01' SAME option specified
    0EF9 3833 Bitstring    1 *              LOADING/GENERATING CMS MODS
    0EFA 3834 Bitstring    1 NLFLAG2        Setup for NUCLDPG field
              1... ....      HOBSET         X'80' Indicate Hihg Order Bit to
                                            be set for SD & LD VCON'S
              .1.. ....      HOBSETSD       X'40' Indicate High Order Bit to
                                            be set for SD VCON'S
              ..1. ....      TRANLOAD       X'20' Indicates that load origin-
                                            ated in the transient area
              ...1 ....      RELODBEL       X'10' Indicates that load above
                                            the line failed, will try reload
                                            below the line
    0EFB 3835 Bitstring    1 *              Reserved for future use
    0EFC 3836 Bitstring   80 SAVIMAGE       REP OR VER CARD IMAGE
    0F4C 3916 Character    8 SAVFTYPE       SAVE AREA FOR FILETYPE
    0F54 3924 Signed       4 PRVCNTX        Extended form of psuedo reg
                                            support. Contains cumlative
                                            length of PRs processed. Also is
                                            the running offset for PR fields
                                            as they are processed. Same
                                            function as PRVCNT but a word
                                            long. Part of removing the
                                            undocumented restrictions of PR
                                            process.
    0F58 3928 Signed       4 APSV4 (16)     Reg savearea, used by DMSLDO
    0F98 3992 Signed       4 TMPPH          TEMP STORAGE OF PH ESD ADDR FOR
                                            RLD PROCESSING
    0F9C 3996 Signed       4 TXTLNTH        save text length for fullmap use
    0FA0 4000 Character    2 FMAPFM         file mode for fullmap information
    0FA2 4002 Bitstring    6 FMAPTIMS       save FSTADATI
    0FA8 4008 Dbl-Word     8 ENDFREE (0)
              000001F5       NEED           (ENDFREE-LDRST)/8 Length of LDRST
                                            in double wrds
              00000FA8       NEEDBYTE       NEED*8 Length of LDRST in bytes

#### LDRST Storage Layout

    *** LDRST - Loader Storage Area
    *
    *     +-------------------------------------------------------+
    *   0 |                        GPRSAV                         |
    *     |                           +---------------------------+
    *   8 |                           |          LOCSAV           |
    *     +---------------------------+---------------------------+
    *  10 |          NATSAV           |          ENGSAV           |
    *     +---------------------------+---------------------------+
    *  18 |                       NAMORIG                         |
    *     +---------------------------+---------------------------+
    *  20 |           RETT            |          LOCCT            |
    *     +---------------------------+---------------------------+
    *  28 |           BRAD            |          TBLREF           |
    *     +------+------+------+------+-------------+-------------+
    *  30 |FLAG1 |FLAG2 |FLAG3 |FLAG4 |   TBLCT     |/////////////|
    *     +------+------+------+------+-------------+-------------+
    *  38 |         PRIMINFO          |         RLDCONST          |
    *     +---------------------------+---------------------------+
    *  40 |         PARMLIST          |          RETREG           |
    *     +---------------------------+---------------------------+
    *  48 |                                                       |
    *     =                         APSV                          =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    *  88 |          TEMPST           |          TMPLOC           |
    *     +---------------------------+---------------------------+
    *  90 |          CRDPTR           |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  98 |                         FILE                          |
    *     +-------------------------------------------------------+
    *  A0 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  A8 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  B0 |///////////////////////////////////////////////////////|
    *     +-------------+-------------+---------------------------+
    *  B8 |/////////////|/////////////|///////////////////////////|
    *     +-------------+-------------+------+------+------+------+
    *  C0 |///////////////////////////|//////|//////|//////|//////|
    *     +---------------------------+------+------+------+------+
    *  C8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    *  D0 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    *  D8 |///////////////////////////|          FINIS-           |
    *     +---------------------------+---------------------------+
    *  E0 |          -(0DC)           |        LDRFINFN-          |
    *     +---------------------------+---------------------------+
    *  E8 |          -(0E4)           |        LDRFINFT-          |
    *     +---------------------------+-------------+------+------+
    *  F0 |          -(0EC)           |  LDRFINFM   |//////|:FLAG4|
    *     +------+--------------------+-------------+------+------+
    *  F8 |FLAGS |      LDRFREE       |          LDRRLD           |
    *     +------+--------------------+---------------------------+
    * 100 |                        TYPLIN                         |
    *     +-------------------------------------------------------+
    * 108 |                        TYPEAD                         |
    *     +-------------------------------------------------------+
    * 110 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 118 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 120 |///////////////////////////////////////////////////////|
    *     +-------------+-------------+---------------------------+
    * 128 |/////////////|/////////////|///////////////////////////|
    *     +-------------+-------------+------+------+------+------+
    * 130 |///////////////////////////|//////|//////|//////|//////|
    *     +---------------------------+------+------+------+------+
    * 138 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 140 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 148 |///////////////////////////|                           |
    *     +---------------------------+                           |
    *     |                        HEXCON                         |
    *     |                    +--------------------+------+------+
    * 158 |                    |////////////////////|OUTPUT|:BUFL |
    *     +--------------------+--------------------+------+------+
    * 160 |                                                       |
    *     =                        OUTBUF                         =
    *     |                           +-------------+-------------+
    * 1C0 |                           |   PRVCNT    |/////////////|
    *     +---------------------------+-------------+-------------+
    * 1C8 |                        SAV67                          |
    *     +-------------------------------------------------------+
    * 1D0 |                       ENTNAME                         |
    *     +---------------------------+---------------------------+
    * 1D8 |          ENTADR           |         MEMBOUND          |
    *     +---------------------------+---------------------------+
    * 1E0 |                                                       |
    *     =                       PLISTSAV                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 3E0 |         REG13SAV          |         FRSTSDID          |
    *     +---------------------------+---------------------------+
    * 3E8 |         LDRRLDAT          |          LDR14A           |
    *     +---------------------------+---------------------------+
    * 3F0 |         LDRESIDA          |         LDRESIDL          |
    *     +---------------------------+---------------------------+
    * 3F8 |                                                       |
    *     =                       LDRESID                         =
    *     |                                                       |
    *     +------+------------------------------------------------+
    * BF8 |:ESSL |                                                |
    *     +------+                                                |
    * C00 |                                                       |
    *     =                        PRMESS                         =
    *     |                    +------+---------------------------+
    * C28 |                    |:ESSL2|                           |
    *     +--------------------+------+                           |
    * C30 |                                                       |
    *     =                       PRMESS2                         =
    *     |                           +------+--------------------+
    * C78 |                           |:ESSL |                    |
    *     +---------------------------+------+                    |
    * C80 |                                                       |
    *     =                        CMMESS                         =
    *     |                                                +------+
    * CA8 |                                                |:ESSL2|
    *     +------------------------------------------------+------+
    * CB0 |                                                       |
    *     =                       CMMESS2                         =
    *     |                                                       |
    *     +------+------------------------------------------------+
    * D00 |:MESS |                                                |
    *     +------+                                                |
    * D08 |                                                       |
    *     =                        CXDTXT                         =
    *     |                    +------+---------------------------+
    * D30 |                    |INVCRD|                           |
    *     +--------------------+------+                           |
    * D38 |                                                       |
    *     =                        INVTXT                         =
    *     |                                         +------+------+
    * D60 |                                         |PTERR |      |
    *     +-----------------------------------------+------+      |
    * D68 |                                                       |
    *     =                        PTTXT                          =
    *     |      +------+-----------------------------------------+
    * D98 |      |CTLCRD|                                         |
    *     +------+------+                                         |
    * DA0 |                                                       |
    *     =                        CTLTXT                         =
    *     |                           +---------------------------+
    *     |                           |                           |
    *     +---------------------------+                           |
    * DD0 |                                                       |
    *     =                         SPEC                          =
    *     |                           +---------------------------+
    * E68 |                           |         LDRBUFS           |
    *     +---------------------------+---------------------------+
    * E70 |         LDRBUFE           |         LDRLICMD          |
    *     +---------------------------+---------------------------+
    * E78 |         OTXTAREA          |         CTXTAREA          |
    *     +---------------------------+---------------------------+
    * E80 |         OBRADENT          |         CBRADENT          |
    *     +---------------------------+---------------------------+
    * E88 |         ESDPCSA           |         READSIZE          |
    *     +---------------------------+---------------------------+
    * E90 |                       FSTTNAME                        |
    *     +-------------------------------------------------------+
    * E98 |                       MEMBNAME                        |
    *     +-------------------------------------------------------+
    * EA0 |                                                       |
    *     =                        APSV2                          =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * EE0 |                                                       |
    *     =                        APSV3                          =
    *     |                                                       |
    *     +------+------+------+------+---------------------------+
    * EF8 |:LAG1 |//////|:LAG2 |//////|                           |
    *     +------+------+------+------+                           |
    * F00 |                                                       |
    *     =                       SAVIMAGE                        =
    *     |                           +---------------------------+
    *     |                           |        SAVFTYPE-          |
    *     +---------------------------+---------------------------+
    * F50 |          -(F4C)           |         PRVCNTX           |
    *     +---------------------------+---------------------------+
    * F58 |                                                       |
    *     =                        APSV4                          =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * F98 |          TMPPH            |         TXTLNTH           |
    *     +-------------+-------------+---------------------------+
    * FA0 |   FMAPFM    |                FMAPTIMS                 |
    *     +-------------+-----------------------------------------+
    *
    *** LDRST - Loader Storage Area

#### LDRST Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    ABSOLUTE       0030 80
    APRILB         0031 20
    APSV           0048
    APSV2          0EA0
    APSV3          0EE0
    APSV4          0F58
    A24INLD        0EF8 40
    BRAD           0028
    CBRADENT       0E84
    CLOSELIB       00F8 04
    CMD            0032 80
    CMMESS         0C7D
    CMMESSL        0C7C
    CMMESSL2       0CAF
    CMMESS2        0CB0
    COMMONEX       0030 20
    CRDPTR         0090
    CTLCRD         0D99
    CTLTXT         0D9A
    CTXTAREA       0E7C
    CURRCSID       00D8 000000BA
    CXDMESS        0D00
    CXDTXT         0D01
    DATAFND        00F7 01
    DSKAD          0148 0000012C
    DSKFV          0148 00000134
    DSKLIN         0110
    DSKLINFN       0148 00000118
    DSKLINFT       0148 00000120
    ENDCDADR       0030 08
    ENDFREE        0FA8
    ENGSAV         0014
    ENTADR         01D8
    ENTNAME        01D0
    ESDPCSA        0E88
    ESD1ST         00F8 20
    ESD1STN        00F7 80
    FILE           0098
    FINIS          00DC
    FLAGS          00F8
    FLAG1          0030
    FLAG2          0031
    FLAG3          0032
    FLAG4          0033
    FMAPFM         0FA0
    FMAPTIMS       0FA2
    FMODE          00D8 000000B8
    FNAME          00D8 000000A8
    FRSTSDID       03E4
    FSTTNAME       0E90
    FSTXTADR       0030 40
    FTFLAG         0033 08
    FTYPE          00D8 000000B0
    FULLMAP        0EF8 04
    GPRSAV         0000
    HEXCON         014C
    HIGH           0032 08
    HISTORY        0032 20
    HOBSET         0EFA 80
    HOBSETSD       0EFA 40
    INVCRD         0D33
    INVTXT         0D34
    LDRBUFE        0E70
    LDRBUFS        0E6C
    LDRCRLD        00F7 40
    LDRESID        03F8
    LDRESIDA       03F0
    LDRESIDD       03F8 0LDRESID
    LDRESIDL       03F4
    LDRESIDX       00F7 10
    LDRFILE        00D8 000000A8
    LDRFINFM       00F4
    LDRFINFN       00E4
    LDRFINFT       00EC
    LDRFINIS       00DC
    LDRFLAG4       00F7
    LDRFREE        00F9
    LDRINIT        00F7 02
    LDRLICMD       0E74
    LDRPR          00F7 08
    LDRREAD        00A0
    LDRRLD         00FC
    LDRRLDAT       03E8
    LDR14A         03EC
    LOCCT          0024
    LOCCTSET       0032 0C
    LOCSAV         000C
    LOW            0032 04
    LUNDEF         00F8 02
    MEMBNAME       0E98
    MEMBOUND       01DC
    NAMORIG        0018
    NATSAV         0010
    NCHIST         0EF8 08
    NEED           0FA8 000001F5
    NEEDBYTE       0FA8 00000FA8
    NLFLAG1        0EF8
    NLFLAG2        0EFA
    NOAUTO         0031 10
    NODUP          0030 01
    NOERASE        0030 04
    NOINV          0031 02
    NOLIBE         0031 01
    NOMAP          0031 40
    NOREP          0031 04
    NOUNDEF        0033 02
    NOVER          0033 04
    NUMBYTE        00D8 000000C8
    OBRADENT       0E80
    ONEDYNA        00F8 40
    ORGFLG         0033 80
    OTXTAREA       0E78
    OUTBUF         0160
    OUTBUFL        015F
    OUTPUT         015E
    PACK           014C 00HEXCON
    PARMLIST       0040
    PBKNFND        00F7 04
    PLISTSAV       01E0
    PREALLOC       0033 01
    PRESFLAG       0033 20
    PREXIST        0030 10
    PRIMINFO       0038
    PRMESS         0BF9
    PRMESSL        0BF8
    PRMESSL2       0C2B
    PRMESS2        0C2C
    PRVCNT         01C4
    PRVCNTX        0F54
    PRVMAP         0EF8 02
    PTERR          0D66
    PTTXT          0D67
    RADD           00D8 000000BC
    RAOVRRID       0EF8 80
    READBUF        00D8 000000A0
    READFSCB       00A0
    READSIZE       0E8C
    REG13SAV       03E0
    RELOADFL       0033 10
    RELODBEL       0EFA 10
    REPL           00D8 000000C5
    RESET          00F8 01
    RETREG         0044
    RETT           0020
    RFIX           00D8 000000C4
    RITEM          00D8 000000CC
    RLDCONST       003C
    RLDSAVE        0032 40
    RLENG          00D8 000000C0
    RMANYOVR       0EF8 10
    RMODEFLG       0033 40
    RNUM           00D8 000000D0
    RRDPT          00D8 000000D8
    RWRPT          00D8 000000D4
    R24INLD        0EF8 20
    SAMEOPT        0EF8 01
    SAVFTYPE       0F4C
    SAVIMAGE       0EFC
    SAV67          01C8
    SETLIB         00F8 08
    SLCBIT         0032 10
    SPEC           0DCC
    START          00F8 80
    STRINITC       0031 80
    STRTAMOD       0032 03
    TBLCT          0034
    TBLREF         002C
    TEMPST         0088
    TMPLOC         008C
    TMPPH          0F98
    TRANLOAD       0EFA 20
    TXTLNTH        0F9C
    TYPE           0031 08
    TYPEAD         0108
    TYPLIN         0100
    UNPACK         014C 00HEXCON
    WORKFILE       0030 02

This information is based on z/VM V4R3.0.
Last updated on 1 May 2002 at 14:22:52 EDT.
Copyright IBM Corporation, 1990, 2002