Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### GSXBK

Prolog

Control Block Contents
GSXBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### GSXBK Prolog

     NAME       : HCPGSXBK
     DESCRIPTION: Cross system communication block
     DSECT      : GSXBK
     FUNCTION   : Maps the GSDDATA field in the HCPGSDBK for use
                  by CSE in cross system communication.
                  This DSECT is used to pass the user ID and
                  other pertinent information about the user
                  who issued a CP command sent to this system
                  from another system in this CSE complex.
                  The control block is created when a QITEM
                  is received representing a CP command that
                  is to be executed on this system.  The
                  CP command processors, such as HCPCSC for
                  the TRANSFER command, and HCPTHI for the
                  INDICATE command, use the information in
                  this control block in lieu of the VMDBK.
                  HCPQCNWT uses this information to determine
                  to which system responses should be sent.
     LOCATED BY : (Overlay of) GSDDATA field of HCPGSDBK
     CREATED BY : HCPXCC
     DELETED BY : HCPXCC

#### GSXBK Control Block Content

#### GSXBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      GSXBK          Cross system communication block
         Information common to all CSE protocols
    0000    0 Character    8 GSXUSER        VMDUSER of command issuer
    0008    8 Signed       4 GSXSYS         SHPBK of issuing CSE system
    000C   12 Signed       4 GSXQTRN        QITEM transaction number
    0010   16 Bitstring    1 GSXFC          CSE Function Code
    0011   17 Bitstring    1 GSXCTYPE       VMDCTYPE of command issuer
         Information used for the CHANGE, ORDER, and TRANSFER commands.
    0012   18 Bitstring    1 GSXMLVL        VMDMLVL of command issuer
    0013   19 Bitstring    1 GSXSYSX        SHPINDEX of issuing system
    0014   20 Bitstring    1 GSXCMDAU       VMDCMDAU of command issuer
    0015   21 Bitstring    1 GSXCMDPR       VMDCMDPR of command issuer
    0016   22 Bitstring    1 GSXSECU1       VMDSECU1 of command issuer
    0017   23 Bitstring    1 GSXRSVD1       Reserved for IBM use
    0018   24 Character    8 GSXDIST        VMDDIST of command issuer
    0020   32 Character    8 GSXGRPN        VMDGRPN of command issuer
    0028   40 Character    8 GSXALTID       VMDALTID, if specified
              00000030       GSXSSIZE       *-GSXUSER Size in bytes CSE Info
                                            spooling area
         Information used for QUERY and INDICATE commands
    0012   18 Bitstring    1 GSXDEVTP       Device Type
    0013   19 Bitstring    1 GSXTC          Type Code
    0014   20 Character    6 GSXVOLID       DASD Volume id
    001A   26 Signed       2 GSXSDISP       Starting minidisk cyl
    001C   28 Signed       2 GSXEDISP       Ending minidisk cyl
    001E   30 Signed       2 GSXRETCD       Return Code
              00000020       GSXQSIZE       *-GSXUSER Size in bytes of CSE
                                            Info Query/Indicate area
              1... ....      GSXQLST        X'80' QUERY LINKS stable option
                                            requested

#### GSXBK Storage Layout

    *** GSXBK - Cross system communication block
    *
    *     +-------------------------------------------------------+
    *   0 |                       GSXUSER                         |
    *     +---------------------------+---------------------------+
    *   8 |          GSXSYS           |         GSXQTRN           |
    *     +------+------+------+------+------+------+------+------+
    *  10 |GSXFC |:CTYPE|:MLVL |:SYSX |:CMDAU|:CMDPR|:SECU1|:RSVD1|
    *     +------+------+------+------+------+------+------+------+
    *  18 |                       GSXDIST                         |
    *     +-------------------------------------------------------+
    *  20 |                       GSXGRPN                         |
    *     +-------------------------------------------------------+
    *  28 |                       GSXALTID                        |
    *     +-------------------------------------------------------+
    *  30
    *
    *** GSXBK - Cross system communication block

    *** Overlay for GSXMLVL in GSXBK
    *
    *                   +------+------+---------------------------+
    *  10 ...        12 |:DEVTP|GSXTC |        GSXVOLID-          |
    *     +-------------+------+------+-------------+-------------+
    *  18 |   -(014)    |  GSXSDISP   |  GSXEDISP   |  GSXRETCD   |
    *     +-------------+-------------+-------------+-------------+
    *  20
    *
    *** Overlay for GSXMLVL in GSXBK

#### GSXBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    GSXALTID       0028
    GSXCMDAU       0014
    GSXCMDPR       0015
    GSXCTYPE       0011
    GSXDEVTP       0012
    GSXDIST        0018
    GSXEDISP       001C
    GSXFC          0010
    GSXGRPN        0020
    GSXMLVL        0012
    GSXQLST        001E 80
    GSXQSIZE       001E 00000020
    GSXQTRN        000C
    GSXRETCD       001E
    GSXRSVD1       0017
    GSXSDISP       001A
    GSXSECU1       0016
    GSXSSIZE       0028 00000030
    GSXSYS         0008
    GSXSYSX        0013
    GSXTC          0013
    GSXUSER        0000
    GSXVOLID       0014

This information is based on z/VM V4R3.0. Last updated on 1 May 2002 at 08:55:40 EDT.
Copyright IBM Corporation, 1990, 2002