UWKPG - 64-bit CP - V4R4.0

Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### UWKPG

Prolog

Control Block Contents
UWKPG DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### UWKPG Prolog

     Name       : HCPUWKPG
     Description: INDICATE USER data block
     DSECT      : UWKPG
     Function   : Contain information gathered to process the
                  INDICATE USER command.
     Located by : Registers in INDICATE USER modules
     Created by : HCPTHLU
     Deleted by : HCPTHLU
     Serialized : Task execution: each time the task is run a new set
                  of pages is obtained to hold the UWKPG maps; the
                  data is first collected, then used, and finally the
                  pages are deleted
     Comments   :
                  This control block is used to map entries in
                  storage that is fetched and released by the
                  page.
                  This control block is used to map the data gathered
                  for both the old response and the expanded response
                  to the Indicate user command.  Some fields are not
                  used when processing the old response format.

#### UWKPG Control Block Content

#### UWKPG DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      UWKPG          INDICATE USER data block
    0000    0 Character    8 UWKUSER        Userid
    0008    8 Bitstring    1 UWKFLAG        Flags for various states;
                                            contains BITS, so TM must be
                                            used.
              1... ....      UWK370         X'80' Machine Mode = 370
              .1.. ....      UWKXA          X'40' Machine Mode = XA
              ..1. ....      UWKESA         X'20' Machine Mode = ESA
              ...1 ....      UWKXC          X'10' Machine Mode = XC
              .... 1...      UWKHADVF       X'08' User had virtual vector
                                            facility
              .... .1..      UWKBASE        X'04' Entry is for virtual MP
                                            configuration
    0009    9 Bitstring    1 UWKPVTSH       Flags indicating type of primary
                                            address space.
              1... ....      UWKPRIVT       X'80' Primary space is private
              .1.. ....      UWKSHARD       X'40' Primary space is shared
    000A   10 Bitstring    1 UWKIOPT        IO passthrough indication
    000B   11 Bitstring    1 UWKVIRT        Storage type
    000C   12 Bitstring    1 UWKTYPE        VMDBK type
    000D   13 Bitstring    1 UWKADJFL       ADJUNCT TYPE
    000E   14 Bitstring    1 * (2)          Reserved
    0010   16 Dbl-Word     8 UWKGSTOR       Total configured size of user's
                                            primary address space in bytes-1
    0018   24 Signed       4 UWKXSTR        Xstore size (if attached), or
                                            'NONE'
         For the EXPanded response, UWKIPLN is filled in only for base VMDBK
         UWKPG entries, and is filled in with the IPL system name or device that
         is in effect for the virtual configuration, or 'DEV NONE' if none. For
         the non-EXPanded response, UWKIPLN is filled in for each UWKPG entry
         with the IPL system name or device that is in effect for the virtual
         configuration if it was IPL'd on that virtual CPU, or 'DEV NONE.'
    001C   28 Character    8 UWKIPLN (0)    Name of IPL device or name, or
                                            'DEV NONE' if none.
    001C   28 Character    4 UWKIPDEV       'DEV '
    0020   32 Character    4 UWKIPNUM       IPL device number
    0024   36 Signed       4 UWKDEVN        Number of attached devices
    0028   40 Signed       4 UWKSPLRD       Number of spooling pages read
                                            from DASD
    002C   44 Signed       4 UWKSPLWT       Number of spooling pages written
                                            to DASD
    0030   48 Character    8 UWKPRMUS       Userid of primary space owner
    0038   56 Character   24 UWKPRMNM       Space name of primary space
    0050   80 Dbl-Word     8 UWKGPRMAD      Addressable size of primary
                                            address space - 1
         The following two fields represent totals for all address spaces.
    0058   88 Signed       4 UWKTOTSP       Number of spaces owned by user
    0060   96 Dbl-Word     8 UWKGTOTSZ      Total size, in pages, of all
                                            spaces owned by this user
         The following counts are the totals of the values for all private
         address spaces.
    0068  104 Signed       4 UWKPVTSP       Number of private spaces owned by
                                            this user
    0070  112 Dbl-Word     8 UWKGPVTSZ      Size in pages of all private
                                            spaces owned by this user
         Private spaces, pages information These are counts for spaces which are
         currently private.
    0078  120 Signed       4 UWKRES         Number of resident pages in
                                            private address spaces
    007C  124 Signed       4 UWKXBK         Number of pages in xstore for
                                            private address spaces
    0080  128 Signed       4 UWKPDAS        Number of pages on DASD for
                                            private address spaces
    0084  132 Signed       4 UWKLOK         Number of locked pages in private
                                            address spaces
    0088  136 Signed       4 UWKWSS         Working Set Size
    008C  140 Signed       4 UWKRESV        Number of reserved pages in
                                            private address spaces
         End of totals for private spaces
         The following counts are the totals of the values for all shared
         address spaces.
    0090  144 Signed       4 UWKSHRSP       Number of shared spaces owned by
                                            this user
    0098  152 Dbl-Word     8 UWKGSHRSZ      Size in pages of all shared
                                            spaces owned by this user
         Shared spaces, pages information These are counts for spaces which are
         currently shared.
    00A0  160 Signed       4 UWKSRES        Number of resident pages in
                                            shared address spaces
    00A4  164 Signed       4 UWKSXBK        Number of pages in xstore for
                                            shared address spaces
    00A8  168 Signed       4 UWKSDAS        Number of pages on DASD for
                                            shared address spaces
    00AC  172 Signed       4 UWKSLOK        Number of locked pages in shared
                                            address spaces
         End of totals for shared spaces.
         The following counts are the totals of the values for all address
         spaces:
         These are the cummulative counts of private and shared paging for all
         address spaces regardless of whether they are currently private or
         shared.
         Private paging information:
    00B0  176 Signed       4 UWKXRD         Number reads from xstore to
                                            private address spaces
    00B4  180 Signed       4 UWKXWT         Number writes to xstore from
                                            private address spaces
    00B8  184 Signed       4 UWKMIG         Number of migrates for private
                                            address spaces
    00BC  188 Signed       4 UWKREAD        Number of reads from DASD to
                                            private address spaces
    00C0  192 Signed       4 UWKWRIT        Number of writes to DASD from
                                            private address spaces
         Shared paging information:
    00C4  196 Signed       4 UWKSXRD        Number of reads from xstore to
                                            shared address spaces
    00C8  200 Signed       4 UWKSXWT        Number of writes to xstore from
                                            shared address spaces
    00CC  204 Signed       4 UWKSMIG        Number of migrates for shared
                                            address spaces
    00D0  208 Signed       4 UWKSREAD       Number of reads from DASD to
                                            shared address spaces
    00D4  212 Signed       4 UWKSWRIT       Number of writes to DASD from
                                            shared address spaces.
         End of totals for all address spaces
         The following fields are significant for each virtual processor in a
         virtual configuration.
    00D8  216 Signed       4 UWKCPUAD       Virtual CPU address
    00DC  220 Signed       4 UWKTODON       Connect time. The current TOD
                                            minus the time of logon (or
                                            creation for a non origin VMDBK).
                                            Only the high order word of the
                                            TOD clock value is used.
    00E0  224 Dbl-Word     8 UWKVTIM        Total virtual time
    00E8  232 Dbl-Word     8 UWKTTIM        Total virtual and simulation time
    00F0  240 Dbl-Word     8 UWKVVECT       VVECTIME
    00F8  248 Dbl-Word     8 UWKTVECT       TVECTIME
    0100  256 Signed       4 UWKRDR         Number of virtual cards read
    0104  260 Signed       4 UWKPRT         Number of virtual lines printed
    0108  264 Signed       4 UWKPCH         Number of virutal cards punched
    010C  268 Signed       4 UWKIOS         Number of IO requests
         End of fields significant for each virtual processor
         End of control block
              00000110       UWKSIZE        *-UWKPG Single entry size (bytes)
              00000022       UWKDWSZ        ((*-UWKPG)+7)/8 Single entry size
                                            (dbl words)

#### UWKPG Storage Layout

    *** UWKPG - INDICATE USER data block
    *
    *     +-------------------------------------------------------+
    *   0 |                       UWKUSER                         |
    *     +------+------+------+------+------+------+-------------+
    *   8 |:FLAG |:PVTSH|:IOPT |:VIRT |:TYPE |:ADJFL|/////////////|
    *     +------+------+------+------+------+------+-------------+
    *  10 |                       UWKGSTOR                        |
    *     +---------------------------+---------------------------+
    *  18 |         UWKXSTR           |         UWKIPDEV          |
    *     +---------------------------+---------------------------+
    *  20 |         UWKIPNUM          |         UWKDEVN           |
    *     +---------------------------+---------------------------+
    *  28 |         UWKSPLRD          |         UWKSPLWT          |
    *     +---------------------------+---------------------------+
    *  30 |                       UWKPRMUS                        |
    *     +-------------------------------------------------------+
    *  38 |                                                       |
    *     =                       UWKPRMNM                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  50 |                      UWKGPRMAD                        |
    *     +---------------------------+---------------------------+
    *  58 |         UWKTOTSP          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  60 |                      UWKGTOTSZ                        |
    *     +---------------------------+---------------------------+
    *  68 |         UWKPVTSP          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  70 |                      UWKGPVTSZ                        |
    *     +---------------------------+---------------------------+
    *  78 |          UWKRES           |          UWKXBK           |
    *     +---------------------------+---------------------------+
    *  80 |         UWKPDAS           |          UWKLOK           |
    *     +---------------------------+---------------------------+
    *  88 |          UWKWSS           |         UWKRESV           |
    *     +---------------------------+---------------------------+
    *  90 |         UWKSHRSP          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  98 |                      UWKGSHRSZ                        |
    *     +---------------------------+---------------------------+
    *  A0 |         UWKSRES           |         UWKSXBK           |
    *     +---------------------------+---------------------------+
    *  A8 |         UWKSDAS           |         UWKSLOK           |
    *     +---------------------------+---------------------------+
    *  B0 |          UWKXRD           |          UWKXWT           |
    *     +---------------------------+---------------------------+
    *  B8 |          UWKMIG           |         UWKREAD           |
    *     +---------------------------+---------------------------+
    *  C0 |         UWKWRIT           |         UWKSXRD           |
    *     +---------------------------+---------------------------+
    *  C8 |         UWKSXWT           |         UWKSMIG           |
    *     +---------------------------+---------------------------+
    *  D0 |         UWKSREAD          |         UWKSWRIT          |
    *     +---------------------------+---------------------------+
    *  D8 |         UWKCPUAD          |         UWKTODON          |
    *     +---------------------------+---------------------------+
    *  E0 |                       UWKVTIM                         |
    *     +-------------------------------------------------------+
    *  E8 |                       UWKTTIM                         |
    *     +-------------------------------------------------------+
    *  F0 |                       UWKVVECT                        |
    *     +-------------------------------------------------------+
    *  F8 |                       UWKTVECT                        |
    *     +---------------------------+---------------------------+
    * 100 |          UWKRDR           |          UWKPRT           |
    *     +---------------------------+---------------------------+
    * 108 |          UWKPCH           |          UWKIOS           |
    *     +---------------------------+---------------------------+
    * 110
    *
    *** UWKPG - INDICATE USER data block

#### UWKPG Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    UWKADJFL       000D
    UWKBASE        0008 04
    UWKCPUAD       00D8
    UWKDEVN        0024
    UWKDWSZ        010C 00000022
    UWKESA         0008 20
    UWKFLAG        0008
    UWKGPRMAD      0050
    UWKGPVTSZ      0070
    UWKGSHRSZ      0098
    UWKGSTOR       0010
    UWKGTOTSZ      0060
    UWKHADVF       0008 08
    UWKIOPT        000A
    UWKIOS         010C
    UWKIPDEV       001C
    UWKIPLN        001C
    UWKIPNUM       0020
    UWKLOK         0084
    UWKMIG         00B8
    UWKPCH         0108
    UWKPDAS        0080
    UWKPRIVT       0009 80
    UWKPRMNM       0038
    UWKPRMUS       0030
    UWKPRT         0104
    UWKPVTSH       0009
    UWKPVTSP       0068
    UWKRDR         0100
    UWKREAD        00BC
    UWKRES         0078
    UWKRESV        008C
    UWKSDAS        00A8
    UWKSHARD       0009 40
    UWKSHRSP       0090
    UWKSIZE        010C 00000110
    UWKSLOK        00AC
    UWKSMIG        00CC
    UWKSPLRD       0028
    UWKSPLWT       002C
    UWKSREAD       00D0
    UWKSRES        00A0
    UWKSWRIT       00D4
    UWKSXBK        00A4
    UWKSXRD        00C4
    UWKSXWT        00C8
    UWKTODON       00DC
    UWKTOTSP       0058
    UWKTTIM        00E8
    UWKTVECT       00F8
    UWKTYPE        000C
    UWKUSER        0000
    UWKVIRT        000B
    UWKVTIM        00E0
    UWKVVECT       00F0
    UWKWRIT        00C0
    UWKWSS         0088
    UWKXA          0008 40
    UWKXBK         007C
    UWKXC          0008 10
    UWKXRD         00B0
    UWKXSTR        0018
    UWKXWT         00B4
    UWK370         0008 80

This information is based on z/VM V4R4.0. Last updated on 30 Jul 2003 at 13:25:48 EDT.
Copyright IBM Corporation, 1990, 2003