Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSCLSQD

Prolog
Control Block Contents
Cross Reference

#### MRSCLSQD Prolog

####

####

     DSECT NAME - SCLSQD
     FUNCTION - Map a Monitor record.
     LOCATED BY -
               Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSCLSQD
     DESCRIPTIVE NAME - Monitor Event Record
                        Domain 2 - Scheduler Domain
                        Record 10 - SET QUICKDSP Changes
     DESCRIPTION - Record of changes made by a SET QUICKDSP command.
                   Generated only if the user who is the target of the
                   command is enabled for scheduler domain (not to be
                   confused with the user that issued the command).

    MRSCLSQD Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)          Description

      0   0  Structure   32  SCLSQD              Start of monitor record
      0   0  Character    0  SCLSQD_MRHDR        Record header. See MRRECHDR for
                                                 details.
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN            record length in bytes
      2   2  Unsigned     2  MRHDRZER            field of zeros
      4   4  Unsigned     1  MRHDRDM             domain identifier
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC             record identifier
      8   8  Character    8  MRHDRTOD            Time at which this record was
                                                 built. In time-of-day (TOD) clock
                                                 format. See IBM System 370 XA
                                                 Principle of Operation for
                                                 explanation of format.
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END           End of header
     20  14  Character    8  SCLSQD_VMDUSER      Userid
     28  1C  Bitstring    1  SCLSQD_CALFLAG1     Flag byte 1
              1... ....      *
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      SCLSQD_VMDQDSPU     When set on, user is classified
                                                 as QUICKDSP. Set by the user's
                                                 directory or by the SET QUICKDSP
                                                 command.
              .... .1..      *
              .... ..1.      *
              .... ...1      *
     29  1D  Character    3  *                   Reserved for IBM use
     32  20  Character    0  SCLSQD_END

    MRSCLSQD Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                   0     20
    MRHDR_END              14      0
    MRHDRDM                 4      1
    MRHDRLEN                0      2
    MRHDRRC                 6      2
    MRHDRTOD                8      8
    MRHDRZER                2      2
    SCLSQD                  0     32
    SCLSQD_CALFLAG1        1C      1
    SCLSQD_END             20      0
    SCLSQD_MRHDR            0      0
    SCLSQD_VMDQDSPU        1C           08
    SCLSQD_VMDUSER         14      8

    This information is
    based on z/VM V4R4.0.

    Last updated on 22 Jul 2003 at 15:04:23.

    Copyright IBM Corporation, 1990, 2003