Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSCLAEL

Prolog
Control Block Contents
Cross Reference

#### MRSCLAEL Prolog

####

####

     DSECT NAME - SCLAEL
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSCLAEL
     DESCRIPTIVE NAME - Monitor Event Record
                        Domain 2 - Scheduler
                        Record 6 - Add User To Eligible List
     DESCRIPTION - Indicates conditions after this user has been
                   added to the eligible list.  A separate
                   record is generated for each VMDBK in the
                   virtual MP complex.

    MRSCLAEL Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)          Description

      0   0  Structure  132  SCLAEL              Start of monitor record
      0   0  Character    0  SCLAEL_MRHDR        Record header. See MRRECHDR for
                                                 details.
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN            record length in bytes
      2   2  Unsigned     2  MRHDRZER            field of zeros
      4   4  Unsigned     1  MRHDRDM             domain identifier
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC             record identifier
      8   8  Character    8  MRHDRTOD            Time at which this record was
                                                 built. In time-of-day (TOD) clock
                                                 format. See IBM System 370 XA
                                                 Principle of Operation for
                                                 explanation of format.
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END           End of header
     20  14  Character    8  SCLAEL_VMDUSER      Userid
     28  1C  Unsigned     2  SCLAEL_SRMC1ELG     Cardinal count of short, medium
                                                 and long-running users in the
                                                 eligible list. This includes all
                                                 E1, E2 and E3 users. It includes
                                                 no E0 users.
     30  1E  Unsigned     2  SCLAEL_SRMC2ELG     Cardinal count of short, medium
                                                 and long-running users in the
                                                 eligible list. This includes all
                                                 E2 and E3 users. It includes no E0
                                                 or E1 users.
     32  20  Unsigned     2  SCLAEL_SRMC3ELG     Cardinal count of short, medium
                                                 and long-running users in the
                                                 eligible list. This includes all
                                                 E3 users. It includes no no E0,
                                                 E1, or E2 users.
     34  22  Unsigned     2  SCLAEL_VMDCPUAD     Virtual processor address
     36  24  Character    8  SCLAEL_VMDSVMID     VMDBK name for the last
                                                 successful IUCV, VMCF or APPC/VM
                                                 Send for this virtual machine.
                                                 Valid in base VMDBK only.
     44  2C  Bitstring    1  SCLAEL_VMDSVMWT     Service-virtual-machine (SVM)
                                                 wait flag byte - valid in base
                                                 VMDBK only.
              1... ....      SCLAEL_VMDSVMWF     VMDBK is waiting for a response
                                                 from IUCV, VMCF or APPC.
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
     45  2D  Character    0  SCLAEL_VMDSVMW2     Back-up byte to the VMDSVMWT
                                                 byte. Its contents will persist
                                                 longer than they would in
                                                 VMDSVMWT. Valid in base VMDBK
                                                 only.
     45  2D  Bitstring    1  SCLAEL_VMDSVMWT     Service-virtual-machine (SVM)
                                                 wait flag byte - valid in base
                                                 VMDBK only.
              1... ....      SCLAEL_VMDSVMWF     VMDBK is waiting for a response
                                                 from IUCV, VMCF or APPC.
     46  2E  Character    0  SCLAEL_VMDRDYCM     Flag byte set by IUCV, VMCF, or
                                                 APPC whenever IUCV/VMCF/APPC makes
                                                 an external interrupt. It is sort
                                                 of a "reference byte" that tells
                                                 the scheduler that IUCV/VMCF/APPC
                                                 had been active recently. Valid in
                                                 base VMDBK only.
     46  2E  Bitstring    1  SCLAEL_VMDSVMWT     Service-virtual-machine (SVM)
                                                 wait flag byte - valid in base
                                                 VMDBK only.
              1... ....      SCLAEL_VMDSVMWF     VMDBK is waiting for a response
                                                 from IUCV, VMCF or APPC.
     47  2F  Bitstring    1  SCLAEL_CALFLAG1     Flag byte
              1... ....      SCLAEL_CALBASE      If on, this is the base VMDBK.
                                                 VMDBASE
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
     48  30  Unsigned     4  SCLAEL_VMDWSSPR     This user's projected working
                                                 set size. This is the scheduler's
                                                 estimate of the amount of storage
                                                 this user will require to be
                                                 resident as it runs during its
                                                 next stay in the dispatch list. It
                                                 is based upon the user's past
                                                 behavior and in some cases, on the
                                                 behavior of similar types of
                                                 users.
     52  34  Unsigned     4  SCLAEL_VMDPGRTE     Number of pages per second which
                                                 this user read in during its last
                                                 stay in the dispatch list
     56  38  Bitstring    1  SCLAEL_CALQSTAT     Scheduling status of user
              1... ....      SCLAEL_VMDHOTRQ     Hot Shot scheduling requested
              .1.. ....      SCLAEL_VMDHOTST     Hot Shot user scheduling granted
              ..1. ....      SCLAEL_VMDLOADU     Loading user designation
              ...1 ....      SCLAEL_VMDIABIA     Interactive bias is in effect
              .... 1...      SCLAEL_VMDPGBIA     Paging bias is in effect
              .... .1..      SCLAEL_VMDLKSHT     "Lockshot" scheduling in effect
                                                 for this user. Set only in the
                                                 base VMDBK.
              .... ..1.      *
              .... ...1      SCLAEL_VMDNULL      User is logging off
     57  39  Unsigned     1  SCLAEL_VMDELIST     This user's eligible list class.
                                                 It can be 0, 1, 2, or 3. Classes
                                                 1-3 relate to the time this
                                                 (scheduler-determined) transaction
                                                 has been running. Class 1 is
                                                 short-running, class 2,
                                                 medium-running and class 3,
                                                 long-running.
     58  3A  Bitstring    1  SCLAEL_VMDWRKCS     Type of work which must be done
                                                 on the VMDBK
     59  3B  Bitstring    1  SCLAEL_CALOSTAT     Virtual machine operating status
              1... ....      SCLAEL_VMDSYSOP     User is primary system operator
              .1.. ....      SCLAEL_VMDUSRCT     User is counted as being logged
                                                 on
              ..1. ....      *
              ...1 ....      SCLAEL_VMDFORCE     User is to be logged off. This
                                                 may be requested by CP, a forced
                                                 logoff, or user's logoff command.
              .... 1...      SCLAEL_VMDUFORC     User is forced to logoff the
                                                 system
              .... .1..      SCLAEL_VMDDISC      User is running disconnected
              .... ..1.      SCLAEL_VMDAUTOL     AUTOLOG/XAUTOLOG in progress.
                                                 User has been automatically logged
                                                 on. This bit is set off when the
                                                 user's IPL statement is processed,
                                                 or (if there is no IPL to process)
                                                 when the user enters a LOGON
                                                 command from a terminal to
                                                 RECONNECT.
              .... ...1      SCLAEL_VMDXAUTO     The original command was
                                                 XAUTOLOG. Valid for the base VMDBK
                                                 only.
     60  3C  Character    8  SCLAEL_VMDEPRTY     Eligible list priority. This
                                                 represents the scheduler's
                                                 estimate of the latest time this
                                                 VMDBK should be selected to go
                                                 into the dispatch list from the
                                                 eligible list. It is used to order
                                                 users in the eligible list.
     68  44  Unsigned     4  SCLAEL_VMDCTPVR     Cardinal count of resident pages
                                                 in private address spaces
                                                 belonging to this user. This
                                                 monitor field is actually the sum
                                                 of VMDCTPVR + VMDCTPVG which is
                                                 the resident pages above and below
                                                 the 2GB line. To get the count of
                                                 resident pages below the 2GB line,
                                                 subtract SCLAEL_VMDCTPVG from
                                                 SCLAEL_VMDCTPVR.
     72  48  Unsigned     4  SCLAEL_VMDCTXBK     Number of Expanded Storage
                                                 blocks allocated to a virtual
                                                 machine by CP for paging
     76  4C  Unsigned     4  SCLAEL_CALCPPST     Cumulative count of pages stolen
                                                 from this user's address spaces
                                                 while they were private.
     80  50  Unsigned     4  SCLAEL_VMDRELSH     This user's RELATIVE share of
                                                 the system, as set in the user's
                                                 directory or via the SET SHARE
                                                 command. Set to zero if the user
                                                 is an ABSOLUTE share user or if
                                                 this VMDBK has a virtual processor
                                                 dedicated to it, and this is a
                                                 virtual MP user. Set to a negative
                                                 value if VMDBK has a virtual
                                                 processor dedicated to it, and the
                                                 user is a virtual UP user.
     84  54  Unsigned     4  SCLAEL_VMDABSSH     This user's ABSOLUTE share of
                                                 the system, as set in the user's
                                                 directory or via the SET SHARE
                                                 command. Unit of value is a
                                                 hexadecimal factor scaled 16 bits.
                                                 For example X'00010000' = 1.00
                                                 (100%), X'0000C000' = 0.75 (75%),
                                                 X'00008000' = 0.50 (50%), etc. Set
                                                 to zero if user is a RELATIVE
                                                 share user.
     88  58  Signed       4  SCLAEL_VMDURRSP     User's resource requirement for
                                                 storage and paging
     92  5C  Signed       4  SCLAEL_SRMABSDE     Cardinal count of total absolute
                                                 shares of all VMDBKs in the
                                                 dispatch and eligible lists. Unit
                                                 of value is same as
                                                 SCLAEL_VMDABSSH.
     96  60  Signed       4  SCLAEL_SRMRELDE     Cardinal count of total relative
                                                 shares of all VMDBKs in the
                                                 dispatch and eligible lists.
    100  64  Unsigned     4  SCLAEL_VMDCTCRT     Count of CP critical-processes
                                                 this VMDBK is responsible for.
                                                 VMDBK must not wait in eligible
                                                 list while this count is greater
                                                 than 0. Valid only in base VMDBK.
    104  68  Bitstring    1  SCLAEL_CALSHARF     Set Share flags
              1... ....      SCLAEL_VMDMXSHA     Max share is Absolute if ON. Max
                                                 share is Relative if OFF.
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      SCLAEL_VMDLIMTH     Max Share is Limithard if ON.
                                                 Max Share is Limitsoft if OFF.
              .... ...1      *
    105  69  Unsigned     3  *                   Reserved and available for IBM
                                                 use.
    108  6C  Unsigned     4  SCLAEL_VMDMXSHR     The user's Max share of the
                                                 system, as set in the user's
                                                 directory or via the SET SHARE
                                                 command. This value is set to zero
                                                 if no Max share exists. If the Max
                                                 share is Absolute, then the unit
                                                 of the value is a hexadecimal
                                                 factor scaled 16 bits. For
                                                 example, X'00010000' = 1.00(100%),
                                                 X'0000C000' = 0.75(75%),
                                                 X'00008000' = 0.50(50%), etc.
                                                 Check SCLAEL_VMDMXSHA to determine
                                                 if Max share is absolute or
                                                 relative.
    112  70  Character    8  SCLAEL_SRMATOD      Artificial TOD. This TOD only
                                                 advances at the rate the system is
                                                 running user work.
    120  78  Character    8  SCLAEL_SRMATOD2     Artificial TOD2. This TOD only
                                                 advances with each CPU's user time
                                                 and each CPU's wait time.
    128  80  Unsigned     4  SCLAEL_VMDCTPVG     Count of private address space
                                                 resident pages in DPA owned by
                                                 this virtual machine which are
                                                 above the 2GB line. Valid only in
                                                 base VMDBK. To get total resident
                                                 pages under the 2GB line, subtract
                                                 this field from SCLAEL_VMDCTPVR.
    132  84  Character    0  SCLAEL_END

    MRSCLAEL Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                   0     20
    MRHDR_END              14      0
    MRHDRDM                 4      1
    MRHDRLEN                0      2
    MRHDRRC                 6      2
    MRHDRTOD                8      8
    MRHDRZER                2      2
    SCLAEL                  0    132
    SCLAEL_CALBASE         2F           80
    SCLAEL_CALCPPST        4C      4
    SCLAEL_CALFLAG1        2F      1
    SCLAEL_CALOSTAT        3B      1
    SCLAEL_CALQSTAT        38      1
    SCLAEL_CALSHARF        68      1
    SCLAEL_END             84      0
    SCLAEL_MRHDR            0      0
    SCLAEL_SRMABSDE        5C      4
    SCLAEL_SRMATOD         70      8
    SCLAEL_SRMATOD2        78      8
    SCLAEL_SRMC1ELG        1C      2
    SCLAEL_SRMC2ELG        1E      2
    SCLAEL_SRMC3ELG        20      2
    SCLAEL_SRMRELDE        60      4
    SCLAEL_VMDABSSH        54      4
    SCLAEL_VMDAUTOL        3B           02
    SCLAEL_VMDCPUAD        22      2
    SCLAEL_VMDCTCRT        64      4
    SCLAEL_VMDCTPVG        80      4
    SCLAEL_VMDCTPVR        44      4
    SCLAEL_VMDCTXBK        48      4
    SCLAEL_VMDDISC         3B           04
    SCLAEL_VMDELIST        39      1
    SCLAEL_VMDEPRTY        3C      8
    SCLAEL_VMDFORCE        3B           10
    SCLAEL_VMDHOTRQ        38           80
    SCLAEL_VMDHOTST        38           40
    SCLAEL_VMDIABIA        38           10
    SCLAEL_VMDLIMTH        68           02
    SCLAEL_VMDLKSHT        38           04
    SCLAEL_VMDLOADU        38           20
    SCLAEL_VMDMXSHA        68           80
    SCLAEL_VMDMXSHR        6C      4
    SCLAEL_VMDNULL         38           01
    SCLAEL_VMDPGBIA        38           08
    SCLAEL_VMDPGRTE        34      4
    SCLAEL_VMDRDYCM        2E      0
    SCLAEL_VMDRELSH        50      4
    SCLAEL_VMDSVMID        24      8
    SCLAEL_VMDSVMWF        2C           80
    SCLAEL_VMDSVMWF        2D           80
    SCLAEL_VMDSVMWF        2E           80
    SCLAEL_VMDSVMWT        2C      1
    SCLAEL_VMDSVMWT        2D      1
    SCLAEL_VMDSVMWT        2E      1
    SCLAEL_VMDSVMW2        2D      0
    SCLAEL_VMDSYSOP        3B           80
    SCLAEL_VMDUFORC        3B           08
    SCLAEL_VMDURRSP        58      4
    SCLAEL_VMDUSER         14      8
    SCLAEL_VMDUSRCT        3B           40
    SCLAEL_VMDWRKCS        3A      1
    SCLAEL_VMDWSSPR        30      4
    SCLAEL_VMDXAUTO        3B           01

    This information is
    based on z/VM V4R4.0.

    Last updated on 22 Jul 2003 at 15:04:23.

    Copyright IBM Corporation, 1990, 2003