Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRUSEINT

Prolog
Control Block Contents
Cross Reference

#### MRUSEINT Prolog

####

####

     DSECT NAME - USEINT
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRUSEINT
     DESCRIPTIVE NAME - Monitor Sample Record
                        Domain 4 - User Domain
                        Record 4 - User Interaction Data
     DESCRIPTION - Describes a VMDBK's use of the system.  Included
                   are such things as its use of IUCV, APPC and the
                   number of times it occupied various queues.  A
                   separate record is generated for each VMDBK defined
                   in the user's virtual complex.
     NOTES:
       - Fields labeled by the prefix, 'USEINT_HF', are high-frequency
         counters.
       - The following is the order of high-frequency counters in which
         the user is tested for its wait state.  If the user is in more
         than one state, it is counted only in the first of the list.
                     USEINT_HFIOWT
                     USEINT_HFCFWT
                     USEINT_HFSIMWT
                     USEINT_HFWTPAG
                     USEINT_HFLLIST
                     USEINT_HFCPUWT
                     USEINT_HFCPURN
                     USEINT_HFESVM
                     USEINT_HFLOAD
                     USEINT_HFDORM
                     USEINT_HFDSVM
                     USEINT_HFIOACT
                     USEINT_HFTIDL
                     USEINT_HFTSVM
                     USEINT_HFPGACT
                     USEINT_HFOTHR

    MRUSEINT Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)          Description

      0   0  Structure  228  USEINT              Start of monitor record
      0   0  Character    0  USEINT_MRHDR        Record header. See MRRECHDR for
                                                 details.
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN            record length in bytes
      2   2  Unsigned     2  MRHDRZER            field of zeros
      4   4  Unsigned     1  MRHDRDM             domain identifier
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC             record identifier
      8   8  Character    8  MRHDRTOD            Time at which this record was
                                                 built. In time-of-day (TOD) clock
                                                 format. See IBM System 370 XA
                                                 Principle of Operation for
                                                 explanation of format.
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END           End of header
     20  14  Character    8  USEINT_VMDUSER      User logon identification
     28  1C  Unsigned     2  USEINT_VMDCPUAD     Processor address
     30  1E  Bitstring    1  USEINT_CALFLAG      Flag byte
              1... ....      USEINT_CALBASE      If on, this is the base VMDBK.
                                                 VMDBASE
              .1.. ....      USEINT_CALTRQFL     If on, there is a TRQ block set
                                                 to either time the user in a sleep
                                                 state for a limited period of time
                                                 or to time 15 minutes before
                                                 logging off a disconnected user
                                                 following an attempted display I/O
                                                 (time bomb logoff).
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
     31  1F  Unsigned     1  *                   Reserved for IBM use
     32  20  Character    4  USEINT_CALINTRN     'YES ' = this VMDBK is currently
                                                 contributing to a transaction. 'NO
                                                 ' = this VMDBK is not currently
                                                 contributing to a transaction.
                                                 'UNDE' = this VMDBK is currently
                                                 idle and may or may not contribute
                                                 to a transaction.
     36  24  Unsigned     4  USEINT_VMDSVMFX     Number of times the SVM-wait
                                                 flag was left on at the end of a
                                                 transaction and had to be
                                                 corrected by the scheduler by
                                                 resetting it.
     40  28  Character    8  USEINT_VMDSVMID     VMDBK name for the last
                                                 successful IUCV, VMCF, or APPC/VM
                                                 Send for this virtual machine.
                                                 Valid in base VMDBK only.
     48  30  Bitstring    1  USEINT_VMDSVMWT     Service-virtual-machine (SVM)
                                                 wait flag byte - valid in base
                                                 VMDBK only.
              1... ....      USEINT_VMDSVMWF     VMDBK is waiting for a response
                                                 from IUCV, VMCF, or APPC.
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
     49  31  Character    0  USEINT_VMDSVMW2     Back-up byte to the VMDSVMWT
                                                 byte. Its contents will persist
                                                 longer than they would in
                                                 VMDSVMWT. Valid in base VMDBK
                                                 only.
     49  31  Bitstring    1  USEINT_VMDSVMWT     Service-virtual-machine (SVM)
                                                 wait flag byte - valid in base
                                                 VMDBK only.
              1... ....      USEINT_VMDSVMWF     VMDBK is waiting for a response
                                                 from IUCV, VMCF, or APPC.
     50  32  Character    0  USEINT_VMDRDYCM     Flag byte set by IUCV, VMCF, or
                                                 APPC whenever IUCV/VMCF/APPC makes
                                                 an external interrupt. It is sort
                                                 of a "reference byte" that tells
                                                 the scheduler that IUCV/VMCF/APPC
                                                 had been active recently. Valid in
                                                 base VMDBK only.
     50  32  Bitstring    1  USEINT_VMDSVMWT     Service-virtual-machine (SVM)
                                                 wait flag byte - valid in base
                                                 VMDBK only.
              1... ....      USEINT_VMDSVMWF     VMDBK is waiting for a response
                                                 from IUCV, VMCF, or APPC.
     51  33  Unsigned     1  *                   Reserved for IBM use
     52  34  Unsigned     4  USEINT_HFQUCT       Number of times VMDBK was high
                                                 frequency sampled.
     56  38  Unsigned     4  USEINT_HFDISP0      Number of times the VMDBK was in
                                                 Q0. VMDSLIST = VMDDISPL and
                                                 VMDELIST = 0.
     60  3C  Unsigned     4  USEINT_HFDISP1      Number of times the VMDBK was in
                                                 Q1. VMDSLIST = VMDDISPL and
                                                 VMDELIST = 1.
     64  40  Unsigned     4  USEINT_HFDISP2      Number of times the VMDBK was in
                                                 Q2. VMDSLIST = VMDDISPL and
                                                 VMDELIST = 2.
     68  44  Unsigned     4  USEINT_HFDISP3      Number of times the VMDBK was in
                                                 Q3. VMDSLIST = VMDDISPL and
                                                 VMDELIST = 3.
     72  48  Unsigned     4  USEINT_HFELIG0      Number of times the VMDBK was in
                                                 E0. VMDSLIST = VMDELIG and
                                                 VMDELIST = 0.
     76  4C  Unsigned     4  USEINT_HFELIG1      Number of times the VMDBK was in
                                                 E1. VMDSLIST = VMDELIG and
                                                 VMDELIST = 1.
     80  50  Unsigned     4  USEINT_HFELIG2      Number of times the VMDBK was in
                                                 E2. VMDSLIST = VMDELIG and
                                                 VMDELIST = 2.
     84  54  Unsigned     4  USEINT_HFELIG3      Number of times the VMDBK was in
                                                 E3. VMDSLIST = VMDELIG and
                                                 VMDELIST = 3.
     88  58  Unsigned     4  USEINT_HFSTCT       Number of times VMDBK was high
                                                 frequency sampled. This was once
                                                 distinguishable from USEINT_HFQUCT
                                                 but is now the same and is
                                                 retained for migration or
                                                 compatibility purposes.
     92  5C  Unsigned     4  USEINT_HFTIDL       Count of times user was found in
                                                 test idle and not in SVM wait
     96  60  Unsigned     4  USEINT_HFTSVM       Count of times user was found in
                                                 test idle and in SVM wait
    100  64  Unsigned     4  USEINT_HFIOWT       Number of times this user was in
                                                 synchronous I/O wait. This I/O
                                                 wait indicates that a guest is
                                                 waiting for I/O completion status
                                                 and thus is prevented from
                                                 running. VMDIOWT
    104  68  Unsigned     4  USEINT_HFCFWT       Number of times this user was
                                                 found in console-function wait.
                                                 During such a wait, the virtual
                                                 cpu is not permitted to run.
                                                 VMDCFWT
    108  6C  Unsigned     4  USEINT_HFSIMWT      Number of times this user was
                                                 found in 'simulation wait' in
                                                 which the CPU is simulating some
                                                 hardware functions such as
                                                 instructions, interrupts, or timer
                                                 updates, and the virtual machine
                                                 is thus prevented from running to
                                                 avoid potential conflicts with the
                                                 simulations. VMDSIMWT
    112  70  Unsigned     4  USEINT_HFWTPAG      Count of times this user was
                                                 found in page wait. Page wait is
                                                 when the current guest instruction
                                                 refers to a guest page which is
                                                 not present in host storage and
                                                 must be brought in from auxiliary
                                                 storage. Page wait prevents the
                                                 virtual CPU from running, however
                                                 it is a "soft wait" condition, and
                                                 as such can be cleared by a guest
                                                 PSW swap. VMDWTPAG
    116  74  Unsigned     4  USEINT_HFCPUWT      Count of times this user was
                                                 found waiting to run on the real
                                                 processor. VMDSTATE = VMDREADY
    120  78  Unsigned     4  USEINT_HFCPURN      Count of times this user was
                                                 found running on the real
                                                 processor. VMDSTATE = VMDISPCH
    124  7C  Unsigned     4  USEINT_HFESVM       Count of times this user was
                                                 found in SVM wait and in the
                                                 eligible list
    128  80  Unsigned     4  USEINT_HFLOAD       Count of times this user was
                                                 considered a loading user.
                                                 VMDLOADU = on and VMDSLIST ^=
                                                 VMDDORM
    132  84  Unsigned     4  USEINT_HFDORM       Count of times this user was
                                                 found dormant. VMDSLIST = VMDDORM
    136  88  Signed       4  USEINT_HFDSVM       Count of times this user was
                                                 found in SVM wait and in the
                                                 dormant list. Note: this count is
                                                 also included in USEINT_HFDORM.
                                                 VMDSVMWF of VMDSVMWT = on and
                                                 VMDSLIST = VMDDORM
    140  8C  Unsigned     4  USEINT_HFOTHR       Count of times this user was not
                                                 found in any of the above states
    144  90  Unsigned     2  USEINT_VMDCNTID     Number of times user was not
                                                 granted a test idle time when it
                                                 went idle in the dispatch list
    146  92  Unsigned     2  USEINT_VMDCTIDL     Number of times this user was
                                                 granted a test idle time when it
                                                 went idle in the dispatch list
    148  94  Unsigned     4  USEINT_VMDDFRWK     Count of 'deferred' work items
                                                 for the VMDBK. A 'deferred' work
                                                 item is an asynchronous task that
                                                 has yet to run. This VMDBK shall
                                                 be prevented from completing its
                                                 logoff until this count is zero,
                                                 i.e., when all such work items
                                                 have been run.
    152  98  Bitstring    1  USEINT_VMDSTATE     Scheduler/Dispatcher State.
                                                 X'63' = Review-suspended. VMDBK is
                                                 in transition to the suspended
                                                 state. X'58' = Review-idle. VMDBK
                                                 is in transition to the idle
                                                 state. X'4D' = VMDBK has been
                                                 selected by dispatcher for
                                                 processing. X'42' = VMDBK is ready
                                                 for selection by dispatcher once
                                                 it goes to the dispatch list.
                                                 X'37' = Test-idle. VMDBK is ready
                                                 for selection by the dispatcher
                                                 but should be dropped from the
                                                 dispatch list when selected the
                                                 next time. X'08' = VMDBK is
                                                 suspended, probably waiting for a
                                                 short-term event to occur. X'00' =
                                                 VMDBK is idle. No work is
                                                 available.
    153  99  Bitstring    1  USEINT_CALOSTAT     Virtual machine operating status
              1... ....      USEINT_VMDSYSOP     User is primary system operator
              .1.. ....      USEINT_VMDUSRCT     User is counted as being logged
                                                 on
              ..1. ....      *
              ...1 ....      USEINT_VMDFORCE     User is to be logged off. This
                                                 may be requested by CP, a forced
                                                 logoff, or user's logoff command.
              .... 1...      USEINT_VMDUFORC     User is forced to logoff the
                                                 system
              .... .1..      USEINT_VMDDISC      User is running disconnected
              .... ..1.      USEINT_VMDAUTOL     AUTOLOG/XAUTOLOG in progress.
                                                 User has been automatically logged
                                                 on. This bit is set off when the
                                                 user's IPL statement is processed,
                                                 or (if there is no IPL to process)
                                                 when the user enters a LOGON
                                                 command from a terminal to
                                                 RECONNECT.
              .... ...1      USEINT_VMDXAUTO     The original command was
                                                 XAUTOLOG. Valid for the base VMDBK
                                                 only (see USEINT_CALBASE).
    154  9A  Bitstring    1  USEINT_CALRSTAT     Reason(s) the dispatched VMDBK
                                                 is not being run
              1... ....      *
              .1.. ....      USEINT_VMDCFWT      VMDBK is in console function
                                                 wait. Either a console function is
                                                 active, or the virtual machine is
                                                 waiting for the remaining VMDBKs
                                                 in the configuration to enter
                                                 console function mode.
              ..1. ....      USEINT_VMDSIMWT     CP is simulating some hardware
                                                 function for the guest such as
                                                 instructions, interrupts, and
                                                 timer updates. Virtual machine is
                                                 prevented from running to avoid
                                                 potential conflicts with the
                                                 simulations.
              ...1 ....      USEINT_VMDIOWT      Instruction waiting for I/O
                                                 status for completion. (May be
                                                 cancelled without loss of system
                                                 integrity.)
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
    155  9B  Bitstring    1  USEINT_CALCWAIT     Console Function Wait control
                                                 flags.
              1... ....      USEINT_VMDSTOP      virtual machine in stop state.
              .1.. ....      USEINT_VMDSLEEP     virtual machine is sleeping.
              ..1. ....      USEINT_VMDCKST      virtual cpu in check stop state.
              ...1 ....      USEINT_VMDDSCWT     virtual machine is in
                                                 disconnected wait mode. I/O was
                                                 attempted to the display and the
                                                 user was disconnected, so a timer
                                                 is set to log the user off if not
                                                 reconnected within 15 minutes.
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
    156  9C  Unsigned     2  USEINT_VMDCPRMD(4)  Number of times this user was
                                                 was pre-emptied from the dispatch
                                                 list (Q0, Q1, Q2, Q3) due to a
                                                 requirement for storage for E1
                                                 users
    164  A4  Unsigned     2  USEINT_VMDCWSGD(4)  Number of times this user was
                                                 removed from the dispatch list
                                                 (Q0, Q1, Q2, Q3) because it
                                                 reached its working set size
                                                 growth limit, and its new working
                                                 set size would no longer fit
                                                 available storage.
    172  AC  Unsigned     2  USEINT_VMDCETSD(4)  Number of times this user was
                                                 removed from the dispatch list
                                                 (Q0, Q1, Q2, Q3) because it
                                                 reached elapsed time slice end.
    180  B4  Unsigned     2  USEINT_VMDCIDLD(4)  Number of times this user was
                                                 removed from the dispatch list
                                                 (Q0, Q1, Q2, Q3) because its test
                                                 idle time had expired or because
                                                 it was granted no test idle time
    188  BC  Character    8  USEINT_VMDDQTOD     Time of day clock at the time
                                                 that the VMDBK was dropped from
                                                 the dispatch list
    196  C4  Character    8  USEINT_VMDSUSCK     Time of day clock at the time
                                                 the VMDBK was last marked
                                                 suspended
    204  CC  Character    8  USEINT_VMDMTTOD     Time of day clock when the last
                                                 transaction started. Valid for the
                                                 base VMDBK only (see
                                                 USEINT_CALBASE).
    212  D4  Unsigned     4  USEINT_HFIOACT      High Frequency Count. Cardinal
                                                 number of times the user had an
                                                 asynchronous I/O outstanding,
                                                 causing the user to be left in the
                                                 dispatch list. VMDIOACT
    216  D8  Unsigned     4  USEINT_HFLLIST      High Frequency Count. Number of
                                                 times the user was in dispatch
                                                 list waiting for CPU but was on
                                                 the Limit List, prevented from
                                                 running by max share.
    220  DC  Unsigned     4  USEINT_HFPGACT      High Frequency Count. Number of
                                                 times the virtual machine had page
                                                 fault requests active, but was not
                                                 in page wait (VMDWTPAG was not
                                                 set). This would occur if
                                                 asynchronous page fault was being
                                                 used and there was an outstanding
                                                 page fault, but the virtual
                                                 machine loaded a wait state
                                                 because it had no other work to
                                                 do. A virtual machine can have
                                                 page faults handled asynchronously
                                                 if using the PAGEX feature or the
                                                 Page-Fault Handshaking CP services
                                                 via the CP PFAULT MACRO.
    224  E0  Signed       2  USEINT_VMDSLCNT     Count of minor time slices that
                                                 have expired since the start of
                                                 current transaction.
    226  E2  Unsigned     2  *                   Reserved and available for IBM
                                                 use.
    228  E4  Character    0  USEINT_END

    MRUSEINT Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                   0     20
    MRHDR_END              14      0
    MRHDRDM                 4      1
    MRHDRLEN                0      2
    MRHDRRC                 6      2
    MRHDRTOD                8      8
    MRHDRZER                2      2
    USEINT                  0    228
    USEINT_CALBASE         1E           80
    USEINT_CALCWAIT        9B      1
    USEINT_CALFLAG         1E      1
    USEINT_CALINTRN        20      4
    USEINT_CALOSTAT        99      1
    USEINT_CALRSTAT        9A      1
    USEINT_CALTRQFL        1E           40
    USEINT_END             E4      0
    USEINT_HFCFWT          68      4
    USEINT_HFCPURN         78      4
    USEINT_HFCPUWT         74      4
    USEINT_HFDISP0         38      4
    USEINT_HFDISP1         3C      4
    USEINT_HFDISP2         40      4
    USEINT_HFDISP3         44      4
    USEINT_HFDORM          84      4
    USEINT_HFDSVM          88      4
    USEINT_HFELIG0         48      4
    USEINT_HFELIG1         4C      4
    USEINT_HFELIG2         50      4
    USEINT_HFELIG3         54      4
    USEINT_HFESVM          7C      4
    USEINT_HFIOACT         D4      4
    USEINT_HFIOWT          64      4
    USEINT_HFLLIST         D8      4
    USEINT_HFLOAD          80      4
    USEINT_HFOTHR          8C      4
    USEINT_HFPGACT         DC      4
    USEINT_HFQUCT          34      4
    USEINT_HFSIMWT         6C      4
    USEINT_HFSTCT          58      4
    USEINT_HFTIDL          5C      4
    USEINT_HFTSVM          60      4
    USEINT_HFWTPAG         70      4
    USEINT_MRHDR            0      0
    USEINT_VMDAUTOL        99           02
    USEINT_VMDCETSD        AC      8
    USEINT_VMDCFWT         9A           40
    USEINT_VMDCIDLD        B4      8
    USEINT_VMDCKST         9B           20
    USEINT_VMDCNTID        90      2
    USEINT_VMDCPRMD        9C      8
    USEINT_VMDCPUAD        1C      2
    USEINT_VMDCTIDL        92      2
    USEINT_VMDCWSGD        A4      8
    USEINT_VMDDFRWK        94      4
    USEINT_VMDDISC         99           04
    USEINT_VMDDQTOD        BC      8
    USEINT_VMDDSCWT        9B           10
    USEINT_VMDFORCE        99           10
    USEINT_VMDIOWT         9A           10
    USEINT_VMDMTTOD        CC      8
    USEINT_VMDRDYCM        32      0
    USEINT_VMDSIMWT        9A           20
    USEINT_VMDSLCNT        E0      2
    USEINT_VMDSLEEP        9B           40
    USEINT_VMDSTATE        98      1
    USEINT_VMDSTOP         9B           80
    USEINT_VMDSUSCK        C4      8
    USEINT_VMDSVMFX        24      4
    USEINT_VMDSVMID        28      8
    USEINT_VMDSVMWF        30           80
    USEINT_VMDSVMWF        31           80
    USEINT_VMDSVMWF        32           80
    USEINT_VMDSVMWT        30      1
    USEINT_VMDSVMWT        31      1
    USEINT_VMDSVMWT        32      1
    USEINT_VMDSVMW2        31      0
    USEINT_VMDSYSOP        99           80
    USEINT_VMDUFORC        99           08
    USEINT_VMDUSER         14      8
    USEINT_VMDUSRCT        99           40
    USEINT_VMDXAUTO        99           01

    This information is
    based on z/VM V4R4.0.

    Last updated on 22 Jul 2003 at 15:04:23.

    Copyright IBM Corporation, 1990, 2003