LGNBK - 64-bit CP - V4R4.0

Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### LGNBK

Prolog

Control Block Contents
LGNBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### LGNBK Prolog

     NAME       : HCPLGNBK
     DESCRIPTION: LOGON work buffer
     DSECT      : LGNBK
     FUNCTION   : Used by the LOGON/(X)AUTOLOG code as a work area
                  for LOGON/(X)AUTOLOG processing.
     LOCATED BY : NONE
     CREATED BY : HCPAUT   HCPLOG
     DELETED BY : HCPLGB

#### LGNBK Control Block Content

#### LGNBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      LGNBK          LOGON work buffer
    0000    0 Signed       4 LGNFLGS (0)    Parameter flags for logon
    0000    0 Bitstring    1 LGNFLAG        Command line option flag 1
              1... ....      LGNAUTO        X'80' An AUTOLOG command in
                                            process
              .1.. ....      LGNNOIPL       X'40' No system IPL to be
                                            performed
              ..1. ....      LGNAPL         X'20' APL option specified
              ...1 ....      LGNTEXT        X'10' TEXT option specified
              .... 1...      LGNQUIET       X'08' QUIET option specified
              .... .1..      LGNDATA        X'04' Data line present with
                                            command
              .... ..1.      LGNIPL         X'02' IPL option specified
              .... ...1      LGNNORUN       X'01' NORUN option specified
    0001    1 Bitstring    1 LGNFLAG2       Command line option flag 2
              1... ....      LGNPASS        X'80' PASSWORD option specified
              .1.. ....      LGNPROMT       X'40' PROMPT option specified
              ..1. ....      LGNDIRCT       X'20' DIRECTORY option specified
              ...1 ....      LGNHERE        X'10' HERE option specified
              .... 1...      LGNSYNCH       X'08' SYNCH option specified
              .... .1..      LGNMASK        X'04' Mask option specified
              .... ..1.      LGNSECLB       X'02' SECLABEL option specified
              .... ...1      LGNMCH         X'01' MACHINE option specified
    0002    2 Bitstring    1 LGNFLAG3       Program execution flag 1
              1... ....      LGNNOFAT       X'80' Nonfatal error - return to
                                            caller
              .1.. ....      LGNRECON       X'40' User to be reconnected
              ..1. ....      LGNMAXU        X'20' This user is allowed to
                                            LOGON even if the maxusers limit
                                            has been exceeded.
              ...1 ....      LGNIS663       X'10' Issued message 663 to user
                                            already
              .... 1...      LGNASYNC       X'08' Processing Asynchronous
                                            XAUTOLOG
              .... ..1.      LGNALOGS       X'02' Autolog process - first
                                            pass through (X)AUTOLOG/LOGON
                                            modules
              .... ...1      LGNDLOCK       X'01' User directory entry is
                                            locked
    0003    3 Bitstring    1 LGNFLAG4       Program execution flag 2
              1... ....      LGNDFRWK       X'80' Indicates that the deferred
                                            work counter for target VMDBK of
                                            a reconnect has been incremented.
              .1.. ....      LGNDEV         X'40' ON option specified
              ..1. ....      LGNLDEV        X'20' Logical device address
                                            supplied
              ...1 ....      LGNNOCSA       X'10' Indicate no CSABK or domain
              .... 1...      LGNNOCRY       X'08' Indicate no real crypto
                                            facility
              .... .1..      LGNNOCMD       X'04' Indicates this is a dummy
                                            logon from the LOGO panel.
              .... ..1.      LGNNAUDT       X'02' Indicates that
                                            LOGON/(X)AUTOLOG has gone far
                                            enough that HCPLGALF should no
                                            longer be called.
              .... ...1      LGNNOPAS       X'01' Password=NOPASS in the
                                            directory.
    0004    4 Bitstring    1 LGNFLAG5       Logon work area flag 5
              1... ....      LGNAUTH        X'80' User passed password(ESM)
                                            check so we need to call HCPJRLOG
              .1.. ....      LGNBADPW       X'40' User fail password(ESM)
                                            check so we need to call HCPJRLPW
              ..1. ....      LGNPRMPT       X'20' Causes HCPLGALF to display
                                            logon prompt on exit.
              ...1 ....      LGNNOPMT       X'10' Do not force the user even
                                            though we should not display the
                                            logon prompt.
              .... 1...      LGNLOGBY       X'08' A BYUSER entered the LOGON
                                            command
              .... .1..      LGNADJ         X'04' Adjunct virtual machine
                                            logon
    0005    5 Bitstring    1 LGNCMD
              00000004       LGNLOGON       X'04' This is a LOGON command
              00000008       LGNAUTOL       X'08' This is an AUTOLOG command
              0000000C       LGNXAUT        X'0C' This is a CLASS A or B
                                            XAUTOLOG
              00000010       LGNXAUTG       X'10' This is a CLASS G XAUTOLOG
              00000014       LGNAUTSI       X'14' This is a system
                                            initialization autolog.
              00000018       LGNAUTPR       X'18' This is a TSAF private
                                            server autolog.
              0000001C       LGNLOGOP       X'1C' This is the operator
                                            logging on system initialization.
    0006    6 Bitstring    1 LGNMLVL
              1... ....      VMDMSGON       X'80' CONTROLS WHETHER MESSAGES
                                            SENT BY OTHER USERS ARE
                                            DISPLAYED. (CONTROLLED BY THE SET
                                            MSG OR TERMINAL MSG COMMANDS)
              .1.. ....      VMDWNGON       X'40' CONTROLS WHETHER MESSAGES
                                            SENT USING THE WARNING COMMAND
                                            ARE DISPLAYED. (CONTROLLED BY THE
                                            SET WNG OR TERMINAL WNG COMMANDS)
              ..1. ....      VMDMCODE       X'20' CONTROLS ERROR MESSAGE
                                            DISPLAY OF THE ERROR MESSAGE
                                            CODE. (CONTROLLED BY THE SET EMSG
                                            OR TERMINAL EMSG COMMANDS)
              ...1 ....      VMDMTEXT       X'10' CONTROLS ERROR MESSAGE
                                            DISPLAY OF THE ERROR MESSAGE
                                            TEXT. (CONTROLLED BY THE SET EMSG
                                            OR TERMINAL EMSG COMMANDS)
              .... 1...      VMDSPMSG       X'08' CONTROLS WHETHER SPECIAL
                                            MESSAGES SENT BY OTHER USERS CAN
                                            BE RECEIVED. (CONTROLLED BY THE
                                            SET SMSG COMMAND)
              .... .1..      VMDMIMSG       X'04' CONTROLS THE DISPLAY OF
                                            SELECTED CP COMMAND INFORMATIONAL
                                            RESPONSES. IF SET THE RESPONSES
                                            ARE DISPLAYED, IF NOT THE
                                            RESPONSES WILL NOT BE DISPLAYED.
                                            (CONTROLLED BY THE SET IMSG AND
                                            TERMINAL IMSG COMMANDS)
              .... ...1      VMDMCNFG       X'01' Message level set from
                                            system configuration file
    0007    7 Bitstring    1 *              Reserved for IBM use
    0008    8 Character    8 LGNACNUM       Account number
    0010   16 Signed       4 LGNILEN        IPL command length
    0014   20 Address      4 LGNIADDR       IPL command address
    0018   24 Address      4 LGNDVMD        Directory buffer address
    001C   28 Address      4 LGNCDATA       Pointer to console input data.
    0020   32 Signed       4 LGNCDATL       Length of console input data.
    0028   40 Dbl-Word     8 LGNKSTOR       Storage size in K
    0028   40 Signed       4 LGNKSTR0       High word of LGNKSTOR
    002C   44 Signed       4 LGNKSTR1       Low word of LGNLSTOR
    0030   48 Character    3 LGNMACH        Machine setting (i.e. 370, etc)
    0033   51 Bitstring    1 LGNDDEF        Maps to DVMDDEF
              1... ....      DVMDXSTR       X'80' EXTENDED STORAGE FACILITY
                                            ALLOWED
              .1.. ....      DVMDNOP        X'40' 'NOPDATA' STATEMENT IN
                                            ENTRY
              ..1. ....      DVMDNLG        X'20' VIRTUAL MACHINE'S PSWD IS
                                            NOLOG
              ...1 ....      DVMDVXC        X'10' GUEST IS A VIRTUAL ESA/XC
                                            MACHINE
              .... 1...      DVMDVESA       X'08' GUEST IS A VIRTUAL ESA
              .... .1..      DVMDYES        X'04' USER HAS AT LEAST ONE DDEV
              .... ..1.      DVMDVXA        X'02' GUEST IS A VIRTUAL XA
              .... ...1      DVMDV370       X'01' GUEST IS A VIRTUAL 370
    0034   52 Signed       4 LGNVMDBK       VMDBK address of target VMDBK for
                                            a reconnect.
    0038   56 Signed       4 LGNTODON       VMDTODON of the target VMDBK for
                                            a reconnect.
    003C   60 Address      4 LGNEFTID       The address of the effective
                                            userid that is causing a LGNAUTPR
                                            autolog to be done.
         This following is the paramter section for HCPRPWRD.
    0040   64 Dbl-Word     8 LGNPWDPM (0)   Parameters for HCPPWDRD
    0040   64 Address      4 LGNPWDIN       Address of input password area
    0044   68 Address      4 LGNPWDPP       Address of the password prompt
    0048   72 Bitstring    1 LGNPWLEN       Password length
         The following byte is to manage the fretting for the LGNBK and its
         related control blocks. It is zero if this process should not fret the
         LGNBK and is X'FF' if this process should fret the LGNBK. It is updated
         with TEST AND SET.
    0049   73 Bitstring    1 LGNFRET        Fret byte
    004A   74 Signed       2 LGNDEVNO       Console device number
    004C   76 Character  139 LGNBUFF        Message buffer (see description
                                            on the next page)
    00D7  215 Bitstring    1 *              Alignment
    00D8  216 Character    5 LGNLNG         Language ID Work Area for HCPLGN
    00DD  221 Bitstring    3 *              Reserved for IBM use
    00E0  224 Dbl-Word     8 LGNACIPM (0)   Area for ACIPARMS
              0000001C       LGNBKL         (*-LGNBK+7)/8 Size of LGNBK in
                                            doublewords
         LGNBUFF - Buffer/work area for constructing message substitution data.
         The first field in this area (MSGPDUID) contains the userid padded with
         blanks (if necessary) of the user being logged on. This field is
         constructed from the userid on the command line and is preserved
         throughout the process of logging on the user. It is used for a couple
         of purposes. First, it is used as input to all routines requiring a
         userid (such as HCPUDR). Second, it is used as substitution data for
         the "tag" placed on messages issued for the asynchronous XAUTOLOG
         command. For this reason, it is immediately followed by a delimiter
         (initially set to X'FF').
         Immediately following MSGPDUID and its delimiter (MSGPUDLM), all other
         substitution data for "tagged" and untagged messages are constructed.
         This area is labelled MSGSUB. The first field (that is always
         constructed at the same time as MSGPDUID) is MSGUID, which contains the
         userid with trailing blanks removed. It is delimited with X'FF'. This
         the most common substitution data in messages issued by these modules.
         This field should not be overlaid when issueing non-fatal messages
         because it may be required by a subsequent fatal error message.
         For fatal error messages having substitution data other than the
         userid, the substitution data should be constructed starting at label
         MSGSUB (overlaying the userid). This area may be redefined in a
         particular module for various messages to be issued by the module. This
         is done in the module by placing the local definitions following this
         mapping and using an ORG MSGSUB in front of the definition(s) for each
         message.
         For non-fatal (informational) messages, MSGUID should not be overlaid.
         In these cases, start building the substitution data at label MSGODATA.
         Use of the message buffer area:
         - For "tagged" asynchronous XAUTOLOG messages with no substitution data
         other than in the tag, point R1 to the field MSGPDUID.
         - For "tagged" asynchronous XAUTOLOG messages with substitution data in
         the basic message text, change the delimiter MSGPUDLM to X'00' and
         point R1 to the field MSGPDUID.
         - For untagged error messages with substitution data, point R1 to the
         field MSGSUB.
         - For informational (non-fatal) messages with substitution data, point
         R1 to the field MSGODATA.
    004C   76 Character    8 LGNPDUID       Padded userid
    0054   84 Character    1 LGNPUDLM       Userid delimiter
    0055   85 Character    1 LGNSUB (0)     Message substitution fields
    0055   85 Character    8 LGNUID         Non-padded userid for messages
    005D   93 Character    1 LGNUIDLM       Userid delimiter
    005E   94 Character    1 LGNODATA (0)   Other substitution data
         Some overlays used by different messages.
    0055   85 Character    8 LGNLUNAM       LUNAME
    005D   93 Character    1 LGNLUEND       Message substitution end
                                            delimiter
    0055   85 Character    5 LGNDVADR       Device address
    005A   90 Character    1 LGNDVEND       Message substitution end
                                            delimiter
    0055   85 Character    8 LGNSYSNM       "Other" system name
    005D   93 Character    1 LGNSYSND       Message substitution end
                                            delimiter Substitutions unique to
                                            message 1513
    0055   85 Character    4 LGN13DNA       Device name
    0059   89 Character    1 LGN13DL1       Substitution delimiter
    005A   90 Character    5 LGN13DNU       Device number
    005F   95 Character    1 LGN13END       Message substitution end
                                            delimiter
         Here are some constants used by logon.
              .... .1..      LGNLIMIT       X'04' Number of LOGON cmds before
                                            a skeleton is forced.
              .... ...1      LGNPWLMT       X'01' Number of times to prompt
                                            for a password.

#### LGNBK Storage Layout

    *** LGNBK - LOGON work buffer
    *
    *     +------+------+------+------+------+------+------+------+
    *   0 |:FLAG |:FLAG2|:FLAG3|:FLAG4|:FLAG5|LGNCMD|:MLVL |//////|
    *     +------+------+------+------+------+------+------+------+
    *   8 |                       LGNACNUM                        |
    *     +---------------------------+---------------------------+
    *  10 |         LGNILEN           |         LGNIADDR          |
    *     +---------------------------+---------------------------+
    *  18 |         LGNDVMD           |         LGNCDATA          |
    *     +---------------------------+---------------------------+
    *  20 |         LGNCDATL          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  28 |                       LGNKSTOR                        |
    *     +-------------------------------------------------------+
    *  30
    *
    *** LGNBK - LOGON work buffer

    *** Overlay for LGNKSTOR in LGNBK
    *
    *     +---------------------------+---------------------------+
    *  28 |         LGNKSTR0          |         LGNKSTR1          |
    *     +--------------------+------+---------------------------+
    *  30 |      LGNMACH       |:DDEF |         LGNVMDBK          |
    *     +--------------------+------+---------------------------+
    *  38 |         LGNTODON          |         LGNEFTID          |
    *     +---------------------------+---------------------------+
    *  40 |         LGNPWDIN          |         LGNPWDPP          |
    *     +------+------+-------------+---------------------------+
    *  48 |:PWLEN|:FRET |  LGNDEVNO   |                           |
    *     +------+------+-------------+                           |
    *  50 |                                                       |
    *     =                       LGNBUFF                         =
    *     |                                                +------+
    *  D0 |                                                |//////|
    *     +----------------------------------+-------------+------+
    *  D8 |             LGNLNG               |////////////////////|
    *     +----------------------------------+--------------------+
    *
    *** Overlay for LGNKSTOR in LGNBK

    *** Overlay for LGNBUFF in LGNBK
    *
    *                                 +---------------------------+
    *     ...                      4C |        LGNPDUID-          |
    *     +---------------------------+------+--------------------+
    *  50 |          -(04C)           |:PUDLM|      (055)-        |
    *     +---------------------------+------+------+-------------+
    *  58 |             -LGNUID              |:UIDLM|
    *     +----------------------------------+------+
    *
    *** Overlay for LGNBUFF in LGNBK

    *** Overlay for LGNSUB in LGNBK
    *
    *                                        +--------------------+
    *     ...                             55 |      (055)-        |
    *     +----------------------------------+------+-------------+
    *  58 |            -LGNLUNAM             |:LUEND| 5E
    *     +----------------------------------+------+
    *
    *** Overlay for LGNSUB in LGNBK

    *** Overlay for LGNSUB in LGNBK
    *
    *                                        +--------------------+
    *     ...                             55 |     LGNDVADR-      |
    *     +-------------+------+-------------+--------------------+
    *  58 |   -(055)    |:DVEND| 5B
    *     +-------------+------+
    *
    *** Overlay for LGNSUB in LGNBK

    *** Overlay for LGNSUB in LGNBK
    *
    *                                        +--------------------+
    *     ...                             55 |      (055)-        |
    *     +----------------------------------+------+-------------+
    *  58 |            -LGNSYSNM             |:SYSND| 5E
    *     +----------------------------------+------+
    *
    *** Overlay for LGNSUB in LGNBK

    *** Overlay for LGNSUB in LGNBK
    *
    *                                        +--------------------+
    *     ...                             55 |     LGN13DNA-      |
    *     +------+------+--------------------+-------------+------+
    *  58 |-(055)|:13DL1|            LGN13DNU              |:13END|
    *     +------+------+----------------------------------+------+
    *  60
    *
    *** Overlay for LGNSUB in LGNBK

#### LGNBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    DVMDNLG        0033 20
    DVMDNOP        0033 40
    DVMDVESA       0033 08
    DVMDVXA        0033 02
    DVMDVXC        0033 10
    DVMDV370       0033 01
    DVMDXSTR       0033 80
    DVMDYES        0033 04
    LGNACIPM       00E0
    LGNACNUM       0008
    LGNADJ         0004 04
    LGNALOGS       0002 02
    LGNAPL         0000 20
    LGNASYNC       0002 08
    LGNAUTH        0004 80
    LGNAUTO        0000 80
    LGNAUTOL       0005 00000008
    LGNAUTPR       0005 00000018
    LGNAUTSI       0005 00000014
    LGNBADPW       0004 40
    LGNBKL         00E0 0000001C
    LGNBUFF        004C
    LGNCDATA       001C
    LGNCDATL       0020
    LGNCMD         0005
    LGNDATA        0000 04
    LGNDDEF        0033
    LGNDEV         0003 40
    LGNDEVNO       004A
    LGNDFRWK       0003 80
    LGNDIRCT       0001 20
    LGNDLOCK       0002 01
    LGNDVADR       0055
    LGNDVEND       005A
    LGNDVMD        0018
    LGNEFTID       003C
    LGNFLAG        0000
    LGNFLAG2       0001
    LGNFLAG3       0002
    LGNFLAG4       0003
    LGNFLAG5       0004
    LGNFLGS        0000
    LGNFRET        0049
    LGNHERE        0001 10
    LGNIADDR       0014
    LGNILEN        0010
    LGNIPL         0000 02
    LGNIS663       0002 10
    LGNKSTOR       0028
    LGNKSTR0       0028
    LGNKSTR1       002C
    LGNLDEV        0003 20
    LGNLIMIT       005F 04
    LGNLNG         00D8
    LGNLOGBY       0004 08
    LGNLOGON       0005 00000004
    LGNLOGOP       0005 0000001C
    LGNLUEND       005D
    LGNLUNAM       0055
    LGNMACH        0030
    LGNMASK        0001 04
    LGNMAXU        0002 20
    LGNMCH         0001 01
    LGNMLVL        0006
    LGNNAUDT       0003 02
    LGNNOCMD       0003 04
    LGNNOCRY       0003 08
    LGNNOCSA       0003 10
    LGNNOFAT       0002 80
    LGNNOIPL       0000 40
    LGNNOPAS       0003 01
    LGNNOPMT       0004 10
    LGNNORUN       0000 01
    LGNODATA       005E
    LGNPASS        0001 80
    LGNPDUID       004C
    LGNPRMPT       0004 20
    LGNPROMT       0001 40
    LGNPUDLM       0054
    LGNPWDIN       0040
    LGNPWDPM       0040
    LGNPWDPP       0044
    LGNPWLEN       0048
    LGNPWLMT       005F 01
    LGNQUIET       0000 08
    LGNRECON       0002 40
    LGNSECLB       0001 02
    LGNSUB         0055
    LGNSYNCH       0001 08
    LGNSYSND       005D
    LGNSYSNM       0055
    LGNTEXT        0000 10
    LGNTODON       0038
    LGNUID         0055
    LGNUIDLM       005D
    LGNVMDBK       0034
    LGNXAUT        0005 0000000C
    LGNXAUTG       0005 00000010
    LGN13DL1       0059
    LGN13DNA       0055
    LGN13DNU       005A
    LGN13END       005F
    VMDMCNFG       0006 01
    VMDMCODE       0006 20
    VMDMIMSG       0006 04
    VMDMSGON       0006 80
    VMDMTEXT       0006 10
    VMDSPMSG       0006 08
    VMDWNGON       0006 40

This information is based on z/VM V4R4.0. Last updated on 30 Jul 2003 at 12:55:27 EDT.
Copyright IBM Corporation, 1990, 2003