MCRBK - 32-bit CP - V4R4.0

Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### MCRBK

Prolog

Control Block Contents
MCRBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### MCRBK Prolog

     NAME       : HCPMCRBK
     DESCRIPTION: Machine Check Record Block
     DSECT      : MCRBK
     FUNCTION   : HCPMCRBK contains information relative to a
                  machine check incident which (incident) is to be
                  reflected to a guest.
     LOCATED BY : Is a mapping of the parameters passed for
                  manufacturing a machine check or building the
                  message information when communicating a machine
                  check incident.
     CREATED BY : Any caller who wants to pass a machine check record
                  information.
     DELETED BY : The caller who creates it or the callee. This is
                  communicated via MCRFLAG1 in this control block.

#### MCRBK Control Block Content

#### MCRBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      MCRBK          Machine Check Record Block
    0000    0 Dbl-Word     8 MCRMCIC (0)    Machine Check Interruption Code
    0000    0 Signed       4 MCRMCWD0 (0)   MCRMCIC word 0
    0000    0 Bitstring    2 MCRMCB01 (0)   MCRMCIC byte 0 and 1
    0000    0 Bitstring    1 MCRMCIC0       MCRMCIC byte 0
              1111 1111      MCIPRIM0       X'FF' PRIMARY MACHINE CHECK BITS
                                            - BYTE 0
              1... ....      MCICSD         X'80' SYSTEM DAMAGE BIT.
              .1.. ....      MCICPD         X'40' PROCESSING DAMAGE BIT.
              ..1. ....      MCICSR         X'20' SYSTEM RECOVERY BIT.
              ...1 ....      MCICITD        X'10' INTERVAL TIMER DAMAGE. (370
                                            GUESTS)
              .... 1...      MCICCD         X'08' TIMING (CLOCK) FACILITY
                                            DAMAGE.
              .... .1..      MCICED         X'04' EXTERNAL DAMAGE.
              .... ..1.      MCICVFF        X'02' VECTOR FACILITY FAILURE
              .... ...1      MCICDG         X'01' DEGRADATION BIT.
    0001    1 Bitstring    1 MCRMCIC1       MCRMCIC byte 1
              1111 ....      MCIPRIM1       X'F0' PRIMARY MACHINE CHECK BITS
                                            - BYTE 1
              1... ....      MCICW          X'80' WARNING BIT.
              .1.. ....      MCICCRW        X'40' PENDING-CRW REPORT.
              ..1. ....      MCICSP         X'20' SERVICE PROCESSOR DAMAGE.
              ...1 ....      MCICCSD        X'10' CHANNEL-SUBSYSTEM DAMAGE.
              .... .1..      MCICVFS        X'04' VECTOR FACILITY SOURCE
              .... ..1.      MCICBU         X'02' 'BACKED UP' BIT.
              .... ...1      MCICDL         X'01' 'DELAYED' BIT. (370 GUESTS)
    0002    2 Bitstring    1 MCRMCIC2       MCRMCIC byte 2
              1... ....      MCICSE         X'80' STORAGE ERROR UNCORRECTED.
              .1.. ....      MCICSC         X'40' STORAGE ERROR CORRECTED.
              ..1. ....      MCICKE         X'20' STORAGE-KEY ERROR
                                            UNCORRECTED.
              ...1 ....      MCICSDG        X'10' STORAGE DEGRADATION.
                                            MODIFIES STORAGE ERROR CORRECTED.
              .... 1...      MCICVWP        X'08' BITS 12-15 OF MC OLD PSW
                                            VALID.
              .... .1..      MCICVMS        X'04' SYSTEM MASK & KEY OF MC OLD
                                            PSW VALID.
              .... ..1.      MCICVPM        X'02' PROGRAM MASK & CC OF MC OLD
                                            PSW VALID.
              .... ...1      MCICVIA        X'01' INSTR ADDR OF MC OLD PSW IS
                                            VALID.
    0003    3 Bitstring    1 MCRMCIC3       MCRMCIC byte 3
              1... ....      MCICVFA        X'80' FAILING STORAGE ADDRESS IS
                                            VALID.
              ..1. ....      MCICVED        X'20' EXTERNAL-DAMAGE CODE IS
                                            VALID.
              ...1 ....      MCICVFP        X'10' FP REGISTERS STORED ARE
                                            VALID.
              .... 1...      MCICVGR        X'08' GP REGISTERS STORED ARE
                                            VALID.
              .... .1..      MCICVCR        X'04' CONTROL REGISTERS STORED
                                            VALID.
              .... ..1.      MCICVLG        X'02' EXTENDED LOGOUT AREA IS
                                            VALID.
              .... ...1      MCICVST        X'01' INST. MODIFIED STORAGE IS
                                            VALID.
    0004    4 Signed       4 MCRMCWD1 (0)   MCRMCIC word 1
    0004    4 Bitstring    1 MCRMCIC4       MCRMCIC byte 4
              1... ....      MCICIE         X'80' INDIRECT STORAGE ERROR
              .1.. ....      MCICVAR        X'40' ACCESS REGISTERS STORED ARE
                                            VALID
              ..1. ....      MCICDA         X'20' DELAYED ACCESS EXCEPTION
                                            BIT
    0005    5 Bitstring    1 MCRMCIC5       MCRMCIC byte 5
              ...1 ....      MCICVXFP       X'10' Additional FP Registers
                                            Validity (ESA390) FP Control
                                            Register Validity (ESAME)
              .... 1...      MCICAR         X'08' Ancillary Report Bit
              .... ..1.      MCICVCT        X'02' CPU TIMER STORED IS VALID.
              .... ...1      MCICVCC        X'01' CLOCK COMPARATOR STORED IS
                                            VALID.
    0006    6 Bitstring    1 MCRMCIC6       MCRMCIC byte 6
    0007    7 Bitstring    1 MCRMCIC7       MCRMCIC byte 7
    0008    8 Signed       4 *
    000C   12 Signed       4 MCREDC (0)     Machine check external-damage
                                            code
    000C   12 Bitstring    1 MCREDCB0       MCREDC byte 0
              .... ....      MCEXTD0        X'00' No bits defined
    000D   13 Bitstring    1 MCREDCB1       MCREDC byte 1
              1... ....      MCEXTDXN       X'80' Bit 8 - Extended storage
                                            not operational
              .1.. ....      MCEXTDXF       X'40' Bit 9 - Extended storage
                                            control failure
    000E   14 Bitstring    1 MCREDCB2       MCREDC byte 2
              1... ....      MCEXTDPS       X'80' Bit 16 - Primary-Sync
                                            Damage
              .1.. ....      MCEXTDEA       X'40' Bit 17 - ETR Attachement
                                            Damage
              ..1. ....      MCEXTDSL       X'20' Bit 18 - Switch to local
              ...1 ....      MCEXTDES       X'10' Bit 19 - ETR Sync check
    000F   15 Bitstring    1 MCREDCB3       MCREDC byte 3
              .... ....      MCEXTD3        X'00' No bits defined
    0010   16 Signed       4 MCRMCICX       Machine check interruption code
                                            extension
    0014   20 Bitstring    1 MCRFLAG1       Flag byte 1
              1... ....      MCRREAL        X'80' Failing storage address is
                                            real. If this bit is zero the
                                            failing storage address (if
                                            specified) is absolute. This bit
                                            is meaningful only when the
                                            MCRNULLA bit is 0.
              .1.. ....      MCRRELST       X'40' MCRBK storage is to be
                                            released by the guest machine
                                            service routines when this
                                            machine check is presented.
              ..1. ....      MCRNULLA       X'20' Indicates that
                                            MCRFSAD/MCRGFAD contains a null
                                            address
    0015   21 Bitstring    1 *              Reserved for IBM use.
    0016   22 Bitstring    1 *              Reserved for IBM use.
    0017   23 Bitstring    1 *              Reserved for IBM use
    0018   24 Dbl-Word     8 MCRFLOG (2)    Fixed logout area
    0028   40 Dbl-Word     8 MCRGFAD (0)    ESAME 64 bit failing stor addr
    0028   40 Signed       4 MCR64HI        High order 32 bits of 64 bit addr
    002C   44 Signed       4 MCRFSAD        Guest failing storage address
              0000002C       MCR64LO        MCRFSAD Low order 32 bits of 64
                                            bit addr
              00000030       MCRLEN         *-MCRBK MCRBK block size in bytes
              00000006       MCRSIZE        (MCRLEN+7)/8 MCRBK block size in
                                            doublewords
    0018   24 Dbl-Word     8 MCRFASIT       Failing-storage internal ASIT
    0000    0 Bitstring    2 *
    0002    2 Bitstring    4 MCRMCB25       MCRMCIC bytes 2-5
    0006    6 Bitstring    2 *

#### MCRBK Storage Layout

    *** MCRBK - Machine Check Record Block
    *
    *     +------+------+------+------+------+------+------+------+
    *   0 |:MCIC0|:MCIC1|:MCIC2|:MCIC3|:MCIC4|:MCIC5|:MCIC6|:MCIC7|
    *     +------+------+------+------+------+------+------+------+
    *   8 |///////////////////////////|:EDCB0|:EDCB1|:EDCB2|:EDCB3|
    *     +---------------------------+------+------+------+------+
    *  10 |         MCRMCICX          |:FLAG1|//////|//////|//////|
    *     +---------------------------+------+------+------+------+
    *  18 |                       MCRFLOG                         |
    *     |                                                       |
    *     +---------------------------+---------------------------+
    *  28 |         MCR64HI           |         MCRFSAD           |
    *     +---------------------------+---------------------------+
    *  30
    *
    *** MCRBK - Machine Check Record Block

    *** Overlay for MCRFLOG in MCRBK
    *
    *     +-------------------------------------------------------+
    *  18 |                       MCRFASIT                        |
    *     +-------------------------------------------------------+
    *  20
    *
    *** Overlay for MCRFLOG in MCRBK

    *** Overlay for MCRMCIC in MCRBK
    *
    *     +-------------+---------------------------+-------------+
    *   0 |/////////////|         MCRMCB25          |/////////////|
    *     +-------------+---------------------------+-------------+
    *   8
    *
    *** Overlay for MCRMCIC in MCRBK

#### MCRBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    MCEXTDEA       000E 40
    MCEXTDES       000E 10
    MCEXTDPS       000E 80
    MCEXTDSL       000E 20
    MCEXTDXF       000D 40
    MCEXTDXN       000D 80
    MCEXTD0        000C 00
    MCEXTD3        000F 00
    MCICAR         0005 08
    MCICBU         0001 02
    MCICCD         0000 08
    MCICCRW        0001 40
    MCICCSD        0001 10
    MCICDA         0004 20
    MCICDG         0000 01
    MCICDL         0001 01
    MCICED         0000 04
    MCICIE         0004 80
    MCICITD        0000 10
    MCICKE         0002 20
    MCICPD         0000 40
    MCICSC         0002 40
    MCICSD         0000 80
    MCICSDG        0002 10
    MCICSE         0002 80
    MCICSP         0001 20
    MCICSR         0000 20
    MCICVAR        0004 40
    MCICVCC        0005 01
    MCICVCR        0003 04
    MCICVCT        0005 02
    MCICVED        0003 20
    MCICVFA        0003 80
    MCICVFF        0000 02
    MCICVFP        0003 10
    MCICVFS        0001 04
    MCICVGR        0003 08
    MCICVIA        0002 01
    MCICVLG        0003 02
    MCICVMS        0002 04
    MCICVPM        0002 02
    MCICVST        0003 01
    MCICVWP        0002 08
    MCICVXFP       0005 10
    MCICW          0001 80
    MCIPRIM0       0000 FF
    MCIPRIM1       0001 F0
    MCREDC         000C
    MCREDCB0       000C
    MCREDCB1       000D
    MCREDCB2       000E
    MCREDCB3       000F
    MCRFASIT       0018
    MCRFLAG1       0014
    MCRFLOG        0018
    MCRFSAD        002C
    MCRGFAD        0028
    MCRLEN         002C 00000030
    MCRMCB01       0000
    MCRMCB25       0002
    MCRMCIC        0000
    MCRMCICX       0010
    MCRMCIC0       0000
    MCRMCIC1       0001
    MCRMCIC2       0002
    MCRMCIC3       0003
    MCRMCIC4       0004
    MCRMCIC5       0005
    MCRMCIC6       0006
    MCRMCIC7       0007
    MCRMCWD0       0000
    MCRMCWD1       0004
    MCRNULLA       0014 20
    MCRREAL        0014 80
    MCRRELST       0014 40
    MCRSIZE        002C 00000006
    MCR64HI        0028
    MCR64LO        002C 0000002C

This information is based on z/VM V4R4.0. Last updated on 29 Jul 2003 at 15:49:27 EDT.
Copyright IBM Corporation, 1990, 2003