CSLPL - 64-bit CP - V4R4.0

Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### CSLPL

Prolog

Control Block Contents
CSLPL DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### CSLPL Prolog

     NAME       : HCPCSLPL
     DESCRIPTION: Console macro parameter list
     DSECT      : CSLPL
     LOCATED BY : HCPCONSL passes the address in a register
     CREATED BY : The HCPCSLPL is created by the HCPCONSL macro
                  whenever a read or write is to be done.
     DELETED BY : The HCPCSLPL is deleted by the HCPCONSL macro
     REFERENCES : None.
     SERIALIZED : HCPCONSL gets free storage for each instance of this
                  control block, so only one processor will be looking at
                  any one instance of this control block at any one time.

#### CSLPL Control Block Content

#### CSLPL DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CSLPL          Console macro parameter list
    0000    0 Character    2 CSLCOMMN (0)   common part
    0000    0 Bitstring    2 CSLNEST        how many caller's register to go
                                            back
    0002    2 Character    1 CSLFUNDE (0)   start of variable length data
    0002    2 Character   12 CSLWRITE (0)
    0002    2 Signed       2 CSLDADDR       bddd of data
    0004    4 Bitstring    1 CSLDATA        data information flags
              1... ....      CSLNUM         X'80' repository entry number
              .1.. ....      CSLNUMRG       X'40' repository entry number
              ..1. ....      CSLIST         X'20' list of repository numbers
              ...1 ....      CSLDLNRG       X'10' length of data is in a
                                            register
              .... 1...      CSLSUBDT       X'08' substitution data is passed
              .... .1..      CSLSUBRG       X'04' substitution data is in a
                                            register
              .... ..1.      CSLHLNRG       X'02' header length is in a
                                            register
              .... ...1      CSLVMDRG       X'01' VMDBK address is in a
                                            register
    0005    5 Bitstring    1 CSLTYPE        data type flags
              1... ....      CSLEMSG        X'80' error message
              .1.. ....      CSLIMSG        X'40' informational message
              ..1. ....      CSLFEMSG       X'20' full error message
              ...1 ....      CSLCRESP       X'10' command response
              .... 1...      CSLRDISP       X'08' input redisplay
              .... .1..      CSLWNG         X'04' warning message
              .... ..1.      CSLMSG         X'02' message to a user
              .... ...1      CSLMSGNH       X'01' message no-header to a user
    0006    6 Bitstring    1 CSLDFLG        destination flags
              1... ....      CSLALTVM       X'80' alternate vmdbk is
                                            specified
              .1.. ....      CSLOPER        X'40' data to be sent to the
                                            operator
              ..1. ....      CSLTERM        X'20' send data to terminal(not
                                            over IUCV, Diag 8 to buff,etc )
              ...1 ....      CSLGSDBK       X'10' return data in a GSDBK
              .... 1...      CSLTRMA        X'08' force data to terminal also
              .... .1..      CSLTRMO        X'04' force data to terminal only
              .... ..1.      CSLINITP       X'02' initial logon prompt
              .... ...1      CSLISSUS       X'01' issuer's userid is
                                            specified
    0007    7 Bitstring    1 CSLEFLG        data edit flags
              .1.. ....      CSLADTIM       X'40' add timestamp to data
              ..1. ....      CSLSPTIM       X'20' suppress time stamp and cpu
                                            id
              ...1 ....      CSLBRITE       X'10' hilight this data
              .... 1...      CSLCOLFM       X'08' error message in column
                                            format
              .... .1..      CSLBLNKS       X'04' do not delete trailing
                                            blanks
              .... ..1.      CSLOBSRV       X'02' message to observer
              .... ...1      CSLPRND        X'01' prompt with no-display read
    0008    8 Bitstring    1 CSLSFLG        screen control flags
              1... ....      CSLALARM       X'80' sound alarm
              .1.. ....      CSLHIPRI       X'40' this is high priority data,
                                            if user is in full screen, post
                                            an attention to the user
              ..1. ....      CSLNDISP       X'20' do not display data (or
                                            spool for reads)
              ...1 ....      CSLCLEAR       X'10' clear screen prior to
                                            displaying data
              .... 1...      CSLIOCMP       X'08' return after users IO
                                            completed
              .... .1..      CSLSCRFL       X'04' return if data can fit on
                                            current screen
              .... ..1.      CSLDROP        X'02' drops the connection
              .... ...1      CSLIMMED       X'01' if the user is in full
                                            screen, this message will break
                                            the user out of full screen.
    0009    9 Bitstring    1 CSLPFLG        Parameter address flag (address
                                            of address)
              1... ....      CSLDPTR        X'80' parameter list points to
                                            address of data
              .1.. ....      CSLIPTR        X'40' parameter list points to
                                            address of issuers USERID
              ..1. ....      CSLAPTR        X'20' parameter list points to
                                            address of alternate VMDBK
              ...1 ....      CSLSPTR        X'10' parameter list points to
                                            address of substitution data/reg
              .... 1...      CSLLPTR        X'08' parameter list points to
                                            address of data length
              .... .1..      CSLHPTR        X'04' parameter list points to
                                            address of header length
    000A   10 Signed       2 CSLISSID       bddd of the issuer's userid
    000C   12 Signed       2 CSLVMDBK       bddd of alternate VMDBK address
    000E   14 Address      2 CSLCMPID       bddd of 3-char component ID
    0010   16 Character    1 CSLWTYDE (0)   start of variable length data
         Write Type dependent parts
    0010   16 Character    2 CSLSUBDA (0)
    0010   16 Signed       2 CSLSBDAT       bddd of substitution data
              00000012       CSLSSIZE       *-CSLPL
    0010   16 Character    2 CSLSUBR (0)
    0010   16 Signed       2 CSLSBREG       register containing substitution
                                            data
              00000012       CSLESIZE       *-CSLPL
    0010   16 Character    4 CSLBDAT (0)
    0010   16 Signed       2 CSLDLGTH       bddd of length of data being
                                            passed
    0012   18 Signed       2 CSLHDRSZ       bddd of length of message header
    0014   20 Character    1 CSLPRMDE (0)   start of variable length data
              00000014       CSLQSIZE       *-CSLPL
         Read dependent parts
         Any changes to the read fields should also be made to the prompted read
         fields.
    0002    2 Character    1 CSLREAD (0)
    0002    2 Bitstring    1 CSLRPARM       read data flags
              1... ....      CSLNODSP       X'80' do not display or spool
                                            this data
              .1.. ....      CSLNOLED       X'40' do not perform line editing
              ..1. ....      CSLUPPER       X'20' translate input line to
                                            upper case
              ...1 ....      CSLCDRDR       X'10' data from a card reader
              00000003       CSLRSIZE       *-CSLPL
         Prompted read dependent parts
         Any changes to the prompted read fields should also be made to the read
         fields.
    0014   20 Character    1 CSLPREAD (0)
    0014   20 Bitstring    1 CSLRFLAG       read data flags
              1... ....      CSLNODIS       X'80' do not display or spool
                                            this data
              .1.. ....      CSLPNLED       X'40' do not perform line editing
              ..1. ....      CSLUPPR        X'20' translate input line to
                                            upper case
              ...1 ....      CSLCARDR       X'10' data from a card reader
              00000015       CSLPSIZE       *-CSLPL
         Labels for XRef Purposes only
              .... ....      CSLWRTEF       X'00' WRITE to console specified
              .... ....      CSLFRMTF       X'00' WRITE(format) to GSDBK
              .... ....      CSLREADF       X'00' READ func specified
              .... ....      CSLPRMPT       X'00' PROMPT func specified
              .... ....      CSLWAITF       X'00' WAIT func specified
              .... ....      CSLDATAK       X'00' DATA keyword specified
              .... ....      CSLCPDAT       X'00' DATATYPE NONE
              .... ....      CSLDSPCH       X'00' DESTINATION dispatched
              .... ....      CSLXNDSP       X'00' DISPLAY NO
              .... ....      CSLXNLED       X'00' LINEEDIT NO
              .... ....      CSLXUPPR       X'00' CASE UPPER
              .... ....      CSLXCRDR       X'00' DEVICE CARDRDR

#### CSLPL Storage Layout

    *** CSLPL - Console macro parameter list
    *
    *     +-------------+
    *   0 |  CSLNEST    |
    *     +-------------+
    *
    *** CSLPL - Console macro parameter list

    *** Overlay for CSLFUNDE in CSLPL
    *
    *                   +-------------+------+------+------+------+
    *   0 ...         2 |  CSLDADDR   |:DATA |:TYPE |:DFLG |:EFLG |
    *     +------+------+-------------+------+------+------+------+
    *   8 |:SFLG |:PFLG |  CSLISSID   |  CSLVMDBK   |  CSLCMPID   |
    *     +------+------+-------------+-------------+-------------+
    *
    *** Overlay for CSLFUNDE in CSLPL

    *** Overlay for CSLWTYDE in CSLPL
    *
    *     +-------------+
    *  10 |  CSLSBDAT   | 12
    *     +-------------+
    *
    *** Overlay for CSLWTYDE in CSLPL

    *** Overlay for CSLWTYDE in CSLPL
    *
    *     +-------------+
    *  10 |  CSLSBREG   | 12
    *     +-------------+
    *
    *** Overlay for CSLWTYDE in CSLPL

    *** Overlay for CSLWTYDE in CSLPL
    *
    *     +-------------+-------------+
    *  10 |  CSLDLGTH   |  CSLHDRSZ   |
    *     +-------------+-------------+
    *
    *** Overlay for CSLWTYDE in CSLPL

    *** Overlay for CSLFUNDE in CSLPL
    *
    *                   +------+
    *   0 ...         2 |:RPARM| 3
    *                   +------+
    *
    *** Overlay for CSLFUNDE in CSLPL

    *** Overlay for CSLPRMDE in CSLPL
    *
    *                                 +------+
    *  10 ...                      14 |:RFLAG| 15
    *                                 +------+
    *
    *** Overlay for CSLPRMDE in CSLPL

#### CSLPL Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    CSLADTIM       0007 40
    CSLALARM       0008 80
    CSLALTVM       0006 80
    CSLAPTR        0009 20
    CSLBDAT        0010
    CSLBLNKS       0007 04
    CSLBRITE       0007 10
    CSLCARDR       0014 10
    CSLCDRDR       0002 10
    CSLCLEAR       0008 10
    CSLCMPID       000E
    CSLCOLFM       0007 08
    CSLCOMMN       0000
    CSLCPDAT       0014 00
    CSLCRESP       0005 10
    CSLDADDR       0002
    CSLDATA        0004
    CSLDATAK       0014 00
    CSLDFLG        0006
    CSLDLGTH       0010
    CSLDLNRG       0004 10
    CSLDPTR        0009 80
    CSLDROP        0008 02
    CSLDSPCH       0014 00
    CSLEFLG        0007
    CSLEMSG        0005 80
    CSLESIZE       0010 00000012
    CSLFEMSG       0005 20
    CSLFRMTF       0014 00
    CSLFUNDE       0002
    CSLGSDBK       0006 10
    CSLHDRSZ       0012
    CSLHIPRI       0008 40
    CSLHLNRG       0004 02
    CSLHPTR        0009 04
    CSLIMMED       0008 01
    CSLIMSG        0005 40
    CSLINITP       0006 02
    CSLIOCMP       0008 08
    CSLIPTR        0009 40
    CSLISSID       000A
    CSLISSUS       0006 01
    CSLIST         0004 20
    CSLLPTR        0009 08
    CSLMSG         0005 02
    CSLMSGNH       0005 01
    CSLNDISP       0008 20
    CSLNEST        0000
    CSLNODIS       0014 80
    CSLNODSP       0002 80
    CSLNOLED       0002 40
    CSLNUM         0004 80
    CSLNUMRG       0004 40
    CSLOBSRV       0007 02
    CSLOPER        0006 40
    CSLPFLG        0009
    CSLPNLED       0014 40
    CSLPREAD       0014
    CSLPRMDE       0014
    CSLPRMPT       0014 00
    CSLPRND        0007 01
    CSLPSIZE       0014 00000015
    CSLQSIZE       0014 00000014
    CSLRDISP       0005 08
    CSLREAD        0002
    CSLREADF       0014 00
    CSLRFLAG       0014
    CSLRPARM       0002
    CSLRSIZE       0002 00000003
    CSLSBDAT       0010
    CSLSBREG       0010
    CSLSCRFL       0008 04
    CSLSFLG        0008
    CSLSPTIM       0007 20
    CSLSPTR        0009 10
    CSLSSIZE       0010 00000012
    CSLSUBDA       0010
    CSLSUBDT       0004 08
    CSLSUBR        0010
    CSLSUBRG       0004 04
    CSLTERM        0006 20
    CSLTRMA        0006 08
    CSLTRMO        0006 04
    CSLTYPE        0005
    CSLUPPER       0002 20
    CSLUPPR        0014 20
    CSLVMDBK       000C
    CSLVMDRG       0004 01
    CSLWAITF       0014 00
    CSLWNG         0005 04
    CSLWRITE       0002
    CSLWRTEF       0014 00
    CSLWTYDE       0010
    CSLXCRDR       0014 00
    CSLXNDSP       0014 00
    CSLXNLED       0014 00
    CSLXUPPR       0014 00

This information is based on z/VM V4R4.0. Last updated on 30 Jul 2003 at 12:35:48 EDT.
Copyright IBM Corporation, 1990, 2003