VDEV - 64-bit CP - V4R4.0

Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### VDEV

Prolog

Control Block Contents
VDEV DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### VDEV Prolog

     NAME       : HCPVDEV
     DESCRIPTION: VIRTUAL DEVICE CONTROL BLOCK
     DSECT      : VDEV
     FUNCTION   : DESCRIBE THE STATUS OF AN I/O DEVICE (REAL OR VIRTUAL)
                  ACCESSABLE BY A VIRTUAL MACHINE.
     LOCATED BY - A POINTER IN THE LOWEST LEVEL INDEX VECTOR IN THE
                  FOUR-LEVEL TREE ANCHORED IN:
                    VMDCHRSN - FOR ACCESS VIA SUBCHANNEL NUMBER
                    VMDCHRDN - FOR ACCESS VIA DEVICE NUMBER
                  RDEVVDEV - DEDICATED DEVICE ONLY
                  BLKVDEVA - DEVICES CONNECTED TO DASD BLOCK I/O
                             SYSTEM SERVICE
                  VDEVBASE - MULTIPLE EXPOSURE DEVICE ONLY
                  VMDVSPRT - PRINTER TO USE IN DUMP, TRACE, ... CMDS
                  VMDVCONS - CONSOLE
                  MDIRVDEV - VDEV TO WHICH A MINI-DISK EXTENT IS
                             VIRTUALLY RESERVED.
                  WHILE AN I/O EVENT IS OUTSTANDING FOR A VIRTUAL
                  MACHINE, THE ADDRESS OF A VDEV MAY APPEAR IN:
                    CHCQUEUE(I) - FIRST DEVICE WITH AN INTERRUPT PENDING
                                  ON CHANNEL I (OR IN CHANNEL CLASS I)
                    VDEVFPNT - NEXT DEVICE WITH INTERRUPT PENDING ON
                               THIS CHANNEL (OR THIS VDEV, IF LAST)
                    VDEVBPNT - PREVIOUS INTERRUPT PENDING DEVICE ON THIS
                               CHANNEL (OR THIS VDEV, IF FIRST)
                    VMDWVDEV - DEVICE CAUSING I/O WAIT CONDITION
                               - SYNCHRONOUS I/O VIA DIAGNOSE 18 OR 20
                               - VIRTUAL MACHINE LOOPING ON TIO INSTR.
                    IORVDEV -  VDEV WITH WHICH VIRTUAL MACHINE'S I/O
                               REQUEST IS ASSOCIATED.
                  WHEN A GUEST REQUESTS AN ASYNCHRONOUS MESSAGE,
                  THE ADDRESS OF A VDEV MAY APPEAR IN:
                    AEBKVDEV - VDEV WITH WHICH VIRTUAL MACHINE'S
                               ASYNCHRONOUS MESSAGE REQUEST IS
                               ASSOCIATED.
                  I/O SUPERVISOR ROUTINES NORMALLY USE REGISTER 6 TO
                  ADDRESS THE VDEV ASSOCIATED WITH THE EVENT BEING
                  PROCESSED.
     CREATED BY : HCPVDB
     DELETED BY : HCPVDB

#### VDEV Control Block Content

#### VDEV DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      VDEV           VIRTUAL DEVICE CONTROL BLOCK
    0000    0 Signed       4 VDEVFPNT       FORWARD INTERRUPTION POINTER
    0004    4 Signed       4 VDEVBPNT       BACKWARD INTERRUPTION POINTER
    0008    8 Dbl-Word     8 VDEVLOCK (0)   VIRTUAL DEVICE LOCKWORD
    0008    8 Address      4 VDEVLOWN       ADDRESS OF LOCK OWNER'S VMDBK
    000C   12 Address      4 VDEVTSKQ       ANCHOR FOR QUEUE OF WAITING TASKS
    0010   16 Signed       2 VDEVSUB        VIRTUAL SUBCHANNEL NUMBER
    0012   18 Signed       2 VDEVCODE (0)   VIRTUAL DEVICE IDENTITY CODE
    0012   18 Bitstring    1 VDEVCLAS       DEVICE CLASS
              1... ....      CLASTERM       X'80' TERMINAL DEVICE CLASS
              .1.. ....      CLASGRAF       X'40' GRAPHIC DISPLAY DEVICE
                                            CLASS
              .1.. ...1      CLASGRFR       X'41' GRAPHIC DISPLAY DEVICE
                                            CLASS (REMOTE)
              ..1. ....      CLASPOOL       X'20' UNIT RECORD SPOOLING DEVICE
                                            CLASS
              ...1 ....      CLASSVCM       X'10' SIMULATED DEVICE CLASS
              .... 1...      CLASTAPE       X'08' MAGNETIC TAPE DEVICE CLASS
              .... .1..      CLASDASD       X'04' DIRECT ACCESS STORAGE
                                            DEVICE CLASS
              .... ..1.      CLASSPEC       X'02' SPECIAL DEVICE CLASS
              .... ...1      CLASSWCH       X'01' Switch device class
              1111 1111      CLASAIF        X'FF' Adapter-Interrupt-Facility
                                            (AIF) Class
    0013   19 Bitstring    1 VDEVTYPE       DEVICE TYPE
              1... ....      TYP2700        X'80' TERM - 2700 BISYNC LINE
              1... 1...      TYPBSC         X'88' TERM - BISYNC LINE FOR 3270
                                            REMOTE STATION
              .1.. ....      TYPCONS        X'40' TERM - CONSOLE DEVICE
              .1.. ....      TYP3215        X'40' TERM - 3215 CONSOLE
              .1.. ....      TYP1052        X'40' TERM - 1052 CONSOLE
              ..1. ....      TYPTTY         X'20' TERM - USASCII-8 TELEGRAPH
                                            TERMINAL
              ...1 ....      TYPIBM1        X'10' TERM - IBM TERMINAL CONTROL
                                            TYPE 1
              ...1 11..      TYPUNDEF       X'1C' TERM - TERMINAL TYPE
                                            UNDEFINED
              ...1 1...      TYP2741        X'18' TERM - 2741 COMMUNICATIONS
                                            TERMINAL
              ...1 1...      TYP3767        X'18' TERM - 3767 IN 2741
                                            COMPATIBILITY MOD
              ...1 .1..      TYP1050        X'14' TERM - 1050 COMMUNICATIONS
                                            TERMINAL
              .... 1...      TYPSDLC        X'08' TERM - SDLC Integrated
                                            Adapter
              ..1. ....      TYPTELE2       X'20' TERM - TELE2 Integrated
                                            Adapter
              ..1. .1..      TYPHDLC        X'24' TERM - HDLC Integrated
                                            Adapter
              ..1. 1...      TYPILAN        X'28' TERM - ILAN Integrated
                                            Adapter
              ..1. 1...      TYPELAN        X'28' TERM - ELAN Integrated
                                            Adapter
              .1.. ....      TYP3270        X'40' GRAF - 3270 GENERIC DISPLAY
                                            STATION
              1... ....      TYP3277        X'80' GRAF - 3277 DISPLAY STATION
              .1.. ....      TYP3278        X'40' GRAF - 3278 DISPLAY STATION
              .1.. ....      TYP3178        X'40' GRAF - 3178 DISPLAY STATION
              .1.. ....      TYP3279        X'40' GRAF - 3279 DISPLAY STATION
              .1.. ....      TYP3179        X'40' GRAF - 3179 DISPLAY STATION
              .1.. ....      TYP3180        X'40' GRAF - 3180 DISPLAY STATION
              .1.. ....      TYP3290        X'40' GRAF - 3290 DISPLAY STATION
              .1.. ....      TYP3190        X'40' GRAF - 3190 DISPLAY STATION
              ..1. ....      TYP3271        X'20' GRAF - 3271 CONTROLLER
                                            (REMOTE)
              ...1 ....      TYP3275        X'10' GRAF - 3275 DISPLAY STATION
              .... 1...      TYP3284        X'08' GRAF - 3284 PRINTER
              .... 1...      TYP3286        X'08' GRAF - 3286 PRINTER
              .... 1..1      TYP3287        X'09' GRAF - 3287 PRINTER
              .... 1...      TYP3288        X'08' GRAF - 3288 PRINTER
              .... 1..1      TYP3289        X'09' GRAF - 3289 PRINTER
              .... 1...      TYP3287L       X'08' GRAF - 3287 LOGICAL PRINTER
              .... 1...      TYP3289L       X'08' GRAF - 3289 LOGICAL PRINTER
              .... .1..      TYP2250        X'04' GRAF - 2250 DISPLAY UNIT
              .... .1..      TYP3250        X'04' GRAF - 3250 DISPLAY UNIT
              .... .11.      TYP5080        X'06' GRAF - 5080 DISPLAY UNIT
              ..11 ....      TYPCLUST       X'30' GRAF - CLUSTER CTLR (3271
                                            OR 3275)
              .... ..1.      TYPIC          X'02' TERM - Integrated console
                                            GRAF - Integrated 3270
              1... ....      TYPRDR         X'80' SPOL - CARD READER DEVICE
              1... ...1      TYP2501        X'81' SPOL - 2501 CARD READER
              1... ..1.      TYP2540R       X'82' SPOL - 2540 CARD READER
              1... .1..      TYP3505        X'84' SPOL - 3505 CARD READER
              .1.. ....      TYPPUN         X'40' SPOL - CARD PUNCH DEVICE
              .1.. ..1.      TYP2540P       X'42' SPOL - 2540 CARD PUNCH
              .1.. .1..      TYP3525        X'44' SPOL - 3525 CARD PUNCH
              ..1. ....      TYPPRT         X'20' SPOL - PRINTER TYPE DEVICE
              ..1. ...1      TYP1403        X'21' SPOL - 1403 PRINTER
              ..1. ..1.      TYP32XX        X'22' SPOL - 3203 OR 3211 PRINTER
              ..1. .11.      TYP3203        X'26' SPOL - 3203 PRINTER
              ..1. ..1.      TYP3211        X'22' SPOL - 3211 PRINTER
              ..1. 1...      TYP3800        X'28' SPOL - 3800 PRINTER
              ..1. ..11      TYP3262        X'23' SPOL - 3262 PRINTER
              ..1. .1..      TYP4245        X'24' SPOL - 4245 PRINTER
              ..1. 1..1      TYP4248        X'29' SPOL - 4248 PRINTER
              ..1. .1.1      TYP3820        X'25' SPOL - 3820 PRINTER -
                                            dedicated only
              ..1. .111      TYPAFP1        X'27' SPOL - AFP1 PRINTER -
                                            dedicated only
              ..1. 1.1.      TYPVAFP        X'2A' SPOL - VAFP PRINTER -
                                            simulated only
              ...1 ....      TYPSYS         X'10' SPOL - SYSTEM VIRT DEVICE
                                            FOR DUMPS
              ...1 ....      TYP3420        X'10' TAPE - 3420 TAPE DRIVE
              ..1. ....      TYP3430        X'20' TAPE - 3430 TAPE DRIVE
              .1.. ....      TYP3480        X'40' TAPE - 3480 TAPE DRIVE
              .1.. ..1.      TYP3424        X'42' TAPE - 3424 TAPE DRIVE
              .1.. .1..      TYP9348        X'44' TAPE - 9348 TAPE DRIVE
              1... ....      TYP3422        X'80' TAPE - 3422 TAPE DRIVE
              1... ...1      TYP3490        X'81' TAPE - 3490 TAPE DRIVE
              1... ..11      TYP3590        X'83' TAPE - 3590 TAPE DRIVE
              .1.. ....      TYP3330        X'40' DASD - 3330 DISK STORAGE
                                            FACILITY
              ..1. ....      TYP3340        X'20' DASD - 3340 DISK STORAGE
                                            FACILITY
              ...1 ....      TYP3350        X'10' DASD - 3350 DISK STORAGE
                                            FACILITY
              ...1 ...1      TYP3350C       X'11' DASD - 3350 4 X 8 PAGING
                                            STORAGE
              ...1 ..1.      TYP3350D       X'12' DASD - 3350 4 X 4 PAGING
                                            STORAGE
              .... 1...      TYP2305        X'08' DASD - 2305 FIXED HEAD
                                            STORAGE FACILITY
              .... .1..      TYP3380        X'04' DASD - 3380 DISK STORAGE
                                            FACILITY
              1... ..1.      TYP3390        X'82' DASD - 3390 DISK STORAGE
                                            FACILITY
              1... ....      TYP3375        X'80' DASD - 3375 DISK STORAGE
                                            FACILITY
              .... ..1.      TYP3370        X'02' DASD - 3370 DISK STORAGE
                                            FACILITY
              1... ...1      TYP9345        X'81' DASD - 9345 DISK STORAGE
                                            FACILITY
              ..1. ...1      TYP9332        X'21' DASD - 9332 FBA Direct
                                            Access Storage
              ..1. ..1.      TYP9335        X'22' DASD - 9335 FBA Direct
                                            Access Storage
              ..1. .1..      TYP9336        X'24' DASD - 9336 FBA Direct
                                            Access Storage
              ..1. 1...      TYPFBA         X'28' DASD - Generic FBA DAS
              .1.. ....      TYP9033        X'40' SWCH - 9033 Switch device
              1... ....      TYP9032        X'80' SWCH - 9032 Switch device
              ..1. ....      TYP2032        X'20' SWCH - 2032 FICON Switch
                                            device
              1... ....      TYPCTCA        X'80' SPEC - CHANNEL TO CHANNEL
                                            ADAPTER
              1... ....      TYP3088        X'80' SPEC - 3088 MULTISYSTEM
                                            CHANNEL COMMUNICATION UNIT
              .1.. ....      TYP3704        X'40' SPEC - 3704 PROGRAMMABLE
                                            COMMUNICATION CONTROL UNIT
              .1.. ....      TYP3705        X'40' SPEC - 3705 PROGRAMMABLE
                                            COMMUNICATION CONTROL UNIT
              ..1. ....      TYPOSA         X'20' SPEC - Open Systems Adapter
                                            (OSA)
              ...1 ....      TYPFCP         X'10' SPEC - Open FCP Adapter
                                            (FCP)
              .... .1..      TYPE3SCH       X'04' SPEC - Type 3 subchannel
              .... ..1.      TYP3851        X'02' SPEC - MSS MASS STORAGE
                                            COMMUNICATOR
              .... 1...      TYP3890        X'08' SPEC - 3890 DOCUMENT
                                            PROCESSOR
              .... ...1      TYPUNSUP       X'01' SPEC - DEVICE UNSUPPORTED
                                            BY * THE VM/ 370 MIGRATION AID
              .... .1..      TYP3SIM        X'04' VCM - Simulated type 3
                                            subchannel
              .... ..1.      TYPDYNIO       X'02' VCM - Dynamic I/O
              .... ...1      TYPMSGF        X'01' VCM - Message Facility
    0014   20 Signed       4 VDEVUSER       POINTER TO VMDBK OF OWNER
    0018   24 Bitstring    1 VDEVSTAT       DEVICE STATUS - OWNED BY VIRTUAL
                                            I/O INSTRUCTION SIMULATION. THIS
                                            IS NOT TO BE USED BY VIRTUAL
                                            DEVICE SIMULA- TION.
              1... ....      VDEVBUSY       X'80' START FUNCTION
              .1.. ....      VDEVPRCE       X'40' CHANNEL END RECEIVED
              ..1. ....      VDEVCLRF       X'20' CLEAR FUNCTION
              ...1 ....      VDEVHLTF       X'10' HALT FUNCTION
              1111 ....      VDEVACTV       VDEVBUSY+VDEVPRCE+VDEVCLRF+VDEVHL
                                            TF
              .... 1...      VDEVSUSP       X'08' SUBCHANNEL SUSPENDED
              .... .1..      VDEVRPND       X'04' RESUME PENDING
              .... ..1.      VDEVQUED       X'02' DEVICE-BUSY RECEIVED -
                                            VDEVNIOR CONTAINS THE ADDRESS OF
                                            AN IORBK WHICH RECEIVED AN
                                            INITIAL STATUS OF BUSY-ALONE AND
                                            IS AWAITING AN UNSOLICITED DEVICE
                                            END.
              .... ...1      VDEVCATT       X'01' ATTACHED VIA CONSOLE
                                            COMMAND
    0019   25 Bitstring    1 VDEVWAIT       WAIT STATUS CONTROLS
              1... ....      VDEVIMRS       X'80' VM SUSPENDED PENDING I/O
                                            RESPONSE
              .1.. ....      VDEVWINT       X'40' CPU(S) AWAITING STATUS
                                            (TIO/TSCH BUSY)
    001A   26 Bitstring    1 VDEVAFLG       DEVICE ALLOCATION FLAG
              1... ....      VDEVINTV       X'80' SIMULATED INTERVENTION
                                            REQUIRED
              .1.. ....      VDEVTDSK       X'40' DEVICE IS DASD TDISK
              ..1. ....      VDEVVSIM       X'20' DEVICE IS SIMULATED BY
                                            VDSBK
              ...1 ....      VDEVFULL       X'10' DEVICE IS A COMPLETE VOLUME
              .... 1...      VDEVDED        X'08' DEVICE IS ATTACHED TO
                                            VDEVRDEV
              .... .1..      VDEVMPLX       X'04' MULTIPLE EXPOSURE DEVICE
              .... ..1.      VDEVFPO        X'02' THE DEVICE IS A
                                            FULL-PACK-OVERLAY MINIDISK
              .... ...1      VDEVDTCH       X'01' THE DEVICE IS BEING
                                            DETACHED
    001B   27 Bitstring    1 VDEVBFLG       HALT flags plus some misc flags
              1... ....      VDEVBCC0       X'80' BACKUP CONFIRMED CC 0 FLAG
              .1.. ....      VDEVBPCI       X'40' BACKUP PCI FLAG
              ..1. ....      VDEVBSUI       X'20' BACKUP SUSPENSION INTERRUPT
                                            FLAG
              .... 1...      VDEVQACT       X'08' BACKUP QDIO Active Status
              .... .1..      VDEVCMS        X'04' Device is attached to
                                            adjunct
              .... ..1.      VDEVVMIO       X'02' Update VMDIOACT for active
                                            I/O
    001C   28 Bitstring    1 VDEVDFLG       DEVICE CONTROL FLAGS
              1... ....      VDEVRO         X'80' DEVICE- READ ONLY ACCESS
              .1.. ....      VDEVENAB       X'40' COMMUNICATION LINE -
                                            ENABLED
              ..1. ....      VDEVDIAL       X'20' COMMUNICATION LINE - DIALED
              ...1 ....      VDEVSDIA       X'10' COMMUNICATION LINE - SNA
                                            DIALED
              .... 1...      VDEVNOTO       X'08' If on, means that this VDEV
                                            is no longer operational, because
                                            it is soon going away. Set by
                                            Detach processing.
              .... .1..      VDEVRSRL       X'04' RESERVE/RELEASE VALID CCW'S
              .... ..1.      VDEVNSEG       X'02' NO CHAN PROG SEGMENTATION
                                            ALLOWED
              .... ...1      VDEVGCWE       X'01' GLOBAL CCW EXPECTED FOR
                                            THIS DEVICE
    001D   29 Bitstring    1 VDEVCFLG       CONSOLE PROCESSING CONTROLS
              1... ....      VDEVINT3       X'80' Device used as integrated
                                            3270
              .1.. ....      VDEVPPA1       X'40' REFLECT PA1 KEY TO THE
                                            VIRTUAL MACHINE
              ..1. ....      VDEVGSUS       X'20' FULL SCREEN GUEST WAS
                                            SUSPENDED WITH UNIT EXCEPTION. CP
                                            MUST GENERATE AN UNSOLICITED
                                            DEVICE END TO RESUME GUEST
              ...1 ....      VDEVDING       X'10' dial in progress
              .... 1...      VDEVATTN       X'08' ATTENTION INTERRUPT MUST BE
                                            GENERATED
              .... .1..      VDEVBRGS       X'04' Set RDEVGSUS when
                                            reconnected to console RDEV
    001E   30 Bitstring    1 VDEVFFLG       MINIDISK FLAGS
              1... ....      VDEVLNKS       X'80' STABLE MINIDISK LINK
              .1.. ....      VDEVLNKE       X'40' EXCLUSIVE MINIDISK LINK
              ..1. ....      VDEVDVFP       X'20' THE DEVICE IS A DEVNO
                                            DEFINED FULL-PACK MINIDISK
              ...1 ....      VDEVQDSK       X'10' The device is a VDISK
              .... 1...      VDEVFBA        X'08' FBA disk or minidisk
              .... .1..      VDEVRMLF       X'04' Minidisk can use real MPLF
                                            facility
              .... ..1.      VDEVSULF       X'02' Suppress CFLF and MPLF
    001F   31 Bitstring    1 VDEVPFLG       DEVICE PROCESSING FLAG
              1... ....      VDEVCPCL       X'80' DEVICE CLOSED BY CP COMMAND
              .1.. ....      VDEVPURG       X'40' DEVICE CLOSED AND PURGED BY
                                            CP COMMAND
              ..1. ....      VDEVNRSM       X'20' DEVICE CANNOT RESUME
                                            CHANNEL PROGRAM
              ...1 ....      VDEVDPRE       X'10' DYMAMIC PATHING HAS BEEN
                                            REQUESTED
              .... 1...      VDEVTRCW       X'08' FORCE TRANSLATION OF
                                            CHANNEL PROGRAM FOR THIS DEVICE
              .... .1..      VDEVTENB       X'04' TAPE Device has not been
                                            enabled. Device End has not been
                                            presented.
              .... ..1.      VDEVSHRD       X'02' Multiuser device bit
              .... ...1      VDEVSHND       X'01' Multiuser/Detach ALL fails
                                            for vdev
    0020   32 Bitstring   28 VDEVPMCW       PATH MANAGEMENT CONTROL WORD
    003C   60 Signed       4 VDEVAIOR       POINTER TO THE ACTIVE IORBK
    0040   64 Signed       4 VDEVNIOR       SSCH PNDING (NOT YET STARTED)
                                            IORBK
    0044   68 Address      4 VDEVSIOR       IORBK HOLDING SENSE DATA FOR
                                            DEVICE
    0048   72 Signed       4 VDEVIORQ       RDEV-TO-VDEV LOCK SWAPPING PIVOT
    004C   76 Signed       4 VDEVPIOR       PENDING INTERRUPT IORBK
    0050   80 Signed       4 VDEVENDQ       COMPLETION TASK QUEUE ANCHOR
    0054   84 Address      4 VDEVDEOT       DELAYED ENDOP TRQBK ANCHOR
    0058   88 Signed       4 VDEVRDEV       POINTER TO RDEV OF ACTUAL DEVICE
    005C   92 Address      4 VDEVAEVT       POINTER TO LIST OF ASYNCHRONOUS
                                            EVENTS IN THIS VDEV.
    0060   96 Address      4 VDEVREVT       POINTER TO RESERVED ASYNCHRONOUS
                                            EVENT
    0064  100 Address      4 VDEVCEOT       POINTER TO 20 SECOND TIMER
    0068  104 Address      4 VDEVLMSG       CFLF In-line Message Block
                                            Pointer
    006C  108 Signed       4 VDEVIOCT       Count of virtual I/O requests
                                            issued to the virtual device.
                                            (See VDEVIOCA). Not applicable to
                                            consoles, virtual spool or I/O
                                            Assist devices.
    0070  112 Dbl-Word     8 VDEVTIME (0)   TOD CLOCK AT DEVICE CREATION
    0070  112 Signed       4 VDEVTIMH       HI ORDER TOD CLOCK ROUGHLY IN
                                            SECONDS
    0074  116 Signed       4 VDEVTIML       LO ORDER TOD CLOCK
    0078  120 Signed       4 VDEVSPEC (10)  DEVICE-DEPENDENT SPECIFICATIONS
    00A0  160 Address      4 VDEVIOMI       Address of Virtual I/O Management
                                            Info
    00A4  164 Address      4 VDEVUIOR       Pending unsolicited IORBK came in
                                            after unit check
    00A8  168 Signed       4 VDEVIOCA       Count of actual I/O operations
                                            initiated by CP for this virtual
                                            device. Not applicable to
                                            consoles, virtual spool or I/O
                                            Assist devices. Notes : This
                                            value may be lower than the
                                            number of virtual I/O requests if
                                            data can be obtained thru MDC, or
                                            it may be higher, if a virtual
                                            I/O request is broken up by CP
                                            into more than one actual I/O
                                            request (e.g., a diagnose x'A4'
                                            request for blocks on multiple
                                            cylinders.
    00AC  172 Signed       4 VDEVATIM       Time of device creation or last
                                            ACNT, whichever is later
    00B0  176 Bitstring    1 VDEVIOP1       I/O PASS THROUGH FLAGS
              1... ....      VDEVIOPQ       X'80' User set QIOAssist off for
                                            the device
              .1.. ....      VDEVIOPA       X'40' DEV IS OPERATING UNDER PASS
                                            THROUGH
              ..1. ....      VDEVIOPI       X'20' DEV BEING PUT UNDER I/O
                                            PASS THROUGH
              ...1 ....      VDEVIOPO       X'10' TAKE DEVICE OUT OF PASS
                                            THROUGH AT NEXT OPPORTUNITY
              .... 1...      VDEVIOPR       X'08' DEV BEING REMOVED FROM PASS
                                            THROUGH
              .... .1..      VDEVIOPS       X'04' User set I/O Assist off for
                                            the device
              .... ..1.      VDEVIOPX       X'02' DEVICE IS ELIGIBLE FOR XA
                                            I/O PASS THROUGH
              .... ...1      VDEVIOP3       X'01' DEVICE IS ELIGIBLE FOR 370
                                            I/O PASS THROUGH
    00B1  177 Bitstring    1 VDEVMODL       VIRTUAL DEVICE MODEL NUMBER
    00B2  178 Bitstring    1 VDEVCPIE       CHANNEL PATH IN ERROR MASK
    00B3  179 Bitstring    1 VDEVCRDR       Count of I/O redrives to
                                            simulation
    00B4  180 Signed       4 VDEVIUBK       I/O Assist Utilization Block
                                            Address
    00B8  184 Bitstring    1 VDEVLCNT       CURRENT LINE COUNT
    00B9  185 Bitstring    1 VDEVLTOD (3)   BYTES 2-4 OF TOD CLOCK WHEN LCNT
                                            RESET
    00BC  188 Address      4 VDEVBKIA       Address of the BKIBK This field
                                            is serialized by: If = 0,
                                            compare-and-swap if ^=0, BKILOCK
                                            held exclusive and
                                            single-access-word-current-store.
    00C0  192 Address      4 VDEVIPTS       Used by HCPIPT to contain a
                                            pointer to the SCHIB before a
                                            CSCH is done.
    00C4  196 Bitstring    1 VDEVSCHT       Subchannel type (Must remain like
                                            RDEVSCHT and SCHVISC)
              .... ....      VDEVSTP0       X'00' Type 0 Subchannel
              .11. ....      VDEVSTP3       X'60' Type 3 Subchannel
    00C5  197 Bitstring    1 VDEVPMSK       Mask of path on which the
                                            Quiesce/Resume message was
                                            received
    00C6  198 Bitstring    1 VDEVVNET       Virtual Network Simulation flags
              1... ....      VDEVNSIM       X'80' Virtual Network Simulation
                                            is ACTIVE (this means VDEVNIP is
                                            active)
              .1.. ....      VDEVVSW        X'40' Virtual SWITCH (VSWITCH)
                                            device
    00C7  199 Bitstring    1 *              RESERVED FOR FUTURE IBM USE
         RESERVED FIELDS FOR INSTALLATION USE
         THIS AREA IS PERMANENTLY AVAILABLE, BUT MAY BE MOVED TO ANOTHER OFFSET
         IN THE BLOCK AT A LATER RELEASE OF THE SYSTEM.
    00C8  200 Signed       4 VDEVUSR1       RESERVED FOR INSTALLATION USE
    00CC  204 Signed       4 VDEVUSR2       RESERVED FOR INSTALLATION USE
    00D0  208 Signed       4 VDEVUSR3       RESERVED FOR INSTALLATION USE
    00D4  212 Signed       4 VDEVUSR4       RESERVED FOR INSTALLATION USE
         End of Installation reserved fields
    00D8  216 Signed       4 *              Reserved for future IBM use
    00DC  220 Signed       4 VDEVRTMR       Pointer to RESET TRQBK. This
                                            field is serialized by VDEV lock
                                            when it is set and the dispatch
                                            lock when the field is reset.
    00E0  224 Signed       4 VDEVTRKF       First relative track for device
    00E4  228 Signed       4 VDEVTRKL       Last relative track for device
    00E8  232 Signed       4 VDEVARSL       Pointer to next Diag 254 pseudo
                                            vdev
    00EC  236 Signed       4 VDEVARSI       Pointer to Diag 254 information
                                            block
    00F0  240 Signed       4 VDEVARPV       Pointer to Diag 254 parent vdev
    00F4  244 Bitstring    1 VDEVMDFG       Message Device Flag
              1... ....      VDEVMDEL       X'80' Message Device Deleted
    00F5  245 Bitstring    1 * (3)          Reserved for future IBM use
    00F8  248 Address      4 VDEVQDIO       Anchor for the QDIO Data Queues
    00FC  252 Address      4 VDEVAIF        Anchor for Adapter IRPT Facility
                                            Block
    0100  256 Address      4 VDEVSHTP       MULTIuser tape device forward
                                            pointer
    0104  260 Address      4 VDEVIODD       CCW TRACE IODATA buffer
    0108  264 Dbl-Word     8 VDEVMBLK (0)   64-bit measurement block address
    0108  264 Signed       4 VDEVMBAH       High order MBA word
    010C  268 Signed       4 VDEVMBAL       Low order MBA word
              VDEVMBAL       VDEVMBAO       VDEVMBAL 390 measurement block
                                            address
         Start VDEV overlay area
              00000110       VDEVBYSZ       *-VDEV VDEV size in bytes
              00000022       VDEVSIZE       ((*-VDEV)+7)/8 VDEV SIZE IN
                                            DOUBLE-WORDS
    0078  120 Signed       4 VDEVPOSN (0)   VIRTUAL DASD ARM POSITION
    0078  120 Signed       2 VDEVCYLN       VIRTUAL DASD CYLINDER NUMBER
              .111 1...      VDEVCYL0       VDEVCYLN,1 1ST BYTE OF CYLINDER
                                            INFORMATION
              .111 1..1      VDEVCYL1       VDEVCYLN+1,1 2ND BYTE OF CYLINDER
                                            INFORMATION
    007A  122 Signed       2 VDEVHEAD       VIRTUAL DASD HEAD NUMBER
              .111 1.1.      VDEVHED0       VDEVHEAD,1 1ST BYTE OF HEAD
                                            INFORMATION
              .111 1.11      VDEVHED1       VDEVHEAD+1,1 2ND BYTE OF HEAD
                                            INFORMATION
    007C  124 Signed       4 VDEVSEXT (0)   Minidisk Start of EXTent. May be
                                            in cylinders (CKD/ECKD) or
                                            blocks(FBA)
    007C  124 Signed       2 *              Filler for beginning cylinder
    007E  126 Signed       2 VDEVBCYL       Minidisk beginning cylinder
    0080  128 Signed       4 VDEVEEXT (0)   Minidisk End of EXTent. May be in
                                            cylinders (CKD/ECKD) or
                                            blocks(FBA)
    0080  128 Signed       2 *              Filler for last cylinder
    0082  130 Signed       2 VDEVLCYL       Minidisk last cylinder
    0084  132 Signed       4 VDEVLINK       Next VDEV on this MDISK (cf.
                                            VDEVLINP)
    0088  136 Signed       4 VDEVBIOA       BLOCK I/O CONNECT BLOCK
    008C  140 Signed       4 VDEVMDSK       MINI-DISK BLOCK FOR
                                            RESERVE/RELEASE
    0090  144 Signed       4 VDEVBASE       BASE ADDRESS VDEV FOR
                                            MULT-EXPOSURE
    0094  148 Bitstring    1 VDEVMNGT       LEVEL OF CONTROL FOR CACHED DASD
              1... ....      VDEVCA         X'80' CACHING AVAILABLE TO A
                                            MINIDISK
              .1.. ....      VDEVCNA        X'40' CACHING NOT AVAILABLE TO A
                                            MINIDISK
              ..1. ....      VDEVSCTL       X'20' SYSTEM CONTROL FOR CACHED
                                            DASD
              ...1 ....      VDEVDCTL       X'10' DEVICE CONTROL FOR CACHED
                                            DASD
              .... 1...      VDEVNCTL       X'08' NO CONTROL FOR CACHED DASD
    0095  149 Bitstring    1 VDEVSFLG       DASD SPECIFIC FLAG
              ...1 ....      VDEVRFID       X'10' READ CACHE FASTWRITE ID CCW
                                            ISSUED
              .... 1...      VDEVSCPI       X'08' REFLECT A STATE-CHANGE
                                            INTERRUPT WHEN A
                                            STATE-CHANGE-PENDING CONDITION
                                            ENDS
    0096  150 Bitstring    2 *              RESERVED FOR FUTURE IBM USE
    0098  152 Signed       2 VDEVMPCT       COUNT OF EXTENTS DEFINED FOR THIS
                                            MINIDISK.
    009A  154 Signed       2 *              RESERVED FOR IBM USE
    009C  156 Signed       4 VDEVLINP       Prev VDEV on this MDISK
                                            (cf.VDEVLINK) (Previous of head
                                            is tail but Next of tail is
                                            zero.)
    0078  120 Bitstring   36 *              RESERVED FOR FUTURE IBM USE
    009C  156 Address      4 VDEVDYPT       Pointer to Tape Pathing Control
                                            Block
    0078  120 Character    8 VDEVCUSR       RESTRICTED USERID FOR COUPLING
    0080  128 Address      4 VDEVCTCA       ADDRESS OF CACBK
    0084  132 Bitstring    4 VDEVCTCD       CTCA designation 3088 = 3088
                                            emulation SCTC = ESCON SCTC
                                            emulation BCTC = ESCON BCTC
                                            emulation CNC = ESCON CNC
                                            emulation FCTC = FICON emulation
    0088  136 Bitstring   24 *              Reserved for IBM use
         Overlay for a fully-simulated Virtual Network device. This definition
         is active whenever VDEVNSIM is ON.
              00000078       VDEVNIP        * Network Interface Properties
    0078  120 Character    4 VDEVNIFT       Interface Type (e.g. c'IQDC')
    007C  124 Signed       4 VDEVNIDX       Index of this NID in the adapter
    0080  128 Address      4 VDEVNIC        Pointer to adapter NICBK
    0084  132 Address      4 VDEVNID        Pointer to device NIDBK
    0088  136 Address      4 VDEVSIGA       SIGA Simulation Routine
    008C  140 Bitstring    4 VDEVQMSK       QDIO Queue Selection Mask
    0090  144 Bitstring    1 VDEVOTSK       QDIO Output Queue Processing Task
    0091  145 Bitstring    1 VDEVITSK       QDIO Input Queue Processing Task
    0092  146 Bitstring    1 VDEVSWFL       VSWITCH Flags
              1... ....      VDEVSWDD       X'80' VSWITCH DATA device
    0093  147 Bitstring    1 *              Reserved for IBM Use
    0094  148 Signed       4 VDEVCHKQ       Checking queues (stacked call)
    0098  152 Bitstring    8 *              Reserved for IBM Use
    0078  120 Signed       4 *              RESERVED FOR FUTURE IBM USE
    007C  124 Address      4 VDEVVSP        ADDRESS OF THE VIRTUAL SPOOL
                                            BLOCK
    0080  128 Address      4 VDEVVPX        ADDRESS OF PRT EXTENSION BLOCK
    0084  132 Address      4 VDEVVDS        DEVICE SIMULATION POINTER
    0088  136 Bitstring   24 *              RESERVED FOR FUTURE IBM USE
    0078  120 Address      4 VDEVMNPT       Pointer to Next Message Device
    007C  124 Address      4 VDEVLCF        Address of Lock Facility Data
                                            Block
    0080  128 Address      4 VDEVLFIO       Address Of Lock Facility IORBK
    0084  132 Bitstring   28 *              Reserved for Future IBM Use
    0020   32 Signed       4 VDEVPMW0 (0)   WORD 0 OF PMCW
    0020   32 Signed       4 VDEVINTP       INTERRUPT PARAMETER
    0024   36 Signed       4 VDEVPMW1 (0)   WORD 1 OF PMCW
    0024   36 Bitstring    1 VDEVIRCF       SUBCHANNEL INTERUPT REQUEST CODE
              ..11 1...      CSWIRC         X'38' INTERRUPTION SUBCLASS
                                            EXTRACT MASK
              1... ....      CSWQDIO        X'80' QDIO Facility (Q) Available
              .... .1..      CSWIOINC       X'04' I/O Initiation Control bit
              .... ..1.      CSWHDVA        X'02' HALT DEVICE (HDV) Assist
                                            Control bit
              .... ...1      CSWABC         X'01' ALTERNATE BLOCK CONTROL BIT
              1... ....      CSWPATH        X'80' MODEL DEPENDENT PATH FOR
                                            MSG SUBCHANL
              ..11 111.      CSWMSV         X'3E' MESSAGE SUBCHANNEL VALID
                                            BITS
              .1.. ....      CSWMINS        X'40' MESSAGE DEVICE MAY BE
                                            INSTALLED
    0025   37 Bitstring    1 VDEVCTL        SUBCHANNEL STATUS CONTROL
    0026   38 Bitstring    2 VDEVDEV (0)    INTERNAL DEVICE NUMBER
    0026   38 Bitstring    1 VDEVDEVC       CHANNEL NUMBER
    0027   39 Bitstring    1 VDEVDEVU       DEVICE/CONTROL UNIT NUMBER
    0028   40 Signed       4 VDEVPMW2 (0)   WORD 2 OF PMCW
    0028   40 Bitstring    1 VDEVLPM        SUBCHANNEL LOGICAL PATH MASK
    0029   41 Bitstring    1 VDEVPNOM       SUBCHANNEL PATH NOT OPERATIONAL
                                            MASK
    002A   42 Bitstring    1 VDEVLPUM       SUBCHANNEL LAST PATH USED MASK
    002B   43 Bitstring    1 VDEVPIM        SUBCHANNEL PATH INSTALLED MASK
    002C   44 Signed       4 VDEVPMW3 (0)   WORD 3 OF PMCW
    002C   44 Signed       2 VDEVMBI        MEASUREMENT BLOCK INDEX
    002E   46 Bitstring    1 VDEVPOM        SUBCHANNEL OPERATIONAL MASK
    002F   47 Bitstring    1 VDEVPAM        SUBCHANNEL PATH AVAILABLE MASK
    0030   48 Bitstring    1 VDEVCPID (8)   CHANNEL PATH IDENTIFIERS 0 - 7
    0038   56 Signed       4 VDEVPMW6 (0)   WORD 6 OF PMCW
    0038   56 Bitstring    1 VDEVZONE       ZONE
    0039   57 Bitstring    1 VDEVVISC       GUEST ISC
              .11. ....      VDEVADM        X'60' Type of Subchannel is ADM
                                            (ST=3)
              .1.. ....      VDEVMSGS       X'40' Type of Subchannel is
                                            Message
              ..1. ....      VDEVDYN        X'20' Type of Subchaneel is DYN
                                            I/O (ST=1)
    003A   58 Bitstring    1 *              RESERVED
    003B   59 Bitstring    1 VDEVECFG       EXTENDED CONTROL FLAGS
    0010   16 Bitstring    1 VDEVSUBL       LEFT DIGIT OF SUBCHANNEL NUMBER
    0011   17 Bitstring    1 VDEVSUBR       RIGHT DIGIT OF SUBCHANNEL NUMBER

#### VDEV Storage Layout

    *** VDEV - VIRTUAL DEVICE CONTROL BLOCK
    *
    *     +---------------------------+---------------------------+
    *   0 |         VDEVFPNT          |         VDEVBPNT          |
    *     +---------------------------+---------------------------+
    *   8 |         VDEVLOWN          |         VDEVTSKQ          |
    *     +-------------+------+------+---------------------------+
    *  10 |  VDEVSUB    |:VCLAS|:VTYPE|         VDEVUSER          |
    *     +------+------+------+------+------+------+------+------+
    *  18 |:VSTAT|:VWAIT|:VAFLG|:VBFLG|:VDFLG|:VCFLG|:VFFLG|:VPFLG|
    *     +------+------+------+------+------+------+------+------+
    *  20 |                                                       |
    *     =                       VDEVPMCW                        =
    *     |                           +---------------------------+
    *  38 |                           |         VDEVAIOR          |
    *     +---------------------------+---------------------------+
    *  40 |         VDEVNIOR          |         VDEVSIOR          |
    *     +---------------------------+---------------------------+
    *  48 |         VDEVIORQ          |         VDEVPIOR          |
    *     +---------------------------+---------------------------+
    *  50 |         VDEVENDQ          |         VDEVDEOT          |
    *     +---------------------------+---------------------------+
    *  58 |         VDEVRDEV          |         VDEVAEVT          |
    *     +---------------------------+---------------------------+
    *  60 |         VDEVREVT          |         VDEVCEOT          |
    *     +---------------------------+---------------------------+
    *  68 |         VDEVLMSG          |         VDEVIOCT          |
    *     +---------------------------+---------------------------+
    *  70 |         VDEVTIMH          |         VDEVTIML          |
    *     +---------------------------+---------------------------+
    *  78 |                                                       |
    *     =                       VDEVSPEC                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    *  A0 |         VDEVIOMI          |         VDEVUIOR          |
    *     +---------------------------+---------------------------+
    *  A8 |         VDEVIOCA          |         VDEVATIM          |
    *     +------+------+------+------+---------------------------+
    *  B0 |:VIOP1|:VMODL|:VCPIE|:VCRDR|         VDEVIUBK          |
    *     +------+------+------+------+---------------------------+
    *  B8 |:VLCNT|     VDEVLTOD       |         VDEVBKIA          |
    *     +------+--------------------+------+------+------+------+
    *  C0 |         VDEVIPTS          |:VSCHT|:VPMSK|:VVNET|//////|
    *     +---------------------------+------+------+------+------+
    *  C8 |         VDEVUSR1          |         VDEVUSR2          |
    *     +---------------------------+---------------------------+
    *  D0 |         VDEVUSR3          |         VDEVUSR4          |
    *     +---------------------------+---------------------------+
    *  D8 |///////////////////////////|         VDEVRTMR          |
    *     +---------------------------+---------------------------+
    *  E0 |         VDEVTRKF          |         VDEVTRKL          |
    *     +---------------------------+---------------------------+
    *  E8 |         VDEVARSL          |         VDEVARSI          |
    *     +---------------------------+------+--------------------+
    *  F0 |         VDEVARPV          |:VMDFG|////////////////////|
    *     +---------------------------+------+--------------------+
    *  F8 |         VDEVQDIO          |         VDEVAIF           |
    *     +---------------------------+---------------------------+
    * 100 |         VDEVSHTP          |         VDEVIODD          |
    *     +---------------------------+---------------------------+
    * 108 |         VDEVMBAH          |         VDEVMBAL          |
    *     +---------------------------+---------------------------+
    * 110
    *
    *** VDEV - VIRTUAL DEVICE CONTROL BLOCK

    *** Overlay for VDEVSPEC in VDEV
    *
    *     +-------------+-------------+-------------+-------------+
    *  78 |  VDEVCYLN   |  VDEVHEAD   |/////////////|  VDEVBCYL   |
    *     +-------------+-------------+-------------+-------------+
    *  80 |/////////////|  VDEVLCYL   |         VDEVLINK          |
    *     +-------------+-------------+---------------------------+
    *  88 |         VDEVBIOA          |         VDEVMDSK          |
    *     +---------------------------+------+------+-------------+
    *  90 |         VDEVBASE          |:VMNGT|:VSFLG|/////////////|
    *     +-------------+-------------+------+------+-------------+
    *  98 |  VDEVMPCT   |/////////////|         VDEVLINP          |
    *     +-------------+-------------+---------------------------+
    *  A0
    *
    *** Overlay for VDEVSPEC in VDEV

    *** Overlay for VDEVSPEC in VDEV
    *
    *     +-------------------------------------------------------+
    *  78 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////+---------------------------+
    *  98 |///////////////////////////|         VDEVDYPT          |
    *     +---------------------------+---------------------------+
    *  A0
    *
    *** Overlay for VDEVSPEC in VDEV

    *** Overlay for VDEVSPEC in VDEV
    *
    *     +-------------------------------------------------------+
    *  78 |                       VDEVCUSR                        |
    *     +---------------------------+---------------------------+
    *  80 |         VDEVCTCA          |         VDEVCTCD          |
    *     +---------------------------+---------------------------+
    *  88 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  A0
    *
    *** Overlay for VDEVSPEC in VDEV

    *** Overlay for VDEVSPEC in VDEV
    *
    *     +---------------------------+---------------------------+
    *  78 |         VDEVNIFT          |         VDEVNIDX          |
    *     +---------------------------+---------------------------+
    *  80 |         VDEVNIC           |         VDEVNID           |
    *     +---------------------------+---------------------------+
    *  88 |         VDEVSIGA          |         VDEVQMSK          |
    *     +------+------+------+------+---------------------------+
    *  90 |:VOTSK|:VITSK|:VSWFL|//////|         VDEVCHKQ          |
    *     +------+------+------+------+---------------------------+
    *  98 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  A0
    *
    *** Overlay for VDEVSPEC in VDEV

    *** Overlay for VDEVSPEC in VDEV
    *
    *     +---------------------------+---------------------------+
    *  78 |///////////////////////////|         VDEVVSP           |
    *     +---------------------------+---------------------------+
    *  80 |         VDEVVPX           |         VDEVVDS           |
    *     +---------------------------+---------------------------+
    *  88 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  A0
    *
    *** Overlay for VDEVSPEC in VDEV

    *** Overlay for VDEVSPEC in VDEV
    *
    *     +---------------------------+---------------------------+
    *  78 |         VDEVMNPT          |         VDEVLCF           |
    *     +---------------------------+---------------------------+
    *  80 |         VDEVLFIO          |///////////////////////////|
    *     +---------------------------+///////////////////////////|
    *  88 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  A0
    *
    *** Overlay for VDEVSPEC in VDEV

    *** Overlay for VDEVPMCW in VDEV
    *
    *     +---------------------------+------+------+------+------+
    *  20 |         VDEVINTP          |:VIRCF|:VCTL |:VDEVC|:VDEVU|
    *     +------+------+------+------+------+------+------+------+
    *  28 |:VLPM |:VPNOM|:VLPUM|:VPIM |  VDEVMBI    |:VPOM |:VPAM |
    *     +------+------+------+------+-------------+------+------+
    *  30 |                       VDEVCPID                        |
    *     +------+------+------+------+---------------------------+
    *  38 |:VZONE|:VVISC|//////|:VECFG| 3C
    *     +------+------+------+------+
    *
    *** Overlay for VDEVPMCW in VDEV

    *** Overlay for VDEVSUB in VDEV
    *
    *     +------+------+
    *  10 |:VSUBL|:VSUBR| 12
    *     +------+------+
    *
    *** Overlay for VDEVSUB in VDEV

#### VDEV Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    CLASAIF        0012 FF
    CLASDASD       0012 04
    CLASGRAF       0012 40
    CLASGRFR       0012 41
    CLASPOOL       0012 20
    CLASSPEC       0012 02
    CLASSVCM       0012 10
    CLASSWCH       0012 01
    CLASTAPE       0012 08
    CLASTERM       0012 80
    CSWABC         0024 01
    CSWHDVA        0024 02
    CSWIOINC       0024 04
    CSWIRC         0024 38
    CSWMINS        0024 40
    CSWMSV         0024 3E
    CSWPATH        0024 80
    CSWQDIO        0024 80
    TYPAFP1        0013 27
    TYPBSC         0013 88
    TYPCLUST       0013 30
    TYPCONS        0013 40
    TYPCTCA        0013 80
    TYPDYNIO       0013 02
    TYPELAN        0013 28
    TYPE3SCH       0013 04
    TYPFBA         0013 28
    TYPFCP         0013 10
    TYPHDLC        0013 24
    TYPIBM1        0013 10
    TYPIC          0013 02
    TYPILAN        0013 28
    TYPMSGF        0013 01
    TYPOSA         0013 20
    TYPPRT         0013 20
    TYPPUN         0013 40
    TYPRDR         0013 80
    TYPSDLC        0013 08
    TYPSYS         0013 10
    TYPTELE2       0013 20
    TYPTTY         0013 20
    TYPUNDEF       0013 1C
    TYPUNSUP       0013 01
    TYPVAFP        0013 2A
    TYP1050        0013 14
    TYP1052        0013 40
    TYP1403        0013 21
    TYP2032        0013 20
    TYP2250        0013 04
    TYP2305        0013 08
    TYP2501        0013 81
    TYP2540P       0013 42
    TYP2540R       0013 82
    TYP2700        0013 80
    TYP2741        0013 18
    TYP3SIM        0013 04
    TYP3088        0013 80
    TYP3178        0013 40
    TYP3179        0013 40
    TYP3180        0013 40
    TYP3190        0013 40
    TYP32XX        0013 22
    TYP3203        0013 26
    TYP3211        0013 22
    TYP3215        0013 40
    TYP3250        0013 04
    TYP3262        0013 23
    TYP3270        0013 40
    TYP3271        0013 20
    TYP3275        0013 10
    TYP3277        0013 80
    TYP3278        0013 40
    TYP3279        0013 40
    TYP3284        0013 08
    TYP3286        0013 08
    TYP3287        0013 09
    TYP3287L       0013 08
    TYP3288        0013 08
    TYP3289        0013 09
    TYP3289L       0013 08
    TYP3290        0013 40
    TYP3330        0013 40
    TYP3340        0013 20
    TYP3350        0013 10
    TYP3350C       0013 11
    TYP3350D       0013 12
    TYP3370        0013 02
    TYP3375        0013 80
    TYP3380        0013 04
    TYP3390        0013 82
    TYP3420        0013 10
    TYP3422        0013 80
    TYP3424        0013 42
    TYP3430        0013 20
    TYP3480        0013 40
    TYP3490        0013 81
    TYP3505        0013 84
    TYP3525        0013 44
    TYP3590        0013 83
    TYP3704        0013 40
    TYP3705        0013 40
    TYP3767        0013 18
    TYP3800        0013 28
    TYP3820        0013 25
    TYP3851        0013 02
    TYP3890        0013 08
    TYP4245        0013 24
    TYP4248        0013 29
    TYP5080        0013 06
    TYP9032        0013 80
    TYP9033        0013 40
    TYP9332        0013 21
    TYP9335        0013 22
    TYP9336        0013 24
    TYP9345        0013 81
    TYP9348        0013 44
    VDEVACTV       0018 F0
    VDEVADM        0039 60
    VDEVAEVT       005C
    VDEVAFLG       001A
    VDEVAIF        00FC
    VDEVAIOR       003C
    VDEVARPV       00F0
    VDEVARSI       00EC
    VDEVARSL       00E8
    VDEVATIM       00AC
    VDEVATTN       001D 08
    VDEVBASE       0090
    VDEVBCC0       001B 80
    VDEVBCYL       007E
    VDEVBFLG       001B
    VDEVBIOA       0088
    VDEVBKIA       00BC
    VDEVBPCI       001B 40
    VDEVBPNT       0004
    VDEVBRGS       001D 04
    VDEVBSUI       001B 20
    VDEVBUSY       0018 80
    VDEVBYSZ       010C 00000110
    VDEVCA         0094 80
    VDEVCATT       0018 01
    VDEVCEOT       0064
    VDEVCFLG       001D
    VDEVCHKQ       0094
    VDEVCLAS       0012
    VDEVCLRF       0018 20
    VDEVCMS        001B 04
    VDEVCNA        0094 40
    VDEVCODE       0012
    VDEVCPCL       001F 80
    VDEVCPID       0030
    VDEVCPIE       00B2
    VDEVCRDR       00B3
    VDEVCTCA       0080
    VDEVCTCD       0084
    VDEVCTL        0025
    VDEVCUSR       0078
    VDEVCYLN       0078
    VDEVCYL0       0078 78
    VDEVCYL1       0078 79
    VDEVDCTL       0094 10
    VDEVDED        001A 08
    VDEVDEOT       0054
    VDEVDEV        0026
    VDEVDEVC       0026
    VDEVDEVU       0027
    VDEVDFLG       001C
    VDEVDIAL       001C 20
    VDEVDING       001D 10
    VDEVDPRE       001F 10
    VDEVDTCH       001A 01
    VDEVDVFP       001E 20
    VDEVDYN        0039 20
    VDEVDYPT       009C
    VDEVECFG       003B
    VDEVEEXT       0080
    VDEVENAB       001C 40
    VDEVENDQ       0050
    VDEVFBA        001E 08
    VDEVFFLG       001E
    VDEVFPNT       0000
    VDEVFPO        001A 02
    VDEVFULL       001A 10
    VDEVGCWE       001C 01
    VDEVGSUS       001D 20
    VDEVHEAD       007A
    VDEVHED0       007A 7A
    VDEVHED1       007A 7B
    VDEVHLTF       0018 10
    VDEVIMRS       0019 80
    VDEVINTP       0020
    VDEVINTV       001A 80
    VDEVINT3       001D 80
    VDEVIOCA       00A8
    VDEVIOCT       006C
    VDEVIODD       0104
    VDEVIOMI       00A0
    VDEVIOPA       00B0 40
    VDEVIOPI       00B0 20
    VDEVIOPO       00B0 10
    VDEVIOPQ       00B0 80
    VDEVIOPR       00B0 08
    VDEVIOPS       00B0 04
    VDEVIOPX       00B0 02
    VDEVIOP1       00B0
    VDEVIOP3       00B0 01
    VDEVIORQ       0048
    VDEVIPTS       00C0
    VDEVIRCF       0024
    VDEVITSK       0091
    VDEVIUBK       00B4
    VDEVLCF        007C
    VDEVLCNT       00B8
    VDEVLCYL       0082
    VDEVLFIO       0080
    VDEVLINK       0084
    VDEVLINP       009C
    VDEVLMSG       0068
    VDEVLNKE       001E 40
    VDEVLNKS       001E 80
    VDEVLOCK       0008
    VDEVLOWN       0008
    VDEVLPM        0028
    VDEVLPUM       002A
    VDEVLTOD       00B9
    VDEVMBAH       0108
    VDEVMBAL       010C
    VDEVMBAO       010C VDEVMBAL
    VDEVMBI        002C
    VDEVMBLK       0108
    VDEVMDEL       00F4 80
    VDEVMDFG       00F4
    VDEVMDSK       008C
    VDEVMNGT       0094
    VDEVMNPT       0078
    VDEVMODL       00B1
    VDEVMPCT       0098
    VDEVMPLX       001A 04
    VDEVMSGS       0039 40
    VDEVNCTL       0094 08
    VDEVNIC        0080
    VDEVNID        0084
    VDEVNIDX       007C
    VDEVNIFT       0078
    VDEVNIOR       0040
    VDEVNIP        0088 00000078
    VDEVNOTO       001C 08
    VDEVNRSM       001F 20
    VDEVNSEG       001C 02
    VDEVNSIM       00C6 80
    VDEVOTSK       0090
    VDEVPAM        002F
    VDEVPFLG       001F
    VDEVPIM        002B
    VDEVPIOR       004C
    VDEVPMCW       0020
    VDEVPMSK       00C5
    VDEVPMW0       0020
    VDEVPMW1       0024
    VDEVPMW2       0028
    VDEVPMW3       002C
    VDEVPMW6       0038
    VDEVPNOM       0029
    VDEVPOM        002E
    VDEVPOSN       0078
    VDEVPPA1       001D 40
    VDEVPRCE       0018 40
    VDEVPURG       001F 40
    VDEVQACT       001B 08
    VDEVQDIO       00F8
    VDEVQDSK       001E 10
    VDEVQMSK       008C
    VDEVQUED       0018 02
    VDEVRDEV       0058
    VDEVREVT       0060
    VDEVRFID       0095 10
    VDEVRMLF       001E 04
    VDEVRO         001C 80
    VDEVRPND       0018 04
    VDEVRSRL       001C 04
    VDEVRTMR       00DC
    VDEVSCHT       00C4
    VDEVSCPI       0095 08
    VDEVSCTL       0094 20
    VDEVSDIA       001C 10
    VDEVSEXT       007C
    VDEVSFLG       0095
    VDEVSHND       001F 01
    VDEVSHRD       001F 02
    VDEVSHTP       0100
    VDEVSIGA       0088
    VDEVSIOR       0044
    VDEVSIZE       010C 00000022
    VDEVSPEC       0078
    VDEVSTAT       0018
    VDEVSTP0       00C4 00
    VDEVSTP3       00C4 60
    VDEVSUB        0010
    VDEVSUBL       0010
    VDEVSUBR       0011
    VDEVSULF       001E 02
    VDEVSUSP       0018 08
    VDEVSWDD       0092 80
    VDEVSWFL       0092
    VDEVTDSK       001A 40
    VDEVTENB       001F 04
    VDEVTIME       0070
    VDEVTIMH       0070
    VDEVTIML       0074
    VDEVTRCW       001F 08
    VDEVTRKF       00E0
    VDEVTRKL       00E4
    VDEVTSKQ       000C
    VDEVTYPE       0013
    VDEVUIOR       00A4
    VDEVUSER       0014
    VDEVUSR1       00C8
    VDEVUSR2       00CC
    VDEVUSR3       00D0
    VDEVUSR4       00D4
    VDEVVDS        0084
    VDEVVISC       0039
    VDEVVMIO       001B 02
    VDEVVNET       00C6
    VDEVVPX        0080
    VDEVVSIM       001A 20
    VDEVVSP        007C
    VDEVVSW        00C6 40
    VDEVWAIT       0019
    VDEVWINT       0019 40
    VDEVZONE       0038

This information is based on z/VM V4R4.0. Last updated on 30 Jul 2003 at 13:26:17 EDT.
Copyright IBM Corporation, 1990, 2003