Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### SFSCB

Prolog

Control Block Contents
SFSCB DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### SFSCB Prolog

     Name       : DMSSFSCB
     Description: Shared File System Control Block
     DSECT      : SFSCB
     Function   : This macro maps data used by the CMS
                  file system support of file sharing.

#### SFSCB Control Block Content

#### SFSCB DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SFSCB          Yes Miscellaneous fields
    0000    0 Character    8 SFSFPOOL       Current filepool
    0008    8 Character    8 SFSPPOOL       Primary filepool
    0010   16 Address      4 SFSODTAD       => List of ODTs
    0014   20 Signed       4 SFSSEQCT       Sequence counter
    0018   24 Dbl-Word     8 SFSTOKEN (0)   Unique identifier for SFS object
    0018   24 Address      4 SFSTOKAD       Object address
    001C   28 Signed       4 SFSTOKSQ       Object sequence number
              00000008       SFSTOKLN       *-SFSTOKEN Token length
    0020   32 Signed       4 *              Reserved
    0024   36 Signed       4 SFSOSECB       OS ECB for READ and WRITE
    0028   40 Address      4 SFSSDE         => Common Error Handler
    002C   44 Address      4 SFSSDM         => Common Message Handler
                                            Asynchronous Request fields
    0030   48 Signed       4 SFSARCHD (0)   Asynchronous Request Chain Header
    0030   48 Signed       4 *              Reserved
    0034   52 Address      4 SFSARCF        Points to first ARCE
    0038   56 Address      4 SFSARCL        Points to last ARCE Caching
                                            fields
    003C   60 Signed       4 SFSCAWAR (18)  Cache Work Area
    0084  132 Signed       4 SFSCARET       Cache Build Return Code
    0088  136 Address      4 SFSCAADT       => Cache Build Anchor ADT
    008C  140 Address      4 SFSREFST       => Rename FST
    0090  144 Address      4 SFSREHYP       => Rename Hyperblock
    0094  148 Address      4 SFSUCCAD       => Unaccessed Cache Chain
    0098  152 Bitstring    1 SFSCAFLG       Cache flags
              1... ....      SFSFRESH       X'80' Issue Refresh_directory
              .1.. ....      SFSCACLN       X'40' Cache end-command cleanup
                                            required
              ..1. ....      SFSCACLA       X'20' A disk cleanup required
              ...1 ....      SFSFRSH6       X'10' Issue Refresh_directory for
                                            Release 6 file pool
    0099  153 Bitstring    1 *              Reserved
    009A  154 Signed       2 SFSUACNT       Count of directories on UACC
    009C  156 Bitstring    4 SFSCALWM       Caching storage low water mark
    00A0  160 Signed       4 *              Reserved UCT anchors
    00A4  164 Signed       4 * (0)          Explicit alignment
    00A4  164 Address      4 SFSUCTA        UCT anchor
    00A8  168 Signed       4 SFSUCTC        UCT count
    00AC  172 Bitstring   28 SFSUCTA1       UCT anchor block
    00C8  200 Bitstring   28 SFSUCTA2       UCT anchor block
    00E4  228 Bitstring   28 SFSUCTA3       UCT anchor block
    0100  256 Bitstring   28 SFSUCTA4       UCT anchor block
    011C  284 Bitstring   28 SFSUCTA5       UCT anchor block
    0138  312 Bitstring   28 SFSUCTA6       UCT anchor block Logical block
                                            processing fields
    0154  340 Bitstring  124 SFSWBNL        Logical block number list
    01D0  464 Bitstring  124 SFSWBAL        4K buffer address list Work unit
                                            processing
    024C  588 Address      4 SFSWUIDC       Initial counter value
    0250  592 Address      4 SFSWUBAS       Base work unit
              .... ...1      SFSWUBAI       1 Initial base work unit ID value
              .... 1...      SFSWURES       8 Number of reserved workunit IDs
              .... ...1      SFSREADO       1 Read/Only ID
              .... ..1.      SFSATOMC       2 Atomic write ID
              .... ..11      SFSSSLOG       3 Session services logging ID
              .... .1..      SFSCOPYF       4 COPYFILE write ID
    0254  596 Address      4 SFSWUSTP       => Last block of stack storage
    0258  600 Character    8 SFSWUCUR (0)   Current default work unit ID
    0258  600 Signed       4 SFSWUCU1       First half of work unit ID
                                            (zeros)
    025C  604 Signed       4 SFSWUCU2       Second half of work unit ID
    0260  608 Signed       4 SFSWUSTK (22)  Stack storage for work units
    0260  608 Address      4 *
    0264  612 Signed       4 * (2)
    026C  620 Signed       4 * (19)
    02B8  696 Bitstring    1 SFSWUFLG       Workunit flags
              1... ....      SFSWURET       X'80' There are workunits to be
                                            returned
              .1.. ....      SFSWUPOP       X'40' There are workunits to be
                                            popped
    02B9  697 Bitstring    1 * (3)          Reserved for future use
                                            OPEN/CLOSE CATALOG processing
    02BC  700 Address      4 SFSRESPA       pointer to the address of the
                                            response data returned from OPEN
                                            CATALOG or CLOSE CATALOG
    02C0  704 Signed       4 SFSRESPL       length of the response data
                                            returned from OPEN CATALOG or
                                            CLOSE CATALOG NAMEDEF processing
    02C4  708 Address      4 SFSDNT         => Dirid NAMDEF Table
    02C8  712 Address      4 SFSFNT         => File NAMDEF Table
    02CC  716 Address      4 SFSMNT         => Filemode NAMDEF Table
    02D0  720 Address      4 SFSCNT         => Command NAMDEF Table
    02D4  724 Signed       4 SFSCNTBL (0)   Command NAMDEF Table
    02D4  724 Address      4 SFSCRES        Reserved for future use
    02D8  728 Address      4 SFSCFRE        Chain of unused NAMEDEF entries
    02DC  732 Address      4 SFSCUSED       Chain of used NAMEDEF entries
    02E0  736 Signed       4 SFSCENT0 (0)   Compatability NAMEDEF entry
    02E0  736 Address      4 SFSC0NXT       => Next entry
    02E4  740 Character   16 SFSC0NAM       Compatability NAMEDEF
    02F4  756 Character  168 SFSC0PDC       Make room for PDCB
    039C  924 Signed       4 SFSCENT1 (0)   First command NAMEDEF entry
    039C  924 Address      4 SFSC1NXT       => Next entry
    03A0  928 Character   16 SFSC1NAM       First command NAMEDEF
    03B0  944 Character  168 SFSC1PDC       Make room for PDCB
    0458 1112 Signed       4 SFSCENT2 (0)   Second command NAMEDEF entry
    0458 1112 Address      4 SFSC2NXT       => Next entry
    045C 1116 Character   16 SFSC2NAM       Second command NAMEDEF
    046C 1132 Character  168 SFSC2PDC       Make room for PDCB SFSODT
    0514 1300 Bitstring  248 SFSODT         ODT for general usage SPSCA
    060C 1548 Bitstring  208 SFSSPSCA       SPSCA for general usage
    06DC 1756 Signed       4 *              Reserved for future use DMSJNL
                                            (NAMELIST) processing fields
    06E0 1760 Signed       4 SFSJNLPL (0)   Plist to call DMSJNL (NAMELIST)
    06E0 1760 Character  255 SFSJNLNK       Nickname
    07DF 2015 Bitstring    1 SFSJNLMD       Message disposition for DMSMSG
    07E0 2016 Address      4 SFSJNLAL       Address of userid length, list
    07E4 2020 Signed       4 SFSJNLSL       Length of storage to be released
    07E8 2024 Character    8 SFSJNLFP       File pool id
    07F0 2032 Character   84 SFSJNLST       Storage for 10 userids List of
                                            file pools with file space
                                            threshold exceeded (SFSFPCNT is
                                            number of filemodes available to
                                            users)
    0844 2116 Character    8 SFSFPLST (25)  Array of file pool identifiers
              000000C8       SFSFPLEN       *-SFSFPLST Length of the array in
                                            bytes
    0844 2116 Bitstring    1 SFSFPCHR (200) Initialize array to zeros ARCE
                                            (asynchronous request chain)
                                            storage management
              ...1 1..1      SFSFPCNT       25 Number of names in the array
    090C 2316 Signed       4 SFSARCHB (0)
    090C 2316 Address      4 SFSAVAIL       Addr(chain of usable ARCE
                                            storage)
    0910 2320 Bitstring    1 SFSASFLG       Asynch flags
              1... ....      SFSAFLG        X'80' Flag whether any asynch
                                            processing
    0911 2321 Bitstring    1 * (3)          Reserved for future use File
                                            Attribute Stack related
                                            information
    0914 2324 Bitstring   12 SFSFASTK       Current File Attribute Defaults
                                            in DMSFATTR MACRO format Work
                                            Unit Table management for Release
                                            1.1 Multiple Userid Support.
    0920 2336 Address      4 SFSWUTAP       => Array of table entry ptrs.
    0924 2340 Address      4 SFSWUTFP       => Free storage pool.
    0928 2344 Address      4 SFSWUTSP       => Deallocation stack.
              00000400       SFSWUTAN       1024 # Elements in ptr array.
              00001000       SFSWUTAL       4096 # Bytes in ptr array.
              00002A30       SFSWUTFL       10800 # Bytes of storage to
                                            allocate per free pool storage
                                            request. Other Miscellaneous
                                            Information
    092C 2348 Bitstring    1 SFSOFLAG       Other Miscellaneous Flags
              1... ....      SFSRECIN       X'80' Indicates whether DFSMS
                                            Implicit file Recall processing
                                            has been inhibited. '1' means
                                            RECALL OFF.
              .1.. ....      SFSRORES       X'40' Indicates whether R/O
                                            access should be respected. (Used
                                            by XEDIT & COPYFILE). '1' means
                                            RORESPECT set to ON.
    092D 2349 Bitstring    1 * (3)          Reserved for future use File I/O
                                            related information
    0930 2352 Address      4 SFSSDF         => File I/O Message handler
                                            RCM storage management For DMSRCM
                                            (File system Record Manager)
                                            storage management, store in the
                                            SFSCB the pointer (SFSRCMAV) to
                                            the first available storage chunk
                                            in the page of storage obtained
                                            by DMSRCM. Also, store the flag
                                            (SFSRCMFL.SFSARCM) that indicates
                                            whether asynchronous processing
                                            has occurred since the last
                                            end-of-command.
    0934 2356 Signed       4 SFSASRCM (0)
    0934 2356 Address      4 SFSRCMAV       Address of the first available
                                            storage chunk in the DMSRCMAS
                                            subpool
    0938 2360 Bitstring    1 SFSRCMFL       DMSRCM asynchronous flags
              1... ....      SFSARCM        X'80' When on indicates a prior
                                            asynchronous function has
                                            occurred
    0939 2361 Bitstring    1 * (3)          Reserved
    093C 2364 Bitstring    1 * (4)          Reserved File space Usage Block
                                            (FUB) Management
    0940 2368 Address      4 SFSFUBPT       Pointer to FUB Chain
    0944 2372 Signed       4 SFSFUBNA       Number of Active FUBs.
              .... ..11      SFSFUBNP       3 Number of pre-allocated FUBs
                                            Note. If the value of SFSFUBNP
                                            changes then the number of FUBs
                                            allocated here in the SFSCB must
                                            change accordingly.
    0948 2376 Dbl-Word     8 SFSFUB1 (0)    First FUB in chain
    0948 2376 Character    3 SFSF1EYE       File Space Usage Block
    094B 2379 Bitstring    1 SFSF1FLG       FUB flags FUBPREAL flag indicates
                                            that this FUB is preallocated.
                                            This flag must never be set to 0
                                            here.
    094C 2380 Address      4 SFSF1FPT       Pointer to next FUB in chain
    0950 2384 Bitstring   40 SFSF1FLD       Additional FUB fields
    0978 2424 Dbl-Word     8 SFSFUB2 (0)    Second FUB in chain
    0978 2424 Character    3 SFSF2EYE       File Space Usage Block
    097B 2427 Bitstring    1 SFSF2FLG       FUB flags FUBPREAL flag indicates
                                            that this FUB is preallocated.
                                            This flag must never be set to 0
                                            here.
    097C 2428 Address      4 SFSF2FPT       Pointer to next FUB in chain
    0980 2432 Bitstring   40 SFSF2FLD       Additional FUB fields
    09A8 2472 Dbl-Word     8 SFSFUB3 (0)    Third FUB in chain
    09A8 2472 Character    3 SFSF3EYE       File Space Usage Block
    09AB 2475 Bitstring    1 SFSF3FLG       FUB flags FUBPREAL flag indicates
                                            that this FUB is preallocated.
                                            This flag must never be set to 0
                                            here.
    09AC 2476 Address      4 SFSF3FPT       Pointer to next FUB in chain
    09B0 2480 Bitstring   40 SFSF3FLD       Additional FUB fields
    09D8 2520 Address      4 SFSBFSCB       Pointer to the DMSBFSCP block
    09DC 2524 Address      4 SFSFSSM        Pointer to the FSSM anchor Useful
                                            Equates
              00000099       SFSDIRMX       153 Maximum size of compressed
                                            dirid
              000009E0       SFSCBSIZ       *-SFSCB Length of SFSCB

#### SFSCB Storage Layout

    *** SFSCB - Control Block in SFSCB
    *
    *     +-------------------------------------------------------+
    *   0 |                       SFSFPOOL                        |
    *     +-------------------------------------------------------+
    *   8 |                       SFSPPOOL                        |
    *     +---------------------------+---------------------------+
    *  10 |         SFSODTAD          |         SFSSEQCT          |
    *     +---------------------------+---------------------------+
    *  18 |         SFSTOKAD          |         SFSTOKSQ          |
    *     +---------------------------+---------------------------+
    *  20 |///////////////////////////|         SFSOSECB          |
    *     +---------------------------+---------------------------+
    *  28 |          SFSSDE           |          SFSSDM           |
    *     +---------------------------+---------------------------+
    *  30 |///////////////////////////|         SFSARCF           |
    *     +---------------------------+---------------------------+
    *  38 |         SFSARCL           |                           |
    *     +---------------------------+                           |
    *  40 |                                                       |
    *     =                       SFSCAWAR                        =
    *     |                           +---------------------------+
    *  80 |                           |         SFSCARET          |
    *     +---------------------------+---------------------------+
    *  88 |         SFSCAADT          |         SFSREFST          |
    *     +---------------------------+---------------------------+
    *  90 |         SFSREHYP          |         SFSUCCAD          |
    *     +------+------+-------------+---------------------------+
    *  98 |:CAFLG|//////|  SFSUACNT   |         SFSCALWM          |
    *     +------+------+-------------+---------------------------+
    *  A0 |///////////////////////////|         SFSUCTA           |
    *     +---------------------------+---------------------------+
    *  A8 |         SFSUCTC           |                           |
    *     +---------------------------+                           |
    *  B0 |                                                       |
    *     =                       SFSUCTA1                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  C8 |                                                       |
    *     =                       SFSUCTA2                        =
    *     |                           +---------------------------+
    *     |                           |                           |
    *     +---------------------------+                           |
    *  E8 |                                                       |
    *     =                       SFSUCTA3                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 100 |                                                       |
    *     =                       SFSUCTA4                        =
    *     |                           +---------------------------+
    *     |                           |                           |
    *     +---------------------------+                           |
    * 120 |                                                       |
    *     =                       SFSUCTA5                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 138 |                                                       |
    *     =                       SFSUCTA6                        =
    *     |                           +---------------------------+
    *     |                           |                           |
    *     +---------------------------+                           |
    * 158 |                                                       |
    *     =                       SFSWBNL                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 1D0 |                                                       |
    *     =                       SFSWBAL                         =
    *     |                           +---------------------------+
    * 248 |                           |         SFSWUIDC          |
    *     +---------------------------+---------------------------+
    * 250 |         SFSWUBAS          |         SFSWUSTP          |
    *     +---------------------------+---------------------------+
    * 258 |         SFSWUCU1          |         SFSWUCU2          |
    *     +---------------------------+---------------------------+
    * 260 |                                                       |
    *     =                       SFSWUSTK                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 2B8
    *
    *** SFSCB - Control Block in SFSCB

    *** Overlay for SFSWUSTK in SFSCB
    *
    *     +---------------------------+---------------------------+
    * 260 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 268 |///////////////////////////|///////////////////////////|
    *     +---------------------------+///////////////////////////|
    * 270 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +------+--------------------+---------------------------+
    * 2B8 |:WUFLG|////////////////////|         SFSRESPA          |
    *     +------+--------------------+---------------------------+
    * 2C0 |         SFSRESPL          |          SFSDNT           |
    *     +---------------------------+---------------------------+
    * 2C8 |          SFSFNT           |          SFSMNT           |
    *     +---------------------------+---------------------------+
    * 2D0 |          SFSCNT           |         SFSCRES           |
    *     +---------------------------+---------------------------+
    * 2D8 |         SFSCFRE           |         SFSCUSED          |
    *     +---------------------------+---------------------------+
    * 2E0 |         SFSC0NXT          |                           |
    *     +---------------------------+                           |
    *     |                       SFSC0NAM                        |
    *     |                           +---------------------------+
    *     |                           |                           |
    *     +---------------------------+                           |
    * 2F8 |                                                       |
    *     =                       SFSC0PDC                        =
    *     |                           +---------------------------+
    * 398 |                           |         SFSC1NXT          |
    *     +---------------------------+---------------------------+
    * 3A0 |                       SFSC1NAM                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 3B0 |                                                       |
    *     =                       SFSC1PDC                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 458 |         SFSC2NXT          |                           |
    *     +---------------------------+                           |
    *     |                       SFSC2NAM                        |
    *     |                           +---------------------------+
    *     |                           |                           |
    *     +---------------------------+                           |
    * 470 |                                                       |
    *     =                       SFSC2PDC                        =
    *     |                           +---------------------------+
    *     |                           |                           |
    *     +---------------------------+                           |
    * 518 |                                                       |
    *     =                        SFSODT                         =
    *     |                           +---------------------------+
    *     |                           |                           |
    *     +---------------------------+                           |
    * 610 |                                                       |
    *     =                       SFSSPSCA                        =
    *     |                           +---------------------------+
    * 6D8 |                           |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 6E0 |                                                       |
    *     =                       SFSJNLNK                        =
    *     |                                                +------+
    * 7D8 |                                                |:JNLMD|
    *     +---------------------------+--------------------+------+
    * 7E0 |         SFSJNLAL          |         SFSJNLSL          |
    *     +---------------------------+---------------------------+
    * 7E8 |                       SFSJNLFP                        |
    *     +-------------------------------------------------------+
    * 7F0 |                                                       |
    *     =                       SFSJNLST                        =
    *     |                           +---------------------------+
    *     |                           |                           |
    *     +---------------------------+                           |
    * 848 |                                                       |
    *     =                       SFSFPLST                        =
    *     |                           +---------------------------+
    *     |                           | 90C
    *     +---------------------------+
    *
    *** Overlay for SFSWUSTK in SFSCB

    *** Overlay for SFSFPLST in SFSCB
    *
    *                                 +---------------------------+
    *     ...                     844 |                           |
    *     +---------------------------+                           |
    * 848 |                                                       |
    *     =                       SFSFPCHR                        =
    *     |                           +---------------------------+
    * 908 |                           |         SFSAVAIL          |
    *     +------+--------------------+---------------------------+
    * 910 |:ASFLG|////////////////////|         SFSFASTK          |
    *     +------+--------------------+                           |
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 920 |         SFSWUTAP          |         SFSWUTFP          |
    *     +---------------------------+------+--------------------+
    * 928 |         SFSWUTSP          |:OFLAG|////////////////////|
    *     +---------------------------+------+--------------------+
    * 930 |          SFSSDF           |         SFSRCMAV          |
    *     +------+--------------------+---------------------------+
    * 938 |:RCMFL|////////////////////|///////////////////////////|
    *     +------+--------------------+---------------------------+
    * 940 |         SFSFUBPT          |         SFSFUBNA          |
    *     +--------------------+------+---------------------------+
    * 948 |     SFSF1EYE       |:F1FLG|         SFSF1FPT          |
    *     +--------------------+------+---------------------------+
    * 950 |                                                       |
    *     =                       SFSF1FLD                        =
    *     |                                                       |
    *     +--------------------+------+---------------------------+
    * 978 |     SFSF2EYE       |:F2FLG|         SFSF2FPT          |
    *     +--------------------+------+---------------------------+
    * 980 |                                                       |
    *     =                       SFSF2FLD                        =
    *     |                                                       |
    *     +--------------------+------+---------------------------+
    * 9A8 |     SFSF3EYE       |:F3FLG|         SFSF3FPT          |
    *     +--------------------+------+---------------------------+
    * 9B0 |                                                       |
    *     =                       SFSF3FLD                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 9D8 |         SFSBFSCB          |         SFSFSSM           |
    *     +---------------------------+---------------------------+
    * 9E0
    *
    *** Overlay for SFSFPLST in SFSCB

#### SFSCB Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    SFSAFLG        0910 80
    SFSARCF        0034
    SFSARCHB       090C
    SFSARCHD       0030
    SFSARCL        0038
    SFSARCM        0938 80
    SFSASFLG       0910
    SFSASRCM       0934
    SFSATOMC       0250 02
    SFSAVAIL       090C
    SFSBFSCB       09D8
    SFSCAADT       0088
    SFSCACLA       0098 20
    SFSCACLN       0098 40
    SFSCAFLG       0098
    SFSCALWM       009C
    SFSCARET       0084
    SFSCAWAR       003C
    SFSCBSIZ       09DC 000009E0
    SFSCENT0       02E0
    SFSCENT1       039C
    SFSCENT2       0458
    SFSCFRE        02D8
    SFSCNT         02D0
    SFSCNTBL       02D4
    SFSCOPYF       0250 04
    SFSCRES        02D4
    SFSCUSED       02DC
    SFSC0NAM       02E4
    SFSC0NXT       02E0
    SFSC0PDC       02F4
    SFSC1NAM       03A0
    SFSC1NXT       039C
    SFSC1PDC       03B0
    SFSC2NAM       045C
    SFSC2NXT       0458
    SFSC2PDC       046C
    SFSDIRMX       09DC 00000099
    SFSDNT         02C4
    SFSFASTK       0914
    SFSFNT         02C8
    SFSFPCHR       0844
    SFSFPCNT       0844 19
    SFSFPLEN       0844 000000C8
    SFSFPLST       0844
    SFSFPOOL       0000
    SFSFRESH       0098 80
    SFSFRSH6       0098 10
    SFSFSSM        09DC
    SFSFUBNA       0944
    SFSFUBNP       0944 03
    SFSFUBPT       0940
    SFSFUB1        0948
    SFSFUB2        0978
    SFSFUB3        09A8
    SFSF1EYE       0948
    SFSF1FLD       0950
    SFSF1FLG       094B
    SFSF1FPT       094C
    SFSF2EYE       0978
    SFSF2FLD       0980
    SFSF2FLG       097B
    SFSF2FPT       097C
    SFSF3EYE       09A8
    SFSF3FLD       09B0
    SFSF3FLG       09AB
    SFSF3FPT       09AC
    SFSJNLAL       07E0
    SFSJNLFP       07E8
    SFSJNLMD       07DF
    SFSJNLNK       06E0
    SFSJNLPL       06E0
    SFSJNLSL       07E4
    SFSJNLST       07F0
    SFSMNT         02CC
    SFSODT         0514
    SFSODTAD       0010
    SFSOFLAG       092C
    SFSOSECB       0024
    SFSPPOOL       0008
    SFSRCMAV       0934
    SFSRCMFL       0938
    SFSREADO       0250 01
    SFSRECIN       092C 80
    SFSREFST       008C
    SFSREHYP       0090
    SFSRESPA       02BC
    SFSRESPL       02C0
    SFSRORES       092C 40
    SFSSDE         0028
    SFSSDF         0930
    SFSSDM         002C
    SFSSEQCT       0014
    SFSSPSCA       060C
    SFSSSLOG       0250 03
    SFSTOKAD       0018
    SFSTOKEN       0018
    SFSTOKLN       001C 00000008
    SFSTOKSQ       001C
    SFSUACNT       009A
    SFSUCCAD       0094
    SFSUCTA        00A4
    SFSUCTA1       00AC
    SFSUCTA2       00C8
    SFSUCTA3       00E4
    SFSUCTA4       0100
    SFSUCTA5       011C
    SFSUCTA6       0138
    SFSUCTC        00A8
    SFSWBAL        01D0
    SFSWBNL        0154
    SFSWUBAI       0250 01
    SFSWUBAS       0250
    SFSWUCUR       0258
    SFSWUCU1       0258
    SFSWUCU2       025C
    SFSWUFLG       02B8
    SFSWUIDC       024C
    SFSWUPOP       02B8 40
    SFSWURES       0250 08
    SFSWURET       02B8 80
    SFSWUSTK       0260
    SFSWUSTP       0254
    SFSWUTAL       0928 00001000
    SFSWUTAN       0928 00000400
    SFSWUTAP       0920
    SFSWUTFL       0928 00002A30
    SFSWUTFP       0924
    SFSWUTSP       0928

This information is based on z/VM V4R4.0.
Last updated on 28 Jul 2003 at 08:11:05 EDT.
Copyright IBM Corporation, 1990, 2003