STCONFIG - 64-bit CP - V4R4.0

Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### STCONFIG

Prolog

Control Block Contents
STCONFIG DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### STCONFIG Control Block Content

#### STCONFIG DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      STCONFIG       Address-Space-Control Block
    0000    0 Dbl-Word     8 STCEXTSA       Extent start address
    0008    8 Dbl-Word     8 STCEXTEA       Extent end address (highes byte)
    0010   16 Dbl-Word     8 STCNEXT (0)    Next storage config element
              00000010       STCLEN         *-STCONFIG Length of one config
                                            element

#### STCONFIG Storage Layout

    *** STCONFIG - Address-Space-Control Block
    *
    *     +-------------------------------------------------------+
    *   0 |                       STCEXTSA                        |
    *     +-------------------------------------------------------+
    *   8 |                       STCEXTEA                        |
    *     +-------------------------------------------------------+
    *
    *** STCONFIG - Address-Space-Control Block

#### STCONFIG Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    STCEXTEA       0008
    STCEXTSA       0000
    STCLEN         0010 00000010
    STCNEXT        0010

This information is based on z/VM V4R4.0. Last updated on 30 Jul 2003 at 12:28:58 EDT.
Copyright IBM Corporation, 1990, 2003