BITMP - 64-bit CP - V4R4.0

Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### BITMP

Prolog

Control Block Contents
BITMP DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### BITMP Prolog

     NAME       : HCPBITMP
     DESCRIPTION: Bit Map Control Block
     DSECT      : BITMP
     FUNCTION   : The Bit Map Control Block contains fields that control
                  access to the bits, pointers to the bits, and other
                  useful stuff.
     LOCATED BY : R2 at entry to HCPBIT routines points to a full
                  word that points to the BITMP.
     CREATED BY : HCPBIT
     DELETED BY : HCPBITRL
     REFERENCES : None
     SERIALIZED : Changes to the contents of bit maps need not be done
                  under the control of the BITMP lock, because
                  Compare-and-Swap is used to change the bits and the
                  pointers to the bits.  However, if serialization is
                  needed, the users of the bit maps should call the
                  HCPBIT entry points AS, AX, RS, RX, SX, etc., which
                  call the analogous HCPLCK entry points for control
                  over the BITMP lock.

#### BITMP Control Block Content

#### BITMP DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      BITMP          Bit Map Control Block
         This portion of the BITMP is fixed length. The final size of the BITMP
         depends on how many pointers are actually stored at BITMPPTR.
              00000000       BITMPFXD       * Fixed portion of the BITMP
    0000    0 Dbl-Word     8 BITMPLCK (3)   The BITMP lock
    0018   24 Signed       4 BITMPMAX       The max bit number allowed
    001C   28 Signed       4 BITMPPGS       How many pointers at BITMPPTR
              00000020       BITMPFSZ       *-BITMP Size of fixed portion of
                                            BITMP expressed in bytes.
    0020   32 Address      4 BITMPPTR (0)   Start of variable length data.
                                            Pointers to pages of bits. The
                                            upper bound of the subscript for
                                            this array is contained in
                                            BITMPPGS.

#### BITMP Storage Layout

    *** BITMP - Bit Map Control Block
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       BITMPLCK                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    *  18 |         BITMPMAX          |         BITMPPGS          |
    *     +---------------------------+---------------------------+
    *
    *** BITMP - Bit Map Control Block

#### BITMP Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    BITMPFSZ       001C 00000020
    BITMPFXD       0000 00000000
    BITMPLCK       0000
    BITMPMAX       0018
    BITMPPGS       001C
    BITMPPTR       0020

This information is based on z/VM V4R4.0. Last updated on 30 Jul 2003 at 12:29:49 EDT.
Copyright IBM Corporation, 1990, 2003