DUCT - 64-bit CP - V4R4.0

Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### DUCT

Prolog

Control Block Contents
DUCT DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### DUCT Prolog

     Name       : HCPDUCT
     Description: Dispatchable Unit Control Table
     DSECT      : DUCT
     Function   : The DUCT maps the storage associated with the
                  Dispatchable Unit Control Table
     Located by : The DUCTO in CR2
     Created by : None.
     Deleted by : None.
     References : None.
     Serialized : When used to map a guest DUCT, the DUCT is serialized by
                  instruction stream serialization.
     Notes      : None.

#### DUCT Control Block Content

#### DUCT DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      DUCT           Dispatchable Unit Control Table
    0000    0 Signed       4 DUIBM1         Reserved for IBM use
    0004    4 Signed       4 DUIBM2         Reserved for IBM use
    0008    8 Signed       4 *              Reserved for IBM use
    000C   12 Signed       4 DUIBM4         Reserved for IBM use
    0010   16 Signed       4 DUALD          Dispatchable-Unit Access- List
                                            Designation
         ** From this point on, the DUCT varies by guest mode ** (ESA/390 vs
         ESAME) and by addressing mode (24-bit, ** 31-bit or 64-bit) when CP is
         in ESAME mode.
         * ESA/390 mode guest
    0014   20 Bitstring   44 DUBSA515 (0)   Words 5-15 for ESA/390 guest
    0014   20 Bitstring    8 *              Reserved for IBM use
    001C   28 Signed       4 DUPRGM         For use by programming
    0020   32 Signed       4 DUBSAADR       BSA addr mode & return addr First
                                            bit of the DUBSAADR field
              1... ....      DUBSAADM       X'80' BSA address mode bit
    0024   36 Signed       4 DUBSAPSW       PSW info for BSA instruction
    0028   40 Bitstring    4 *              Reserved for IBM use
    002C   44 Address      4 DUTRPCTL       Trap-Control-Block address
    0030   48 Bitstring   16 *              Reserved for IBM use
         * ESAME mode guest
    0014   20 Bitstring   44 DUG515 (0)     Words 5-15 for ESAME guest
    0014   20 Signed       4 DUGSAPSW       PSW info for BSA instruction
    0018   24 Bitstring    4 *              Reserved for IBM use
    001C   28 Signed       4 DUGPRGM        For use by programming
    0020   32 Address      8 DUG64ADR (0)   Bits 0-63 of 64-bit addr in
                                            64-bit addressing mode
    0020   32 Bitstring    4 DUG64AHI       Bits 0-31 of 64-bit addr in
                                            64-bit addressing mode Zeros in
                                            24-bit or 31-bit addressing modes
    0024   36 Signed       4 DUGSAADR       BSA addr mode & return addr in
                                            24-bit or 31-bit addressing modes
                                            Bits 32-63 of 64-bit addr in
                                            64-bit addressing mode First bit
                                            of the DUGSAADR field
              1... ....      DUGSAADM       X'80' BSA address mode bit
    0028   40 Bitstring    4 *              Reserved for IBM use
    002C   44 Address      4 DUGTRPCT       Trap-Control-Block address
    0030   48 Bitstring   16 *              Reserved for IBM use
              00000040       DUCTLEN        *-DUCT Length in bytes
              00000008       DUCTSIZE       (*-DUCT+7)/8 Length in
                                            doublewords
         Redefinition of DUBSAPSW
    0024   36 Bitstring    2 DUBSAPKM       PSW key mask
    0026   38 Bitstring    1 *              Reserved for IBM use
    0027   39 Bitstring    1 DUBSAPS1       Misc PSW stuff
              1111 ....      DUBSAPSK       X'F0' PSW key
              .... 1...      DUBSARA        X'08' Reduced authority bit
              .... ...1      DUBSAPSB       X'01' Problem state bit
         Redefinition of DUGSAPSW
    0014   20 Bitstring    2 DUGSAPKM       PSW key mask
    0016   22 Bitstring    1 *              Reserved for IBM use
    0017   23 Bitstring    1 DUGSAPS1       Misc PSW stuff
              1111 ....      DUGSAPSK       X'F0' PSW key
              .... 1...      DUGSARA        X'08' Reduced authority bit
              .... ...1      DUGSAPSB       X'01' Problem state bit

#### DUCT Storage Layout

    *** DUCT - Dispatchable Unit Control Table
    *
    *     +---------------------------+---------------------------+
    *   0 |          DUIBM1           |          DUIBM2           |
    *     +---------------------------+---------------------------+
    *   8 |///////////////////////////|          DUIBM4           |
    *     +---------------------------+---------------------------+
    *  10 |          DUALD            |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  18 |///////////////////////////|          DUPRGM           |
    *     +---------------------------+---------------------------+
    *  20 |         DUBSAADR          |         DUBSAPSW          |
    *     +---------------------------+---------------------------+
    *  28 |///////////////////////////|         DUTRPCTL          |
    *     +---------------------------+---------------------------+
    *  30 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  40
    *
    *** DUCT - Dispatchable Unit Control Table

    *** Overlay for DUBSA515 in DUCT
    *
    *                                 +---------------------------+
    *  10 ...                      14 |         DUGSAPSW          |
    *     +---------------------------+---------------------------+
    *  18 |///////////////////////////|         DUGPRGM           |
    *     +---------------------------+---------------------------+
    *  20 |         DUG64AHI          |         DUGSAADR          |
    *     +---------------------------+---------------------------+
    *  28 |///////////////////////////|         DUGTRPCT          |
    *     +---------------------------+---------------------------+
    *  30 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  40
    *
    *** Overlay for DUBSA515 in DUCT

    *** Overlay for DUBSAPSW in DUCT
    *
    *                                 +-------------+------+------+
    *  20 ...                      24 |  DUBSAPKM   |//////|:SAPS1|
    *                                 +-------------+------+------+
    *  28
    *
    *** Overlay for DUBSAPSW in DUCT

    *** Overlay for DUGSAPSW in DUCT
    *
    *                                 +-------------+------+------+
    *  10 ...                      14 |  DUGSAPKM   |//////|:SAPS1|
    *                                 +-------------+------+------+
    *  18
    *
    *** Overlay for DUGSAPSW in DUCT

#### DUCT Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    DUALD          0010
    DUBSAADM       0020 80
    DUBSAADR       0020
    DUBSAPKM       0024
    DUBSAPSB       0027 01
    DUBSAPSK       0027 F0
    DUBSAPSW       0024
    DUBSAPS1       0027
    DUBSARA        0027 08
    DUBSA515       0014
    DUCTLEN        0030 00000040
    DUCTSIZE       0030 00000008
    DUGPRGM        001C
    DUGSAADM       0024 80
    DUGSAADR       0024
    DUGSAPKM       0014
    DUGSAPSB       0017 01
    DUGSAPSK       0017 F0
    DUGSAPSW       0014
    DUGSAPS1       0017
    DUGSARA        0017 08
    DUGTRPCT       002C
    DUG515         0014
    DUG64ADR       0020
    DUG64AHI       0020
    DUIBM1         0000
    DUIBM2         0004
    DUIBM4         000C
    DUPRGM         001C
    DUTRPCTL       002C

This information is based on z/VM V4R4.0. Last updated on 30 Jul 2003 at 12:41:55 EDT.
Copyright IBM Corporation, 1990, 2003