Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSYTRSP

Prolog
Control Block Contents
Cross Reference

#### MRSYTRSP Prolog

####

####

     DSECT NAME - SYTRSP
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSYTRSP
     DESCRIPTIVE NAME - Monitor Sample Record
                        Domain 0 - System Record
                        Record 4 - Real Storage Data (Per Processor)
     DESCRIPTION - Real storage exception conditions. Provides
                   an indication of memory contention and load.
                   A separate record is generated per online
                   processor.

    MRSYTRSP Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)          Description

      0   0  Structure   48  SYTRSP              Start of monitor record
      0   0  Character    0  SYTRSP_MRHDR        record header
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN            record length in bytes
      2   2  Unsigned     2  MRHDRZER            field of zeros
      4   4  Unsigned     1  MRHDRDM             domain identifier
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC             record identifier
      8   8  Character    8  MRHDRTOD            Time at which this record was
                                                 built. In time-of-day (TOD) clock
                                                 format. See IBM System 370 XA
                                                 Principle of Operation for
                                                 explanation of format.
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END           End of header
     20  14  Unsigned     2  SYTRSP_PFXCPUAD     Processor address
     22  16  Unsigned     2  *                   Reserved for IBM use
     24  18  Unsigned     4  SYTRSP_PLSSTLFR     Count of frames taken to satisfy
                                                 the free storage extend condition.
     28  1C  Unsigned     4  SYTRSP_PLSPRQDF     Count of tasks deferred while
                                                 waiting for a page.
     32  20  Unsigned     4  SYTRSP_PLSSHRRD     Total number of page reads and
                                                 PAGINs for shared pages
     36  24  Unsigned     4  SYTRSP_PLSALEMP     Number of times the available
                                                 list became empty
     40  28  Unsigned     4  SYTRSP_PLSNOCMP     Number of times the demand scan
                                                 ran and was unable to obtain
                                                 enough frames.
     44  2C  Unsigned     4  SYTRSP_PLSMVB2G     Number of page translations that
                                                 resulted in the page being moved
                                                 from a frame >= 2GB to one < 2GB.
     48  30  Character    0  SYTRSP_END

    MRSYTRSP Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                   0     20
    MRHDR_END              14      0
    MRHDRDM                 4      1
    MRHDRLEN                0      2
    MRHDRRC                 6      2
    MRHDRTOD                8      8
    MRHDRZER                2      2
    SYTRSP                  0     48
    SYTRSP_END             30      0
    SYTRSP_MRHDR            0      0
    SYTRSP_PFXCPUAD        14      2
    SYTRSP_PLSALEMP        24      4
    SYTRSP_PLSMVB2G        2C      4
    SYTRSP_PLSNOCMP        28      4
    SYTRSP_PLSPRQDF        1C      4
    SYTRSP_PLSSHRRD        20      4
    SYTRSP_PLSSTLFR        18      4

    This information is
    based on z/VM V4R4.0.

    Last updated on 22 Jul 2003 at 15:04:23.

    Copyright IBM Corporation, 1990, 2003