Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### LKSBK

Prolog

Control Block Contents
LKSBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### LKSBK Prolog

     NAME       : HCPLKSBK
     DESCRIPTION: Linkage Stack block
     DSECT      : LKSBK
     FUNCTION   : The LKSBK maps the storage associated with a linkage
                  stack section.
     LOCATED BY : Is a mapping for the entries in a
                  linkage stack section.
     CREATED BY : n/a
     DELETED BY : n/a
     SERIALIZED : The user of the Control Block is responsi-
                  ble for the serialization which is:
                  Instruction stream or Console Funct. Mode

#### LKSBK Control Block Content

#### LKSBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      LKSBK          Linkage Stack block
                                      stack section entry
                 Mapping for a Linkage stack state entry
    0000    0 Bitstring  160 LKSENTRY (0)   Map the contents of a linkage
                                            stack state entry.(The declared
                                            length (160) does not include the
                                            state descriptor length(8)).
                 Values of general purpose registers
    0000    0 Bitstring   64 LKSGPRS (0)    General Purp. Regs. of the caller
              .... ....      LKSGPRH0       LKSGPRS+0,2 GPR halfword 0
              .... ....      LKSGPRB0       LKSGPRS+0,1 GPR byte 0
              .... ...1      LKSGPRB1       LKSGPRS+1,1 GPR byte 1
              .... ..1.      LKSGPRH1       LKSGPRS+2,2 GPR halfword 1
              .... ..1.      LKSGPRB2       LKSGPRS+2,1 GPR byte 2
              .... ..11      LKSGPRB3       LKSGPRS+3,1 GPR byte 3
    0000    0 Signed       4 LKSGPR0        General purpose register 0
    0004    4 Signed       4 LKSGPR1        General purpose register 1
    0008    8 Bitstring   52 LKSGR214 (0)   General purpose registers 2-14
    0008    8 Signed       4 LKSGPR2        General purpose register 2
    000C   12 Signed       4 LKSGPR3        General purpose register 3
    0010   16 Signed       4 LKSGPR4        General purpose register 4
    0014   20 Signed       4 LKSGPR5        General purpose register 5
    0018   24 Signed       4 LKSGPR6        General purpose register 6
    001C   28 Signed       4 LKSGPR7        General purpose register 7
    0020   32 Signed       4 LKSGPR8        General purpose register 8
    0024   36 Signed       4 LKSGPR9        General purpose register 9
    0028   40 Signed       4 LKSGPR10       General purpose register 10
    002C   44 Signed       4 LKSGPR11       General purpose register 11
    0030   48 Signed       4 LKSGPR12       General purpose register 12
    0034   52 Signed       4 LKSGPR13       General purpose register 13
    0038   56 Signed       4 LKSGPR14       General purpose register 14
    003C   60 Signed       4 LKSGPR15       General purpose register 15
                 Values of Access Registers
    0040   64 Bitstring   64 LKSARS (0)     Access registers of the caller
              .1.. ....      LKSARH0        LKSARS+0,2 AR halfword 0
              .1.. ....      LKSARB0        LKSARS+0,1 AR byte 0
              .1.. ...1      LKSARB1        LKSARS+1,1 AR byte 1
              .1.. ..1.      LKSARH1        LKSARS+2,2 AR halfword 1
              .1.. ..1.      LKSARB2        LKSARS+2,1 AR byte 2
              .1.. ..11      LKSARB3        LKSARS+3,1 AR byte 3
    0040   64 Signed       4 LKSAR0         Access register 0
    0044   68 Signed       4 LKSAR1         Access register 1
    0048   72 Bitstring   52 LKSAR214 (0)   Access registers 2-14
    0048   72 Signed       4 LKSAR2         Access register 2
    004C   76 Signed       4 LKSAR3         Access register 3
    0050   80 Signed       4 LKSAR4         Access register 4
    0054   84 Signed       4 LKSAR5         Access register 5
    0058   88 Signed       4 LKSAR6         Access register 6
    005C   92 Signed       4 LKSAR7         Access register 7
    0060   96 Signed       4 LKSAR8         Access register 8
    0064  100 Signed       4 LKSAR9         Access register 9
    0068  104 Signed       4 LKSAR10        Access register 10
    006C  108 Signed       4 LKSAR11        Access register 11
    0070  112 Signed       4 LKSAR12        Access register 12
    0074  116 Signed       4 LKSAR13        Access register 13
    0078  120 Signed       4 LKSAR14        Access register 14
    007C  124 Signed       4 LKSAR15        Access register 15
                 Mapping for a z/Arch Linkage stack state entry
    0000    0 Bitstring  288 LKSGENTY (0)   Map the contents of a z/Arch
                                            linkage stack state entry.(The
                                            length (288) does not include the
                                            state descriptor length(8)).
                 Values of z/Arch general purpose registers
                 - remap GPRs and ARs in ESA/390 format
    0000    0 Bitstring  128 LKSGGPRS (0)   General Purp. Regs. of the caller
              .... ....      LKSGGRW0       LKSGGPRS+0,4 GPR word 0 -
                                            high-order half
              .... ....      LKSGGRH0       LKSGGPRS+0,2 GPR halfword 0
              .... ....      LKSGGRB0       LKSGGPRS+0,1 GPR byte 0
              .... ...1      LKSGGRB1       LKSGGPRS+1,1 GPR byte 1
              .... ..1.      LKSGGRH1       LKSGGPRS+2,2 GPR halfword 1
              .... ..1.      LKSGGRB2       LKSGGPRS+2,1 GPR byte 2
              .... ..11      LKSGGRB3       LKSGGPRS+3,1 GPR byte 3
              .... .1..      LKSGGRW1       LKSGGPRS+4,4 GPR word 1 -
                                            low-order half
              .... .1..      LKSGGRH2       LKSGGPRS+4,2 GPR halfword 2
              .... .1..      LKSGGRB4       LKSGGPRS+4,1 GPR byte 4
              .... .1.1      LKSGGRB5       LKSGGPRS+5,1 GPR byte 5
              .... .11.      LKSGGRH3       LKSGGPRS+6,2 GPR halfword 3
              .... .11.      LKSGGRB6       LKSGGPRS+6,1 GPR byte 6
              .... .111      LKSGGRB7       LKSGGPRS+7,1 GPR byte 7
    0000    0 Dbl-Word     8 LKSGGPR0       General purpose register 0
    0008    8 Dbl-Word     8 LKSGGPR1       General purpose register 1
    0010   16 Bitstring  104 LKSGGR2E (0)   General purpose registers 2-14
    0010   16 Dbl-Word     8 LKSGGPR2       General purpose register 2
    0018   24 Dbl-Word     8 LKSGGPR3       General purpose register 3
    0020   32 Dbl-Word     8 LKSGGPR4       General purpose register 4
    0028   40 Dbl-Word     8 LKSGGPR5       General purpose register 5
    0030   48 Dbl-Word     8 LKSGGPR6       General purpose register 6
    0038   56 Dbl-Word     8 LKSGGPR7       General purpose register 7
    0040   64 Dbl-Word     8 LKSGGPR8       General purpose register 8
    0048   72 Dbl-Word     8 LKSGGPR9       General purpose register 9
    0050   80 Dbl-Word     8 LKSGGPRA       General purpose register 10
    0058   88 Dbl-Word     8 LKSGGPRB       General purpose register 11
    0060   96 Dbl-Word     8 LKSGGPRC       General purpose register 12
    0068  104 Dbl-Word     8 LKSGGPRD       General purpose register 13
    0070  112 Dbl-Word     8 LKSGGPRE       General purpose register 14
    0078  120 Dbl-Word     8 LKSGGPRF       General purpose register 15
                 Control field
    0080  128 Dbl-Word     8 LKSCR384 (0)   CR3 and pieces of CRs 8,4
    0080  128 Signed       4 LKSCR3 (0)     Control register 3
    0080  128 Bitstring    2 LKSPKM         PSW-key mask of caller
    0082  130 Bitstring    2 LKSSASN        Secondary ASN of caller
    0084  132 Signed       2 LKSCR8H1 (0)   CR8 bits 0-15
    0084  132 Bitstring    2 LKSEAX         Extended authorization index
    0086  134 Signed       2 LKSCR4H2 (0)   CR4 bits 16-31
    0086  134 Bitstring    2 LKSPASN        Primary ASN of caller
                Program Status Word
    0088  136 Dbl-Word     8 LKSPSW (0)     PSW of caller (points past instr)
                                            for a 390 guest, PSW bits 0-63
                                            for a z/Arch guest.
    0088  136 Signed       4 LKSPSW0F (0)   Caller PSW bits 0-31
    0088  136 Bitstring    1 LKSPSW0        Caller PSW byte zero, Syst. Mask
              .1.. ....      PSWPERA        X'40' PROGRAM EVENT RECORDING
                                            ACTIVE
              .... .1..      PSWTRAN        X'04' ADDRESS TRANSLATE MODE
                                            ACTIVE
              .... ..1.      PSWIOSM        X'02' I/O INTERRUPTION SUMMARY
                                            MASK
              .... ...1      PSWEXSM        X'01' EXTERNAL INTERRUPT SUMMARY
                                            MASK
              1111 11..      PSWIOMSK       X'FC' CHANNEL MASK, CHANNELS 0-5
              .... ..1.      PSWIOSMB       X'02' I/O SUMMARY MASK, CHANNEL
                                            6-15
              .... ...1      PSWEXSMB       X'01' EXTERNAL INTERRUPT SUMMARY
                                            MASK
    0089  137 Bitstring    1 LKSPSW1        Caller PSW byte one, key/emwp
              1111 ....      PSWKEY         X'F0' PSW ACCESS KEY EXTRACTION
                                            MASK
              .... 1...      PSWECMD        X'08' EXTENDED CONTROL MODE
                                            ACTIVE
              .... .1..      PSWMCHK        X'04' MACHINE CHECK SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PROGRAM PROBLEM STATE
              .... ...1      PSWMAPPD       X'01' For BC-mode PSWs created by
                                            the 370 Accommodation facility,
                                            this bit being set indicates that
                                            the PSW is really a "mapped" PSW.
                                            See HCPPSW.
    008A  138 Bitstring    1 LKSPSW2        Caller PSW byte two, EC mode
                                            Secondary/Cond. Code/Pgm mask
              11.. ....      PSWASMSK       X'C0' ADDRESS SPACE CONTROL MASK
              11.. ....      PSWHMODE       X'C0' HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' ACCESS-REGISTER MODE
              ..11 ....      PSWCOND        X'30' PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSW CONDITION CODE BIT FOR
                                            CC=2,3
              ...1 ....      PSWCOND1       X'10' PSW CONDITION CODE BIT FOR
                                            CC=1,3
              .... 1111      PSWPMSK        X'0F' FIXO+DECO+EXUN+SIGN PROGRAM
                                            MASK
              .... 1...      PSWFIXO        X'08' FIXED-PT OVERFLOW INTRPT
                                            MASK
              .... .1..      PSWDECO        X'04' DECIMAL OVERFLOW INTRPT
                                            MASK
              .... ..1.      PSWEXUN        X'02' EXPONENT UNDERFLOW INTRPT
                                            MASK
              .... ...1      PSWSIGN        X'01' SIGNIFICANCE INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PRIMARY-SPACE MODE
    008B  139 Bitstring    1 LKSPSW3        Caller PSW byte three,
    008C  140 Signed       4 LKSPSW4F (0)   PSW instruction address for a
                                            non-z/Arch guest (S/370 bits
                                            32-39 zero) z/Arch: bit32 =
                                            AMode, b33-63=0 LKS2PSW has
                                            remaining psw fields
    008C  140 Bitstring    1 LKSPSW4        Caller EC PSW byte four, AMode
              1... ....      PSW31BT        X'80' 31-BIT LOGICAL ADDRESSING
                                            MODE
              1... ....      PSWBA          PSW31BT Basic Addressing Mode
              .111 1111      PSWHIADR       X'7F' INSTRUCTION COUNTER BITS
                                            1-7 - MUST BE ZERO IN 24-BIT
                                            MODE.
              .... ....      PSW31AMF       X'80000000' ADDRESS MODE FULLWORD
                                            MASK - CORRESPONDS TO PSW31BT
    008D  141 Bitstring    3 LKSPSW57       Caller EC PSW byte 5,6,7 BC
                                            Instr.
    0090  144 Dbl-Word     8 LKSDATA (0)    Data for specific types of
                                            entries
                 Mapping for LKSDATA for a Branch state entry
    0090  144 Dbl-Word     8 LKSGBADR (0)   z/Arch guest branch address for a
                                            branch state entry
    0090  144 Signed       4 *              Reserved
    0094  148 Address      4 LKSBADDR (0)   Branch address for a branch state
                                            entry for non-z/Arch guest
    0094  148 Bitstring    1 LKSBADD0       Byte 0
              1... ....      LKSAMODE       X'80' Addressing mode bit for a
                                            branch state entry
    0095  149 Bitstring    3 *              Byte 1-3 of the branch address
    0098  152 Dbl-Word     8 LKSMODFA       Modifiable area
              000000A0       LKSENLEN       *-LKSENTRY Number of bytes to
                                            back up pointer for a state entry
                                            dsect
                 Mapping for a Linkage stack entry descriptor
                 - offset is changed in z/Arch, but no content change
    00A0  160 Dbl-Word     8 LKSEDESC (0)   Entry descriptor
    00A0  160 Bitstring    1 LKSETYPE       Entry type
              00000001       LKSHEADR       1 Header entry
              00000002       LKSTRAIL       2 Trailer entry
              00000004       LKSBRSTT       4 Branch and stack state entry
              00000005       LKSPCSTT       5 Program call state entry
              0000007F       LKSETMSK       127 Mask to obtain entry type
              1... ....      LKSUSUPR       X'80' Unstack suppression bit,
                                            valid for header or state entries
    00A1  161 Bitstring    1 LKSSECID       Section identification
    00A2  162 Bitstring    2 LKSRFS         Remaining free space in bytes
                                            between this entry and the
                                            trailer entry.
    00A4  164 Bitstring    2 LKSNES         Next entry size in bytes, zero if
                                            the current entry
    00A6  166 Bitstring    2 *              Reserved
              00000008       LKSEDSIZ       *-LKSEDESC Number of bytes in
                                            entry descriptor
                 Size of  state entry = Number of bytes in state
                                        entry DSECT + Number of bytes
                                        in entry descriptor
              000000A8       LKSENSIZ       LKSENLEN+LKSEDSIZ Number of bytes
                                            in state entry
                 Mapping for Other Status Information (after the
                 modifiable area) for z/Arch
                 - remap at entry descriptor field of ESA/390 format
    00A0  160 Bitstring   64 LKSGSTAT (0)   more status info for z/Arch
    00A0  160 Bitstring    1 LKSGRSV1 (8)   map to edesc of ESA/390 (all 0s)
    00A8  168 Dbl-Word     8 LKSPSWIA (0)   2nd half of 16-byte psw
    00A8  168 Signed       4 LKSPSW8F       1st word of IA (bit64-95 of psw)
    00AC  172 Signed       4 LKSPSWCF       2nd word of IA (bit96-127 of psw)
    00B0  176 Dbl-Word     8 LKSINSTNS (0)  Instance numbers
    00B0  176 Signed       4 LKSSASTEIN     SASTE instance number
    00B4  180 Signed       4 LKSPASTEIN     PASTE instance number
    00B8  184 Bitstring    1 LKSGRSV2 (40)  remaining reserved area
                 Values of z/Arch Access Registers
    00E0  224 Bitstring   64 LKSGARS (0)    Access registers of the caller
              111. ....      LKSGARH0       LKSGARS+0,2 AR halfword 0
              111. ....      LKSGARB0       LKSGARS+0,1 AR byte 0
              111. ...1      LKSGARB1       LKSGARS+1,1 AR byte 1
              111. ..1.      LKSGARH1       LKSGARS+2,2 AR halfword 1
              111. ..1.      LKSGARB2       LKSGARS+2,1 AR byte 2
              111. ..11      LKSGARB3       LKSGARS+3,1 AR byte 3
    00E0  224 Signed       4 LKSGAR0        Access register 0
    00E4  228 Signed       4 LKSGAR1        Access register 1
    00E8  232 Bitstring   52 LKSGAR2E (0)   Access registers 2-14
    00E8  232 Signed       4 LKSGAR2        Access register 2
    00EC  236 Signed       4 LKSGAR3        Access register 3
    00F0  240 Signed       4 LKSGAR4        Access register 4
    00F4  244 Signed       4 LKSGAR5        Access register 5
    00F8  248 Signed       4 LKSGAR6        Access register 6
    00FC  252 Signed       4 LKSGAR7        Access register 7
    0100  256 Signed       4 LKSGAR8        Access register 8
    0104  260 Signed       4 LKSGAR9        Access register 9
    0108  264 Signed       4 LKSGARA        Access register 10
    010C  268 Signed       4 LKSGARB        Access register 11
    0110  272 Signed       4 LKSGARC        Access register 12
    0114  276 Signed       4 LKSGARD        Access register 13
    0118  280 Signed       4 LKSGARE        Access register 14
    011C  284 Signed       4 LKSGARF        Access register 15
              00000120       LKSGENLN       *-LKSGENTY Number of bytes to
                                            back up ptr for a z/Arch state
                                            entry dsect
                 Mapping for z/Arch Linkage stack entry descriptor
                 - the content is the same as the ESA/390 entry desc
    0120  288 Dbl-Word     8 LKSGEDES (0)   z/Arch Entry descriptor
    0120  288 Bitstring    1 LKSGETYP       z/Arch Entry type
              00000009       LKSGHEAD       9 z/Arch Header entry
              0000000A       LKSGTRAI       10 z/Arch Trailer entry
              0000000C       LKSGBRST       12 z/Arch Branch and stack entry
              0000000D       LKSGPCST       13 z/Arch Program call state
                                            entry
    0121  289 Bitstring    1 LKSGSEID       z/Arch Section identification
    0122  290 Bitstring    2 LKSGRFS        Remaining free space in bytes
                                            bet. this entry and the trailer
                                            entry in a z/Arch linkage stack
    0124  292 Bitstring    2 LKSGNES        Next entry size in bytes, zero if
                                            the current entry
    0126  294 Bitstring    2 *              Reserved
          LKSEDSIZ EQU   *-LKSEDESC   Number of bytes in entry desc.
                                      is the same as in ESA/390
                 Size of  state entry = Number of bytes in state
                 (for z/Arch)           entry DSECT + Number of bytes
                                        in entry descriptor
              00000128       LKSGENSZ       LKSGENLN+LKSEDSIZ Number of bytes
                                            in state entry
                 Mapping for LKSDATA for a PC state entry
    0090  144 Signed       4 *              Reserved
    0094  148 Signed       4 LKSPCNUM       PC number for a program-call
                                            state entry
                 Mapping for linkage stack Header or Trailer
                        (non-z/Arch guest)
    0098  152 Bitstring    8 LKSHDTR (0)    Map the contents of the linkage
                                            stack Header or Trailer
    0098  152 Signed       4 *              Reserved
    009C  156 Address      4 LKSBFSA (0)    Backward stack-entry address or
                                            forward-section-header address
                                            respectively for header and
                                            trailer entries
    009C  156 Bitstring    1 LKSNXST0       Byte 0
              1... ....      LKSVALID       X'80' LLSBFSA pointer is valid.
    009D  157 Bitstring    3 *
              00000008       LKSHLEN        *-LKSHDTR Number of bytes to back
                                            up pointer for a Header or
                                            Trailer DSECT

#### LKSBK Storage Layout

    *** LKSBK - Linkage Stack block
    *
    *     +---------------------------+---------------------------+
    *   0 |         LKSGPR0           |         LKSGPR1           |
    *     +---------------------------+---------------------------+
    *   8 |         LKSGPR2           |         LKSGPR3           |
    *     +---------------------------+---------------------------+
    *  10 |         LKSGPR4           |         LKSGPR5           |
    *     +---------------------------+---------------------------+
    *  18 |         LKSGPR6           |         LKSGPR7           |
    *     +---------------------------+---------------------------+
    *  20 |         LKSGPR8           |         LKSGPR9           |
    *     +---------------------------+---------------------------+
    *  28 |         LKSGPR10          |         LKSGPR11          |
    *     +---------------------------+---------------------------+
    *  30 |         LKSGPR12          |         LKSGPR13          |
    *     +---------------------------+---------------------------+
    *  38 |         LKSGPR14          |         LKSGPR15          |
    *     +---------------------------+---------------------------+
    *  40 |          LKSAR0           |          LKSAR1           |
    *     +---------------------------+---------------------------+
    *  48 |          LKSAR2           |          LKSAR3           |
    *     +---------------------------+---------------------------+
    *  50 |          LKSAR4           |          LKSAR5           |
    *     +---------------------------+---------------------------+
    *  58 |          LKSAR6           |          LKSAR7           |
    *     +---------------------------+---------------------------+
    *  60 |          LKSAR8           |          LKSAR9           |
    *     +---------------------------+---------------------------+
    *  68 |         LKSAR10           |         LKSAR11           |
    *     +---------------------------+---------------------------+
    *  70 |         LKSAR12           |         LKSAR13           |
    *     +---------------------------+---------------------------+
    *  78 |         LKSAR14           |         LKSAR15           |
    *     +---------------------------+---------------------------+
    *  80
    *
    *** LKSBK - Linkage Stack block

    *** Overlay for LKSENTRY in LKSBK
    *
    *     +-------------------------------------------------------+
    *   0 |                       LKSGGPR0                        |
    *     +-------------------------------------------------------+
    *   8 |                       LKSGGPR1                        |
    *     +-------------------------------------------------------+
    *  10 |                       LKSGGPR2                        |
    *     +-------------------------------------------------------+
    *  18 |                       LKSGGPR3                        |
    *     +-------------------------------------------------------+
    *  20 |                       LKSGGPR4                        |
    *     +-------------------------------------------------------+
    *  28 |                       LKSGGPR5                        |
    *     +-------------------------------------------------------+
    *  30 |                       LKSGGPR6                        |
    *     +-------------------------------------------------------+
    *  38 |                       LKSGGPR7                        |
    *     +-------------------------------------------------------+
    *  40 |                       LKSGGPR8                        |
    *     +-------------------------------------------------------+
    *  48 |                       LKSGGPR9                        |
    *     +-------------------------------------------------------+
    *  50 |                       LKSGGPRA                        |
    *     +-------------------------------------------------------+
    *  58 |                       LKSGGPRB                        |
    *     +-------------------------------------------------------+
    *  60 |                       LKSGGPRC                        |
    *     +-------------------------------------------------------+
    *  68 |                       LKSGGPRD                        |
    *     +-------------------------------------------------------+
    *  70 |                       LKSGGPRE                        |
    *     +-------------------------------------------------------+
    *  78 |                       LKSGGPRF                        |
    *     +-------------+-------------+-------------+-------------+
    *  80 |   LKSPKM    |  LKSSASN    |   LKSEAX    |  LKSPASN    |
    *     +------+------+------+------+------+------+-------------+
    *  88 |:PSW0 |:PSW1 |:PSW2 |:PSW3 |:PSW4 |     LKSPSW57       |
    *     +------+------+------+------+------+--------------------+
    *  90 |///////////////////////////|:BADD0|////////////////////|
    *     +---------------------------+------+--------------------+
    *  98 |                       LKSMODFA                        |
    *     +------+------+-------------+-------------+-------------+
    *  A0 |:ETYPE|:SECID|   LKSRFS    |   LKSNES    |/////////////|
    *     +------+------+-------------+-------------+-------------+
    *  A8
    *
    *** Overlay for LKSENTRY in LKSBK

    *** Overlay for LKSEDESC in LKSBK
    *
    *     +-------------------------------------------------------+
    *  A0 |                       LKSGRSV1                        |
    *     +---------------------------+---------------------------+
    *  A8 |         LKSPSW8F          |         LKSPSWCF          |
    *     +---------------------------+---------------------------+
    *  B0 |        LKSSASTEIN         |        LKSPASTEIN         |
    *     +---------------------------+---------------------------+
    *  B8 |                                                       |
    *     =                       LKSGRSV2                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    *  E0 |         LKSGAR0           |         LKSGAR1           |
    *     +---------------------------+---------------------------+
    *  E8 |         LKSGAR2           |         LKSGAR3           |
    *     +---------------------------+---------------------------+
    *  F0 |         LKSGAR4           |         LKSGAR5           |
    *     +---------------------------+---------------------------+
    *  F8 |         LKSGAR6           |         LKSGAR7           |
    *     +---------------------------+---------------------------+
    * 100 |         LKSGAR8           |         LKSGAR9           |
    *     +---------------------------+---------------------------+
    * 108 |         LKSGARA           |         LKSGARB           |
    *     +---------------------------+---------------------------+
    * 110 |         LKSGARC           |         LKSGARD           |
    *     +---------------------------+---------------------------+
    * 118 |         LKSGARE           |         LKSGARF           |
    *     +------+------+-------------+-------------+-------------+
    * 120 |:GETYP|:GSEID|  LKSGRFS    |  LKSGNES    |/////////////|
    *     +------+------+-------------+-------------+-------------+
    * 128
    *
    *** Overlay for LKSEDESC in LKSBK

    *** Overlay for LKSDATA in LKSBK
    *
    *     +---------------------------+---------------------------+
    *  90 |///////////////////////////|         LKSPCNUM          |
    *     +---------------------------+---------------------------+
    *  98
    *
    *** Overlay for LKSDATA in LKSBK

    *** Overlay for LKSEDESC-LKSHLEN in LKSBK
    *
    *     +---------------------------+------+--------------------+
    *  98 |///////////////////////////|:NXST0|////////////////////|
    *     +---------------------------+------+--------------------+
    *  A0
    *
    *** Overlay for LKSEDESC-LKSHLEN in LKSBK

#### LKSBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    LKSAMODE       0094 80
    LKSARB0        0040 40
    LKSARB1        0040 41
    LKSARB2        0040 42
    LKSARB3        0040 43
    LKSARH0        0040 40
    LKSARH1        0040 42
    LKSARS         0040
    LKSAR0         0040
    LKSAR1         0044
    LKSAR10        0068
    LKSAR11        006C
    LKSAR12        0070
    LKSAR13        0074
    LKSAR14        0078
    LKSAR15        007C
    LKSAR2         0048
    LKSAR214       0048
    LKSAR3         004C
    LKSAR4         0050
    LKSAR5         0054
    LKSAR6         0058
    LKSAR7         005C
    LKSAR8         0060
    LKSAR9         0064
    LKSBADDR       0094
    LKSBADD0       0094
    LKSBFSA        009C
    LKSBRSTT       00A0 00000004
    LKSCR3         0080
    LKSCR384       0080
    LKSCR4H2       0086
    LKSCR8H1       0084
    LKSDATA        0090
    LKSEAX         0084
    LKSEDESC       00A0
    LKSEDSIZ       00A6 00000008
    LKSENLEN       0098 000000A0
    LKSENSIZ       00A6 000000A8
    LKSENTRY       0000
    LKSETMSK       00A0 0000007F
    LKSETYPE       00A0
    LKSGARA        0108
    LKSGARB        010C
    LKSGARB0       00E0 E0
    LKSGARB1       00E0 E1
    LKSGARB2       00E0 E2
    LKSGARB3       00E0 E3
    LKSGARC        0110
    LKSGARD        0114
    LKSGARE        0118
    LKSGARF        011C
    LKSGARH0       00E0 E0
    LKSGARH1       00E0 E2
    LKSGARS        00E0
    LKSGAR0        00E0
    LKSGAR1        00E4
    LKSGAR2        00E8
    LKSGAR2E       00E8
    LKSGAR3        00EC
    LKSGAR4        00F0
    LKSGAR5        00F4
    LKSGAR6        00F8
    LKSGAR7        00FC
    LKSGAR8        0100
    LKSGAR9        0104
    LKSGBADR       0090
    LKSGBRST       0120 0000000C
    LKSGEDES       0120
    LKSGENLN       011C 00000120
    LKSGENSZ       0126 00000128
    LKSGENTY       0000
    LKSGETYP       0120
    LKSGGPRA       0050
    LKSGGPRB       0058
    LKSGGPRC       0060
    LKSGGPRD       0068
    LKSGGPRE       0070
    LKSGGPRF       0078
    LKSGGPRS       0000
    LKSGGPR0       0000
    LKSGGPR1       0008
    LKSGGPR2       0010
    LKSGGPR3       0018
    LKSGGPR4       0020
    LKSGGPR5       0028
    LKSGGPR6       0030
    LKSGGPR7       0038
    LKSGGPR8       0040
    LKSGGPR9       0048
    LKSGGRB0       0000 00
    LKSGGRB1       0000 01
    LKSGGRB2       0000 02
    LKSGGRB3       0000 03
    LKSGGRB4       0000 04
    LKSGGRB5       0000 05
    LKSGGRB6       0000 06
    LKSGGRB7       0000 07
    LKSGGRH0       0000 00
    LKSGGRH1       0000 02
    LKSGGRH2       0000 04
    LKSGGRH3       0000 06
    LKSGGRW0       0000 00
    LKSGGRW1       0000 04
    LKSGGR2E       0010
    LKSGHEAD       0120 00000009
    LKSGNES        0124
    LKSGPCST       0120 0000000D
    LKSGPRB0       0000 00
    LKSGPRB1       0000 01
    LKSGPRB2       0000 02
    LKSGPRB3       0000 03
    LKSGPRH0       0000 00
    LKSGPRH1       0000 02
    LKSGPRS        0000
    LKSGPR0        0000
    LKSGPR1        0004
    LKSGPR10       0028
    LKSGPR11       002C
    LKSGPR12       0030
    LKSGPR13       0034
    LKSGPR14       0038
    LKSGPR15       003C
    LKSGPR2        0008
    LKSGPR3        000C
    LKSGPR4        0010
    LKSGPR5        0014
    LKSGPR6        0018
    LKSGPR7        001C
    LKSGPR8        0020
    LKSGPR9        0024
    LKSGRFS        0122
    LKSGRSV1       00A0
    LKSGRSV2       00B8
    LKSGR214       0008
    LKSGSEID       0121
    LKSGSTAT       00A0
    LKSGTRAI       0120 0000000A
    LKSHDTR        0098
    LKSHEADR       00A0 00000001
    LKSHLEN        009D 00000008
    LKSINSTNS      00B0
    LKSMODFA       0098
    LKSNES         00A4
    LKSNXST0       009C
    LKSPASN        0086
    LKSPASTEIN     00B4
    LKSPCNUM       0094
    LKSPCSTT       00A0 00000005
    LKSPKM         0080
    LKSPSW         0088
    LKSPSWCF       00AC
    LKSPSWIA       00A8
    LKSPSW0        0088
    LKSPSW0F       0088
    LKSPSW1        0089
    LKSPSW2        008A
    LKSPSW3        008B
    LKSPSW4        008C
    LKSPSW4F       008C
    LKSPSW57       008D
    LKSPSW8F       00A8
    LKSRFS         00A2
    LKSSASN        0082
    LKSSASTEIN     00B0
    LKSSECID       00A1
    LKSTRAIL       00A0 00000002
    LKSUSUPR       00A0 80
    LKSVALID       009C 80
    PSWAMODE       008A 40
    PSWASMSK       008A C0
    PSWBA          008C 80
    PSWCOND        008A 30
    PSWCOND1       008A 10
    PSWCOND2       008A 20
    PSWDECO        008A 04
    PSWECMD        0089 08
    PSWEXSM        0088 01
    PSWEXSMB       0088 01
    PSWEXUN        008A 02
    PSWFIXO        008A 08
    PSWHIADR       008C 7F
    PSWHMODE       008A C0
    PSWIOMSK       0088 FC
    PSWIOSM        0088 02
    PSWIOSMB       0088 02
    PSWKEY         0089 F0
    PSWMAPPD       0089 01
    PSWMCHK        0089 04
    PSWPERA        0088 40
    PSWPMODE       008A 00
    PSWPMSK        008A 0F
    PSWPROB        0089 01
    PSWSIGN        008A 01
    PSWSMODE       008A 80
    PSWTRAN        0088 04
    PSWWAIT        0089 02
    PSW31AMF       008C 00
    PSW31BT        008C 80

This information is based on z/VM V5R2.0. Last updated on 12 Apr 2006 at 17:02:44 EDT.
Copyright IBM Corporation, 1990, 2005