Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### RTEBK

Prolog

Control Block Contents
RTEBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### RTEBK Prolog

     Name       : HCPRTEBK
     Description: Region-Table Entry
     DSECT      : RTEBK
     Function   : This DSECT maps a z/Arch region-table entry (RTE).
                  The RTE defines three types of table entries:
                  region-first-table (RFT), region-second-table (RST)
                  and region-third-table (RTT).
                  An RFT entry contains an RST designation.  An RST
                  entry contains an RTT designation.  An RTT entry
                  contains a segment-table designation.
                  The format of a region-table entry is architected,
                  and described in the Principles of Operation.
     Located by : CR1      is the ASCE for the primary address space.
                  CR7      is the ASCE for the secondary address space.
                  CR13     is the ASCE for the home address space.
                  VMDPASCE is the ASCE for the primary address space.
                  ASTASCE
     Created by : HCPASMCR when an address space equal to or greater
                  than 2 gigabytes is created.
     Deleted by : HCPASMDS when the address space is destroyed.

#### RTEBK Control Block Content

#### RTEBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      RTEBK          Region-Table Entry
          RTEBK - 8 bytes, 64 bits
    0000    0 Dbl-Word     8 RTEENTRY       Entire region-table entry
          64-bit mask  X'FFFFFFFFFFFFF000'
              00FFFFFF       RTETOMH        X'FFFFFFFF' Isolate table origin
                                            (high word)
              00FFF000       RTETOML        X'FFFFF000' Isolate table origin
                                            (low word)
          64-bit mask  X'00000000000000C0'
          32-bit high  X'00000000'
              11.. ....      RTETFMSK       X'000000C0' Isolate table offset
                                            bits
          64-bit mask  X'0000000000000020'
          32-bit high  X'00000000'
              ..1. ....      RTEINVMK       X'00000020' Isolate invalid bit
          64-bit mask  X'0000000000000010'
          32-bit high  X'00000000'
              ...1 ....      RTENULMK       X'00000010' Isolate null bit - CP
                                            internal use only. See RTENBIT.
          64-bit mask  X'000000000000000C'
          32-bit high  X'00000000'
              .... 11..      RTETTMSK       X'0000000C' Isolate table type
                                            bits
          64-bit mask  X'0000000000000003'
          32-bit high  X'00000000'
              .... ..11      RTETLMSK       X'00000003' Isolate table length
                                            of region-second table or
                                            region-third table or segment
                                            table
              00000002       RTETFNUM       2 Number of table-offset bits
              00000002       RTETLNUM       2 Number of table-length bits
              00000006       RTETFSHF       6 Offset of table-offset (TF)
                                            field from right edge of RTE
              00000006       RTETFBYT       6 Bits to shift TF to get number
                                            of bytes from table origin to
                                            actual start of table
              0000000C       RTETLBYT       12 Bits to shift (TL+1) to get
                                            number of bytes from origin to
                                            end of table
              0000000B       RTERXNUM       11 Number of bits in Rx index
              0000000B       RTESXNUM       RTERXNUM Number of bits in
                                            Segment index
              000007FF       RTERXRIT       X'7FF' Mask to select a right-
                                            justified RX
              0000000B       RTERFNUM       RTERXNUM Number of bits in RFX
                                            portion of virtual address
              0000000B       RTERSNUM       RTERXNUM Number of bits in RSX
                                            portion of virtual address
              0000000B       RTERTNUM       RTERXNUM Number of bits in RTX
                                            portion of virtual address
              0000000B       RTESNUM        RTERXNUM Number of bits in SX
                                            portion of virtual address
              0000003E       RTERFXTL       64-RTETLNUM Number of bits to
                                            shift to convert between an
                                            isolated RFX and the
                                            corresponding RFTL. Also the
                                            number of bits to shift to
                                            convert between RFTL units and
                                            addressable bytes.
              00000033       RTERSXTL       64-RTERSNUM-RTETLNUM Number of
                                            bits to shift to convert between
                                            an isolated RSX and the
                                            corresponding RSTL. Also the
                                            number of bits to shift to
                                            convert between RSTL units and
                                            addressable bytes.
              00000028       RTERTXTL       64-RTERFNUM-RTERSNUM-RTETLNUM
                                            Number of bits to shift to
                                            convert between an isolated RTX
                                            and the corresponding RTTL. Also
                                            the number of bits to shift to
                                            convert between RTTL units and
                                            addressable bytes.
              0000001D       RTESXSTL       64-RTERFNUM-RTERSNUM-RTERTNUM-RTE
                                            TLNUM Number of bits to shift to
                                            convert between an isolated SX
                                            and the corresponding STL. Also
                                            the number of bits to shift to
                                            convert between STL units and
                                            addressable bytes.
              0000000B       RTEFCLR        RTERFNUM Number of bits to shift
                                            out RFX portion of virtual
                                            address, i.e. left-align RSX
              00000016       RTEFSCLR       RTERFNUM+RTERSNUM Number of bits
                                            to shift out RFX and RSX portions
                                            of virtual address, i.e.
                                            left-align RTX
              00000035       RTESHIFT       64-RTERXNUM Number of bits to
                                            shift to right-align a
                                            left-aligned Rx index
              00000008       RTELENTH       *-RTEENTRY Length of one RTE
              00000003       RTESZSHF       3 Shift to multiply by size of an
                                            RTE
    0008    8 Dbl-Word     8 RTENEXT (0)    Next RTE
    0000    0 Signed       4 RTEW0          Word 0 of RTE
    0004    4 Signed       4 RTEW1          Word 1 of RTE
    0004    4 Bitstring    1 RTEW1B0        Word 1 Byte 0 of RTE
    0005    5 Bitstring    1 RTEW1B1        Word 1 Byte 1 of RTE
    0006    6 Bitstring    1 RTEW1B2        Word 1 Byte 2 of RTE
    0007    7 Bitstring    1 RTEW1B3        Word 1 Byte 3 of RTE
    0007    7 Bitstring    1 RTEFLAG        RTE Flag Byte
              .1.. ....      RTETRANS       X'40' RTE is in the process of
                                            being validated. This bit is a
                                            non-architected CP software
                                            definition and is used to
                                            serialize RTE validation. Note
                                            that TMLL is used to test RTEIBIT
                                            and RTENBIT at the same time.
                                            This creates a dependency on
                                            RETIBIT being to the left of and
                                            in the same halfword as RTENBIT.
              ..1. ....      RTEIBIT        X'20' RTE is invalid.
              ...1 ....      RTENBIT        X'10' RTE is null and cannot be
                                            validated. This bit is a
                                            non-architected CP software
                                            definition used to identify RTEs
                                            representing non- addressable
                                            storage.
              .... 11..      RTETTBTS       X'0C' RTE table type bits
              .... 11..      RTETTF         X'0C' RTE is an RFT entry
              .... 1...      RTETTS         X'08' RTE is an RST entry
              .... .1..      RTETTT         X'04' RTE is an RTT entry

#### RTEBK Storage Layout

    *** RTEBK - Region-Table Entry
    *
    *
    *** RTEBK - Region-Table Entry

    *** Overlay for RTEBK in RTEBK
    *
    *     +-------------------------------------------------------+
    *   0 |                       RTEENTRY                        |
    *     +-------------------------------------------------------+
    *
    *** Overlay for RTEBK in RTEBK

    *** Overlay for RTEENTRY in RTEBK
    *
    *     +---------------------------+---------------------------+
    *   0 |          RTEW0            |          RTEW1            |
    *     +---------------------------+---------------------------+
    *   8
    *
    *** Overlay for RTEENTRY in RTEBK

    *** Overlay for RTEW1 in RTEBK
    *
    *                                 +------+------+------+------+
    *   0 ...                       4 |:W1B0 |:W1B1 |:W1B2 |:W1B3 |
    *                                 +------+------+------+------+
    *   8
    *
    *** Overlay for RTEW1 in RTEBK

    *** Overlay for RTEW1B3 in RTEBK
    *
    *                                                      +------+
    *   0 ...                                            7 |:FLAG |
    *                                                      +------+
    *   8
    *
    *** Overlay for RTEW1B3 in RTEBK

#### RTEBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    RTEENTRY       0000
    RTEFCLR        0000 0000000B
    RTEFLAG        0007
    RTEFSCLR       0000 00000016
    RTEIBIT        0007 20
    RTEINVMK       0000 20
    RTELENTH       0000 00000008
    RTENBIT        0007 10
    RTENEXT        0008
    RTENULMK       0000 10
    RTERFNUM       0000 0000000B
    RTERFXTL       0000 0000003E
    RTERSNUM       0000 0000000B
    RTERSXTL       0000 00000033
    RTERTNUM       0000 0000000B
    RTERTXTL       0000 00000028
    RTERXNUM       0000 0000000B
    RTERXRIT       0000 000007FF
    RTESHIFT       0000 00000035
    RTESNUM        0000 0000000B
    RTESXNUM       0000 0000000B
    RTESXSTL       0000 0000001D
    RTESZSHF       0000 00000003
    RTETFBYT       0000 00000006
    RTETFMSK       0000 C0
    RTETFNUM       0000 00000002
    RTETFSHF       0000 00000006
    RTETLBYT       0000 0000000C
    RTETLMSK       0000 03
    RTETLNUM       0000 00000002
    RTETOMH        0000 00FFFFFF
    RTETOML        0000 00FFF000
    RTETRANS       0007 40
    RTETTBTS       0007 0C
    RTETTF         0007 0C
    RTETTMSK       0000 0C
    RTETTS         0007 08
    RTETTT         0007 04
    RTEW0          0000
    RTEW1          0004
    RTEW1B0        0004
    RTEW1B1        0005
    RTEW1B2        0006
    RTEW1B3        0007

This information is based on z/VM V5R2.0. Last updated on 12 Apr 2006 at 17:41:09 EDT.
Copyright IBM Corporation, 1990, 2005