Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### WEBBK

Prolog

Control Block Contents
WEBBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### WEBBK Prolog

     Name       : HCPWEBBK
     Description: Work Element Block
     DSECT      : WEBBK
     Function   : Interface control block passed between SNA/CCS
                  and a VSM (known there as DTIWEB).  It is used
                  to request the other component to do a certain
                  piece of work.
                  Also contains IPTRGMAP, a DSECT used to map
                  the IPTRGCLS field contained in IPARML COPY
                  to the WEBBK fields WEBFUN, WEBMODE, and
                  WEBCHAR.
     Located by : WEIWEBBK  Field of WEIBK
                  VSMWEBBK  Field of VSMBK - for initial logo
     Created by : HCPVCVEB - Building a WEBBK (regular)
                  HCPVCXGO - Building a WEBBK for logo
                  HCPVCXSA - Processing an error in a WEBBK from VSM
     Deleted by : HCPVCPIL - Processing asynchronous input from VSM
                  HCPVCQSR - Processing a return from an IUCV SEND
                  with no reply
                  HCPVCVEB - Building a WEBBK (regular)
                  HCPVCVIN - Clean-up SNABK input chain
                  HCPVCVUT - Clean-up SNABK output chain
                  HCPVCXFU - Processing a non-zero IUCV return code
                  HCPVCXSA - Processing an error in a WEBBK from VSM
     Serialized : SNALOCK   Shared-exclusive lock that serializes
                  the fields SNAINN and SNAOUT, which
                  anchor the chains of WEIBKs and WEBBKs

#### WEBBK Control Block Content

#### WEBBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      WEBBK          Work Element Block
    0000    0 Bitstring    1 WEBFMT         Control area format
              00000000       WEBFMT1        X'00' Msg format-single control
                                            area
    0001    1 Bitstring    1 WEBCAN         Number of control areas
              00000001       WEBCAN1        X'01' Number of control areas is
                                            one
    0002    2 Signed       2 WEBCOUNT       Data count - length of WEBDATA
    0004    4 Bitstring    1 WEBFUN         Function code OUTBOUND IN CONSOLE
                                            MODE
              00000000       WEBCPWRT       X'00' Write to next line in
                                            output area
              00000001       WEBCPRED       X'01' Read request
              00000002       WEBCPBRK       X'02' Break connection (CP LOGOFF
                                            or DISCONNECT)
              00000003       WEBCPWIC       X'03' Write to input area,
                                            position cursor as indicated in
                                            WEBCURSR
              00000004       WEBCPCPY       X'04' Copy request
              00000005       WEBCPIED       X'05' Invalid environment
                                            definition
              00000006       WEBCPPFR       X'06' PFk reply-treat as terminal
                                            input
              00000007       WEBCPIA        X'07' Input data accepted -
                                            process
              00000008       WEBCPINA       X'08' Input data not accepted
              00000009       WEBCPREX       X'09' Reply expected by
                                            synchronous path
              0000000A       WEBCPTAB       X'0A' PF key tab operation
              0000000B       WEBCPLER       X'0B' Logical error
              0000000C       WEBCPLGO       X'0C' Logo in WEBDATA
              0000000D       WEBCPTMR       X'0D' Cmd end-no output for cmd
                                            entered
              0000000E       WEBCPPTH       X'0E' IUCV pathid
              0000000F       WEBCPCAH       X'0F' Color & hilite map
              00000010       WEBCPLSA       X'10' User and device info
                                            (accounting and TERMINAL cmd
                                            data) . FUNCTION CODE - OUTBOUND
                                            IN CMS MODE
              00000000       WEBCMWRT       X'00' Write to line number
                                            specified in WEBLINE
              00000001       WEBCMEWT       X'01' Erase output area-write to
                                            WEBLINE
              00000002       WEBCMCLR       X'02' Erase entire screen and
                                            refresh output, input, and status
                                            areas FUNCTION CODE - OUTBOUND IN
                                            FULL-SCREEN SUPPORT MODE
              00000000       WEBFSWRT       X'00' FSSM Write
              00000001       WEBFSEWT       X'01' FSSM Erase/Write
              00000002       WEBFSEWA       X'02' FSSM Erase/Write Alternate
              00000003       WEBFSRDM       X'03' FSSM Read Modified
              00000004       WEBFSRDB       X'04' FSSM Read Buffer
              00000005       WEBFSWSF       X'05' FSSM Write Structured Field
              00000006       WEBFSEAU       X'06' FSSM Erase All Unprotected
              00000007       WEBFSRBP       X'07' FSSM Read Buffer for
                                            Position
              00000008       WEBFSRMP       X'08' FSSM Read Modified for
                                            Position FUNCTION CODE - INBOUND
                                            IN ALL MODES
              00000001       WEBINLOG       X'01' Logon request
              00000002       WEBINATT       X'02' Attention interrupt without
                                            data
              00000003       WEBINERR       X'03' Unrecoverable I/O error,
                                            logoff condition
              00000004       WEBINPUT       X'04' AID and optional data input
              00000005       WEBINCB1       X'05' Cursor back 1 (cursor
                                            attention)
              00000006       WEBINLGF       X'06' VTAM generated logoff
                                            condition - CCS will logoff user
              00000007       WEBINFNU       X'07' FSSM request rejected -
                                            screen not user mode
              00000008       WEBINAOK       X'08' Normal response
              00000009       WEBINACT       X'09' Accounting data for VSM
                                            user
              0000000A       WEBINOPC       X'0A' Operation check for FSSM
                                            request
              0000000B       WEBINLER       X'0B' Logic error in SNA/CCS
                                            WEBBK
              0000000C       WEBINVER       X'0C' VSM logic error
              0000000D       WEBRDERR       X'0D' Line terminal read error
              0000000E       WEBINVTM       X'0E' VTAM machine userid input
              0000000F       WEBINGLA       X'0F' Accounting data for VSM
                                            user sent on global path FUNCTION
                                            CODE - INBOUND IN FULL-SCREEN
                                            SUPPORT MODE
              0000000F       WEBINCC1       X'0F' ATTN + BUSY, with CC1
              00000010       WEBINECU       X'10' EQUIP CHK + UNIT SPEC
              00000011       WEBINDCU       X'11' DATA CHK + UNIT SPEC
              00000012       WEBINEC        X'12' EQUIP CHK
              00000013       WEBINCRJ       X'13' CMD REJ
              00000014       WEBINCDC       X'14' (channel) DATA CHK
              00000015       WEBINCCC       X'15' (channel) CONTROL CHK
    0005    5 Bitstring    5 WEBENVR (0)    Environment definition
    0005    5 Bitstring    1 WEBMODE        Mode of operation
              00000000       WEBCONS        X'00' Console mode
              00000001       WEBCMS         X'01' CMS mode
              00000002       WEBFSSM        X'02' Full-screen support mode
              00000004       WEBVSAN        X'04' VSM internal mode
    0006    6 Bitstring    1 WEBCHAR        Character set
              00000000       WEBCHEBC       X'00' EBCDIC character set
              00000001       WEBCHAPL       X'01' APL character set
              00000002       WEBCHTXT       X'02' Text character set
              00000004       WEBCHDBC       X'04' Mixed DBCS data included
    0007    7 Bitstring    1 WEBEDIT        Editing characteristics
              1... ....      WEBIMMED       X'80' Breakdown FSSM guest
                                            immediately
              .1.. ....      WEBPETCM       X'40' This is the 'PRESS ENTER TO
                                            CONTINUE' message
              ..1. ....      WEBCLRSC       X'20' Clear the screen
              .... 1...      WEBHIEKO       X'08' Highlight input redisplay
              .... .1..      WEBEDPTI       X'04' Inhibit printing (or
                                            non-display)
              .... ..1.      WEBNOEKO       X'02' Do not redisplay input on
                                            next output line
              .... ...1      WEBEDCUP       X'01' Convert to upper case
    0008    8 Bitstring    1 WEBFLAGS       CCS flags for VSM
              1... ....      WEBTTYWT       X'80' TTY write with outstanding
                                            read
              1... ....      WEBCLVMI       WEBTTYWT Reject all outstanding
                                            VM I/O (for graphics only)
              .1.. ....      WEBCONMD       X'40' Operation to terminal with
                                            CONMODE 3270
              ..1. ....      WEBLED         X'20' Limited edit write
              ...1 ....      WEBANFSW       X'10' Allow any FSSM write -
                                            reset done
              .... 1...      WEBDIAL        X'08' Operation to a dialed
                                            device
              .... .1..      WEBNOMOR       X'04' Clear screen but no more
                                            status
              .... ..1.      WEBPRMPT       X'02' Tell VSM initial LOGON
                                            prompt
              .... ..1.      WEBCPFS        X'02' In FSSM mode: a
                                            CP-generated task
              .... ...1      WEBPASPA       X'01' Pass PA1 key to application
    0009    9 Bitstring    1 WEBCPFLG       CCS status flags for VSM outbound
              1... ....      WEBCPNCR       X'80' No carriage return (K/P
                                            only)
              .1.. ....      WEBCPPRI       X'40' Priority msg
              ..1. ....      WEBCPALM       X'20' Alarm
              ...1 ....      WEBCPMDE       X'10' CP
              .... 1...      WEBCPHLW       X'08' Highlight the write
              .... .1..      WEBCPRSP       X'04' CCS response (reply)
              .... ..1.      WEBCPRRR       X'02' CCS request, required
                                            response (send/reply)
              .... ...1      WEBCPRNR       X'01' CCS request, no response
                                            required (send)
    000A   10 Signed       2 WEBLINE        Line number for CMS WEBCMWRT and
                                            WEBCMEWT (0 origin)
    000C   12 Signed       2 WEBCURSR       Relative cursor position
                                            inbound/outbound
    000E   14 Bitstring    1 WEBTABCH       Logical tab character
    000F   15 Bitstring    1 *              Used by the VSM
    0010   16 Signed       2 WEBOFSET       Offset of data within WEBDATA
    0012   18 Signed       2 *              Used by the VSM
    0014   20 Signed       4 WEBVSMWK       VSM workarea
              00000003       WEBSIZE        (*-WEBBK+7)/8 WEBBK fixed size in
                                            doublewords
              00000018       WEBBSIZE       (*-WEBBK) WEBBK fixed size in
                                            bytes
    0018   24 Bitstring    1 WEBDATA (0)    Data area - variable size
    0018   24 Bitstring    1 WEBTYPC        LU device class
              1... ....      WEBTERM        X'80' Keyboard/printer
              .1.. ....      WEBGRAF        X'40' Graphics device
    0019   25 Bitstring    1 WEBDMDL        Device model
              00000002       WEBSCRN2       X'02' Screen size is 24 X 80
              00000003       WEBSCRN3       X'03' Screen size is 32 X 80
              00000004       WEBSCRN4       X'04' Screen size is 43 X 80
              00000005       WEBSCRN5       X'05' Screen size is 27 X 132
    001A   26 Bitstring    1 WEBDFTR        Device features
              1... ....      WEBXCLOR       X'80' Extended color
              .1.. ....      WEBXHILI       X'40' Extended highlight
              ..1. ....      WEBXPSS        X'20' Programmed symbol sets
              ...1 ....      WEBWSFQ        X'10' WSFQ reply data is present
    001B   27 Bitstring    1 WEBLINEL       Device line length
    001C   28 Signed       2 WEBSAPTH       VSM IUCV pathid
    001E   30 Signed       2 WEBPACE        Device pace value
    0020   32 Bitstring    1 WEBDTYPE       APL indicator/device type
              00000000       WEBT3215       X'00' 3215-type terminal
              00000001       WEBT3278       X'01' 3278-type terminal
              00000004       WEBT3277       X'04' 3277-type terminal
              00000018       WEBT2741       X'18' 2741-type terminal
              00000020       WEBTTTY        X'20' TTY-type terminal
              00000009       WEBINLL        *-WEBDATA Size on inbound record
                                            in bytes
    0021   33 Bitstring    1 WEBWSFQD (0)   WSFQ reply data
    0021   33 Bitstring    7 WEBRSRVD       Used for alignment purposes
    0028   40 Dbl-Word     8 WEBPART2 (0)   WEBBK extension
    0028   40 Bitstring    1 WEBTYPE        Type of WEBBK logo extension
              00000001       WEBTYPE1       X'01' Minimum logo data follows
              00000002       WEBTYPE2       X'02' System ID data follows
              00000003       WEBTYPE3       X'03' TTY online msg follows
              00000004       WEBTYPE4       X'04' 2741 online msg follows
              00000005       WEBTYPE5       X'05' Logo input area follows
              00000006       WEBTYPE6       X'06' DBCS Vector follows
              00000007       WEBTYPE7       X'07' Screen status fields follow
    0029   41 Bitstring    1 *              Reserved for future IBM use
    002A   42 Signed       2 WEBCNT2        Length of WEBDATA2
    002C   44 Signed       2 WEBLOGL2       Number of lines in second logo
    002E   46 Signed       2 WEBLOGB2       Number of bytes per line
              00000001       WEBSIZE2       (*-WEBPART2+7)/8 WEBBK extension
                                            size in doublewords
              00000008       WEBBSIZ2       (*-WEBPART2) WEBBK extension size
                                            in bytes
    0030   48 Bitstring    1 WEBDATA2 (0)   Start of variable length data
          Format of WEBTYPE7 WEBBK logo extension data
          Notes      : The format of a WEBTYPE7 WEBBK logo extension can
                NOT be changed without a corresponding change to the
                VSM.
              00000030       WEBSTAT        * Screen status fields
    0030   48 Character    8 WEBCPRD        CP Read status field
    0038   56 Character    8 WEBVMRD        VM Read status field
    0040   64 Character    8 WEBRUNN        Running status field
    0048   72 Character    8 WEBMORE        More status field
    0050   80 Character    8 WEBHOLD        Holding status field
    0058   88 Character   12 WEBNTAC        Not Accepted status field
              00000034       WEBSTATL       *-WEBSTAT Length of screen status
                                            fields
    0009    9 Bitstring    1 WEBSAFLG       VSM status flags for CCS
              ..1. ....      WEBSAHLD       X'20' Holding
              ...1 ....      WEBSAMOR       X'10' More
              .... .1..      WEBSARSP       X'04' Indicates CCS response
              .... ..1.      WEBSARRR       X'02' VSM request, response
                                            required
              .... ...1      WEBSARNR       X'01' VSM request, no response
                                            required
    000A   10 Bitstring    1 WEBLAID        Logical attention identifier
              00000000       WEBLANTR       X'00' Enter
              00000001       WEBLAPA1       X'01' PA1
              00000002       WEBLAPA2       X'02' PA2
              00000003       WEBLAPA3       X'03' PA3
              00000004       WEBLACLR       X'04' Clear key (VSM internal)
              00000005       WEBSATTN       X'05' Single attention
              00000006       WEBMATTN       X'06' Multiple attention
              00000064       WEBLALPD       X'64' Light pen
              00000065       WEBLA001       X'65' PF1
              00000066       WEBLA002       X'66' PF2
              00000067       WEBLA003       X'67' PF3
              00000068       WEBLA004       X'68' PF4
              00000069       WEBLA005       X'69' PF5
              0000006A       WEBLA006       X'6A' PF6
              0000006B       WEBLA007       X'6B' PF7
              0000006C       WEBLA008       X'6C' PF8
              0000006D       WEBLA009       X'6D' PF9
              0000006E       WEBLA010       X'6E' PF10
              0000006F       WEBLA011       X'6F' PF11
              00000070       WEBLA012       X'70' PF12
              00000071       WEBLA013       X'71' PF13
              00000072       WEBLA014       X'72' PF14
              00000073       WEBLA015       X'73' PF15
              00000074       WEBLA016       X'74' PF16
              00000075       WEBLA017       X'75' PF17
              00000076       WEBLA018       X'76' PF18
              00000077       WEBLA019       X'77' PF19
              00000078       WEBLA020       X'78' PF20
              00000079       WEBLA021       X'79' PF21
              0000007A       WEBLA022       X'7A' PF22
              0000007B       WEBLA023       X'7B' PF23
              0000007C       WEBLA024       X'7C' PF24
    000B   11 Bitstring    1 WEBNLLOS       Number lines left on screen
    0010   16 Signed       2 WEBLOGOL       Number of lines for logo
    0012   18 Signed       2 WEBLOGOB       Number of bytes per line
    0010   16 Signed       2 WEBWTCNT       Number of bytes to write prior to
                                            the read for VSM TTY
    0018   24 Bitstring    1 WEBDFLGS       Device information flags
              ..1. ....      WEBDCURR       X'20' MORE and HOLD settings
                                            should be applied to the current
                                            screen
              ...1 ....      WEBDHOLD       X'10' TERM HOLD in effect
              .... 1...      WEBDHILT       X'08' TERM HILITE in effect
              .... .1..      WEBDNBRK       X'04' TERM BRKKEY NONE in effect
              .... ..1.      WEBDMASK       X'02' TERM MASK in effect
              .... ...1      WEBDATTN       X'01' TERM ATTN in effect
    0019   25 Bitstring    2 WEBTRMSZ       DEVICE LINE LENGTH
    001B   27 Bitstring    2 WEBMORTM (0)   Contains the MORE time values
    001B   27 Bitstring    1 WEBMORBP       Contains the time in seconds from
                                            the appearance of MORE to beep
    001C   28 Bitstring    1 WEBMORCL       Contains the time in seconds from
                                            the beep to the screen clearing
    001D   29 Bitstring    3 *              Reserved for future IBM use
    0020   32 Character    8 WEBACTID       Accounting userid
    0028   40 Character    8 WEBACTNO       Account number
              00000018       WEBDINFL       *-WEBDATA Length of user and
                                            device info
    0018   24 Character    8 WEBGLACI       Userid to be charged
    0020   32 Character    8 WEBGLACN       Account number
    0028   40 Character   62 WEBGLACD       Accounting data
              0000004E       WEBGLLEN       *-WEBDATA Length of accounting
                                            data on the global path

#### WEBBK Storage Layout

    *** WEBBK - Work Element Block
    *
    *     +------+------+-------------+------+------+------+------+
    *   0 |WEBFMT|WEBCAN|  WEBCOUNT   |WEBFUN|:MODE |:CHAR |:EDIT |
    *     +------+------+-------------+------+------+------+------+
    *   8 |:FLAGS|:CPFLG|  WEBLINE    |  WEBCURSR   |:TABCH|//////|
    *     +------+------+-------------+-------------+------+------+
    *  10 |  WEBOFSET   |/////////////|         WEBVSMWK          |
    *     +------+------+------+------+-------------+-------------+
    *  18 |:TYPC |:DMDL |:DFTR |:LINEL|  WEBSAPTH   |  WEBPACE    |
    *     +------+------+------+------+-------------+-------------+
    *  20 |:DTYPE|                   WEBRSRVD                     |
    *     +------+------+-------------+-------------+-------------+
    *  28 |:TYPE |//////|  WEBCNT2    |  WEBLOGL2   |  WEBLOGB2   |
    *     +------+------+-------------+-------------+-------------+
    *
    *** WEBBK - Work Element Block

    *** Overlay for WEBDATA2 in WEBBK
    *
    *     +-------------------------------------------------------+
    *  30 |                       WEBCPRD                         |
    *     +-------------------------------------------------------+
    *  38 |                       WEBVMRD                         |
    *     +-------------------------------------------------------+
    *  40 |                       WEBRUNN                         |
    *     +-------------------------------------------------------+
    *  48 |                       WEBMORE                         |
    *     +-------------------------------------------------------+
    *  50 |                       WEBHOLD                         |
    *     +-------------------------------------------------------+
    *  58 |                       WEBNTAC                         |
    *     |                           +---------------------------+
    *     |                           | 64
    *     +---------------------------+
    *
    *** Overlay for WEBDATA2 in WEBBK

    *** Overlay for WEBCPFLG in WEBBK
    *
    *            +------+------+------+
    *   8 ..   9 |:SAFLG|:LAID |:NLLOS| C
    *            +------+------+------+
    *
    *** Overlay for WEBCPFLG in WEBBK

    *** Overlay for WEBOFSET in WEBBK
    *
    *     +-------------+-------------+
    *  10 |  WEBLOGOL   |  WEBLOGOB   | 14
    *     +-------------+-------------+
    *
    *** Overlay for WEBOFSET in WEBBK

    *** Overlay for WEBOFSET in WEBBK
    *
    *     +-------------+
    *  10 |  WEBWTCNT   | 12
    *     +-------------+
    *
    *** Overlay for WEBOFSET in WEBBK

    *** Overlay for WEBDATA in WEBBK
    *
    *     +------+-------------+------+------+--------------------+
    *  18 |:DFLGS|  WEBTRMSZ   |:MORBP|:MORCL|////////////////////|
    *     +------+-------------+------+------+--------------------+
    *  20 |                       WEBACTID                        |
    *     +-------------------------------------------------------+
    *  28 |                       WEBACTNO                        |
    *     +-------------------------------------------------------+
    *  30
    *
    *** Overlay for WEBDATA in WEBBK

    *** Overlay for WEBDATA in WEBBK
    *
    *     +-------------------------------------------------------+
    *  18 |                       WEBGLACI                        |
    *     +-------------------------------------------------------+
    *  20 |                       WEBGLACN                        |
    *     +-------------------------------------------------------+
    *  28 |                                                       |
    *     =                       WEBGLACD                        =
    *     |                                         +-------------+
    *     |                                         | 66
    *     +-----------------------------------------+
    *
    *** Overlay for WEBDATA in WEBBK

#### WEBBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    WEBACTID       0020
    WEBACTNO       0028
    WEBANFSW       0008 10
    WEBBSIZE       0014 00000018
    WEBBSIZ2       002E 00000008
    WEBCAN         0001
    WEBCAN1        0001 00000001
    WEBCHAPL       0006 00000001
    WEBCHAR        0006
    WEBCHDBC       0006 00000004
    WEBCHEBC       0006 00000000
    WEBCHTXT       0006 00000002
    WEBCLRSC       0007 20
    WEBCLVMI       0008 80
    WEBCMCLR       0004 00000002
    WEBCMEWT       0004 00000001
    WEBCMS         0005 00000001
    WEBCMWRT       0004 00000000
    WEBCNT2        002A
    WEBCONMD       0008 40
    WEBCONS        0005 00000000
    WEBCOUNT       0002
    WEBCPALM       0009 20
    WEBCPBRK       0004 00000002
    WEBCPCAH       0004 0000000F
    WEBCPCPY       0004 00000004
    WEBCPFLG       0009
    WEBCPFS        0008 02
    WEBCPHLW       0009 08
    WEBCPIA        0004 00000007
    WEBCPIED       0004 00000005
    WEBCPINA       0004 00000008
    WEBCPLER       0004 0000000B
    WEBCPLGO       0004 0000000C
    WEBCPLSA       0004 00000010
    WEBCPMDE       0009 10
    WEBCPNCR       0009 80
    WEBCPPFR       0004 00000006
    WEBCPPRI       0009 40
    WEBCPPTH       0004 0000000E
    WEBCPRD        0030
    WEBCPRED       0004 00000001
    WEBCPREX       0004 00000009
    WEBCPRNR       0009 01
    WEBCPRRR       0009 02
    WEBCPRSP       0009 04
    WEBCPTAB       0004 0000000A
    WEBCPTMR       0004 0000000D
    WEBCPWIC       0004 00000003
    WEBCPWRT       0004 00000000
    WEBCURSR       000C
    WEBDATA        0018
    WEBDATA2       0030
    WEBDATTN       0018 01
    WEBDCURR       0018 20
    WEBDFLGS       0018
    WEBDFTR        001A
    WEBDHILT       0018 08
    WEBDHOLD       0018 10
    WEBDIAL        0008 08
    WEBDINFL       0028 00000018
    WEBDMASK       0018 02
    WEBDMDL        0019
    WEBDNBRK       0018 04
    WEBDTYPE       0020
    WEBEDCUP       0007 01
    WEBEDIT        0007
    WEBEDPTI       0007 04
    WEBENVR        0005
    WEBFLAGS       0008
    WEBFMT         0000
    WEBFMT1        0000 00000000
    WEBFSEAU       0004 00000006
    WEBFSEWA       0004 00000002
    WEBFSEWT       0004 00000001
    WEBFSRBP       0004 00000007
    WEBFSRDB       0004 00000004
    WEBFSRDM       0004 00000003
    WEBFSRMP       0004 00000008
    WEBFSSM        0005 00000002
    WEBFSWRT       0004 00000000
    WEBFSWSF       0004 00000005
    WEBFUN         0004
    WEBGLACD       0028
    WEBGLACI       0018
    WEBGLACN       0020
    WEBGLLEN       0028 0000004E
    WEBGRAF        0018 40
    WEBHIEKO       0007 08
    WEBHOLD        0050
    WEBIMMED       0007 80
    WEBINACT       0004 00000009
    WEBINAOK       0004 00000008
    WEBINATT       0004 00000002
    WEBINCB1       0004 00000005
    WEBINCCC       0004 00000015
    WEBINCC1       0004 0000000F
    WEBINCDC       0004 00000014
    WEBINCRJ       0004 00000013
    WEBINDCU       0004 00000011
    WEBINEC        0004 00000012
    WEBINECU       0004 00000010
    WEBINERR       0004 00000003
    WEBINFNU       0004 00000007
    WEBINGLA       0004 0000000F
    WEBINLER       0004 0000000B
    WEBINLGF       0004 00000006
    WEBINLL        0020 00000009
    WEBINLOG       0004 00000001
    WEBINOPC       0004 0000000A
    WEBINPUT       0004 00000004
    WEBINVER       0004 0000000C
    WEBINVTM       0004 0000000E
    WEBLACLR       000A 00000004
    WEBLAID        000A
    WEBLALPD       000A 00000064
    WEBLANTR       000A 00000000
    WEBLAPA1       000A 00000001
    WEBLAPA2       000A 00000002
    WEBLAPA3       000A 00000003
    WEBLA001       000A 00000065
    WEBLA002       000A 00000066
    WEBLA003       000A 00000067
    WEBLA004       000A 00000068
    WEBLA005       000A 00000069
    WEBLA006       000A 0000006A
    WEBLA007       000A 0000006B
    WEBLA008       000A 0000006C
    WEBLA009       000A 0000006D
    WEBLA010       000A 0000006E
    WEBLA011       000A 0000006F
    WEBLA012       000A 00000070
    WEBLA013       000A 00000071
    WEBLA014       000A 00000072
    WEBLA015       000A 00000073
    WEBLA016       000A 00000074
    WEBLA017       000A 00000075
    WEBLA018       000A 00000076
    WEBLA019       000A 00000077
    WEBLA020       000A 00000078
    WEBLA021       000A 00000079
    WEBLA022       000A 0000007A
    WEBLA023       000A 0000007B
    WEBLA024       000A 0000007C
    WEBLED         0008 20
    WEBLINE        000A
    WEBLINEL       001B
    WEBLOGB2       002E
    WEBLOGL2       002C
    WEBLOGOB       0012
    WEBLOGOL       0010
    WEBMATTN       000A 00000006
    WEBMODE        0005
    WEBMORBP       001B
    WEBMORCL       001C
    WEBMORE        0048
    WEBMORTM       001B
    WEBNLLOS       000B
    WEBNOEKO       0007 02
    WEBNOMOR       0008 04
    WEBNTAC        0058
    WEBOFSET       0010
    WEBPACE        001E
    WEBPART2       0028
    WEBPASPA       0008 01
    WEBPETCM       0007 40
    WEBPRMPT       0008 02
    WEBRDERR       0004 0000000D
    WEBRSRVD       0021
    WEBRUNN        0040
    WEBSAFLG       0009
    WEBSAHLD       0009 20
    WEBSAMOR       0009 10
    WEBSAPTH       001C
    WEBSARNR       0009 01
    WEBSARRR       0009 02
    WEBSARSP       0009 04
    WEBSATTN       000A 00000005
    WEBSCRN2       0019 00000002
    WEBSCRN3       0019 00000003
    WEBSCRN4       0019 00000004
    WEBSCRN5       0019 00000005
    WEBSIZE        0014 00000003
    WEBSIZE2       002E 00000001
    WEBSTAT        0030 00000030
    WEBSTATL       0058 00000034
    WEBTABCH       000E
    WEBTERM        0018 80
    WEBTRMSZ       0019
    WEBTTTY        0020 00000020
    WEBTTYWT       0008 80
    WEBTYPC        0018
    WEBTYPE        0028
    WEBTYPE1       0028 00000001
    WEBTYPE2       0028 00000002
    WEBTYPE3       0028 00000003
    WEBTYPE4       0028 00000004
    WEBTYPE5       0028 00000005
    WEBTYPE6       0028 00000006
    WEBTYPE7       0028 00000007
    WEBT2741       0020 00000018
    WEBT3215       0020 00000000
    WEBT3277       0020 00000004
    WEBT3278       0020 00000001
    WEBVMRD        0038
    WEBVSAN        0005 00000004
    WEBVSMWK       0014
    WEBWSFQ        001A 10
    WEBWSFQD       0021
    WEBWTCNT       0010
    WEBXCLOR       001A 80
    WEBXHILI       001A 40
    WEBXPSS        001A 20

This information is based on z/VM V5R2.0. Last updated on 12 Apr 2006 at 17:40:06 EDT.
Copyright IBM Corporation, 1990, 2005