Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### FIOBK

Prolog

Control Block Contents
FIOBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### FIOBK Prolog

     NAME       : HCPFIOBK
     DESCRIPTION: FORMATTED I/O BLOCK
     DSECT      : FIOBK
     FUNCTION   : DEFINE DASD I/O REQUEST TO STAND-ALONE DASD I/O ROUTINE
                  WITH A DESCRIPTION OF THE AREA ON THE VOLUME THAT IS TO
                  USED.  THE DATA CAN BE ACCESSED BY using either a
                  relative block number or an ASA.
     LOCATED BY : GENERAL PURPOSE REGISTER 1 ON ENTRY TO HCPLODAS
     CREATED BY : HCPCKPRS - BEFORE SYSTEM INITIALIZATION ON A SYSTEM BOUNCE
                  HCPCKPSH - DURING AN ABNORMAL TERMINATION OR SHUTDOWN
                  HCPLODNC - DURING THE SYSTEM LOAD PROCESS
     DELETED BY : FIOBK IS OBVIATED WHEN SYSTEM BECOMES FUNCTIONAL

#### FIOBK Control Block Content

#### FIOBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      FIOBK          FORMATTED I/O BLOCK
         -                           INITIALIZATION AND TERMINATION
    0000    0 Bitstring    1 FIOCCWOP       CCW OP-CODE, CWODRDTA OR CWODWDTA
    0001    1 Bitstring    1 FIOFLAG        I/O CONDITION FLAG (CC=1)
              1... ....      FIOSTRFL       X'80' I/O STORAGE FAILURE, CANNOT
                                            LOAD BLOCK
              .1.. ....      FIOFAIL        X'40' I/O FAILURE AFTER 10
                                            ATTEMPTS
              ..1. ....      FIODEVIC       X'20' I/0 DEVICE DOES NOT RESPOND
              ...1 ....      FIORANGE       X'10' I/O OUTSIDE OF RANGE OF
                                            CYLINDERS OR PAGES
              .... ....      FIOSUCES       X'00' CC=0 I/O WAS SUCCESSFUL
    0002    2 Bitstring    1 FIOWRPFL       HCPWRP requesting altnuc I/O
                                            flags
              1... ....      FIOIPLRC       X'80' Read IPL rec from vol in
                                            FIOASA
              .1.. ....      FIOLODMD       X'40' Read HCPLOD from Volume in
                                            FIOASA
    0003    3 Bitstring    1 *              Reserved for future IBM use
    0004    4 Signed       4 FIOAREAS       Starting cylinder(CKD/ECKD) or
                                            page(FBA) number of the area on
                                            the volume where I/O can be done
    0008    8 Signed       4 FIOAREAL       Length in cylinders/pages of the
                                            area on the volume where I/O can
                                            done
    000C   12 Signed       2 FIOPCYLS       PAGES PER CYLINDER ON THIS DEVICE
    000E   14 Signed       2 FIOPTRKS       PAGES PER TRACK ON THIS DEVICE
    0010   16 Address      8 FIOPAGAD       Host Absolute address of page to
                                            be read or written.
    0018   24 Signed       4 FIOSUBCH       SUBCHANNEL NUMBER OF UNIT
    001C   28 Signed       4 FIOASA         Spooling ASA(CKD-CCPV, FBA-PPPV)
    0020   32 Signed       4 FIOBLKNO       BLOCK NUMBER WITH 'FILE'
    0024   36 Signed       2 FIOLEN         LENGTH OF RECORD TO BE READ OR
                                            WRITTEN
    0026   38 Signed       2 *              RESERVED FOR FUTURE IBM USE
    0028   40 Signed       4 FIORDEV        Address of RDEV block
              00000006       FIOSIZE        (*-FIOBK+7)/8 LENGTH OF FORMATTED
                                            I/O BLOCK

#### FIOBK Storage Layout

    *** FIOBK - FORMATTED I/O BLOCK
    *
    *     +------+------+------+------+---------------------------+
    *   0 |:CCWOP|:FLAG |:WRPFL|//////|         FIOAREAS          |
    *     +------+------+------+------+-------------+-------------+
    *   8 |         FIOAREAL          |  FIOPCYLS   |  FIOPTRKS   |
    *     +---------------------------+-------------+-------------+
    *  10 |                       FIOPAGAD                        |
    *     +---------------------------+---------------------------+
    *  18 |         FIOSUBCH          |          FIOASA           |
    *     +---------------------------+-------------+-------------+
    *  20 |         FIOBLKNO          |   FIOLEN    |/////////////|
    *     +---------------------------+-------------+-------------+
    *  28 |         FIORDEV           | 2C
    *     +---------------------------+
    *
    *** FIOBK - FORMATTED I/O BLOCK

#### FIOBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    FIOAREAL       0008
    FIOAREAS       0004
    FIOASA         001C
    FIOBLKNO       0020
    FIOCCWOP       0000
    FIODEVIC       0001 20
    FIOFAIL        0001 40
    FIOFLAG        0001
    FIOIPLRC       0002 80
    FIOLEN         0024
    FIOLODMD       0002 40
    FIOPAGAD       0010
    FIOPCYLS       000C
    FIOPTRKS       000E
    FIORANGE       0001 10
    FIORDEV        0028
    FIOSIZE        0028 00000006
    FIOSTRFL       0001 80
    FIOSUBCH       0018
    FIOSUCES       0001 00
    FIOWRPFL       0002

This information is based on z/VM V5R2.0. Last updated on 12 Apr 2006 at 16:55:33 EDT.
Copyright IBM Corporation, 1990, 2005