Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### MCVBK

Prolog

Control Block Contents
MCVBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### MCVBK Prolog

     NAME       : HCPMCVBK
     DESCRIPTION: VIRTUAL MACHINE CHECK BLOCK
     DSECT      : MCVBK
     FUNCTION   : HCPMCVBK MAINTAINS THE DESCRIPTION OF A MACHINE CHECK
                  INCIDENT BEFORE THE INTERRUPT IS REFLECTED TO THE GUEST.
                  THERE ARE THREE TYPES OF MCVBKS MAINTAINED IN THE SYSTEM.
                  MCVBK (DYNAMICALLY ALLOCATED MCVBK)
                  STORAGE  IS OBTAINED  FOR  A DYNAMICALLY  ALLOCATED
                  MCVBK WHEN REQUIRED.  IT HAS  TWO USES. THE CONTROL
                  PROGRAM BUILDS  MCVBKS WHEN  SOME SYSTEM  INCIDENT,
                  THAT  IS  NOT  A  REAL  MACHINE  CHECK,  IS  TO  BE
                  REFLECTED TO THE  GUEST AS A MACHINE  CHECK.  IT IS
                  ALSO USED  TO MAKE  COPIES OF  MCVBKS TO  ALLOW THE
                  REFLECTION OF  MACHINE CHECKS TO  A GUEST  TO OCURR
                  ASYNCHRONOUSLY WITH OTHER CP FUNCTION.
                  MCVBK (CPU MCVBK)
                  WE REFER TO  THIS MCVBK AS THE  'CPU MCVBK' BECAUSE
                  EACH CPU OWNS ONE, AND  ALSO TO DISTINGUISH IT FROM
                  THE  'SYSTEM  TERMINATION MCVBK'  DESCRIBED  BELOW.
                  THE CPU MCVBK  CONTAINS A DESCRIPTION OF A REAL ERROR
                  INCIDENT  (IF ANY)  CURRENTLY IN  PROGRESS ON  THIS
                  CPU.  IT  IS NEEDED MAINLY  FOR THE BENEFIT  OF THE
                  VIRTUAL  SIDE  OF  THE SYSTEM  (HCPGMCMC)  SO  THAT
                  MACHINE CHECKS CAN BE  REFLECTED TO GUESTS.  HCPMCH
                  CALLS HCPGMCMC AND PASSES  THE CPU MCVBK CONTAINING
                  THE DESCRIPTION OF THE INCIDENT.   THE CPU MCVBK IS
                  ANCHORED IN THE PREFIX PAGE BY 'PFXMCVBK'.
                  DATA IS  PLACED IN  THE MCVBK  AT THE  START OF  AN
                  INCIDENT AND IS CLEARED AT  THE END OF THE INCIDENT
                  SO  THAT THE  BLOCK REMAINS  EMPTY  UNTIL THE  NEXT
                  INCIDENT.
                  MCVBK (SYSTEM TERMINATION MCVBK)
                  THERE ARE ALSO 'SYSTEM TERMINATION' MCVBKS (THERE
                  ARE 32 IN THE SYSTEM).  THEY ARE PERMANENTLY ALLO-
                  CATED IN A WORK AREA HCPWRKMV AND REMAIN INTACT
                  ACROSS A SYSTEM TERMINATION AND SOFTWARE-RE-IPL.
                  THEY ARE USED TO PASS REAL MACHINE CHECK (OR OTHER
                  SYSTEM INCIDENT) DESCRIPTIONS TO INDIVIDUAL VMDBKS
                  IN THE V=R GUEST CONFIGURATION SO THAT MACHINE
                  CHECKS MAY BY REFLECTED TO THE V=R GUEST AFTER THE
                  SYSTEM HAS RE-IPL'D.
                  AT SYSTEM  TERMINATION TIME, HCPWRP  CALLS HCPMCWMD.
                  HCPMCWMD GATHERS INFORMATION FROM THE INDIVIDUAL
                  CPU MCVBK'S (AND OTHER SOURCES) AND PLACE IT IN THE
                  SYSTEM TERMINATION MCVBKS (ONE SYSTEM TERMINATION
                  MCVBK IS USED TO RECORD THE STATE OF ONE REAL CPU).
                  AFTER THE SOFTWARE-RE-IPL THESE MCVBKS ARE PASSED
                  TO HCPGMCGS SO THAT A MACHINE CHECK CAN BE
                  REFLECTED TO THE V=R GUEST IF APPROPRIATE.
     LOCATED BY : HCPWRKMC  (ANCHOR) SYSTEM TERMINATION PERMANENT MCVBKS
                  VMDMCV    FIELD OF HCPVMDBK
                  PFXMCVBK  FIELD OF HCPPFXBK (PERMANENTLY ALLOCATED)
                  MCVNEXT   FORWARD CHAIN
                  CHCMCV    FIELD OF HCPCHCBK
     CREATED BY : HCPGMC   TO SEPARATE MCVBKS RECEIVED INTO ELEMENTARY MACHINE
                  CHECKS AND TO GENERATE MCVBKS FOR MACHINE CHECK
                  REFLECTION TO A GUEST.
                  HCPMCH   TO COPY PERMANENTLY ALLOCATED MCVBK.
                  HCPMCW   WHEN GUEST WAS RUNNING ON A PROCESSOR THAT IS RESET.
                  TO COPY MCVBK RECEIVED FROM HCPALL.
                  HCPMPS   ACQUIRES PERMANENTLY ALLOCATED MCVBK FOR EACH
                  PROCESSOR.
                  HCPRFC   CREATES A CRW MCVBK.
                  HCPVDB   CREATES A CRW MCVBK.
                  HCPVOF   CREATES A CRW MCVBK.
                  HCPVSC   CREATES A CRW MCVBK.
     DELETED BY : HCPMCH   DELETES MCVBKS CREATED BY HCPMCH
                  HCPMCW   DELETES MCVBKS CREATED BY HCPMCW
                  HCPMCV   DELETES MCVBK AFTER REFLECTING MACHINE CHECK TO THE
                  GUEST
                  HCPMPS   RETURNS  PERMANENTLY ALLOCATED MCVBK FOR EACH
                  PROCESSOR.

#### MCVBK Control Block Content

#### MCVBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      MCVBK          VIRTUAL MACHINE CHECK BLOCK
    0000    0 Dbl-Word     8 MCVMCIC (0)    MACHINE CHECK INTERRUPTION CODE
                                            (FOR PURPOSES OF HCPGMC, THIS
                                            APPLIES TO THE MCVVMDBK GUEST,
                                            EXCEPT FOR THE STORAGE ERROR BITS
                                            WHICH APPLY TO MCVFSAUS.)
    0000    0 Signed       4 MCVMCWD0 (0)   FIRST WORD OF MCVMCIC
    0000    0 Bitstring    2 MCVMCB01 (0)   BYTES 0 AND 1 OF MCVMCIC
    0000    0 Bitstring    1 MCVMCIC0       MACHINE CHECK IRPT CODE BYTE 0
              1111 1111      MCIPRIM0       X'FF' PRIMARY MACHINE CHECK BITS
                                            - BYTE 0
              1... ....      MCICSD         X'80' SYSTEM DAMAGE BIT.
              .1.. ....      MCICPD         X'40' PROCESSING DAMAGE BIT.
              ..1. ....      MCICSR         X'20' SYSTEM RECOVERY BIT.
              ...1 ....      MCICITD        X'10' INTERVAL TIMER DAMAGE. (370
                                            GUESTS)
              .... 1...      MCICCD         X'08' TIMING (CLOCK) FACILITY
                                            DAMAGE.
              .... .1..      MCICED         X'04' EXTERNAL DAMAGE.
              .... ...1      MCICDG         X'01' DEGRADATION BIT.
    0001    1 Bitstring    1 MCVMCIC1       MACHINE CHECK IRPT CODE BYTE 1
              1111 ....      MCIPRIM1       X'F0' PRIMARY MACHINE CHECK BITS
                                            - BYTE 1
              1... ....      MCICW          X'80' WARNING BIT.
              .1.. ....      MCICCRW        X'40' PENDING-CRW REPORT.
              ..1. ....      MCICSP         X'20' SERVICE PROCESSOR DAMAGE.
              ...1 ....      MCICCSD        X'10' CHANNEL-SUBSYSTEM DAMAGE.
              .... ..1.      MCICBU         X'02' 'BACKED UP' BIT.
              .... ...1      MCICDL         X'01' 'DELAYED' BIT. (370 GUESTS)
    0002    2 Bitstring    1 MCVMCIC2       MACHINE CHECK IRPT CODE BYTE 2
              1... ....      MCICSE         X'80' STORAGE ERROR UNCORRECTED.
              .1.. ....      MCICSC         X'40' STORAGE ERROR CORRECTED.
              ..1. ....      MCICKE         X'20' STORAGE-KEY ERROR
                                            UNCORRECTED.
              ...1 ....      MCICSDG        X'10' STORAGE DEGRADATION.
                                            MODIFIES STORAGE ERROR CORRECTED.
              .... 1...      MCICVWP        X'08' BITS 12-15 OF MC OLD PSW
                                            VALID.
              .... .1..      MCICVMS        X'04' SYSTEM MASK & KEY OF MC OLD
                                            PSW VALID.
              .... ..1.      MCICVPM        X'02' PROGRAM MASK & CC OF MC OLD
                                            PSW VALID.
              .... ...1      MCICVIA        X'01' INSTR ADDR OF MC OLD PSW IS
                                            VALID.
    0003    3 Bitstring    1 MCVMCIC3       MACHINE CHECK IRPT CODE BYTE 3
              1... ....      MCICVFA        X'80' FAILING STORAGE ADDRESS IS
                                            VALID.
              ..1. ....      MCICVED        X'20' EXTERNAL-DAMAGE CODE IS
                                            VALID.
              ...1 ....      MCICVFP        X'10' FP REGISTERS STORED ARE
                                            VALID.
              .... 1...      MCICVGR        X'08' GP REGISTERS STORED ARE
                                            VALID.
              .... .1..      MCICVCR        X'04' CONTROL REGISTERS STORED
                                            VALID.
              .... ..1.      MCICVLG        X'02' EXTENDED LOGOUT AREA IS
                                            VALID.
              .... ...1      MCICVST        X'01' INST. MODIFIED STORAGE IS
                                            VALID.
    0004    4 Signed       4 MCVMCWD1 (0)   SECOND WORD OF MCVMCIC
    0004    4 Bitstring    1 MCVMCIC4       MACHINE CHECK IRPT CODE BYTE 4
              1... ....      MCICIE         X'80' INDIRECT STORAGE ERROR
              .1.. ....      MCICVAR        X'40' ACCESS REGISTERS STORED ARE
                                            VALID
              ..1. ....      MCICDA         X'20' DELAYED ACCESS EXCEPTION
                                            BIT
    0005    5 Bitstring    1 MCVMCIC5       MACHINE CHECK IRPT CODE BYTE 5
              ..1. ....      MCICVTPR       X'20' TOD programmable register
                                            validity
              ...1 ....      MCICVXFP       X'10' Additional FP Registers
                                            Validity (ESA390) FP Control
                                            Register Validity (zArch)
              .... 1...      MCICAR         X'08' Ancillary Report Bit
              .... ..1.      MCICVCT        X'02' CPU TIMER STORED IS VALID.
              .... ...1      MCICVCC        X'01' CLOCK COMPARATOR STORED IS
                                            VALID.
    0006    6 Bitstring    1 MCVMCIC6       MACHINE CHECK IRPT CODE BYTE 6
    0007    7 Bitstring    1 MCVMCIC7       MACHINE CHECK IRPT CODE BYTE 7
    0008    8 Signed       4 MCVCRWS        CHANNEL REPORT WORD ANCHOR
    000C   12 Signed       4 *              Reserved for IBM use
    0010   16 Signed       4 MCVVMDBK       ADDR OF VMDBK RUNNING ON A REAL
                                            CPU AT THE TIME THE REAL CPU
                                            STATE WAS RECORDED IN THIS MCVBK.
                                            (FROM PFXRNUSR)
    0014   20 Signed       4 MCVFSAUS       ADDR OF VMDBK OWNING THE BAD
                                            FRAME IF HOST SEES A STORAGE
                                            ERROR AND VALID FSA. OTHERWISE
                                            ADDR IS ZERO.
    0018   24 Bitstring    1 MCVFLAG        MCVBK BIT FLAGS.
              1... ....      MCVABEND       X'80' FAILURE IS AN ABEND, NOT A
                                            MACHINE CHECK. (APPLIES TO THE
                                            MCVVMDBK GUEST FOR HCPGMC.)
              .1.. ....      MCVCKSTP       X'40' FAILURE IS A CHECK-STOP,
                                            NOT A MACHINE CHECK. OR FAILURE
                                            IS TIME-OUT + CHECK-STOP. MCVMCIC
                                            AND MCVFSAD ARE PROBABLY 0.
                                            (APPLIES TO MCVVMDBK GUEST FOR
                                            HCPGMC.)
              ..1. ....      MCVTMOUT       X'20' FAILURE IS TIMEOUT, NOT A
                                            MACHINE CHECK. MCVCKSTP WILL ALSO
                                            BE SET IF 'SIGP SENSE' SHOWS
                                            CHECK-STOP AS CAUSE. MCVMCIC &
                                            MCVFSAD ARE PROBABLY ZERO.
                                            (APPLIES TO MCVVMDBK GUEST FOR
                                            HCPGMC.)
              ...1 ....      MCVCUTOF       X'10' GUEST WAS TERMINATED
                                            ABRUPTLY. IF RUNNING SIE AT THE
                                            TIME, THE GUEST HAS NOT BEEN
                                            'UN-RUN'. THE ONLY EXAMPLE AT
                                            PRESENT: GUEST WAS STOPPED BY
                                            SIGP RESET. (APPLIES TO R11 GUEST
                                            FOR HCPGMC.)
              .... 1...      MCVCMPLT       X'08' ANY DAMAGE TO THE TASK THAT
                                            WAS RUNNING WAS REPAIRED BY THE
                                            MACHINE-CHECK FLIH. EITHER: (1) A
                                            HOST TASK INTERRUPTED BY MACHINE
                                            CHECK WAS LATER RESUMED AND
                                            COMPLETED SUCCESSFULLY, OR (2)
                                            ALL DAMAGE TO AN INTERRUPTED
                                            GUEST HAS BEEN CORRECTED.
                                            (APPLIES TO THE MCVVMDBK GUEST
                                            FOR HCPGMC.)
              .... .1..      MCVQWRK        X'04' AT THE TIME OF THE INCIDENT
                                            THERE WAS QUEUED WORK FOR THE
                                            GUEST, BUT IT HAS BEEN LOST
                                            (NEVER COMPLETED). (APPLIES TO
                                            R11 GUEST FOR HCPGMC.)
              .... ..1.      MCVSTGFX       X'02' THE STORAGE ERROR OR
                                            STORAGE KEY ERROR IDENTIFIED BY
                                            THE FAILING STORAGE ADDRESS IN
                                            MCVFSAD HAS BEEN CORRECTED BY THE
                                            MACHINE-CHECK FLIH. THIS FLAG IS
                                            MEANINGFUL ONLY IF THERE WAS A
                                            STORAGE ERROR AND A VALID FSA.
                                            (APPLIES TO THE MCVFSAUS GUEST
                                            FOR HCPGMC.)
              .... ...1      MCVSTGLS       X'01' Damage to the the guest's
                                            MCS linkage stack has occurred.
                                            (Applies to the MCVVMDBK guest
                                            for HCPGMC.)
    0019   25 Bitstring    1 MCVFLAG2       MCVBK BIT FLAGS.
              1... ....      MCVFSIE        X'80' If set, CP was in the 'SIE'
                                            state at the time of the error.
                                            (Applies to MCVVMDBK guest for
                                            HCPGMC.) See HCPMCH for how this
                                            was determined.
              .1.. ....      MCVHRUN        X'40' THIS IS A COPY OF PFXHRUN,
                                            TAKEN AT THE TIME OF THE ERROR.
                                            IF SET, THE VMDBK WAS IN THE
                                            'RUN' STATE AT THE TIME OF THE
                                            ERROR. (APPLIES TO MCVVMDBK GUEST
                                            FOR HCPGMC.)
              ..1. ....      MCVUNRUN       X'20' THE MACHINE-CHECK HANDLER
                                            HAS SUCCESSFULLY UN-RUN THE
                                            GUEST. (THIS FLAG HAS MEANING
                                            ONLY IF MCVHRUN IS SET.) (APPLIES
                                            TO MCVVMDBK GUEST FOR HCPGMC.)
              ...1 ....      MCVSCS         X'10' THE VIRTUAL CONFIGURATION
                                            MUST ENTER SYSTEM CHECK-STOP.
    001A   26 Signed       2 MCVCPUAD       THE CPU ADDRESS OF THE CPU IN THE
                                            REAL HARDWARE CONFIGURATION WHOSE
                                            ERROR IS BEING REPORTED THROUGH
                                            THIS MCVBK.
    001C   28 Signed       4 MCVNEXT        NEXT MCVBK IF ANY (APPLIES TO
                                            MCVVMDBK GUEST FOR HCPGMC.)
    0020   32 Signed       4 MCVMCICX       Machine Check Interruption Code
                                            Extension
    0024   36 Signed       4 MCVEDMDC (0)   MACHINE CHECK EXTERNAL-DAMAGE
                                            CODE.
    0024   36 Bitstring    1 MCVEDCB0       Byte 0 of the external damage
                                            code
              .... ....      MCEXTD0        X'00' No bits defined
    0025   37 Bitstring    1 MCVEDCB1       Byte 1 of the external damage
                                            code
              1... ....      MCEXTDXN       X'80' Bit 8 - Extended storage
                                            not operational
              .1.. ....      MCEXTDXF       X'40' Bit 9 - Extended storage
                                            control failure
    0026   38 Bitstring    1 MCVEDCB2       Byte 2 of the external damage
                                            code
              1... ....      MCEXTDPS       X'80' Bit 16 - Primary-Sync
                                            Damage
              .1.. ....      MCEXTDEA       X'40' Bit 17 - ETR Attachement
                                            Damage
              ..1. ....      MCEXTDSL       X'20' Bit 18 - Switch to local
              ...1 ....      MCEXTDES       X'10' Bit 19 - ETR Sync check
    0027   39 Bitstring    1 MCVEDCB3       Byte 3 of the external damage
                                            code
              .... ....      MCEXTD3        X'00' No bits defined
    0028   40 Dbl-Word     8 MCVFASIT       Failing-storage external ASIT (to
                                            be certified at the time of
                                            reflection as to whether the
                                            guest has still access to the
                                            failing space)
    0030   48 Dbl-Word     8 MCVGFAD (0)    64 bit guest absolute failing
                                            addr
    0030   48 Signed       4 MCV64HI        High order word of 64 bit addr
    0034   52 Signed       4 MCVFSAD        31 bit guest absolute failing
                                            addr
              ..11 .1..      MCV64LO        MCVFSAD Low order word of 64 bit
                                            addr FOLLOWING ARITHMETIC USED TO
                                            PRODUCE MCVZNM1.
              00000F00       MCVZNMZ1       (MCICVWP+MCICVMS+MCICVPM+MCICVIA)
                                            *256
                 THE FOLLOWING ARE MASK VALUES WHICH DEFINE VALIDITY
                 BITS WITHIN THE MACHINE CHECK INTERRUPTION CODE
                 WHICH ARE NORMALLY ON (VALID).
                 MCVZNM1 IS FOR MCIC BITS 0-31.
                 MCVZNM2 IS FOR MCIC BITS 32-63.
                 THESE MASK VALUES ALSO DEFINE THE BITS WHICH ARE
                 AND-ED TOGETHER WHEN MERGING TWO MACHINE CHECK
                 INTERRUPTION CODES.  BITS NOT CALLED OUT BY
                 THE MASK VALUES ARE OR-ED TOGETHER.
              00000F1D       MCVZNM1        MCVZNMZ1+MCICVFP+MCICVGR+MCICVCR+
                                            MCICVST
              003B0000       MCVZNM2        ((MCICVAR*256)+MCICAR+MCICVCT+MCI
                                            CVCC+MCICVXFP+MCICVTPR) *65536
              00000038       MCVLEN         *-MCVBK LENGTH OF AN MCVBK.
              00000007       MCVSIZE        (*-MCVBK+7)/8 MCVBK SIZE IN
                                            DOUBLE WORDS
    0000    0 Bitstring    2 *              BYTES 0 AND 1 OF MCVMCIC
    0002    2 Bitstring    4 MCVMCB25       BYTES 2 - 5 OF MCVMCIC
    0006    6 Bitstring    2 *              BYTES 6 AND 7 OF MCVMCIC

#### MCVBK Storage Layout

    *** MCVBK - VIRTUAL MACHINE CHECK BLOCK
    *
    *     +------+------+------+------+------+------+------+------+
    *   0 |:MCIC0|:MCIC1|:MCIC2|:MCIC3|:MCIC4|:MCIC5|:MCIC6|:MCIC7|
    *     +------+------+------+------+------+------+------+------+
    *   8 |         MCVCRWS           |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  10 |         MCVVMDBK          |         MCVFSAUS          |
    *     +------+------+-------------+---------------------------+
    *  18 |:FLAG |:FLAG2|  MCVCPUAD   |         MCVNEXT           |
    *     +------+------+-------------+------+------+------+------+
    *  20 |         MCVMCICX          |:EDCB0|:EDCB1|:EDCB2|:EDCB3|
    *     +---------------------------+------+------+------+------+
    *  28 |                       MCVFASIT                        |
    *     +---------------------------+---------------------------+
    *  30 |         MCV64HI           |         MCVFSAD           |
    *     +---------------------------+---------------------------+
    *  38
    *
    *** MCVBK - VIRTUAL MACHINE CHECK BLOCK

    *** Overlay for MCVMCIC in MCVBK
    *
    *     +-------------+---------------------------+-------------+
    *   0 |/////////////|         MCVMCB25          |/////////////|
    *     +-------------+---------------------------+-------------+
    *   8
    *
    *** Overlay for MCVMCIC in MCVBK

#### MCVBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    MCEXTDEA       0026 40
    MCEXTDES       0026 10
    MCEXTDPS       0026 80
    MCEXTDSL       0026 20
    MCEXTDXF       0025 40
    MCEXTDXN       0025 80
    MCEXTD0        0024 00
    MCEXTD3        0027 00
    MCICAR         0005 08
    MCICBU         0001 02
    MCICCD         0000 08
    MCICCRW        0001 40
    MCICCSD        0001 10
    MCICDA         0004 20
    MCICDG         0000 01
    MCICDL         0001 01
    MCICED         0000 04
    MCICIE         0004 80
    MCICITD        0000 10
    MCICKE         0002 20
    MCICPD         0000 40
    MCICSC         0002 40
    MCICSD         0000 80
    MCICSDG        0002 10
    MCICSE         0002 80
    MCICSP         0001 20
    MCICSR         0000 20
    MCICVAR        0004 40
    MCICVCC        0005 01
    MCICVCR        0003 04
    MCICVCT        0005 02
    MCICVED        0003 20
    MCICVFA        0003 80
    MCICVFP        0003 10
    MCICVGR        0003 08
    MCICVIA        0002 01
    MCICVLG        0003 02
    MCICVMS        0002 04
    MCICVPM        0002 02
    MCICVST        0003 01
    MCICVTPR       0005 20
    MCICVWP        0002 08
    MCICVXFP       0005 10
    MCICW          0001 80
    MCIPRIM0       0000 FF
    MCIPRIM1       0001 F0
    MCVABEND       0018 80
    MCVCKSTP       0018 40
    MCVCMPLT       0018 08
    MCVCPUAD       001A
    MCVCRWS        0008
    MCVCUTOF       0018 10
    MCVEDCB0       0024
    MCVEDCB1       0025
    MCVEDCB2       0026
    MCVEDCB3       0027
    MCVEDMDC       0024
    MCVFASIT       0028
    MCVFLAG        0018
    MCVFLAG2       0019
    MCVFSAD        0034
    MCVFSAUS       0014
    MCVFSIE        0019 80
    MCVGFAD        0030
    MCVHRUN        0019 40
    MCVLEN         0034 00000038
    MCVMCB01       0000
    MCVMCB25       0002
    MCVMCIC        0000
    MCVMCICX       0020
    MCVMCIC0       0000
    MCVMCIC1       0001
    MCVMCIC2       0002
    MCVMCIC3       0003
    MCVMCIC4       0004
    MCVMCIC5       0005
    MCVMCIC6       0006
    MCVMCIC7       0007
    MCVMCWD0       0000
    MCVMCWD1       0004
    MCVNEXT        001C
    MCVQWRK        0018 04
    MCVSCS         0019 10
    MCVSIZE        0034 00000007
    MCVSTGFX       0018 02
    MCVSTGLS       0018 01
    MCVTMOUT       0018 20
    MCVUNRUN       0019 20
    MCVVMDBK       0010
    MCVZNMZ1       0034 00000F00
    MCVZNM1        0034 00000F1D
    MCVZNM2        0034 003B0000
    MCV64HI        0030
    MCV64LO        0034 34

This information is based on z/VM V5R2.0. Last updated on 12 Apr 2006 at 17:04:46 EDT.
Copyright IBM Corporation, 1990, 2005