Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### SXIDABK

Prolog

Control Block Contents
SXIDABK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### SXIDABK Prolog

     NAME       : HCPSXIBK
     DESCRIPTION: DIAGNOSE X'64' SEGMENT EXTENDED INPUT AREA
     DSECT      : SXIDABK
     FUNCTION   : THIS BLOCK WILL MAP THE SEGMENT EXTENDED INPUT AREA
                  FOR DIAGNOSE X'64' SUBCODE X'18'.
     LOCATED BY : THE POINTER TO THIS AREA IS CONTAINED IN THE RX
                  REGISTER OF THE DIAGNOSE X'64' SUBCODE X'18' FUNCTION.
     CREATED BY : THE RX REGISTER OF DIAGNOSE X'64' SUBCODE X'18' IS
                  SETUP BY THE USER TO POINT TO A USER SUPPLIED BUFFER.
                  - THIS BUFFER HAS A MINIMUM LENGTH OF THREE DOUBLEWORDS.
                  - THIS BUFFER MUST RESIDE ON A DOUBLEWORD BOUNDARY AND
                  CANNOT CROSS A PAGE BOUNDARY.
                  - THE SXIOAREA FIELD DEFINES AN OUTPUT AREA. THIS AREA
                  IS USER SUPPLIED AND MUST RESIDE ON A DOUBLEWORD
                  BOUNDARY AND CANNOT CROSS A PAGE BOUNDARY.
                  THIS AREA IS DEFINED BY THE HCPSXOBK DSECT.
     DELETED BY : THIS AREA IS USER SUPPLIED AND USER DELETED.

#### SXIDABK Control Block Content

#### SXIDABK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SXIDABK        DIAGNOSE X'64' SEGMENT EXTENDED
                                            INPUT AREA
    0000    0 Dbl-Word     8 * (0)
    0000    0 Bitstring    1 SXIOPCOD       CODE FOR THE OPERATION TO BE
                                            PERFORMED
    0001    1 Bitstring    3 *              RESERVED FOR IBM USE
    0004    4 Bitstring    1 SXIRCODE       RETURN CODE FROM THE FUNCTION
    0005    5 Bitstring    3 *              RESERVED FOR IBM USE
    0008    8 Character    8 SXIRNAME       THE REQUESTED SEGMENT NAME. THIS
                                            NAME IS LEFT JUSTIFIED AND PADDED
                                            WITH BLANKS
    0010   16 Signed       4 SXIOAREA       ADDRESS OF THE OUTPUT AREA
    0014   20 Bitstring    2 SXIOARLN       THE LENGTH OF THE OUTPUT AREA
    0016   22 Bitstring    2 *              RESERVED FOR IBM USE
              00000003       SXISIZE        (*-SXIDABK+7)/8 SIZE IN DOUBLE
                                            WORDS

#### SXIDABK Storage Layout

    *** SXIDABK - DIAGNOSE X'64' SEGMENT EXTENDED INPUT AREA
    *
    *     +------+--------------------+------+--------------------+
    *   0 |:OPCOD|////////////////////|:RCODE|////////////////////|
    *     +------+--------------------+------+--------------------+
    *   8 |                       SXIRNAME                        |
    *     +---------------------------+-------------+-------------+
    *  10 |         SXIOAREA          |  SXIOARLN   |/////////////|
    *     +---------------------------+-------------+-------------+
    *  18
    *
    *** SXIDABK - DIAGNOSE X'64' SEGMENT EXTENDED INPUT AREA

#### SXIDABK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    SXIOAREA       0010
    SXIOARLN       0014
    SXIOPCOD       0000
    SXIRCODE       0004
    SXIRNAME       0008
    SXISIZE        0016 00000003

This information is based on z/VM V5R2.0. Last updated on 12 Apr 2006 at 17:31:01 EDT.
Copyright IBM Corporation, 1990, 2005