Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSCLSQD

Prolog
Control Block Contents
Cross Reference

#### MRSCLSQD Prolog

####

####

     DSECT NAME - SCLSQD
     FUNCTION - Map a Monitor record.
     LOCATED BY -
               Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSCLSQD
     DESCRIPTIVE NAME - Monitor Event Record
                        Domain 2 - Scheduler Domain
                        Record 10 - SET QUICKDSP Changes
     DESCRIPTION - Record of changes made by a SET QUICKDSP command.
                   Generated only if the user who is the target of the
                   command is enabled for scheduler domain (not to be
                   confused with the user that issued the command).

    MRSCLSQD Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure   32  SCLSQD                 Start of monitor record
      0   0  Character    0  SCLSQD_MRHDR           Record header. See MRRECHDR
                                                    for details.
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN               record length in bytes
      2   2  Unsigned     2  MRHDRZER               field of zeros
      4   4  Unsigned     1  MRHDRDM                domain identifier
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC                record identifier
      8   8  Character    8  MRHDRTOD               Time at which this record was
                                                    built. In time-of-day (TOD)
                                                    clock format. See IBM System
                                                    370 XA Principle of Operation
                                                    for explanation of format.
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END              End of header
     20  14  Character    8  SCLSQD_VMDUSER         Userid
     28  1C  Bitstring    1  SCLSQD_CALFLAG1        Flag byte 1
              1... ....      *
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      SCLSQD_VMDQDSPU        When set on, user is
                                                    classified as QUICKDSP. Set by
                                                    the user's directory or by the
                                                    SET QUICKDSP command.
              .... .1..      *
              .... ..1.      *
              .... ...1      *
     29  1D  Character    3  *                      Reserved for IBM use
     32  20  Character    0  SCLSQD_END

    MRSCLSQD Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    SCLSQD                     0     32
    SCLSQD_CALFLAG1           1C      1
    SCLSQD_END                20      0
    SCLSQD_MRHDR               0      0
    SCLSQD_VMDQDSPU           1C           08
    SCLSQD_VMDUSER            14      8

    This information is
    based on z/VM V5R2.0.

    Last updated on 11 Dec 2005 at 18:48:12.

    Copyright IBM Corporation, 1990, 2005