Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRIODMOF

Prolog
Control Block Contents
Cross Reference

#### MRIODMOF Prolog

####

####

     DSECT NAME - IODMOF
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRIODMOF
     DESCRIPTIVE NAME - Monitor Event Record
                        Domain 6 - I/O Domain
                        Record 14- Set Subchannel Measurement Off
     DESCRIPTION - Indicates the SET SCMEASURE OFF command turned off
                   subchannel measurements for the device.

    MRIODMOF Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure   68  IODMOF
      0   0  Character    0  IODMOF_MRHDR           Record header. See MRRECHDR
                                                    for details.
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN
      2   2  Unsigned     2  MRHDRZER
      4   4  Unsigned     1  MRHDRDM
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC
      8   8  Character    8  MRHDRTOD
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END
     20  14  Unsigned     4  IODMOF_RDEVSID         Host subchannel I.D. number
                                                    defined at initialization
     24  18  Unsigned     2  IODMOF_RDEVDEV         Device number
     26  1A  Unsigned     2  *                      Reserved and available for
                                                    IBM use
     28  1C  Unsigned     2  IODMOF_SCMSSCH         Cumulative count of SSCHs and
                                                    RSCHs for this device. This
                                                    value may be wrapped when
                                                    format-1 measurement blocks are
                                                    being used (MTRSYS_CALFLG2 =
                                                    x'80').
     30  1E  Unsigned     2  IODMOF_SCMCOUNT        Cumulative sample count.
                                                    Incremented whenever any
                                                    measurement fields are updated.
                                                    This value may be wrapped when
                                                    format-1 measurement blocks are
                                                    being used (MTRSYS_CALFLG2 =
                                                    x'80').
     32  20  Unsigned     4  IODMOF_SCMCNTIM        The time the device is
                                                    connected to the channel. This
                                                    is the sum of time intervals
                                                    measured whenever device is
                                                    logically connected to the
                                                    channel path for purposes of
                                                    transferring information
                                                    between it and the channel
                                                    subsystem.
     36  24  Unsigned     4  IODMOF_SCMFPTIM        The accumulated SSCH and RSCH
                                                    function pending time, the time
                                                    interval between acceptance of
                                                    the start function (or resume
                                                    function if the subchannel is
                                                    in the suspend state) at the
                                                    subchannel and acceptance of
                                                    the first command associated
                                                    with the initiation of
                                                    channel-program execution at
                                                    the device.
     40  28  Unsigned     4  IODMOF_SCMDDTIM        Device disconnect time. This
                                                    is the sum of the time
                                                    intervals measured whenever the
                                                    device is logically
                                                    disconnected from the channel
                                                    subsystem while the subchannel
                                                    is active
     44  2C  Unsigned     4  IODMOF_SCMCQTIM        Control unit queueing time.
                                                    The sum of the time intervals
                                                    measured by the control unit
                                                    whenever the device is
                                                    logically disconnected from the
                                                    channel subsystem during an I/O
                                                    operation while the device is
                                                    busy with an operation from a
                                                    different system.
     48  30  Unsigned     4  IODMOF_SCMDATIM        Device-active-only-time. The
                                                    sum of the time intervals when
                                                    the subchannel is device-active
                                                    but not subchannel-active at
                                                    the end of an I/O operation or
                                                    chain of I/O operations
                                                    initiated by START SUBCHANNEL.
     52  34  Unsigned     4  IODMOF_SCMDBTIM        Device-Busy Time. The sum of
                                                    the time intervals when the
                                                    subchannel is busy during an
                                                    attempt to initiate a start
                                                    function or resume function at
                                                    the subchannel.
     56  38  Unsigned     4  IODMOF_SCMIRTIM        Initial-command-response
                                                    time. The
                                                    initial-command-response time
                                                    for a start or resume function
                                                    is the time interval beginning
                                                    from when the first command of
                                                    the channel program is sent to
                                                    the device until the device
                                                    indicates it has accepted the
                                                    command.
     60  3C  Unsigned     4  IODMOF_SCGSSCH         Fullword cumulative count of
                                                    SSCHs and RSCHs for this
                                                    device. Available when format-1
                                                    measurement blocks are being
                                                    used (MTRSYS_CALFLG2 = x'80').
     64  40  Unsigned     4  IODMOF_SCGCOUNT        Fullword cumulative sample
                                                    count incremented whenever any
                                                    measurement fields are updated.
                                                    Available when format-1
                                                    measurement blocks are being
                                                    used (MTRSYS_CALFLG2 = x'80').
     68  44  Character    0  IODMOF_END

    MRIODMOF Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    IODMOF                     0     68
    IODMOF_END                44      0
    IODMOF_MRHDR               0      0
    IODMOF_RDEVDEV            18      2
    IODMOF_RDEVSID            14      4
    IODMOF_SCGCOUNT           40      4
    IODMOF_SCGSSCH            3C      4
    IODMOF_SCMCNTIM           20      4
    IODMOF_SCMCOUNT           1E      2
    IODMOF_SCMCQTIM           2C      4
    IODMOF_SCMDATIM           30      4
    IODMOF_SCMDBTIM           34      4
    IODMOF_SCMDDTIM           28      4
    IODMOF_SCMFPTIM           24      4
    IODMOF_SCMIRTIM           38      4
    IODMOF_SCMSSCH            1C      2
    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2

    This information is
    based on z/VM V5R2.0.

    Last updated on 11 Dec 2005 at 21:05:26.

    Copyright IBM Corporation, 1990, 2005