Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### VSMBK

Prolog

Control Block Contents
VSMBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### VSMBK Prolog

     Name       : HCPVSMBK
     Description: Vtam Service Machine control BlocK
     DSECT      : VSMBK
     Function   :
                  This block is used to contain information about a
                  single Vtam Service Machine.
     Located by :
                  SYSVSMBK - Anchor for the system VSMBK queue (located
                  in SYSCM).
                  VSMNEXT  - VSMBK forward chain pointer (located in
                  VSMBK).
     Created by :
                  HCPVCLDV - DISABLE SNA command processor for a specific
                  VSM
                  HCPVCLEV - ENABLE SNA command processor for a specific
                  VSM
                  HCPVCTCN - VSM global IUCV CONNECT processor
     Deleted by :
                  HCPVCZRL - SNABK/RDEV and VSMBK storage releaser
     Serialized :
                  The updating of all fields in this block is serialized
                  by exclusive ownership of the system vtam service
                  machine lock (SYSVSMLK) located in SYSCM.
                  Interrogation of a field without the lock is permitted
                  as long as no action is taken which could be
                  invalidated by that field's value changing the instant
                  after it was obtained. Otherwise interrogation requires
                  at least a share of the lock.

#### VSMBK Control Block Content

#### VSMBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      VSMBK          Vtam Service Machine control
                                            BlocK
    0000    0 Character    8 VSMUSRID       VSM userid
    0008    8 Character    8 VSMVTMID       VTAM machine userid
    0010   16 Dbl-Word     8 VSMTIMER       Value for redisplay timer
    0018   24 Signed       4 VSMVMDBK       VSM VMDBK address
    001C   28 Signed       4 VSMRTREE       Radix tree anchor
    0020   32 Signed       4 VSMNEXT        Pointer to the next VSMBK
    0024   36 Signed       4 VSMLOGOS       Pointer to logo WEIBK chain
    0028   40 Signed       4 VSMSEVRQ       Queue of SNABKs awaiting SEVER
    002C   44 Signed       2 VSMPATH        IUCV pathid for the VSM
    002E   46 Signed       2 *              Reserved for future IBM use
    0030   48 Signed       2 VSMMSGLM       Message limit
    0032   50 Signed       2 VSMLUCNT       LU count for VSM
    0034   52 Bitstring    1 VSMFLAG1       Status
              1... ....      VSMCONNP       X'80' Connect pending
              .1.. ....      VSMENABL       X'40' VSM devices enabled
              ..1. ....      VSMSEVER       X'20' Global VSM path has been
                                            severed
              ...1 ....      VSMSGLME       X'10' VSM message limit exceeded
    0035   53 Bitstring    1 VSMLEVEL       Level of support in VSM
              00000000       VSMVCNA        X'00' VCNA
              00000001       VSM31          X'01' VSCS VTAM 3.1
              00000002       VSM311         X'02' VSCS VTAM 3.1.1
              00000003       VSM312         X'03' VSCS VTAM 3.1.2
              00000004       VSM32          X'04' VSCS VTAM 3.2
              00000005       VSM33          X'05' VSCS VTAM 3.3
              00000006       VSM34          X'06' VSCS VTAM 3.4
              00000007       VSM341         X'07' VSCS VTAM 3.4.1
              00000008       VSM42          X'08' VSCS VTAM 4.2
         * Define the VSM Function Table
         *
         * This 2-byte table identifies the functions that are
         * supported by a given VSM Level.
    0036   54 Bitstring    2 VSMFCTNS (0)   VSM function flags
    0036   54 Bitstring    1 VSMFCTB1       Function flag byte 1
              1... ....      VSMFDIA        X'80' DIAL function supported
              .1.. ....      VSMFWSF        X'40' WSF query reply data
                                            supported
              ..1. ....      VSMFEAU        X'20' Erase All Unprotected
                                            supported
              ...1 ....      VSMFTTY        X'10' Enhanced TTY device
                                            supported
              .... 1...      VSMFWFP        X'08' Write for Position
                                            supported
              .... .1..      VSMFCON        X'04' CONMODE 3270 supported
              .... ..1.      VSMFVTM        X'02' VTAM userid transaction
                                            supported
              .... ...1      VSMFLOGO       X'01' LOGON from logo supported
    0037   55 Bitstring    1 VSMFCTB2       Function flag byte 2
              1... ....      VSMFBRKN       X'80' BREAKIN GUESTCTL supported
              .1.. ....      VSMFLDIS       X'40' Linemode DBCS input
                                            supported
              ..1. ....      VSMMOHLD       X'20' TERM MORE/HOLD supported
              ...1 ....      VSMFDYNL       X'10' DYNamic Logo updates
                                            supported
              .... 1...      VSMCURSC       X'08' Changes to the MORE/HOLD
                                            settings of the current screen
                                            supported (Clear screen function
                                            also supported)
              .... .1..      VSMFNQN        X'04' Network Qualified Names
                                            supported
              00000007       VSMSIZE        (*-VSMBK+7)/8 VSMBK size in
                                            doublewords

#### VSMBK Storage Layout

    *** VSMBK - Vtam Service Machine control BlocK
    *
    *     +-------------------------------------------------------+
    *   0 |                       VSMUSRID                        |
    *     +-------------------------------------------------------+
    *   8 |                       VSMVTMID                        |
    *     +-------------------------------------------------------+
    *  10 |                       VSMTIMER                        |
    *     +---------------------------+---------------------------+
    *  18 |         VSMVMDBK          |         VSMRTREE          |
    *     +---------------------------+---------------------------+
    *  20 |         VSMNEXT           |         VSMLOGOS          |
    *     +---------------------------+-------------+-------------+
    *  28 |         VSMSEVRQ          |  VSMPATH    |/////////////|
    *     +-------------+-------------+------+------+------+------+
    *  30 |  VSMMSGLM   |  VSMLUCNT   |:FLAG1|:LEVEL|:FCTB1|:FCTB2|
    *     +-------------+-------------+------+------+------+------+
    *  38
    *
    *** VSMBK - Vtam Service Machine control BlocK

#### VSMBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    VSMCONNP       0034 80
    VSMCURSC       0037 08
    VSMENABL       0034 40
    VSMFBRKN       0037 80
    VSMFCON        0036 04
    VSMFCTB1       0036
    VSMFCTB2       0037
    VSMFCTNS       0036
    VSMFDIA        0036 80
    VSMFDYNL       0037 10
    VSMFEAU        0036 20
    VSMFLAG1       0034
    VSMFLDIS       0037 40
    VSMFLOGO       0036 01
    VSMFNQN        0037 04
    VSMFTTY        0036 10
    VSMFVTM        0036 02
    VSMFWFP        0036 08
    VSMFWSF        0036 40
    VSMLEVEL       0035
    VSMLOGOS       0024
    VSMLUCNT       0032
    VSMMOHLD       0037 20
    VSMMSGLM       0030
    VSMNEXT        0020
    VSMPATH        002C
    VSMRTREE       001C
    VSMSEVER       0034 20
    VSMSEVRQ       0028
    VSMSGLME       0034 10
    VSMSIZE        0037 00000007
    VSMTIMER       0010
    VSMUSRID       0000
    VSMVCNA        0035 00000000
    VSMVMDBK       0018
    VSMVTMID       0008
    VSM31          0035 00000001
    VSM311         0035 00000002
    VSM312         0035 00000003
    VSM32          0035 00000004
    VSM33          0035 00000005
    VSM34          0035 00000006
    VSM341         0035 00000007
    VSM42          0035 00000008

This information is based on z/VM V5R2.0. Last updated on 12 Apr 2006 at 17:39:53 EDT.
Copyright IBM Corporation, 1990, 2005