Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### LANBK

Prolog

Control Block Contents
LANBK DSECT
LANVID DSECT
LANRDD DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### LANBK Prolog

     NAME       : HCPLANBK
     DESCRIPTION: Virtual LAN block
     DSECT      : LANBK
     FUNCTION   :
                  Define a structure to represent a Virtual LAN
                  (Local Area Network) in CP.
     LOCATED BY -
       SLMLANTB - The System LAN Table
     CREATED BY :
                  CP DEFINE LAN command
     DELETED BY :
                  CP DETACH LAN processing
     REFERENCES :
                  HCPEQUAT COPY - General CP equates

#### LANBK Control Block Content

#### LANBK DSECT

####

####

####

####

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      LANBK          Virtual LAN block
          Static Area -
            The fields in this area are relatively static.
            They are set when the LANBK is constructed.
    0000    0 Character   16 LANID (0)      LAN Fully-Qualified Identifier
    0000    0 Character    8 LANOWNER       LAN Owner (user who defined it)
    0008    8 Character    8 LANNAME        LAN Name
    0010   16 Character    8 LANDESC        LAN Description
    0018   24 Character    8 LANDEFBY       LAN Defined By <userid>
    0020   32 Signed       4 LANDFTOD       CPU TOD (high-order word) when
                                            this LAN was defined
    0024   36 Bitstring    1 LANTYPE        LAN Type
              00000001       LANHIPR        1 - HiperSockets LAN
              00000002       LANQDIO        2 - QDIO LAN
    0025   37 Bitstring    1 LANPROTO       LAN Protocol
              00000001       LANENET        X'01' - Ethernet / Fast Ethernet
              00000002       LANTRNET       X'02' - High Speed Token Ring
              00000003       LANGBE         X'03' - Gigabit Ethernet
              00000010       LAN10GE        X'10' - 10 Gig Ethernet
              00000080       LANQDIOP       X'80' - QDIO Protocol
              00000081       LANATME        X'81' - ATM Emulated Enet Port
              00000082       LANATMTR       X'82' - ATM Emulated Token Ring
                                            Port
              00000083       LANATMGE       X'83' - ATM Emulated GbEnet + MTU
                                            size
              00000088       LANATMP        X'88' - ATM Emulated Port +
                                            autoconfig
              00000090       LANATM         X'90' - Native ATM
    0026   38 Bitstring    1 LANLEVEL       LAN Level
              00000001       LANGLAN        1 - Level 1 - Guest Lan
              00000002       LANVSW         2 - Level 2 - Vswitch
    0027   39 Bitstring    1 LANTRANP       Transport type
              00000001       LANIP          1 Layer 3 IP datagrams
              00000002       LANETHER       2 Layer 2 Ethernet frames
          LANLKWRD - LKWRD for primary LAN functions
          Note that certain fields are additionally serialized by
          LANCTLCK. See below for more information.
          Notes      : LKWRDSIZ == 3 doublewords.
    0028   40 Dbl-Word     8 LANLKWRD (3)   LAN Lockword
          LAN Management Area -
    0040   64 Bitstring    1 LANCFLG        LAN Configuration Flags
              1... ....      LANINPRG       X'80' - Initialization in
                                            Progress
              .1.. ....      LANDLPRG       X'40' - Delete in Progress
              ..1. ....      LANLIMCN       X'20' - Limit connections by
                                            LANMAXCN
              ...1 ....      LANLIMID       X'10' - Limit connections by
                                            userid
              .... 1...      LANSYSLN       X'08' - Registered System LAN
              .... .1..      LANUSRLN       X'04' - Private LAN
              .... ..1.      LANTRANS       X'02' - Transient LAN
              .... ...1      LANACNT        X'01' - Accounting Enabled
    0041   65 Bitstring    1 LANCFLG2       More LAN Configuration Flags
              1... ....      LANRDV         X'80' - RDEV was specified for
                                            VSWITCH
              .1.. ....      LANDLDIP       X'40' - LANBK on Delete In
                                            Progress Chain
              ..1. ....      LANPRTRQ       X'20' - PRIROUTER was specified
                                            for VSWITCH
              ...1 ....      LANVLFLT       X'10' - VLAN Filtering (VLAN
                                            AWARE)
              .... 1...      LANGVRP        X'08' - GVRP (VLAN Registration)
                                            Requested
    0042   66 Signed       2 LANIPTO        IP Timeout value (in 30 sec tics)
    0044   68 Signed       4 LANRFCTR       LAN Reference Counter
    0048   72 Address      4 LANFPNT        Pointer to next LANBK
    004C   76 Address      4 LANBPNT        Pointer to previous LANBK
    0050   80 Address      4 LANACLHD       Pointer to first ACLBK
    0054   84 Address      4 LANACLTL       Pointer to last ACLBK
    0058   88 Signed       4 LANMFS         Maximum Frame Size in bytes
    005C   92 Signed       4 LANMAXCN       Maximum number of connections
    0060   96 Address      4 LANCNLST       Pointer to Connected NICBK List
    0064  100 Signed       4 LANCNCTR       LAN Connection Counter
    0068  104 Character    8 LANUPDBY       LAN Updated By <userid>
          These fields represent a real OSA-Express interface.
    0070  112 Address      4 LANVQSBK       Pointer to VQSBK for VSWITCH
    0074  116 Signed       2 LANDFVID       Default VLAN ID
    0076  118 Bitstring    1 LANDFPRT       Default Porttype
              .... ...1      LANDFPRT_ACCESS
                                            1 = Access Port (untagged)
              .... ..1.      LANDFPRT_TRUNK 2 = Trunk Port (tagged or mixed)
    0077  119 Bitstring    1 LANFSV         Queuestorage value (1-8)
          LANDFNIC/LANDFNIC - Default Router to External Network.
            These pointers are set when LANRDEV is initialized and
            ready to use.  This NIDBK represents the virtual
            interface between this LAN segment and the external
            VSWITCH RDEV (LANRDEV).
    0078  120 Address      4 LANDFNIC       Pointer to Default Router NICBK
    007C  124 Address      4 LANDFNID       Pointer to Default Router NIDBK
    0080  128 Signed       4 LANTRACE       CTR for tracing on
    0084  132 Address      4 LANPROM        Pointer to list of Prom users
          LANMCTBL - Pointer to LAN Multicast Table
            Each IPNBK in the Multicast Table represents a device
            (NIDBK) which is subscribed to a multicast group.  This
            table is sorted by Multicast IP Address.
    0088  136 Address      4 LANMCTBL       Ptr to IPNBK chain
    008C  140 Signed       2 LANMCCTR       Number of Multicast subscribers
          LANMRCTR - Count Multicast Routers on this LAN
    008E  142 Signed       2 LANMRCTR       Number of Multicast Routers
          LANIDTBL - LAN Link ID Table (MLTBK)
            Each entry in the Link ID Table represents the
            set of devices registered for a Link ID (which
            is a combination of VLAN ID and MAC address).
          BLOCKMAP DEFINE LANIDTBL (4)D
    0090  144 Dbl-Word     8 LANIDTBL (4)   Reserve a MLTBK here
          LANIPTBL - Pointer to LAN IP Table
            This IP Table functions as an "ARP Cache" for the
            LAN segment.  LANIPTBL is the anchor for the table
            of unicast IP Addresses.  Each entry (IPNBK)
            represents an IP Address, and holds a pointer
            to the network device (NIDBK) which owns this
            IP Address.
          Notes      :
            Only unicast addresses should be installed in this
            table.  MAC addresses should be installed in the
            Link ID Table (LANIDTBL) by MAC address.
    00B0  176 Address      4 LANIPTBL       LAN IP Table (unicast)
    00B4  180 Signed       2 LANIPCTR       Number of entries in LANIPTBL
    00B6  182 Bitstring    2 *              Reserved
          LANVLANL - Pointer to LANVID list
            This is the anchor for a list of VLAN groups active
            on this LAN.
    00B8  184 Address      4 LANVLANL       Pointer to LANVID list
    00BC  188 Bitstring    4 *              Reserved
          Following Fields are only relevant when the LAN Sniffer is
          active either with TRSOURCE or SET_PROMISCUOUS_MODE.
    00C0  192 Signed       4 LANTRID        # of active type lan trace ids
    00C4  196 Signed       4 LANSUSR        # of promiscuous users on lan
    00C8  200 Dbl-Word     8 *              Reserved
         ******** Start of Virtual Switch Controller Section
          The Virtual Switch Controller section of this structure is
          serialized by a combination of LANLKWRD and LANCTLCK.
          To reference these fields, the LANLKWRD must be held at
          least SHARED.
          To modify these fields, either:
            1) Obtain the LANLKWRD EXCLUSIVE, or
            2) Obtain the LANLKWRD SHARED and the LANCTLCK EXCLUSIVE.
          The second choice allows access to the controller-
          related fields without interference with data transfer
          among the guest hosts coupled to the virtual switch.
          LANCTLCK - LKWRD for VSWITCH Controller functions
          Notes      : LKWRDSIZ == 3 doublewords.
    00D0  208 Dbl-Word     8 LANCTLCK (3)   LAN CONTROLLER lock word
          Active Interface Definition -
    00E8  232 Character    8 LANCONT        Controller
    00F0  240 Character    8 *              Reserved
                       F              Reserved
    00F8  248 Signed       2 LANRDEV        Rdev
    00FA  250 Signed       2 *              Reserved
    00FC  252 Bitstring    1 LANCTSTA       VSwitch Controller State
              00000001       LANCTDEF       X'01' - Virtual switch defined
              00000002       LANCTNOC       X'02' - Controller not available
              00000003       LANCTOPR       X'03' - Operator intervention
                                            required
              00000004       LANCTDIS       X'04' - Disconnected
              00000005       LANCTATT       X'05' - VDEVs attached to
                                            controller
              00000006       LANCTINI       X'06' - OSA initialization in
                                            progress
              00000007       LANCTNOT       X'07' - OSA device not ready
              00000008       LANCTRDY       X'08' - OSA device ready
              00000009       LANCTDET       X'09' - OSA devices being
                                            detached
              0000000A       LANCTDEL       X'0A' - VSWITCH delete pending
              0000000B       LANCTRCV       X'0B' - VSWITCH failover
                                            recovering
              0000000C       LANCTRES       X'0C' - Autorestart in progress
              0000000D       LANCTLST       X'0D' - High water mark for
                                            validation NOTE: Cannot exceed 99
                                            (X'63'). Mapped to decimal
                                            message number MS2830xx.
    00FD  253 Bitstring    1 LANCTFLG       VSwitch Controller Flag
              1... ....      LANXIPV6       X'80' - VSWITCH RDEV supports
                                            IPv6
              .1.. ....      LANPRTAC       X'40' - PRIROUTER is active on
                                            VSWITCH
              ..1. ....      LANNOARP       X'20' - No Send_Grat_Arp support
              ...1 ....      LANMSARP       X'10' - HCP2859I - ARP message
                                            issued
              .... 1...      LANNOGVR       X'08' - No GVRP support
              .... .1..      LANMSGVR       X'04' - HCP2859I - GVRP message
                                            issued
    00FE  254 Bitstring    2 *              Reserved
    0100  256 Bitstring    6 LANDVMAC       VSwitch RDEV MAC address
    0106  262 Signed       2 LANMXMTU       MaxMTU reported by H/W
    0108  264 Signed       4 LANUSEFX       Adjustment factor for IPNUSAGE
    010C  268 Address      4 LANIPCHN       Chain of deferred SETIP requests
    0110  272 Address      4 LANIPCHE       Last entry - Chain of deferred
                                            SETIP requests
    0114  276 Signed       4 LANIPCNT       Count of incomplete SETIP reqs
    0118  280 Address      4 LANRRDEV       Chain of LANRDD descriptors
    011C  284 Bitstring    4 *              Reserved
         ********  End of Virtual Switch Controller Section
          LANRXTBL - LAN Router Table (MLTBK)
            Each entry in the Router Table represents the
            set of devices registered as a Router (using
            an ID formed by VLAN ID and IPv4/IPv6 value).
          BLOCKMAP DEFINE LANRXTBL (4)D
    0120  288 Dbl-Word     8 LANRXTBL (2)   Reserve a MLTBK here
          End of the LANBK.
              00000140       LAN$END        * End of the LANBK
              00000140       LANBKLN        *-LANBK Length of LANBK in bytes
              00000028       LANBKSZ        (*-LANBK+7)/8 Size of LANBK in
                                            doublewords
          Define the LANVID structure.
            This structure maps one element of the LANVIDLL list.
            Each element represents an active VLAN group on this
            LAN segment.

    LANVID DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      LANVID         Virtual LAN block
    0000    0 Address      4 LANVID_FPNT    Pointer to Next LANVID
    0004    4 Address      4 LANVID_BPNT    Pointer to Previous LANVID
    0008    8 Signed       2 LANVID_ID      VLAN group ID
    000A   10 Bitstring    2 *              Reserved
    000C   12 Signed       4 LANVID_CTR     Number of interfaces active
              00000010       LANVIDLN       *-LANVID Length of LANVID (bytes)
              00000002       LANVIDSZ       (LANVIDLN+7)/8 Length of LANVID
                                            (doublewords)
          Define the LANRDD structure.
            This structure maps each element of the LANRRDEV array.

    LANRDD DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      LANRDD         Virtual LAN block
    0000    0 Address      4 LANRDD_NEXT    Pointer to Next LANRDD
    0004    4 Address      4 LANRDD_CTPTR   Pointer to Controller entry
    0008    8 Signed       2 LANRDD_RDEV    Real device address
    000A   10 Signed       2 LANRDD_VDEV    Virtual device address
    000C   12 Character    8 LANRDD_PORT    Port name for this device
    0014   20 Bitstring    1 LANRDD_FLAG    Device status flags:
              1... ....      LANRDD_ACTIVE  X'80' - Active, primary RDEV.
              .1.. ....      LANRDD_BACKUP  X'40' - Backup RDEV.
              ..1. ....      LANRDD_INOP    X'20' - Inoperative device
              ...1 ....      LANRDD_NOVDEV  X'10' - VDEV not available at
                                            chosen controller
              .... 1...      LANRDD_PRT     X'08' - Port name specified
              .... .1..      LANRDD_DELETE  X'04' - Delete LANRDD when
                                            cleanup is completed
    0015   21 Bitstring    1 LANRDD_RSN     Failure reason
              .... ....      LANRDD_RSNNONE X'00' - None identified
              .... ...1      LANRDD_RSNPORTNAME
                                            X'01' - Portname conflict
              .... ..1.      LANRDD_RSNNOLAYER2
                                            X'02' - No layer 2 support
              .... ..11      LANRDD_RSNNORDEV
                                            X'03' - RDEV does not exist
              .... .1..      LANRDD_RSNRDEVATT
                                            X'04' - RDEV is attached
                                            elsewhere
              .... .1.1      LANRDD_RSNNOTQDIO
                                            X'05' - RDEV not QDIO OSA-E
              .... .11.      LANRDD_RSNINITERR
                                            X'06' - Initialization error
              .... .111      LANRDD_RSNSTALLEDO
                                            X'07' - Stalled OSA
              .... 1...      LANRDD_RSNSTALLEDC
                                            X'08' - Stalled controller
              .... 1..1      LANRDD_RSNSEVER
                                            X'09' - Controller connection
                                            severed
              .... 1.1.      LANRDD_RSNROUTING
                                            X'0A' - Primary or secondary
                                            routing conflict
              .... 1.11      LANRDD_RSNOFFLINE
                                            X'0B' - Device is offline
              .... 11..      LANRDD_RSNDETACHED
                                            X'0C' - Device was detached
              .... 11.1      LANRDD_RSNMISMATCH
                                            X'0D' - Type Mismatch
                                            (IP<->ETHERNET)
              .... 111.      LANRDD_RSNSTORAGE
                                            X'0E' - Insufficient storage in
                                            controller virtual machine
              .... 1111      LANRDD_RSNTCPIPCONF
                                            X'0F' - TCP/IP Configuration
                                            conflict
    0016   22 Signed       2 *              Reserved
              00000018       LANRDDLB       *-LANRDD Length of each LANRDD in
                                            bytes
              00000003       LANRDDLD       (LANRDDLB+7)/8 Length in
                                            doublewords
          Define MLTBK for this compile.
           PREFIX_LEN = 3
          Start of Assembler Control Block

    LANBK Storage Layout

    *** LANBK - Virtual LAN block
    *
    *     +-------------------------------------------------------+
    *   0 |                       LANOWNER                        |
    *     +-------------------------------------------------------+
    *   8 |                       LANNAME                         |
    *     +-------------------------------------------------------+
    *  10 |                       LANDESC                         |
    *     +-------------------------------------------------------+
    *  18 |                       LANDEFBY                        |
    *     +---------------------------+------+------+------+------+
    *  20 |         LANDFTOD          |:TYPE |:PROTO|:LEVEL|:TRANP|
    *     +---------------------------+------+------+------+------+
    *  28 |                                                       |
    *     =                       LANLKWRD                        =
    *     |                                                       |
    *     +------+------+-------------+---------------------------+
    *  40 |:CFLG |:CFLG2|  LANIPTO    |         LANRFCTR          |
    *     +------+------+-------------+---------------------------+
    *  48 |         LANFPNT           |         LANBPNT           |
    *     +---------------------------+---------------------------+
    *  50 |         LANACLHD          |         LANACLTL          |
    *     +---------------------------+---------------------------+
    *  58 |          LANMFS           |         LANMAXCN          |
    *     +---------------------------+---------------------------+
    *  60 |         LANCNLST          |         LANCNCTR          |
    *     +---------------------------+---------------------------+
    *  68 |                       LANUPDBY                        |
    *     +---------------------------+-------------+------+------+
    *  70 |         LANVQSBK          |  LANDFVID   |:DFPRT|LANFSV|
    *     +---------------------------+-------------+------+------+
    *  78 |         LANDFNIC          |         LANDFNID          |
    *     +---------------------------+---------------------------+
    *  80 |         LANTRACE          |         LANPROM           |
    *     +---------------------------+-------------+-------------+
    *  88 |         LANMCTBL          |  LANMCCTR   |  LANMRCTR   |
    *     +---------------------------+-------------+-------------+
    *  90 |                                                       |
    *     =                       LANIDTBL                        =
    *     |                                                       |
    *     +---------------------------+-------------+-------------+
    *  B0 |         LANIPTBL          |  LANIPCTR   |/////////////|
    *     +---------------------------+-------------+-------------+
    *  B8 |         LANVLANL          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  C0 |         LANTRID           |         LANSUSR           |
    *     +---------------------------+---------------------------+
    *  C8 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  D0 |                                                       |
    *     =                       LANCTLCK                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  E8 |                       LANCONT                         |
    *     +-------------------------------------------------------+
    *  F0 |///////////////////////////////////////////////////////|
    *     +-------------+-------------+------+------+-------------+
    *  F8 |  LANRDEV    |/////////////|:CTSTA|:CTFLG|/////////////|
    *     +-------------+-------------+------+------+-------------+
    * 100 |                LANDVMAC                 |  LANMXMTU   |
    *     +---------------------------+-------------+-------------+
    * 108 |         LANUSEFX          |         LANIPCHN          |
    *     +---------------------------+---------------------------+
    * 110 |         LANIPCHE          |         LANIPCNT          |
    *     +---------------------------+---------------------------+
    * 118 |         LANRRDEV          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 120 |                       LANRXTBL                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 130
    *
    *** LANBK - Virtual LAN block

    *** LANVID - Virtual LAN block
    *
    *     +---------------------------+---------------------------+
    *   0 |       LANVID_FPNT         |       LANVID_BPNT         |
    *     +-------------+-------------+---------------------------+
    *   8 | LANVID_ID   |/////////////|        LANVID_CTR         |
    *     +-------------+-------------+---------------------------+
    *  10
    *
    *** LANVID - Virtual LAN block

    *** LANRDD - Virtual LAN block
    *
    *     +---------------------------+---------------------------+
    *   0 |       LANRDD_NEXT         |       LANRDD_CTPTR        |
    *     +-------------+-------------+---------------------------+
    *   8 |LANRDD_RDEV  |LANRDD_VDEV  |       LANRDD_PORT-        |
    *     +-------------+-------------+------+------+-------------+
    *  10 |          -(00C)           |(014) |(015) |/////////////|
    *     +---------------------------+------+------+-------------+
    *  18
    *
    *** LANRDD - Virtual LAN block

    LANBK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    LAN$END        0120 00000140
    LANACLHD       0050
    LANACLTL       0054
    LANACNT        0040 01
    LANATM         0025 00000090
    LANATME        0025 00000081
    LANATMGE       0025 00000083
    LANATMP        0025 00000088
    LANATMTR       0025 00000082
    LANBKLN        0120 00000140
    LANBKSZ        0120 00000028
    LANBPNT        004C
    LANCFLG        0040
    LANCFLG2       0041
    LANCNCTR       0064
    LANCNLST       0060
    LANCONT        00E8
    LANCTATT       00FC 00000005
    LANCTDEF       00FC 00000001
    LANCTDEL       00FC 0000000A
    LANCTDET       00FC 00000009
    LANCTDIS       00FC 00000004
    LANCTFLG       00FD
    LANCTINI       00FC 00000006
    LANCTLCK       00D0
    LANCTLST       00FC 0000000D
    LANCTNOC       00FC 00000002
    LANCTNOT       00FC 00000007
    LANCTOPR       00FC 00000003
    LANCTRCV       00FC 0000000B
    LANCTRDY       00FC 00000008
    LANCTRES       00FC 0000000C
    LANCTSTA       00FC
    LANDEFBY       0018
    LANDESC        0010
    LANDFNIC       0078
    LANDFNID       007C
    LANDFPRT       0076
    LANDFPRT_ACCESS
                   0076 01
    LANDFPRT_TRUNK
                   0076 02
    LANDFTOD       0020
    LANDFVID       0074
    LANDLDIP       0041 40
    LANDLPRG       0040 40
    LANDVMAC       0100
    LANENET        0025 00000001
    LANETHER       0027 00000002
    LANFPNT        0048
    LANFSV         0077
    LANGBE         0025 00000003
    LANGLAN        0026 00000001
    LANGVRP        0041 08
    LANHIPR        0024 00000001
    LANID          0000
    LANIDTBL       0090
    LANINPRG       0040 80
    LANIP          0027 00000001
    LANIPCHE       0110
    LANIPCHN       010C
    LANIPCNT       0114
    LANIPCTR       00B4
    LANIPTBL       00B0
    LANIPTO        0042
    LANLEVEL       0026
    LANLIMCN       0040 20
    LANLIMID       0040 10
    LANLKWRD       0028
    LANMAXCN       005C
    LANMCCTR       008C
    LANMCTBL       0088
    LANMFS         0058
    LANMRCTR       008E
    LANMSARP       00FD 10
    LANMSGVR       00FD 04
    LANMXMTU       0106
    LANNAME        0008
    LANNOARP       00FD 20
    LANNOGVR       00FD 08
    LANOWNER       0000
    LANPROM        0084
    LANPROTO       0025
    LANPRTAC       00FD 40
    LANPRTRQ       0041 20
    LANQDIO        0024 00000002
    LANQDIOP       0025 00000080
    LANRDD_ACTIVE  0014 80
    LANRDD_BACKUP  0014 40
    LANRDD_CTPTR   0004
    LANRDD_DELETE  0014 04
    LANRDD_FLAG    0014
    LANRDD_INOP    0014 20
    LANRDD_NEXT    0000
    LANRDD_NOVDEV  0014 10
    LANRDD_PORT    000C
    LANRDD_PRT     0014 08
    LANRDD_RDEV    0008
    LANRDD_RSN     0015
    LANRDD_RSNDETACHED
                   0015 0C
    LANRDD_RSNINITERR
                   0015 06
    LANRDD_RSNMISMATCH
                   0015 0D
    LANRDD_RSNNOLAYER2
                   0015 02
    LANRDD_RSNNONE
                   0015 00
    LANRDD_RSNNORDEV
                   0015 03
    LANRDD_RSNNOTQDIO
                   0015 05
    LANRDD_RSNOFFLINE
                   0015 0B
    LANRDD_RSNPORTNAME
                   0015 01
    LANRDD_RSNRDEVATT
                   0015 04
    LANRDD_RSNROUTING
                   0015 0A
    LANRDD_RSNSEVER
                   0015 09
    LANRDD_RSNSTALLEDO
                   0015 07
    LANRDD_RSNSTALLEDC
                   0015 08
    LANRDD_RSNSTORAGE
                   0015 0E
    LANRDD_RSNTCPIPCONF
                   0015 0F
    LANRDD_VDEV    000A
    LANRDDLB       0016 00000018
    LANRDDLD       0016 00000003
    LANRDEV        00F8
    LANRDV         0041 80
    LANRFCTR       0044
    LANRRDEV       0118
    LANRXTBL       0120
    LANSUSR        00C4
    LANSYSLN       0040 08
    LANTRACE       0080
    LANTRANP       0027
    LANTRANS       0040 02
    LANTRID        00C0
    LANTRNET       0025 00000002
    LANTYPE        0024
    LANUPDBY       0068
    LANUSEFX       0108
    LANUSRLN       0040 04
    LANVID_BPNT    0004
    LANVID_CTR     000C
    LANVID_FPNT    0000
    LANVID_ID      0008
    LANVIDLN       000C 00000010
    LANVIDSZ       000C 00000002
    LANVLANL       00B8
    LANVLFLT       0041 10
    LANVQSBK       0070
    LANVSW         0026 00000002
    LANXIPV6       00FD 80
    LAN10GE        0025 00000010

    This information is
    based on z/VM V5R2.0.
    Last updated on 12 Apr 2006 at 17:00:31 EDT.

    Copyright IBM Corporation, 1990, 2005