Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRUSEITE

Prolog
Control Block Contents
Cross Reference

#### MRUSEITE Prolog

####

####

     DSECT NAME - USEITE
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRUSEITE
     DESCRIPTIVE NAME - Monitor Event Record
                        Domain 4 - User Domain
                        Record 10 - User Interaction at Transaction End
     DESCRIPTION - Describes a VMDBK's interaction with other VMDBKs
                   during a transaction.  A separate record is generated
                   for each VMDBK in a virtual complex that contributed
                   to the transaction.
     NOTES:
      - Fields labeled by the prefix, 'USEITE_HF', are high-frequency
        counters.
      - The following is the order in which the user is tested for its
        wait state.  If the user is in more than one state, it is
        counted only in the first of the list.
                 USEITE_HFIOWT
                 USEITE_HFCFWT
                 USEITE_HFSIMWT
                 USEITE_HFWTPAG
                 USEITE_HFLLIST
                 USEITE_HFCPUWT
                 USEITE_HFCPURN
                 USEITE_HFESVM
                 USEITE_HFLOAD
                 USEITE_HFDORM
                 USEITE_HFDSVM
                 USEITE_HFIOACT
                 USEITE_HFTIDL
                 USEITE_HFTSVM
                 USEITE_HFPGACT
                 USEITE_HFOTHR

    MRUSEITE Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure  200  USEITE                 Start of monitor record
      0   0  Character    0  USEITE_MRHDR           Record header. See MRRECHDR
                                                    for details.
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN               record length in bytes
      2   2  Unsigned     2  MRHDRZER               field of zeros
      4   4  Unsigned     1  MRHDRDM                domain identifier
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC                record identifier
      8   8  Character    8  MRHDRTOD               Time at which this record was
                                                    built. In time-of-day (TOD)
                                                    clock format. See IBM System
                                                    370 XA Principle of Operation
                                                    for explanation of format.
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END              End of header
     20  14  Character    8  USEITE_VMDUSER         User logon identification
     28  1C  Unsigned     2  USEITE_VMDCPUAD        Processor address
     30  1E  Signed       2  USEITE_VMDSLCNT        Count of minor time slices
                                                    that have expired since the
                                                    start of current transaction.
     32  20  Unsigned     4  USEITE_VMDSVMFX        Number of times the SVM wait
                                                    flag was left on at the end of
                                                    a transaction and had to be
                                                    reset by the scheduler.
     36  24  Character    8  USEITE_VMDSVMID        VMDBK name for the last
                                                    successful IUCV, VMCF or
                                                    APPC/VM Send for this virtual
                                                    machine. Valid in base VMDBK
                                                    only.
     44  2C  Bitstring    1  USEITE_VMDSVMWT        Service-virtual-machine (SVM)
                                                    wait flag byte - valid in base
                                                    VMDBK only.
              1... ....      USEITE_VMDSVMWF        VMDBK is waiting for a
                                                    response from IUCV, VMCF, or
                                                    APPC.
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
     45  2D  Character    0  USEITE_VMDSVMW2        Back-up byte to the VMDSVMWT
                                                    byte. Its contents will persist
                                                    longer than they would in
                                                    VMDSVMWT. Valid in base VMDBK
                                                    only.
     45  2D  Bitstring    1  USEITE_VMDSVMWT        Service-virtual-machine (SVM)
                                                    wait flag byte - valid in base
                                                    VMDBK only.
              1... ....      USEITE_VMDSVMWF        VMDBK is waiting for a
                                                    response from IUCV, VMCF, or
                                                    APPC.
     46  2E  Character    0  USEITE_VMDRDYCM        Flag byte set by IUCV, VMCF,
                                                    or APPC whenever IUCV/VMCF/APPC
                                                    makes an external interrupt. It
                                                    is sort of a "reference bit"
                                                    that tells the scheduler that
                                                    IUCV/VMCF/APPC has been active
                                                    recently. Valid in base VMDBK
                                                    only.
     46  2E  Bitstring    1  USEITE_VMDSVMWT        Service-virtual-machine (SVM)
                                                    wait flag byte - valid in base
                                                    VMDBK only.
              1... ....      USEITE_VMDSVMWF        VMDBK is waiting for a
                                                    response from IUCV, VMCF, or
                                                    APPC.
     47  2F  Bitstring    1  USEITE_CALFLAG1        Flag byte
              1... ....      USEITE_CALBASE         If on, this is the base
                                                    VMDBK. VMDBASE
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
     48  30  Unsigned     4  USEITE_HFQUCT          Number of times VMDBK was
                                                    sampled for high-frequency data
     52  34  Unsigned     4  USEITE_HFDISP0         Number of times the VMDBK was
                                                    in Q0. VMDSLIST = VMDDISPL and
                                                    VMDELIST = 0.
     56  38  Unsigned     4  USEITE_HFDISP1         Number of times the VMDBK was
                                                    in Q1. VMDSLIST = VMDDISPL and
                                                    VMDELIST = 1.
     60  3C  Unsigned     4  USEITE_HFDISP2         Number of times the VMDBK was
                                                    in Q2. VMDSLIST = VMDDISPL and
                                                    VMDELIST = 2.
     64  40  Unsigned     4  USEITE_HFDISP3         Number of times the VMDBK was
                                                    in Q3. VMDSLIST = VMDDISPL and
                                                    VMDELIST = 3.
     68  44  Unsigned     4  USEITE_HFELIG0         Number of times the VMDBK was
                                                    in E0. VMDSLIST = VMDELIG and
                                                    VMDELIST = 0.
     72  48  Unsigned     4  USEITE_HFELIG1         Number of times the VMDBK was
                                                    in E1. VMDSLIST = VMDELIG and
                                                    VMDELIST = 1.
     76  4C  Unsigned     4  USEITE_HFELIG2         Number of times the VMDBK was
                                                    in E2. VMDSLIST = VMDELIG and
                                                    VMDELIST = 2.
     80  50  Unsigned     4  USEITE_HFELIG3         Number of times the VMDBK was
                                                    in E3. VMDSLIST = VMDELIG and
                                                    VMDELIST = 3.
     84  54  Unsigned     4  USEITE_HFSTCT          Number of times VMDBK was
                                                    high-frequency sampled. This
                                                    was once distinguishable from
                                                    USEITE_HFQUCT but is now the
                                                    same and is retained for
                                                    migration and compatibility
                                                    purposes.
     88  58  Unsigned     4  USEITE_HFTIDL          Number of times this user was
                                                    found in test idle and not in
                                                    SVM wait
     92  5C  Unsigned     4  USEITE_HFTSVM          Number of times this user was
                                                    found in test idle and in SVM
                                                    wait
     96  60  Unsigned     4  USEITE_HFIOWT          Number of times this user was
                                                    in I/O wait. I/O wait indicates
                                                    that a guest is waiting for I/O
                                                    completion status and thus is
                                                    prevented from running. VMDIOWT
    100  64  Unsigned     4  USEITE_HFCFWT          Number of times this user was
                                                    found in console-function wait.
                                                    During such a wait, the virtual
                                                    cpu is not permitted to run.
                                                    VMDCFWT
    104  68  Unsigned     4  USEITE_HFSIMWT         Number of times this user was
                                                    found in 'simulation wait,' in
                                                    which the CPU is simulating
                                                    some hardware functions such as
                                                    instructions, interrupts, or
                                                    timer updates, and the virtual
                                                    machine is thus prevented from
                                                    running to avoid potential
                                                    conflicts with the simulations.
                                                    VMDSIMWT
    108  6C  Unsigned     4  USEITE_HFWTPAG         Number of times this user was
                                                    found in page wait. Page wait
                                                    is when the current guest
                                                    instruction refers to a guest
                                                    page which is not present in
                                                    host storage and must be
                                                    brought in from auxiliary
                                                    storage. Page wait prevents the
                                                    virtual CPU from running,
                                                    however it is a "soft wait"
                                                    condition, and as such can be
                                                    cleared by a guest PSW swap.
                                                    VMDWTPAG
    112  70  Unsigned     4  USEITE_HFCPUWT         Number of times this user was
                                                    found waiting to run on the
                                                    real CPU. VMDSTATE = VMDREADY
    116  74  Unsigned     4  USEITE_HFCPURN         Number of times this user was
                                                    found running on the real CPU.
                                                    VMDSTATE = VMDISPCH
    120  78  Unsigned     4  USEITE_HFESVM          Number of times this user was
                                                    found in SVM wait and in the
                                                    eligible list.
    124  7C  Unsigned     4  USEITE_HFLOAD          Number of times this user was
                                                    considered a loading user.
                                                    VMDLOADU is on and VMDSLIST ^=
                                                    VMDDORM.
    128  80  Unsigned     4  USEITE_HFDORM          Number of times this user was
                                                    found dormant. VMDSLIST =
                                                    VMDDORM
    132  84  Signed       4  USEITE_HFDSVM          Number of times this user was
                                                    found in SVM wait and in the
                                                    dormant list. Note: this count
                                                    is also included in
                                                    USEITE_HFDORM. VMDSVMWF of
                                                    VMDSVMWT = on and VMDSLIST =
                                                    VMDDORM
    136  88  Unsigned     4  USEITE_HFOTHR          Number of times this user was
                                                    not found in any of the above
                                                    states
    140  8C  Unsigned     2  USEITE_VMDCNTID        Number of times user was not
                                                    granted a test idle time when
                                                    it went idle in the dispatch
                                                    list
    142  8E  Unsigned     2  USEITE_VMDCTIDL        Number of times this user was
                                                    granted a test idle time when
                                                    it went idle in the dispatch
                                                    list
    144  90  Unsigned     4  USEITE_VMDDFRWK        Count of 'deferred' work
                                                    items for the VMDBK. A
                                                    'deferred' work item is an
                                                    asynchronous task that has yet
                                                    to run. This VMDBK shall be
                                                    prevented from completing its
                                                    logoff until this count is
                                                    zero, i.e., when all such work
                                                    items have been run.
    148  94  Bitstring    1  USEITE_VMDSTATE        Scheduler/Dispatcher State.
                                                    X'63' = Review-suspended. VMDBK
                                                    is in transition to the
                                                    suspended state. X'58' =
                                                    Review-idle. VMDBK is in
                                                    transition to the idle state.
                                                    X'4D' = VMDBK has been selected
                                                    by dispatcher for processing.
                                                    X'42' = VMDBK is ready for
                                                    selection by dispatcher once it
                                                    goes to the dispatch list.
                                                    X'37' = Test-idle. VMDBK is
                                                    ready for selection by the
                                                    dispatcher but should be
                                                    dropped from the dispatch list
                                                    when selected the next time.
                                                    X'08' = VMDBK is suspended,
                                                    probably waiting for a
                                                    short-term event to occur.
                                                    X'2C' = VMDBK is idle. No work
                                                    is available.
    149  95  Bitstring    1  USEITE_CALOSTAT        Virtual machine operating
                                                    status
              1... ....      USEITE_VMDSYSOP        User is primary system
                                                    operator
              .1.. ....      USEITE_VMDUSRCT        User is counted as being
                                                    logged on
              ..1. ....      *
              ...1 ....      USEITE_VMDFORCE        User is to be logged off.
                                                    This may be requested by CP, a
                                                    forced logoff, or user's logoff
                                                    command.
              .... 1...      USEITE_VMDUFORC        User is forced to logoff the
                                                    system
              .... .1..      USEITE_VMDDISC         User is running disconnected
              .... ..1.      USEITE_VMDAUTOL        AUTOLOG/XAUTOLOG in progress.
                                                    User has been automatically
                                                    logged on. This bit is set off
                                                    when the user's IPL statement
                                                    is processed, or (if there is
                                                    no IPL to process) when the
                                                    user enters a LOGON command
                                                    from a terminal to RECONNECT.
              .... ...1      USEITE_VMDXAUTO        The original command was
                                                    XAUTOLOG. Valid for the base
                                                    VMDBK only.
    150  96  Bitstring    1  USEITE_CALRSTAT        Reason(s) the dispatched
                                                    VMDBK is not being run
              1... ....      *
              .1.. ....      USEITE_VMDCFWT         VMDBK is in console function
                                                    wait. Either a console function
                                                    is active, or the virtual
                                                    machine is waiting for the
                                                    remaining VMDBKs in the
                                                    configuration to enter console
                                                    function mode.
              ..1. ....      USEITE_VMDSIMWT        CP is simulating some
                                                    hardware function for the guest
                                                    such as instructions,
                                                    interrupts, and timer updates.
                                                    Virtual machine is prevented
                                                    from running to avoid potential
                                                    conflicts with the simulations.
              ...1 ....      USEITE_VMDIOWT         Instruction waiting for I/O
                                                    status for completion. (May be
                                                    cancelled without loss of
                                                    system integrity.)
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
    151  97  Unsigned     1  *                      Reserved for IBM use
    152  98  Unsigned     2  USEITE_VMDCPRMD(4)     Number of times this user was
                                                    pre-emptied from the dispatch
                                                    list (Q0, Q1, Q2, Q3) due to a
                                                    requirement for storage for E1
                                                    users.
    160  A0  Unsigned     2  USEITE_VMDCWSGD(4)     Number of times this user was
                                                    removed from the dispatch list
                                                    (Q0, Q1, Q2, Q3) because it
                                                    reached its working set size
                                                    growth limit, and its new
                                                    working set size would no
                                                    longer fit into available
                                                    storage.
    168  A8  Unsigned     2  USEITE_VMDCETSD(4)     Number of times this user was
                                                    removed from the dispatch list
                                                    (Q0, Q1, Q2, Q3) because it
                                                    reached elapsed time slice end.
    176  B0  Unsigned     2  USEITE_VMDCIDLD(4)     Number of times this user was
                                                    removed from the dispatch list
                                                    (Q0, Q1, Q2, Q3) because its
                                                    test idle time had expired or
                                                    because it was granted no test
                                                    idle time.
    184  B8  Unsigned     4  USEITE_HFIOACT         High Frequency Count.
                                                    Cardinal number of times the
                                                    user had an asynchronous I/O
                                                    outstanding, causing the user
                                                    to be left in the dispatch
                                                    list. VMDIOACT
    188  BC  Unsigned     4  USEITE_HFLLIST         High Frequency Count. Number
                                                    of times the user was in
                                                    dispatch list waiting for CPU
                                                    but was on the Limit List,
                                                    prevented from running by max
                                                    share.
    192  C0  Unsigned     4  USEITE_HFPGACT         High Frequency Count. Number
                                                    of times the virtual machine
                                                    had page fault requests active,
                                                    but was not in page wait
                                                    (VMDWTPAG was not set). This
                                                    would occur if asynchronous
                                                    page fault was being used and
                                                    there was an outstanding page
                                                    fault, but the virtual machine
                                                    loaded a wait state because it
                                                    had no other work to do. A
                                                    virtual machine can have page
                                                    faults handled asynchronously
                                                    if using the PAGEX feature or
                                                    the Page-Fault Handshaking CP
                                                    services via the CP PFAULT
                                                    MACRO.
    196  C4  Unsigned     1  USEITE_VMDPUTYP        CPU Type. Valid values: X'00'
                                                    - General Purpose (CP) X'02' -
                                                    zSeries Application Assist
                                                    (zAAP) X'03' - Integrated
                                                    Facility for Linux (IFL) X'04'
                                                    - Internal Coupling Facility
                                                    (ICF) X'05' - zSeries
                                                    Integrated Information (zIIP)
    197  C5  Bitstring    1  USEITE_VMDCFGEM        Virtual configuration
                                                    indicators. Valid in base VMDBK
                                                    only
              1... ....      *
              .1.. ....      USEITE_VMDCPUAF        User requested CPU Affinity
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
    198  C6  Bitstring    1  USEITE_VMDPUST         CPU Status flag
              1... ....      USEITE_VMDAFSUP        CPU Affinity suppressed
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
    199  C7  Character    1  *                      Reserved for IBM use
    200  C8  Character    0  USEITE_END

    MRUSEITE Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    USEITE                     0    200
    USEITE_CALBASE            2F           80
    USEITE_CALFLAG1           2F      1
    USEITE_CALOSTAT           95      1
    USEITE_CALRSTAT           96      1
    USEITE_END                C8      0
    USEITE_HFCFWT             64      4
    USEITE_HFCPURN            74      4
    USEITE_HFCPUWT            70      4
    USEITE_HFDISP0            34      4
    USEITE_HFDISP1            38      4
    USEITE_HFDISP2            3C      4
    USEITE_HFDISP3            40      4
    USEITE_HFDORM             80      4
    USEITE_HFDSVM             84      4
    USEITE_HFELIG0            44      4
    USEITE_HFELIG1            48      4
    USEITE_HFELIG2            4C      4
    USEITE_HFELIG3            50      4
    USEITE_HFESVM             78      4
    USEITE_HFIOACT            B8      4
    USEITE_HFIOWT             60      4
    USEITE_HFLLIST            BC      4
    USEITE_HFLOAD             7C      4
    USEITE_HFOTHR             88      4
    USEITE_HFPGACT            C0      4
    USEITE_HFQUCT             30      4
    USEITE_HFSIMWT            68      4
    USEITE_HFSTCT             54      4
    USEITE_HFTIDL             58      4
    USEITE_HFTSVM             5C      4
    USEITE_HFWTPAG            6C      4
    USEITE_MRHDR               0      0
    USEITE_VMDAFSUP           C6           80
    USEITE_VMDAUTOL           95           02
    USEITE_VMDCETSD           A8      8
    USEITE_VMDCFGEM           C5      1
    USEITE_VMDCFWT            96           40
    USEITE_VMDCIDLD           B0      8
    USEITE_VMDCNTID           8C      2
    USEITE_VMDCPRMD           98      8
    USEITE_VMDCPUAD           1C      2
    USEITE_VMDCPUAF           C5           40
    USEITE_VMDCTIDL           8E      2
    USEITE_VMDCWSGD           A0      8
    USEITE_VMDDFRWK           90      4
    USEITE_VMDDISC            95           04
    USEITE_VMDFORCE           95           10
    USEITE_VMDIOWT            96           10
    USEITE_VMDPUST            C6      1
    USEITE_VMDPUTYP           C4      1
    USEITE_VMDRDYCM           2E      0
    USEITE_VMDSIMWT           96           20
    USEITE_VMDSLCNT           1E      2
    USEITE_VMDSTATE           94      1
    USEITE_VMDSVMFX           20      4
    USEITE_VMDSVMID           24      8
    USEITE_VMDSVMWF           2C           80
    USEITE_VMDSVMWF           2D           80
    USEITE_VMDSVMWF           2E           80
    USEITE_VMDSVMWT           2C      1
    USEITE_VMDSVMWT           2D      1
    USEITE_VMDSVMWT           2E      1
    USEITE_VMDSVMW2           2D      0
    USEITE_VMDSYSOP           95           80
    USEITE_VMDUFORC           95           08
    USEITE_VMDUSER            14      8
    USEITE_VMDUSRCT           95           40
    USEITE_VMDXAUTO           95           01

    This information is
    based on z/VM V6R1.0.

    Last updated on 8 Oct 2009 at 21:08:13.

    Copyright IBM Corporation, 1990, 2009