Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRMTRSOS

Prolog
Control Block Contents
Cross Reference

#### MRMTRSOS Prolog

####

####

     DSECT NAME - MTRSOS
     FUNCTION - This record indicates the start of a suspend condition
                for event data collection.
     LOCATED BY -
               Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRMTRSOS
     DESCRIPTIVE NAME - Monitor Event Record
                        Domain 1  - Monitor Domain
                        Record 12 - Event Record Start of Suspend
     DESCRIPTION - Indicates event monitoring has suspended. Placed as
                   the last record in the last block of data that was
                   completed before the suspend begins.  Since space is
                   always reserved for this record, it will always be
                   present even when the cause of suspension is due to
                   no more space in the DCSS.

    MRMTRSOS Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure   20  MTRSOS                 Start of monitor record
      0   0  Character    0  MTRSOS_MRHDR           Record header. See MRRECHDR
                                                    for details.
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN               record length in bytes
      2   2  Unsigned     2  MRHDRZER               field of zeros
      4   4  Unsigned     1  MRHDRDM                domain identifier
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC                record identifier
      8   8  Character    8  MRHDRTOD               Time at which this record was
                                                    built. In time-of-day (TOD)
                                                    clock format. See IBM System
                                                    370 XA Principle of Operation
                                                    for explanation of format.
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END              End of header
     20  14  Character    0  MTRSOS_END

    MRMTRSOS Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    MTRSOS                     0     20
    MTRSOS_END                14      0
    MTRSOS_MRHDR               0      0

    This information is
    based on z/VM V6R1.0.

    Last updated on 8 Oct 2009 at 21:08:13.

    Copyright IBM Corporation, 1990, 2009