Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### NSCPR

Prolog

Control Block Contents
NSCPR DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### NSCPR Prolog

     Name       : HCPNSCPR
     Description: HCPNSCPR parameter list mapping
     DSECT      : NSCPR

#### NSCPR Control Block Content

#### NSCPR DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      NSCPR          HCPNSCPR parameter list mapping
                       THESE FIELDS ARE USED FOR ENTRY TO HCPNSCSG
                 AND HCPNSCSY.
                 - FIRST TIME SEARCH ONLY REQUIRES THAT NSCNAME BE
                   FILLED IN.
                 - SECOND TIME SEARCH OR A RE-SCAN WOULD REQUIRE
                   NSCSNTBK TO BE FILLED IN FOR NSS, DCSS, SEGMENT
                   SPACE, AND MEMBERS.
                   FOR MEMBER SEGMENTS NSCLSNT@ AND NSCLNAME NEED TO
                   FILLED IN TO DETERMINE IF THE MEMBER IS STILL PART
                   OF THE SEGMENT SPACE.
                   NOTES      : NSCSNTBK IS FILLED IN BY BOTH ENTRY POINTS.
                         NSCLSNT@ AND NSCLNAME ARE FILLED IN BY
                         HCPNSCSG ONLY.
                         THE INPUT FOR NSCSNTBK, NSCLSNT@, AND
                         NSCLNAME  ARE FILLED IN BY HCPNSC MODULE
                         AND SHOULD NOT BE FILLED IN BY THE CALLER.
    0000    0 Character    8 NSCNAME        INPUT - NAME USED TO LOCATE THE
                                            SNTBK ADDRESS.
    0008    8 Signed       4 NSCSNTBK       OUTPUT - ADDRESS OF THE SNTBK.
                                            INPUT - IF ZERO START FROM
                                            BEGINNING OF QUEUE. IF NOT ZERO
                                            START AT THE SNTBK POINTED TO BY
                                            THIS FIELD.
    000C   12 Signed       4 NSCLSNT@       OUTPUT - LOGICAL SNTBK ADDRESS
                                            WHEN NSCNAME IS A MEMBER DCSS.
                                            INPUT - IF NOT ZERO THEN START AT
                                            THIS SNTBK ADDRESS TO CONTINUE
                                            SEARCHING FOR OTHER DCSS.
    0010   16 Character    8 NSCLNAME       OUTPUT - THE NAME OF THE LOGICAL
                                            SNTBK THAT CONTAINS THE MEMBER
                                            NAME.
                                     INPUT  - A FURTHER CHECK TO ENSURE THAT
                                              THE SNTBK IS STILL VALID TO
                                              CONTINUE SEARCHING.
              00000018       NSCBSIZE       *-NSCPR BYTE SIZE OF THIS DSECT.
              00000003       NSCSIZE        (NSCBSIZE+7)/8 SIZE IN
                                            DOUBLEWORDS.

#### NSCPR Storage Layout

    *** NSCPR - HCPNSCPR parameter list mapping
    *
    *     +-------------------------------------------------------+
    *   0 |                       NSCNAME                         |
    *     +---------------------------+---------------------------+
    *   8 |         NSCSNTBK          |         NSCLSNT@          |
    *     +---------------------------+---------------------------+
    *  10 |                       NSCLNAME                        |
    *     +-------------------------------------------------------+
    *  18
    *
    *** NSCPR - HCPNSCPR parameter list mapping

#### NSCPR Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    NSCBSIZE       0010 00000018
    NSCLNAME       0010
    NSCLSNT@       000C
    NSCNAME        0000
    NSCSIZE        0010 00000003
    NSCSNTBK       0008

This information is based on z/VM V6R1.0. Last updated on 18 Feb 2010 at 08:52:28 EDT.
Copyright IBM Corporation, 1990, 2008