Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSYTRSG

Prolog
Control Block Contents
Cross Reference

#### MRSYTRSG Prolog

####

####

     DSECT NAME - SYTRSG
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSYTRSG
     DESCRIPTIVE NAME - Monitor Sample Record
                        Domain 0 - System Domain
                        Record 3 - Real Storage Data (Global)
     DESCRIPTION - Real storage allocation and use. Provides
                   dynamically changing classes of usage.
                   Static classes of usage are provided in the
                   MONITOR domain.

    MRSYTRSG Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure  484  SYTRSG                 Start of monitor record
      0   0  Character    0  SYTRSG_MRHDR           Record header. See MRRECHDR
                                                    for details.
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN               record length in bytes
      2   2  Unsigned     2  MRHDRZER               field of zeros
      4   4  Unsigned     1  MRHDRDM                domain identifier
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC                record identifier
      8   8  Character    8  MRHDRTOD               Time at which this record was
                                                    built. In time-of-day (TOD)
                                                    clock format. See IBM System
                                                    370 XA Principle of Operation
                                                    for explanation of format.
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END              End of header
     20  14  Unsigned     4  *                      Reserved for IBM use.
                                                    Previous field is no longer
                                                    meangingul. (SYTRSG_RSAFSTOR)
     24  18  Unsigned     4  *                      Reserved for IBM use.
                                                    Previous field is no longer
                                                    meaningful. (SYTRSG_SYSVRSZ)
     28  1C  Unsigned     4  *                      Reserved for IBM use.
                                                    Previous field is no longer
                                                    meaningful. (SYTRSG_RSAFSYUD)
     32  20  Unsigned     4  *                      Reserved for IBM use.
                                                    Previous field is no longer
                                                    meaningful. (SYTRSG_RSAFVRUD)
     36  24  Unsigned     4  SYTRSG_SYSRSVPG        Cardinal count of reserved
                                                    pages.
     40  28  Unsigned     4  SYTRSG_RSACPLOK        Cardinal count of frames
                                                    locked below 2G by the CP LOCK
                                                    REAL command. See
                                                    SYTRSG_RSACPLKG for the >2G
                                                    count.
     44  2C  Unsigned     4  SYTRSG_RSANONPG        Cardinal count of <2G
                                                    pageable frames in the system
                                                    that have been made
                                                    non-pageable. This includes
                                                    pages locked for I/O, CP LOCK
                                                    command, virtual system lock
                                                    functions, etc. See
                                                    SYTRSG_RSAPGABL and
                                                    SYTRSG_RSALGFRM.
     48  30  Unsigned     4  SYTRSG_RSAPGABL        Cardinal count of <2G
                                                    pageable frames in the system.
                                                    This includes those that had
                                                    been made non-pageable (see
                                                    SYTRSG_RSANONPG). The size of
                                                    the dynamic area (DPA) or the
                                                    count of useable frames may be
                                                    calculated by subtracting
                                                    RSANONPG from RSAPGABL. See
                                                    SYTRSG_RSALGFRM for the >2G
                                                    field for the count of useable
                                                    frames. NOTE: There is no
                                                    separate count for pageable
                                                    frames (RSAPAGBL) and frames
                                                    made non-pageable (RSANONPG)
                                                    >2G.
     52  34  Unsigned     4  SYTRSG_RSAAVAIL        Cardinal count of ALL frames
                                                    that are currently on the <2G
                                                    available lists. This is a
                                                    TOTAL VALUE (Singles+Contig) as
                                                    in previous releases. See
                                                    SYTRSG_RSA2GAVL for the >2G
                                                    count.
     56  38  Unsigned     4  SYTRSG_RSAFRQWT        Cardinal count of deferred
                                                    tasks waiting for a frame. This
                                                    represents the number of
                                                    requests for real frames which
                                                    have not been satisfied yet
                                                    because no frames are
                                                    available. It includes both
                                                    tasks waiting for frames above
                                                    and below the 2GB line. For a
                                                    count of tasks waiting for a
                                                    frame below 2GB, subtract
                                                    SYTRSG_RSA2GDCT from this
                                                    field.
     60  3C  Unsigned     4  SYTRSG_RSAXTEND        Cardinal count of frames
                                                    missing from the free storage
                                                    reserved frames list.
     64  40  Unsigned     4  *                      Reserved for IBM use.
                                                    Previous field is no longer
                                                    meaningful. (SYTRSG_RSAXFREE)
     68  44  Unsigned     4  SYTRSG_RSASAVFR        Cardinal count of frames in
                                                    use for saveareas.
     72  48  Bitstring    1  *                      Reserved for IBM use.
                                                    Previous field is no longer
                                                    meaningful. (SYTRSG_CALSTAT)
     73  49  Bitstring    1  SYTRSG_CALFLAG1        Flags byte.
              1... ....      SYTRSG_TCMCACHE        Minidisk Caching is enabled.
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
     74  4A  Unsigned     2  SYTRSG_HCPSTPMB        Bias for minidisk cache use
                                                    of real storage. A decimal
                                                    point is assumed to the left of
                                                    the low order 2 digits. For
                                                    example, a value of decimal 95
                                                    in this field would be a bias
                                                    setting of .95 .
     76  4C  Unsigned     4  SYTRSG_SYS98XA         Cardinal number of pages
                                                    locked by Diagnose X'98' in
                                                    31-bit mode
     80  50  Unsigned     4  *                      Reserved for IBM use.
                                                    Previous field is no longer
                                                    meaningful. (SYTRSG_SYS98370)
     84  54  Unsigned     4  SYTRSG_TCMMIDSZ        Maximum allowable number of
                                                    pages in mindisk cache (based
                                                    on average age of a page in
                                                    DPA). AKA "ideal main store
                                                    cache size", set by arbiter
                                                    logic in HCPSTP.
     88  58  Unsigned     4  SYTRSG_TCMMAIN         Current number of pages in
                                                    main storage being used as
                                                    track cache pages. For a
                                                    breakdown of pages below and
                                                    above the 2GB line, see
                                                    SYTRSG_TCMMNBLW and
                                                    SYTRSG_TCMMNABV.
     92  5C  Unsigned     4  SYTRSG_TCMMNMIN        Minimum number of main
                                                    storage pages used by cache as
                                                    set by user command
     96  60  Unsigned     4  SYTRSG_TCMMNMAX        Maximum number of main
                                                    storage pages used by cache as
                                                    set by user command
    100  64  Unsigned     4  SYTRSG_TCMMNDL         Number of main storage pages
                                                    deleted from cache
    104  68  Unsigned     4  SYTRSG_TCMSTLMN        Number of times the steal
                                                    function was invoked to steal
                                                    main storage pages from the
                                                    track cache
    108  6C  Unsigned     4  SYTRSG_SYSSCMAV        Number of SCMBKs that are
                                                    available. This field is valid
                                                    only when format-0 measurement
                                                    blocks are being used
                                                    (MTRSYS_CALFLG2 <> x'80').
    112  70  Unsigned     4  SYTRSG_TCMMNBLW        Number of pages in main
                                                    storage below 2GB in use as
                                                    track cache pages. For ESA/390
                                                    systems this field will be
                                                    equal to SYTRSG_TCMMAIN.
    116  74  Unsigned     4  SYTRSG_TCMMNABV        Number of pages in main
                                                    storage at or above 2GB in use
                                                    as track cache pages. For
                                                    ESA/390 systems this field will
                                                    be zero.
    120  78  Unsigned     4  SYTRSG_RSA2GDCT        Cardinal count of deferred
                                                    tasks that are waiting for
                                                    frames that can be above the
                                                    2GB line. See SYTRSG_RSADFRQWT
                                                    for the total count. For a
                                                    count of tasks waiting for
                                                    frames below the 2GB line,
                                                    subtract this field from
                                                    SYTRSG_RSADFRQWT.
    124  7C  Unsigned     4  SYTRSG_SYSSCGCT        Number of SCGBKs currently
                                                    allocated. This field is valid
                                                    only when format-1 measurement
                                                    blocks are being used
                                                    (MTRSYS_CALFLG2 = x'80').
    128  80  Character    8  SYTRSG_RSALGFRM        Cardinal count of >2G useable
                                                    frames. See SYTRSG_RSAPGABL and
                                                    STYRSG_RSANONPG for the <2G
                                                    value.
    136  88  Unsigned     4  SYTRSG_RSACPLKG        Cardinal count of frames
                                                    locked above 2G by the CP LOCK
                                                    REAL command. See
                                                    SYTRSG_RSACPLOK for the <2G
                                                    count.
    140  8C  Character    8  SYTRSG_RSA2GAVL
    140  8C  Unsigned     4  SYTRSG_RSA2GAV1        Top half is always 0
    144  90  Unsigned     4  SYTRSG_RSA2GAV2        Bottom half can represent up
                                                    to 16T
    148  94  Unsigned     4  SYTRSG_RSAFSB2G        Count of doublewords assigned
                                                    to subpool free storage backed
                                                    below 2G.
    152  98  Unsigned     4  SYTRSG_RSAFSA2G        Count of doublewords assigned
                                                    to subpool free storage backed
                                                    above 2G.
    156  9C  Unsigned     4  SYTRSG_RSAFSYUB        Count of doublewords of in
                                                    use subpool free storage backed
                                                    below 2G.
    160  A0  Unsigned     4  SYTRSG_RSAFSYUA        Count of doublewords of in
                                                    use subpool free storage backed
                                                    above 2G.
    164  A4  Unsigned     4  SYTRSG_RSASXCPL        Count of locked System
                                                    Execution Space alias pages
                                                    locked in logical via the CP
                                                    LOCK command.
    168  A8  Unsigned     4  SYTRSG_RSASXCLA        Count of locked System
                                                    Execution Space alias pages
                                                    locked in logical. RSASXCLA >=
                                                    RSASXCPL
    172  AC  Unsigned     4  SYTRSG_RSARFRST        Count of frames allocated for
                                                    real free storage <2G.
    176  B0  Character    8  SYTRSG_RSARFRSG        Count of frames allocated for
                                                    real free storage >2G.
    184  B8  Unsigned     4  SYTRSG_RSASXBCT        Count of SXS pages on the
                                                    queue of SXS pages backed below
                                                    2G.
    188  BC  Unsigned     4  SYTRSG_RSASXACT        Count of SXS pages on the
                                                    queue of SXS pages backed above
                                                    2G.
    192  C0  Unsigned     4  SYTRSG_RSAAFRDB        Count of doublewords of
                                                    aligned real free storage <2G.
                                                    This count includes active as
                                                    well as inactive aligned free
                                                    storage.
    196  C4  Character    8  SYTRSG_RSAAFRDW        Count of doublewords of
                                                    aligned real free storage >2G.
                                                    This count includes active as
                                                    well as inactive aligned free
                                                    storage.
    204  CC  Unsigned     4  SYTRSG_RSAAFRIB        Count of doublewords of in
                                                    use aligned real free storage
                                                    <2G. This count includes only
                                                    active aligned free storage.
    208  D0  Character    8  SYTRSG_RSAAFRIU        Count of doublewords of in
                                                    use aligned real free storage
                                                    >2G. This count includes only
                                                    active aligned free storage.
    216  D8  Character    8  SYTRSG_RSACALCT        Count of the total number of
                                                    frames on the cleared available
                                                    list.
    224  E0  Character    8  SYTRSG_RSASNG2G        Cardinal count of ALL Single
                                                    frames that are currently on
                                                    the >2G available list.
    232  E8  Unsigned     4  SYTRSG_RSASNGAV        Cardinal count of ALL Single
                                                    frames that are currently on
                                                    the <2G available list.
    236  EC  Unsigned     4  SYTRSG_RSALTDB1        Stolen <2G Long Term Dormant
                                                    Pass 1
    240  F0  Unsigned     4  SYTRSG_RSALTDA1        Stolen >2G Long Term Dormant
                                                    Pass 1
    244  F4  Unsigned     4  SYTRSG_RSALTDD1        Stolen contiguous <2G Long
                                                    Term Dormant Pass 1
    248  F8  Unsigned     4  SYTRSG_RSALTDC1        Stolen contiguous >2G Long
                                                    Term Dormant Pass 1
    252  FC  Unsigned     4  SYTRSG_RSALTDB2        Stolen <2G Long Term Dormant
                                                    Pass 2
    256 100  Unsigned     4  SYTRSG_RSALTDA2        Stolen >2G Long Term Dormant
                                                    Pass 2
    260 104  Unsigned     4  SYTRSG_RSALTDD2        Stolen contiguous <2G Long
                                                    Term Dormant Pass 2
    264 108  Unsigned     4  SYTRSG_RSALTDC2        Stolen contiguous >2G Long
                                                    Term Dormant Pass 2
    268 10C  Unsigned     4  SYTRSG_RSALTDBE        Stolen <2G Long Term Dormant
                                                    Emergency Pass
    272 110  Unsigned     4  SYTRSG_RSALTDAE        Stolen >2G Long Term Dormant
                                                    Emergency Pass
    276 114  Unsigned     4  SYTRSG_RSALTDDE        Stolen contiguous <2G Long
                                                    Term Dormant Emergency Pass
    280 118  Unsigned     4  SYTRSG_RSALTDCE        Stolen contiguous >2G Long
                                                    Term Dormant Emergency Pass
    284 11C  Unsigned     4  SYTRSG_RSADRMB1        Stolen <2G Dormant Pass 1
    288 120  Unsigned     4  SYTRSG_RSADRMA1        Stolen >2G Dormant Pass 1
    292 124  Unsigned     4  SYTRSG_RSADRMD1        Stolen contiguous <2G Dormant
                                                    Pass 1
    296 128  Unsigned     4  SYTRSG_RSADRMC1        Stolen contiguous >2G Dormant
                                                    Pass 1
    300 12C  Unsigned     4  SYTRSG_RSADRMB2        Stolen <2G Dormant Pass 2
    304 130  Unsigned     4  SYTRSG_RSADRMA2        Stolen >2G Dormant Pass 2
    308 134  Unsigned     4  SYTRSG_RSADRMD2        Stolen contiguous <2G Dormant
                                                    Pass 2
    312 138  Unsigned     4  SYTRSG_RSADRMC2        Stolen contiguous >2G Dormant
                                                    Pass 2
    316 13C  Unsigned     4  SYTRSG_RSADRMBE        Stolen <2G Dormant Emergency
                                                    Pass
    320 140  Unsigned     4  SYTRSG_RSADRMAE        Stolen >2G Dormant Emergency
                                                    Pass
    324 144  Unsigned     4  SYTRSG_RSADRMDE        Stolen contiguous <2G Dormant
                                                    Emergency Pass
    328 148  Unsigned     4  SYTRSG_RSADRMCE        Stolen contiguous >2G Dormant
                                                    Emergency Pass
    332 14C  Unsigned     4  SYTRSG_RSAELGB1        Stolen <2G Eligible Pass 1
    336 150  Unsigned     4  SYTRSG_RSAELGA1        Stolen >2G Eligible Pass 1
    340 154  Unsigned     4  SYTRSG_RSAELGD1        Stolen contiguous <2G
                                                    Eligible Pass 1
    344 158  Unsigned     4  SYTRSG_RSAELGC1        Stolen contiguous >2G
                                                    Eligible Pass 1
    348 15C  Unsigned     4  SYTRSG_RSAELGB2        Stolen <2G Eligible Pass 2
    352 160  Unsigned     4  SYTRSG_RSAELGA2        Stolen >2G Eligible Pass 2
    356 164  Unsigned     4  SYTRSG_RSAELGD2        Stolen contiguous <2G
                                                    Eligible Pass 2
    360 168  Unsigned     4  SYTRSG_RSAELGC2        Stolen contiguous >2G
                                                    Eligible Pass 2
    364 16C  Unsigned     4  SYTRSG_RSAELGBE        Stolen <2G Eligible Emergency
                                                    Pass
    368 170  Unsigned     4  SYTRSG_RSAELGAE        Stolen >2G Eligible Emergency
                                                    Pass
    372 174  Unsigned     4  SYTRSG_RSAELGDE        Stolen contiguous <2G
                                                    Eligible Emergency Pass
    376 178  Unsigned     4  SYTRSG_RSAELGCE        Stolen contiguous >2G
                                                    Eligible Emergency Pass
    380 17C  Unsigned     4  SYTRSG_RSADSPB1        Stolen <2G Dispatch Pass 1
    384 180  Unsigned     4  SYTRSG_RSADSPA1        Stolen >2G Dispatch Pass 1
    388 184  Unsigned     4  SYTRSG_RSADSPD1        Stolen contiguous <2G
                                                    Dispatch Pass 1
    392 188  Unsigned     4  SYTRSG_RSADSPC1        Stolen contiguous >2G
                                                    Dispatch Pass 1
    396 18C  Unsigned     4  SYTRSG_RSADSPB2        Stolen <2G Dispatch Pass 2
    400 190  Unsigned     4  SYTRSG_RSADSPA2        Stolen >2G Dispatch Pass 2
    404 194  Unsigned     4  SYTRSG_RSADSPD2        Stolen contiguous <2G
                                                    Dispatch Pass 2
    408 198  Unsigned     4  SYTRSG_RSADSPC2        Stolen contiguous >2G
                                                    Dispatch Pass 2
    412 19C  Unsigned     4  SYTRSG_RSADSPBE        Stolen <2G Dispatch Emergency
                                                    Pass
    416 1A0  Unsigned     4  SYTRSG_RSADSPAE        Stolen >2G Dispatch Emergency
                                                    Pass
    420 1A4  Unsigned     4  SYTRSG_RSADSPDE        Stolen contiguous <2G
                                                    Dispatch Emergency Pass
    424 1A8  Unsigned     4  SYTRSG_RSADSPCE        Stolen contiguous >2G
                                                    Dispatch Emergency Pass
    428 1AC  Unsigned     4  SYTRSG_RSASHRB1        Stolen <2G Shared Pass 1
    432 1B0  Unsigned     4  SYTRSG_RSASHRA1        Stolen >2G Shared Pass 1
    436 1B4  Unsigned     4  SYTRSG_RSASHRD1        Stolen contiguous <2G Shared
                                                    Pass 1
    440 1B8  Unsigned     4  SYTRSG_RSASHRC1        Stolen contiguous >2G Shared
                                                    Pass 1
    444 1BC  Unsigned     4  SYTRSG_RSASHRB2        Stolen <2G Shared Pass 2
    448 1C0  Unsigned     4  SYTRSG_RSASHRA2        Stolen >2G Shared Pass 2
    452 1C4  Unsigned     4  SYTRSG_RSASHRD2        Stolen contiguous <2G Shared
                                                    Pass 2
    456 1C8  Unsigned     4  SYTRSG_RSASHRC2        Stolen contiguous >2G Shared
                                                    Pass 2
    460 1CC  Unsigned     4  SYTRSG_RSASHRBE        Stolen <2G Shared Emergency
                                                    Pass
    464 1D0  Unsigned     4  SYTRSG_RSASHRAE        Stolen >2G Shared Emergency
                                                    Pass
    468 1D4  Unsigned     4  SYTRSG_RSASHRDE        Stolen contiguous <2G Shared
                                                    Emergency Pass
    472 1D8  Unsigned     4  SYTRSG_RSASHRCE        Stolen contiguous >2G Shared
                                                    Emergency Pass
    476 1DC  Unsigned     4  SYTRSG_RSARESAC        Count of resident PTRM pages
                                                    i.e. count of resident PGMBK
                                                    frames >= 2G
    480 1E0  Unsigned     4  SYTRSG_RSARESBC        Count of resident PTRM pages
                                                    i.e. count of resident PGMBK
                                                    frames < 2G
    484 1E4  Character    0  SYTRSG_END

    MRSYTRSG Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    SYTRSG                     0    484
    SYTRSG_CALFLAG1           49      1
    SYTRSG_END               1E4      0
    SYTRSG_HCPSTPMB           4A      2
    SYTRSG_MRHDR               0      0
    SYTRSG_RSAAFRDB           C0      4
    SYTRSG_RSAAFRDW           C4      8
    SYTRSG_RSAAFRIB           CC      4
    SYTRSG_RSAAFRIU           D0      8
    SYTRSG_RSAAVAIL           34      4
    SYTRSG_RSACALCT           D8      8
    SYTRSG_RSACPLKG           88      4
    SYTRSG_RSACPLOK           28      4
    SYTRSG_RSADRMAE          140      4
    SYTRSG_RSADRMA1          120      4
    SYTRSG_RSADRMA2          130      4
    SYTRSG_RSADRMBE          13C      4
    SYTRSG_RSADRMB1          11C      4
    SYTRSG_RSADRMB2          12C      4
    SYTRSG_RSADRMCE          148      4
    SYTRSG_RSADRMC1          128      4
    SYTRSG_RSADRMC2          138      4
    SYTRSG_RSADRMDE          144      4
    SYTRSG_RSADRMD1          124      4
    SYTRSG_RSADRMD2          134      4
    SYTRSG_RSADSPAE          1A0      4
    SYTRSG_RSADSPA1          180      4
    SYTRSG_RSADSPA2          190      4
    SYTRSG_RSADSPBE          19C      4
    SYTRSG_RSADSPB1          17C      4
    SYTRSG_RSADSPB2          18C      4
    SYTRSG_RSADSPCE          1A8      4
    SYTRSG_RSADSPC1          188      4
    SYTRSG_RSADSPC2          198      4
    SYTRSG_RSADSPDE          1A4      4
    SYTRSG_RSADSPD1          184      4
    SYTRSG_RSADSPD2          194      4
    SYTRSG_RSAELGAE          170      4
    SYTRSG_RSAELGA1          150      4
    SYTRSG_RSAELGA2          160      4
    SYTRSG_RSAELGBE          16C      4
    SYTRSG_RSAELGB1          14C      4
    SYTRSG_RSAELGB2          15C      4
    SYTRSG_RSAELGCE          178      4
    SYTRSG_RSAELGC1          158      4
    SYTRSG_RSAELGC2          168      4
    SYTRSG_RSAELGDE          174      4
    SYTRSG_RSAELGD1          154      4
    SYTRSG_RSAELGD2          164      4
    SYTRSG_RSAFRQWT           38      4
    SYTRSG_RSAFSA2G           98      4
    SYTRSG_RSAFSB2G           94      4
    SYTRSG_RSAFSYUA           A0      4
    SYTRSG_RSAFSYUB           9C      4
    SYTRSG_RSALGFRM           80      8
    SYTRSG_RSALTDAE          110      4
    SYTRSG_RSALTDA1           F0      4
    SYTRSG_RSALTDA2          100      4
    SYTRSG_RSALTDBE          10C      4
    SYTRSG_RSALTDB1           EC      4
    SYTRSG_RSALTDB2           FC      4
    SYTRSG_RSALTDCE          118      4
    SYTRSG_RSALTDC1           F8      4
    SYTRSG_RSALTDC2          108      4
    SYTRSG_RSALTDDE          114      4
    SYTRSG_RSALTDD1           F4      4
    SYTRSG_RSALTDD2          104      4
    SYTRSG_RSANONPG           2C      4
    SYTRSG_RSAPGABL           30      4
    SYTRSG_RSARESAC          1DC      4
    SYTRSG_RSARESBC          1E0      4
    SYTRSG_RSARFRSG           B0      8
    SYTRSG_RSARFRST           AC      4
    SYTRSG_RSASAVFR           44      4
    SYTRSG_RSASHRAE          1D0      4
    SYTRSG_RSASHRA1          1B0      4
    SYTRSG_RSASHRA2          1C0      4
    SYTRSG_RSASHRBE          1CC      4
    SYTRSG_RSASHRB1          1AC      4
    SYTRSG_RSASHRB2          1BC      4
    SYTRSG_RSASHRCE          1D8      4
    SYTRSG_RSASHRC1          1B8      4
    SYTRSG_RSASHRC2          1C8      4
    SYTRSG_RSASHRDE          1D4      4
    SYTRSG_RSASHRD1          1B4      4
    SYTRSG_RSASHRD2          1C4      4
    SYTRSG_RSASNGAV           E8      4
    SYTRSG_RSASNG2G           E0      8
    SYTRSG_RSASXACT           BC      4
    SYTRSG_RSASXBCT           B8      4
    SYTRSG_RSASXCLA           A8      4
    SYTRSG_RSASXCPL           A4      4
    SYTRSG_RSAXTEND           3C      4
    SYTRSG_RSA2GAVL           8C      8
    SYTRSG_RSA2GAV1           8C      4
    SYTRSG_RSA2GAV2           90      4
    SYTRSG_RSA2GDCT           78      4
    SYTRSG_SYSRSVPG           24      4
    SYTRSG_SYSSCGCT           7C      4
    SYTRSG_SYSSCMAV           6C      4
    SYTRSG_SYS98XA            4C      4
    SYTRSG_TCMCACHE           49           80
    SYTRSG_TCMMAIN            58      4
    SYTRSG_TCMMIDSZ           54      4
    SYTRSG_TCMMNABV           74      4
    SYTRSG_TCMMNBLW           70      4
    SYTRSG_TCMMNDL            64      4
    SYTRSG_TCMMNMAX           60      4
    SYTRSG_TCMMNMIN           5C      4
    SYTRSG_TCMSTLMN           68      4

    This information is
    based on z/VM V6R1.0.

    Last updated on 8 Oct 2009 at 21:08:13.

    Copyright IBM Corporation, 1990, 2009