Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### XITPL

Prolog

Control Block Contents
XITPL DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### XITPL Prolog

     NAME       : HCPXITPL
     DESCRIPTION: Exit Plist
     DSECT      : XITPL
     FUNCTION   : The Exit Plist describes the standard fields in the
                  CP Exit parameters supplied to the exit routines.
                  Additional fields are expected to be appended by the
                  various routines that build exit plists.
     LOCATED BY : R1 at invocation of the HCPXSERV CALL service.
     CREATED BY : Any CP routine that has an exit point defined.
     DELETED BY : The CP routine that created it.
     SERIALIZED : None
     NOTES      : Acqusition and release of the exit plist should use
                  the label XITPL.   This is because the true plist
                  (the addresses of data items) is embedded within the
                  acquired storage.  This is done to facilitate use of
                  BLOCKDEF and BLOCKMAP, as well as provide a simple
                  way for one to extend the plist addresses at XITPLVAR
                  without stomping on data that would come after the
                  plist addresses if we didn't put the data at the
                  front of the acquired storage.
                  The 256 byte TRT table, XITPLTRT, must remain on a
                  double word boundary, just so expectaions in user
                  exit routines for a doubleword aligned work area
                  are met.
                  The last address in the true plist should have its
                  high order bit turned on, just so expectaions in user
                  exit routines for a variable length plist are met.

#### XITPL Control Block Content

#### XITPL DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      XITPL          Exit Plist
           The user fields must remain at the front of the block
    0000    0 Dbl-Word     8 XITPLUD1       Reserved for non-IBM use
    0008    8 Dbl-Word     8 XITPLUD2       Reserved for non-IBM use
    0010   16 Signed       4 XITPLUF1       Reserved for non-IBM use
    0014   20 Signed       4 XITPLUF2       Reserved for non-IBM use
    0018   24 Signed       2 XITPLUH1       Reserved for non-IBM use
    001A   26 Signed       2 XITPLUH2       Reserved for non-IBM use
    001C   28 Bitstring    1 XITPLUX1       Reserved for non-IBM use
    001D   29 Bitstring    1 XITPLUX2       Reserved for non-IBM use
    001E   30 Bitstring    1 XITPLUX3       Reserved for non-IBM use
    001F   31 Bitstring    1 XITPLUX4       Reserved for non-IBM use
    0020   32 Dbl-Word     8 * (0)          Align XITPLTRT
    0020   32 Bitstring  256 XITPLTRT       256 bytes for anything
              00000120       XITPLHSZ       *-XITPL Size of standard plist
                                            header Start of the true plist
                                            (list of addresses)
    0120  288 Address      4 XITPLSTR (0)   Start of the plist
    0120  288 Address      4 XITPL@RS       'RESERVED'
    0124  292 Address      4 XITPL@UW       'USERWORD' pointer
    0128  296 Address      4 XITPL@TT       'TRTTABLE' pointer
    012C  300 Address      4 XITPLVAR (0)   Start of variable length data
                                            Addresses of fields specific to
                                            the exit. (Eventually) the end of
                                            the true plist (list of
                                            addresses)
    012C  300 Address      4 XITPL@04       Address of first field specific
                                            to the exit.
    0130  304 Address      4 XITPL@05       Address of second field specific
                                            to the exit.
           etc.

#### XITPL Storage Layout

    *** XITPL - Exit Plist
    *
    *     +-------------------------------------------------------+
    *   0 |                       XITPLUD1                        |
    *     +-------------------------------------------------------+
    *   8 |                       XITPLUD2                        |
    *     +---------------------------+---------------------------+
    *  10 |         XITPLUF1          |         XITPLUF2          |
    *     +-------------+-------------+------+------+------+------+
    *  18 |  XITPLUH1   |  XITPLUH2   |:PLUX1|:PLUX2|:PLUX3|:PLUX4|
    *     +-------------+-------------+------+------+------+------+
    *  20 |                                                       |
    *     =                       XITPLTRT                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 120 |         XITPL@RS          |         XITPL@UW          |
    *     +---------------------------+---------------------------+
    * 128 |         XITPL@TT          |
    *     +---------------------------+
    *
    *** XITPL - Exit Plist

    *** Overlay for XITPLVAR in XITPL
    *
    *                                 +---------------------------+
    * 128 ...                     12C |         XITPL@04          |
    *     +---------------------------+---------------------------+
    * 130 |         XITPL@05          | 134
    *     +---------------------------+
    *
    *** Overlay for XITPLVAR in XITPL

#### XITPL Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    XITPL@RS       0120
    XITPL@TT       0128
    XITPL@UW       0124
    XITPL@04       012C
    XITPL@05       0130
    XITPLHSZ       0020 00000120
    XITPLSTR       0120
    XITPLTRT       0020
    XITPLUD1       0000
    XITPLUD2       0008
    XITPLUF1       0010
    XITPLUF2       0014
    XITPLUH1       0018
    XITPLUH2       001A
    XITPLUX1       001C
    XITPLUX2       001D
    XITPLUX3       001E
    XITPLUX4       001F
    XITPLVAR       012C

This information is based on z/VM V6R1.0. Last updated on 18 Feb 2010 at 09:26:16 EDT.
Copyright IBM Corporation, 1990, 2008