Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRPRCAPM

Prolog
Control Block Contents
Cross Reference

#### MRPRCAPM Prolog

     DSECT NAME - PRCAPM
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRPRCAPM
     DESCRIPTIVE NAME - Monitor Sample Record
                        Domain 5  - Processor Domain
                        Record 10 - Crypto performance measurement data
     DESCRIPTION - Provides counters and timers for transactions on the
                   PCI crypto cards.  One or more records are generated
                   to include all of the information for the processor
                   configuration.  Each record contains a list of
                   Crypto Measurement Blocks (CMBs) for each AP in the
                   processor configuration.

                   When the P bit is 1, one or more additional monitor
                   records are generated in the same interval with the
                   P bit = 1 in each interim record and the P bit = 0
                   in the final record. Each record contains a set of
                   complete CMBs; CMBs are not split between on record
                   and the next.

     NOTES:
       - This record is generated only if PCI crypto cards are installed
         on the system.
       - This record is a mapping of data provided directly from
         hardware.
       - This record is not generated if the HMC Global
         Performance Data setting is disabled.

#### MRPRCAPM Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure   40+ PRCAPM                 Start of monitor record
      0   0  Character    0  PRCAPM_MRHDR           Record header. See MRRECHDR
                                                    for details.
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN
      2   2  Unsigned     2  MRHDRZER
      4   4  Unsigned     1  MRHDRDM
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC
      8   8  Character    8  MRHDRTOD
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END
     20  14  Character    4  *                      Reserved for IBM use
    The store-crypto-measurement-data command-response block follows. The
    fixed-length data starts here.

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

     24  18  Unsigned     2  PRCAPM_L2              Unsigned integer specifying
                                                    the length in bytes of the
                                                    command response block
     26  1A  Unsigned     2  PRCAPM_RC              Unsigned integer specifying
                                                    the response code from the
                                                    store crypto-measurement-data
                                                    command
     28  1C  Character    4  *                      Reserved/zeroes
     32  20  Unsigned     4  *
              1... ....      PRCAPM_P               P bit: when P=0, the entire
                                                    response is returned, when P=1,
                                                    a partial response is returned
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
     32  20  Character    3  *                      Reserved/zeroes
     36  24  Character    4  *                      Reserved/zeroes
    The variable data contains a crypto-measurement-block (CMB) list which
    contains one or more CMBs. The length of the command response block
    including both the fixed-length data and the variable length data is
    specified by the PRCAPM_L2 field. The length of the variable data
    depends on the type of AP (determined by the PRCAPM_CT field in the
    CMB header) and the number of APs installed.

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

     40  28  Character    0  PRCAPM_VAR_DATA        Start of variable length data
    CMB entry for types 3 5 7 and 9 APs. These are PCICC PCIXCC CEX2C and
    CEX3C, respectively. These AP cryptos have just one crypto engine.

    This CMB mapping is also used for PRCAPM_CT = 10 when PRCAPM_MT = 9.

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure   64  PRCAPM_CMB1
      0   0  Character   16  PRCAPM_CMB1HDR
      0   0  Bitstring    1  *                      Reserved/zeroes
      1   1  Bitstring    1  PRCAPM_CT              Crypto type
                                                       Valid values include:
                                                           3, 5, 7, 9, and 10 (when
                                                                PRCAPM_MT = 9)
      2   2  Bitstring    1  *                      Reserved/zeroes
      3   3  Bitstring    1  *
              1... ....      *
              .1.. ....      *
              ..xx xxxx      PRCAPM_AX              AP index
      4   4  Unsigned     4  PRCAPM_S               32-bit binary floating point
                                                    value indicating the stepping
                                                    interval, in seconds, of the
                                                    timers
      8   8  Unsigned     4  PRCAPM_V               32-bit mask indicating the
                                                    validity of each timer-counter
                                                    pair
     12   C  Unsigned     1  *                      Reserved/zeroes
     13   D  Unsigned     1  PRCAPM_MT              Mapping Type
                                                    used for PRCAPM_CT = 10
                                                    only. Zero for all other
                                                    crypto types.
     14   E  Unsigned     2  PRCAPM_L4              CMB Length in bytes
                                                    If zero, use the default lengths:
                                                    CMB type 3,5,7,9    64 bytes
                                                    CMB type 4         336 bytes
                                                    CMB type 6,8        80 bytes
                                                    CMB type 10         96 bytes
     16  10  Character    8  PRCAPM_CMB1_T0         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time of all
                                                    operations on the AP
     24  18  Character    8  PRCAPM_CMB1_C0         64-bit unsigned integer
                                                    counter of the number of all
                                                    operations on the AP
     32  20  Character    8  PRCAPM_CMB1_T1         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time of RSA-key-
                                                    generation operations on the AP
     40  28  Character    8  PRCAPM_CMB1_C1         64-bit unsigned integer
                                                    counter of the number of RSA-
                                                    key-generation operations on
                                                    the AP
     48  30  Character   16  *                      Reserved/zeroes
    CMB entry for type 4 APs. (PCICA) This type of AP has five crypto
    engines and data is reported separately for each engine.

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure  336  PRCAPM_CMB2
      0   0  Character   16  PRCAPM_CMB2HDR
      0   0  Bitstring    1  *                      Reserved/zeroes
      1   1  Bitstring    1  PRCAPM_CT              Crypto type
                                                       Valid values include:
                                                           4
      2   2  Bitstring    1  *                      Reserved/zeroes
      3   3  Bitstring    1  *
              1... ....      *
              .1.. ....      *
              ..xx xxxx      PRCAPM_AX              AP index
      4   4  Unsigned     4  PRCAPM_S               32-bit binary floating point
                                                    value indicating the stepping
                                                    interval, in seconds, of the
                                                    timers
      8   8  Unsigned     4  PRCAPM_V               32-bit mask indicating the
                                                    validity of each timer-counter
                                                    pair
     12   C  Unsigned     1  *                      Reserved/zeroes
     13   D  Unsigned     1  PRCAPM_MT              Mapping Type
                                                    used for PRCAPM_CT = 10
                                                    only. Zero for all other
                                                    crypto types.
     14   E  Unsigned     2  PRCAPM_L4              CMB Length in bytes
                                                    If zero, use the default lengths:
                                                    CMB type 3,5,7,9    64 bytes
                                                    CMB type 4         336 bytes
                                                    CMB type 6,8        80 bytes
                                                    CMB type 10         96 bytes
    Timer-counter pairs for AP engine-0

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

     16  10  Character    8  PRCAPM_CMB2_T0         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-0
                                                    for 1024-bit ME-format RSA
                                                    operations
     24  18  Character    8  PRCAPM_CMB2_C0         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-0 for
                                                    1024-bit ME-format RSA
                                                    operations
     32  20  Character    8  PRCAPM_CMB2_T1         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-0
                                                    for 2048-bit ME-format RSA
                                                    operations
     40  28  Character    8  PRCAPM_CMB2_C1         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-0 for
                                                    2048-bit ME-format RSA
                                                    operations
     48  30  Character    8  PRCAPM_CMB2_T2         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-0
                                                    for 1024-bit CRT-format RSA
                                                    operations
     56  38  Character    8  PRCAPM_CMB2_C2         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-0 for
                                                    1024-bit CRT-format RSA
                                                    operations
     64  40  Character    8  PRCAPM_CMB2_T3         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-0
                                                    for 2048-bit CRT-format RSA
                                                    operations
     72  48  Character    8  PRCAPM_CMB2_C3         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-0 for
                                                    2048-bit CRT-format RSA
                                                    operations
    Timer-counter pairs for AP engine-1

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

     80  50  Character    8  PRCAPM_CMB2_T4         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-1
                                                    for 1024-bit ME-format RSA
                                                    operations
     88  58  Character    8  PRCAPM_CMB2_C4         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-1 for
                                                    1024-bit ME-format RSA
                                                    operations
     96  60  Character    8  PRCAPM_CMB2_T5         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-1
                                                    for 2048-bit ME-format RSA
                                                    operations
    104  68  Character    8  PRCAPM_CMB2_C5         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-1 for
                                                    2048-bit ME-format RSA
                                                    operations
    112  70  Character    8  PRCAPM_CMB2_T6         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-1
                                                    for 1024-bit CRT-format RSA
                                                    operations
    120  78  Character    8  PRCAPM_CMB2_C6         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-1 for
                                                    1024-bit CRT-format RSA
                                                    operations
    128  80  Character    8  PRCAPM_CMB2_T7         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-1
                                                    for 2048-bit CRT-format RSA
                                                    operations
    136  88  Character    8  PRCAPM_CMB2_C7         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-1 for
                                                    2048-bit CRT-format RSA
                                                    operations
    Timer-counter pairs for AP engine-2

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

    144  90  Character    8  PRCAPM_CMB2_T8         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-2
                                                    for 1024-bit ME-format RSA
                                                    operations
    152  98  Character    8  PRCAPM_CMB2_C8         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-2 for
                                                    1024-bit ME-format RSA
                                                    operations
    160  A0  Character    8  PRCAPM_CMB2_T9         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-2
                                                    for 2048-bit ME-format RSA
                                                    operations
    168  A8  Character    8  PRCAPM_CMB2_C9         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-2 for
                                                    2048-bit ME-format RSA
                                                    operations
    176  B0  Character    8  PRCAPM_CMB2_T10        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-2
                                                    for 1024-bit CRT-format RSA
                                                    operations
    184  B8  Character    8  PRCAPM_CMB2_C10        64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-2 for
                                                    1024-bit CRT-format RSA
                                                    operations
    192  C0  Character    8  PRCAPM_CMB2_T11        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-2
                                                    for 2048-bit CRT-format RSA
                                                    operations
    200  C8  Character    8  PRCAPM_CMB2_C11        64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-2 for
                                                    2048-bit CRT-format RSA
                                                    operations
    Timer-counter pairs for AP engine-3

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

    208  D0  Character    8  PRCAPM_CMB2_T12        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-3
                                                    for 1024-bit ME-format RSA
                                                    operations
    216  D8  Character    8  PRCAPM_CMB2_C12        64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-3 for
                                                    1024-bit ME-format RSA
                                                    operations
    224  E0  Character    8  PRCAPM_CMB2_T13        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-3
                                                    for 2048-bit ME-format RSA
                                                    operations
    232  E8  Character    8  PRCAPM_CMB2_C13        64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-3 for
                                                    2048-bit ME-format RSA
                                                    operations
    240  F0  Character    8  PRCAPM_CMB2_T14        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-3
                                                    for 1024-bit CRT-format RSA
                                                    operations
    248  F8  Character    8  PRCAPM_CMB2_C14        64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-3 for
                                                    1024-bit CRT-format RSA
                                                    operations
    256 100  Character    8  PRCAPM_CMB2_T15        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-3
                                                    for 2048-bit CRT-format RSA
                                                    operations
    264 108  Character    8  PRCAPM_CMB2_C15        64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-3 for
                                                    2048-bit CRT-format RSA
                                                    operations
    Timer-counter pairs for AP engine-4

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

    272 110  Character    8  PRCAPM_CMB2_T16        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-4
                                                    for 1024-bit ME-format RSA
                                                    operations
    280 118  Character    8  PRCAPM_CMB2_C16        64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-4 for
                                                    1024-bit ME-format RSA
                                                    operations
    288 120  Character    8  PRCAPM_CMB2_T17        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-4
                                                    for 2048-bit ME-format RSA
                                                    operations
    296 128  Character    8  PRCAPM_CMB2_C17        64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-4 for
                                                    2048-bit ME-format RSA
                                                    operations
    304 130  Character    8  PRCAPM_CMB2_T18        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-4
                                                    for 1024-bit CRT-format RSA
                                                    operations
    312 138  Character    8  PRCAPM_CMB2_C18        64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-4 for
                                                    1024-bit CRT-format RSA
                                                    operations
    320 140  Character    8  PRCAPM_CMB2_T19        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-4
                                                    for 2048-bit CRT-format RSA
                                                    operations
    328 148  Character    8  PRCAPM_CMB2_C19        64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-4 for
                                                    2048-bit CRT-format RSA
                                                    operations
    CMB entry for types 6 and 8 APs. These are CEX2A and CEX3A, respectively.
    These AP cryptos have just one crypto engine, but the data reported is
    the same as for type 4, engine 0.

    This CMB mapping is also used for PRCAPM_CT = 10 when PRCAPM_MT = 8.

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure  112  PRCAPM_CMB3
      0   0  Character   16  PRCAPM_CMB3HDR
      0   0  Bitstring    1  *                      Reserved/zeroes
      1   1  Bitstring    1  PRCAPM_CT              Crypto type
                                                       Valid values include:
                                                           6, 8, and 10 (when PRCAPM_MT=8)
      2   2  Bitstring    1  *                      Reserved/zeroes
      3   3  Bitstring    1  *
              1... ....      *
              .1.. ....      *
              ..xx xxxx      PRCAPM_AX              AP index
      4   4  Unsigned     4  PRCAPM_S               32-bit binary floating point
                                                    value indicating the stepping
                                                    interval, in seconds, of the
                                                    timers
      8   8  Unsigned     4  PRCAPM_V               32-bit mask indicating the
                                                    validity of each timer-counter
                                                    pair
     12   C  Unsigned     1  *                      Reserved/zeroes
     13   D  Unsigned     1  PRCAPM_MT              Mapping Type
                                                    used for PRCAPM_CT = 10
                                                    only. Zero for all other
                                                    crypto types.
     14   E  Unsigned     2  PRCAPM_L4              CMB Length in bytes
                                                    If zero, use the default lengths:
                                                    CMB type 3,5,7,9    64 bytes
                                                    CMB type 4         336 bytes
                                                    CMB type 6,8        80 bytes
                                                    CMB type 10         96 bytes
    Timer-counter pairs for crypto engine-0

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

     16  10  Character    8  PRCAPM_CMB3_T0         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-0
                                                    for 1024-bit ME-format RSA
                                                    operations
     24  18  Character    8  PRCAPM_CMB3_C0         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-0 for
                                                    1024-bit ME-format RSA
                                                    operations
     32  20  Character    8  PRCAPM_CMB3_T1         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-0
                                                    for 2048-bit ME-format RSA
                                                    operations
     40  28  Character    8  PRCAPM_CMB3_C1         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-0 for
                                                    2048-bit ME-format RSA
                                                    operations
     48  30  Character    8  PRCAPM_CMB3_T2         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-0
                                                    for 1024-bit CRT-format RSA
                                                    operations
     56  38  Character    8  PRCAPM_CMB3_C2         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-0 for
                                                    1024-bit CRT-format RSA
                                                    operations
     64  40  Character    8  PRCAPM_CMB3_T3         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-0
                                                    for 2048-bit CRT-format RSA
                                                    operations
     72  48  Character    8  PRCAPM_CMB3_C3         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-0 for
                                                    2048-bit CRT-format RSA
                                                    operations
     80  50  Character    8  PRCAPM_CMB3_T4         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-0
                                                    for 4096-bit ME-format RSA
                                                    operations
                                                    (not available for type 6
                                                    APs)
     88  58  Character    8  PRCAPM_CMB3_C4         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-0
                                                    for 4096-bit ME-format RSA
                                                    operations.
                                                    (not available for type 6
                                                    APs)
     96  60  Character    8  PRCAPM_CMB3_T5         64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time on AP engine-0
                                                    for 4096-bit CRT-format RSA
                                                    operations
                                                    (not available for type 6
                                                    APs)
    104  68  Character    8  PRCAPM_CMB3_C5         64-bit unsigned integer
                                                    counter of the number of
                                                    operations on AP engine-0
                                                    for 4096-bit CRT-format RSA
                                                    operations.
                                                    (not available for type 6
                                                    APs)
    CMB entry for type 10 APs (PRCAPM_CT = 10) when PRCAPM_MT = 10.

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure   96  PRCAPM_CMB10
      0   0  Character   16  PRCAPM_CMB10HDR
      0   0  Bitstring    1  *                      Reserved/zeroes
      1   1  Bitstring    1  PRCAPM_CT              Crypto type
                                                       Valid values include:
                                                            10 (when PRCAPM_MT=10)
      2   2  Bitstring    1  *                      Reserved/zeroes
      3   3  Bitstring    1  *
              1... ....      *
              .1.. ....      *
              ..xx xxxx      PRCAPM_AX              AP index
      4   4  Unsigned     4  PRCAPM_S               32-bit binary floating point
                                                    value indicating the stepping
                                                    interval, in seconds, of the
                                                    timers
      8   8  Unsigned     4  PRCAPM_V               32-bit mask indicating the
                                                    validity of each timer-counter
                                                    pair
     12   C  Unsigned     1  *                      Reserved/zeroes
     13   D  Unsigned     1  PRCAPM_MT              Mapping Type
                                                    used for PRCAPM_CT = 10
                                                    only. Zero for all other
                                                    crypto types.
     14   E  Unsigned     2  PRCAPM_L4              CMB Length in bytes
                                                    If zero, use the default lengths:
                                                    CMB type 3,5,7,9    64 bytes
                                                    CMB type 4         336 bytes
                                                    CMB type 6,8        80 bytes
                                                    CMB type 10         96 bytes
    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

     16  10  Character    8  PRCAPM_CMB10_T0        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time of slow
                                                    asymmetric-key functions
     24  18  Character    8  PRCAPM_CMB10_C0        64-bit unsigned integer
                                                    counter of the number of
                                                    slow asymmetric-key functions
     32  20  Character    8  PRCAPM_CMB10_T1        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time of fast
                                                    asymmetric-key functions
     40  28  Character    8  PRCAPM_CMB10_C1        64-bit unsigned integer
                                                    counter of the number of
                                                    fast asymmetric-key functions
     48  30  Character    8  PRCAPM_CMB10_T2        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time of
                                                    symmetric-key functions
                                                    that return partial or
                                                    incremental results
     56  38  Character    8  PRCAPM_CMB10_C2        64-bit unsigned integer
                                                    counter of the number of
                                                    operations by symetric-key
                                                    funtions that return partial
                                                    or incremental results
     64  40  Character    8  PRCAPM_CMB10_T3        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time of
                                                    symmetric-key functions
                                                    that return a complete or
                                                    final result.
     72  48  Character    8  PRCAPM_CMB10_C3        64-bit unsigned integer
                                                    counter of the number of
                                                    operations by symetric-key
                                                    funtions that return a
                                                    complete or final result.
     80  48  Character    8  PRCAPM_CMB10_T4        64-bit unsigned integer timer
                                                    value that measures the
                                                    execution time by an
                                                    asymmetric-key generation
                                                    function.
     88  58  Character    8  PRCAPM_CMB10_C4        64-bit unsigned integer
                                                    counter of the number of
                                                    operations by an
                                                    asymmetric-key generation
                                                    function.

#### MRPRCAPM Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    PRCAPM                     0     40+
    PRCAPM_AX                  1      1
    PRCAPM_CMBHDR              0     16
    PRCAPM_CMB1                0     64
    PRCAPM_CMB1_C0            18      8
    PRCAPM_CMB1_C1            28      8
    PRCAPM_CMB1_T0            10      8
    PRCAPM_CMB1_T1            20      8
    PRCAPM_CMB1HDR             0     16
    PRCAPM_CMB2                0    336
    PRCAPM_CMB2_C0            18      8
    PRCAPM_CMB2_C1            28      8
    PRCAPM_CMB2_C10           B8      8
    PRCAPM_CMB2_C11           C8      8
    PRCAPM_CMB2_C12           D8      8
    PRCAPM_CMB2_C13           E8      8
    PRCAPM_CMB2_C14           F8      8
    PRCAPM_CMB2_C15          108      8
    PRCAPM_CMB2_C16          118      8
    PRCAPM_CMB2_C17          128      8
    PRCAPM_CMB2_C18          138      8
    PRCAPM_CMB2_C19          148      8
    PRCAPM_CMB2_C2            38      8
    PRCAPM_CMB2_C3            48      8
    PRCAPM_CMB2_C4            58      8
    PRCAPM_CMB2_C5            68      8
    PRCAPM_CMB2_C6            78      8
    PRCAPM_CMB2_C7            88      8
    PRCAPM_CMB2_C8            98      8
    PRCAPM_CMB2_C9            A8      8
    PRCAPM_CMB2_T0            10      8
    PRCAPM_CMB2_T1            20      8
    PRCAPM_CMB2_T10           B0      8
    PRCAPM_CMB2_T11           C0      8
    PRCAPM_CMB2_T12           D0      8
    PRCAPM_CMB2_T13           E0      8
    PRCAPM_CMB2_T14           F0      8
    PRCAPM_CMB2_T15          100      8
    PRCAPM_CMB2_T16          110      8
    PRCAPM_CMB2_T17          120      8
    PRCAPM_CMB2_T18          130      8
    PRCAPM_CMB2_T19          140      8
    PRCAPM_CMB2_T2            30      8
    PRCAPM_CMB2_T3            40      8
    PRCAPM_CMB2_T4            50      8
    PRCAPM_CMB2_T5            60      8
    PRCAPM_CMB2_T6            70      8
    PRCAPM_CMB2_T7            80      8
    PRCAPM_CMB2_T8            90      8
    PRCAPM_CMB2_T9            A0      8
    PRCAPM_CMB2HDR             0     16
    PRCAPM_CMB3                0    112
    PRCAPM_CMB3_C0            18      8
    PRCAPM_CMB3_C1            28      8
    PRCAPM_CMB3_C2            38      8
    PRCAPM_CMB3_C3            48      8
    PRCAPM_CMB3_C4            58      8
    PRCAPM_CMB3_C5            68      8
    PRCAPM_CMB3_T0            10      8
    PRCAPM_CMB3_T1            20      8
    PRCAPM_CMB3_T2            30      8
    PRCAPM_CMB3_T3            40      8
    PRCAPM_CMB3_T4            50      8
    PRCAPM_CMB3_T5            60      8
    PRCAPM_CMB3HDR             0     16
    PRCAPM_CMB10               0     96
    PRCAPM_CMB10_C0           18      8
    PRCAPM_CMB10_C1           28      8
    PRCAPM_CMB10_C2           38      8
    PRCAPM_CMB10_C3           48      8
    PRCAPM_CMB10_C4           58      8
    PRCAPM_CMB10_T0           10      8
    PRCAPM_CMB10_T1           20      8
    PRCAPM_CMB10_T2           30      8
    PRCAPM_CMB10_T3           40      8
    PRCAPM_CMB10_T4           50      8
    PRCAPM_CMB10HDR            0     16
    PRCAPM_CT                  1      1
    PRCAPM_L2                 18      2
    PRCAPM_L4                  E      2
    PRCAPM_MRHDR               0      0
    PRCAPM_MT                  D      1
    PRCAPM_P                  1A           80
    PRCAPM_RC                 1A      2
    PRCAPM_S                   4      4
    PRCAPM_V                   8      4
    PRCAPM_VAR_DATA           28      0

This information is based on z/VM V6R1.0.
Last updated on 09 November 2012 at 20:42:30.
Copyright IBM Corporation, 1990, 2012