Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### SR5BK

Prolog

Control Block Contents
SR5BK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### SR5BK Prolog

     NAME       : HCPSR5BK
     DESCRIPTION: Symptom Record Section Five
     DSECT      : SR5BK
     FUNCTION   : Map section 5 of the symptom record.
                  This section is optional.  See general
                  notes below for details.
     LOCATED BY : n/a
     CREATED BY : HCPSRB
                  HCPDMP
     DELETED BY : HCPDMP
                  HCPSRB
     Notes      : The first three keys are for section 5 of the symptom
                  record associated with all dumps. For VM dumps this
                  information will follow any guest provided entries
                  in this section.  For CP hard and soft abend symptom
                  records it will be the only data in this section.
                  The entries in this section are in the form of a key,
                  length of variable data and variable data.  The
                  length of the data excludes the length of the key
                  and the field containing the length.

#### SR5BK Control Block Content

#### SR5BK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SR5BK          Symptom Record Section Five
          Keys, X'1000', X'1001' and X'1002', are used to create
          the symptom record by symptom record processing.
          CP symptom record processing always adds the information
          mapped by these three keys.
    0000    0 Bitstring    2 SR5KEY0        Key to specify userid dumped
    0002    2 Bitstring    2 SR5LEN0        Length of data
    0004    4 Character   15 SR5USRT0       Text for VIEWSYM. HCPSRB fills
                                            this with "USERID DUMPED: ".
    0013   19 Character    8 SR5USRD0       Userid dumped followed by blank
                                            used by soft and hard abend
    001B   27 Character    1 SR5BLNK0       Blank
    001C   28 Bitstring    2 SR5KEY1        Key to specify userid dump sent
                                            to
    001E   30 Bitstring    2 SR5LEN1        Length of data
    0020   32 Character   15 SR5USRT1       Text for VIEWSYM. HCPSRB fills
                                            this with "DUMP RECEIVER: ".
    002F   47 Character    8 SR5USRD1       Recipient userid
    0037   55 Character    1 SR5BLNK1       Blank
    0038   56 Bitstring    2 SR5KEY2        Key to specify spool file id of
                                            dump
    003A   58 Bitstring    2 SR5LEN2        Length of data field
    003C   60 Character    9 SR5SPLT        Text for VIEWSYM. HCPSRB fills
                                            this with "SPOOLID: "
    0045   69 Bitstring    4 SR5SPID        Dump Spool ID in printable hex
          Constants for Key '1000'X
              00001000       SR5_KEY0       X'1000'
              00000018       SR5_LEN0       SR5KEY1-SR5USRT0
          Constants for Key '1001'X
              00001001       SR5_KEY1       X'1001'
              00000018       SR5_LEN1       SR5KEY2-SR5USRT1
          Constants for Key '1002'X
              00001002       SR5_KEY2       X'1002'
              0000000D       SR5_LEN2       *-SR5SPLT
          Length of section 5 as provided by symptom record services.
              00000049       SR5BYTL        (*-SR5BK) In bytes..
              0000000A       SR5SIZE        (*-SR5BK+7)/8
    0049   73 Character   50 *              Reserved for IBM use
          DUMPSCAN will update key '1003'X which contains the main
          CMS dump filename and filetype (DUMP0001).
          DUMPSCAN will also update key '1004'X which contains the
          dump format of an address space dumped in a CMS file.
    0000    0 Bitstring    2 SR5KEY3        Key to specify main CMS dump
                                            file(DUMP0001)
    0002    2 Bitstring    2 SR5LEN3        Length of data
    0004    4 Character   19 SR5MNAME       'Name of main dump: '
    0017   23 Character    8 SR5FNAME       Main dump name
    001F   31 Character    1 SR5SP1         Blank
    0020   32 Character    8 SR5FTYPE       Filetype
    0028   40 Character    2 SR5SP2         2 Blanks
    002A   42 Bitstring    2 SR5KEY4        Key to specify dump format
    002C   44 Bitstring    2 SR5LEN4        Length of data
    002E   46 Character   13 SR5DFORM       'Dump format: '
    003B   59 Character    8 SR5FORMN       Format name
          Constants for Key '1003'X
              00001003       SR5_KEY3       X'1003'
              00000026       SR5_LEN3       SR5KEY4-SR5MNAME
          Constants for Key '1004'X
              00001004       SR5_KEY4       X'1004'
              00000015       SR5_LEN4       *-SR5DFORM
          Calculate the length of key '1003' and key '1004'
              00000043       SR5MAINL       *-SR5KEY3
          PRTDUMP and DUMPSCAN will update this key while processing
          a CMS dump file of a VM dump.
    0000    0 Bitstring    2 SR5KEY5        Key to specify dump info
    0002    2 Bitstring    2 SR5LEN5        Length of data
    0004    4 Character   11 SR5TITLE       "DUMP INFO: "
    000F   15 Character   80 SR5TEXT        Text data
          Constants for Key '1005'X
              00001005       SR5_KEY5       X'1005'
              0000005B       SR5_LEN5       *-SR5TITLE
          Calculate the length of key '1005'
              0000005F       SR5INFOL       *-SR5KEY5
          PRTDUMP and DUMPSCAN will update this key while processing
          a CMS dump file of a VM dump.
    0000    0 Bitstring    2 SR5KEY6        Key to specify dump info
    0002    2 Bitstring    2 SR5LEN6        Length of data
    0004    4 Character   33 SR5NUMBH       DVF's HCSSRU fills this with
                                            "NUMBER OF ADDRESS SPACES DUMPED:
                                            "
    0025   37 Character    4 SR5NUMBD       Number of dump files
          Constants for Key '1006'X
              00001006       SR5_KEY6       X'1006'
              00000025       SR5_LEN6       *-SR5NUMBH
          Calculate the length of key '1006'
              00000029       SR5NUMBL       *-SR5KEY6

#### SR5BK Storage Layout

    *** SR5BK - Symptom Record Section Five
    *
    *     +-------------+-------------+---------------------------+
    *   0 |  SR5KEY0    |  SR5LEN0    |                           |
    *     +-------------+-------------+                           |
    *     |                       SR5USRT0                        |
    *     |                    +----------------------------------+
    *     |                    |            SR5USRD0-             |
    *     +--------------------+------+-------------+-------------+
    *  18 |      -(013)        |:BLNK0|  SR5KEY1    |  SR5LEN1    |
    *     +--------------------+------+-------------+-------------+
    *  20 |                       SR5USRT1                        |
    *     |                                                +------+
    *     |                                                |(02F)-|
    *     +------------------------------------------------+------+
    *  30 |                   -SR5USRD1                    |:BLNK1|
    *     +-------------+-------------+--------------------+------+
    *  38 |  SR5KEY2    |  SR5LEN2    |         SR5SPLT           |
    *     +-------------+-------------+      +--------------------+
    *     |                                  |     SR5SPID-       |
    *     +------+---------------------------+--------------------+
    *  48 |-(045)|////////////////////////////////////////////////|
    *     +------+////////////////////////////////////////////////|
    *  50 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |////////////////////+----------------------------------+
    *     |////////////////////| 7B
    *     +--------------------+
    *
    *** SR5BK - Symptom Record Section Five

    *** Overlay for SR5KEY0 in SR5BK
    *
    *     +-------------+-------------+---------------------------+
    *   0 |  SR5KEY3    |  SR5LEN3    |                           |
    *     +-------------+-------------+                           |
    *     |                       SR5MNAME                        |
    *     |                                                +------+
    *     |                                                |(017)-|
    *     +------------------------------------------------+------+
    *  18 |                   -SR5FNAME                    |SR5SP1|
    *     +------------------------------------------------+------+
    *  20 |                       SR5FTYPE                        |
    *     +-------------+-------------+-------------+-------------+
    *  28 |   SR5SP2    |  SR5KEY4    |  SR5LEN4    |             |
    *     +-------------+-------------+-------------+             |
    *     |                       SR5DFORM                        |
    *     |                    +----------------------------------+
    *     |                    |            SR5FORMN-             |
    *     +--------------------+----------------------------------+
    *  40 |      -(03B)        | 43
    *     +--------------------+
    *
    *** Overlay for SR5KEY0 in SR5BK

    *** Overlay for SR5KEY0 in SR5BK
    *
    *     +-------------+-------------+---------------------------+
    *   0 |  SR5KEY5    |  SR5LEN5    |         SR5TITLE          |
    *     +-------------+-------------+                    +------+
    *     |                                                |      |
    *     +------------------------------------------------+      |
    *  10 |                                                       |
    *     =                       SR5TEXT                         =
    *     |                                                +------+
    *     |                                                | 5F
    *     +------------------------------------------------+
    *
    *** Overlay for SR5KEY0 in SR5BK

    *** Overlay for SR5KEY0 in SR5BK
    *
    *     +-------------+-------------+---------------------------+
    *   0 |  SR5KEY6    |  SR5LEN6    |                           |
    *     +-------------+-------------+                           |
    *   8 |                                                       |
    *     =                       SR5NUMBH                        =
    *     |                                  +--------------------+
    *     |                                  |     SR5NUMBD-      |
    *     +------+---------------------------+--------------------+
    *  28 |-(025)| 29
    *     +------+
    *
    *** Overlay for SR5KEY0 in SR5BK

#### SR5BK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    SR5_KEY0       0045 00001000
    SR5_KEY1       0045 00001001
    SR5_KEY2       0045 00001002
    SR5_KEY3       003B 00001003
    SR5_KEY4       003B 00001004
    SR5_KEY5       000F 00001005
    SR5_KEY6       0025 00001006
    SR5_LEN0       0045 00000018
    SR5_LEN1       0045 00000018
    SR5_LEN2       0045 0000000D
    SR5_LEN3       003B 00000026
    SR5_LEN4       003B 00000015
    SR5_LEN5       000F 0000005B
    SR5_LEN6       0025 00000025
    SR5BLNK0       001B
    SR5BLNK1       0037
    SR5BYTL        0045 00000049
    SR5DFORM       002E
    SR5FNAME       0017
    SR5FORMN       003B
    SR5FTYPE       0020
    SR5INFOL       000F 0000005F
    SR5KEY0        0000
    SR5KEY1        001C
    SR5KEY2        0038
    SR5KEY3        0000
    SR5KEY4        002A
    SR5KEY5        0000
    SR5KEY6        0000
    SR5LEN0        0002
    SR5LEN1        001E
    SR5LEN2        003A
    SR5LEN3        0002
    SR5LEN4        002C
    SR5LEN5        0002
    SR5LEN6        0002
    SR5MAINL       003B 00000043
    SR5MNAME       0004
    SR5NUMBD       0025
    SR5NUMBH       0004
    SR5NUMBL       0025 00000029
    SR5SIZE        0045 0000000A
    SR5SPID        0045
    SR5SPLT        003C
    SR5SP1         001F
    SR5SP2         0028
    SR5TEXT        000F
    SR5TITLE       0004
    SR5USRD0       0013
    SR5USRD1       002F
    SR5USRT0       0004
    SR5USRT1       0020

This information is based on z/VM V6R1.0. Last updated on 18 Feb 2010 at 09:07:55 EDT.
Copyright IBM Corporation, 1990, 2008