Programming Interface Information: This page documents intended Programming Interfaces that allow the customer to write programs to obtain the services of z/VM.

#### CPED

Prolog

Control Block Contents
CPED DSECT
CPEFMH5 DSECT
CPEFASI DSECT
CPEFLUW1 DSECT
CPEFLUW2 DSECT
CPEFCOR DSECT
CPEFASIS DSECT
CPESGIDV DSECT
CPEPIP DSECT
CPEPIPMP DSECT
CPECSRV DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### CPED Prolog

     NAME       : CPED
     DESCRIPTION: CONNECTION PENDING EXTENDED DATA (CPED)
     DSECT      : CPED (primary)
     FUNCTION   : PROVIDES A MAPPING OF THE CPED CONTAINING THE
                  ALLOCATE DATA (VM AREA AND FMH5) WITHIN THE
                  INTERRUPT BUFFER EXTENSION.
                  THE MAPPING OF THE VM COMMUNICATION SERVER AREA
                  AND PROGRAM INTIALIZATION PARAMETER(PIP) ARE
                  ALSO PROVIDED.
     HISTORY    : NEW FOR VM/ESA RELEASE 1
     NOTES      :
            1.  ANY CHANGES TO CPED COPY SHOULD ALSO BE MADE IN THE
                INTERNAL CMS VERSION, DMSCPEDP, TO KEEP THE MAPPING IN
                SYNCH BETWEEN CP AND CMS.  THE CMS BILINGUAL MACRO,
                DMSCPED, USES THE ASSEMBLER COPY FUNCTION TO INCLUDE
                CPED COPY WHEN INVOKED FROM AN ASSEMBLER MODULE.
                ALSO NOTE THAT THE INTERNAL CP VERSION (HCPCONBK COPY)
                AS WELL AS THE INTERNAL AVS AND TSAF VERSIONS FOR THE
                ALLOCATE DATA MAPPING MUST BE KEPT IN SYNCH.
            2.  THE VALUE IN 'CPEFLEN' INCLUDES THE LENGTH OF
                'CPEFLEN' ITSELF. IT IS CALCULATED AS LENGTH(CPEFBASE)
                + CPEFTPNL + CPEFASIL + LENGTH(CPEFASIL) + CPEFLUWL +
                LENGTH(CPEFLUWL) + CPEFCORL + LENGTH(CPEFCORL).
            3.  THE VALUES IN 'CPEFTPNL', 'CPEFASIL', 'CPEFLUWL',
                'CPEFCORL', CPEFSUBL', AND 'CPEFFQNL' DO NOT INCLUDE
                THE LENGTHS OF THE LENGTH FIELDS THEMSELVES.
            4.  'CPEFPRML' SPECIFIES THE LENGTH OF THE FIXED PARAMETERS
                THAT APPEAR IN THE FMH5 BETWEEN 'CPEFPRML' ITSELF AND
                THE FIRST VARYING-LENGTH FIELD. THE VALUE IN 'CPEFPRML'
                ADDED TO THE DISPLACEMENT OF THE FIRST FIXED-LENGTH
                FIELD FOLLOWING 'CPEFPRML' WITHIN THE FMH5 GIVES THE
                DISPLACEMENT OF THE FIRST VARYING-LENGTH FIELD IN THE
                FMH5.
            5.  PROGRAM INITIALIZATION PARAMETER (PIP) DATA IS SENT AS
                A GDS VARIABLE IF THE FIELD 'CPEFPIP' INDICATES THAT
                PIP DATA IS PRESENT.
            6.  THE LL FIELDS FOR THE PIP DATA, 'CPEPIPLN' AND
                'CPEPIPSL', INCLUDE THE LENGTH OF THE LENGTH FIELDS
                THEMSELVES.
            7.  WARNING: IF IPRESID IN THE PARAMETER LIST IS *USERID
                AND THE CPED IS BEING PRESENTED TO A TSAF VIRTUAL
                MACHINE THEN THE CPED WILL BE PRECEDED BY AN 8 BYTE
                NODE ID.

#### CPED Control Block Content

#### CPED DSECT

####

####

####

####

####

####

####

####

####

####

####

####

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CPED           CONNECTION PENDING EXTENDED DATA (CPED)
          VM AREA mapping
    0000    0 Signed       2 CPEVTOTL       TOTAL LENGTH OF VM AREA
    0002    2 Signed       2 CPEVFIXL       LENGTH OF THE FIXED LENGTH FIELD
                                            (FROM CPEVSESL TO THE CURRENT END
                                            OF THE VM AREA)
    0004    4 Signed       2 *              RESERVED
    0006    6 Signed       2 CPEVSRVL       LENGTH OF COMMUNICATION SERVER
                                            AREA (USED FOR OUTBOUND REQUESTS
                                            ONLY - OTHERWISE ZERO)
    0008    8 Bitstring    1 CPEVSESL       LENGTH SESSION INSTANCE ID
    0009    9 Bitstring    1 CPEVLLUL       LENGTH LOCAL LU NAME
    000A   10 Bitstring    1 CPEVRLUL       LENGTH REMOTE LU NAME
    000B   11 Character    5 *              RESERVED
    0010   16 Character    8 CPEVMODE       MODE NAME SPECIFIED
    0018   24 Character    8 CPEVSESS       SESSION INSTANCE IDENTIFIER
    0020   32 Character   16 CPEVLKL (0)    LOCALLY KNOWN LUNAME
    0020   32 Character    8 CPEVLUQ        LUNAME QUALIFIER
    0028   40 Character    8 CPEVTLU        TARGET LUNAME
    0030   48 Character   16 CPEVPLKL (0)   PARTNER LOCAL KNOWN LUNAME
    0030   48 Character    8 CPEVPLUQ       PARTNER LUNAME QUALIFIER
    0038   56 Character    8 CPEVPTLU       PARTNER TARGET LUNAME
    0040   64 Character   17 CPEVLLUN       LOCAL FULLY QUALIFIED LUNAME
    0051   81 Character   17 CPEVRLUN       REMOTE FULLY QUAL. LUNAME
    0062   98 Character    6 *              RESERVED
    0068  104 Character    8 CPEVALT        ALTERNATE USERID TO BE SET
    0070  112 Character    8 CPEVCIT        VIRTUAL CONFIGURATION ID TOKEN
          The next set of information, along with the variable-length
          supplementary group ID (SGID) information, is passed on
          each connect so that the server at the other end can have
          access to POSIX access control information.
    0078  120 Bitstring    1 CPEVIDFL       Access control flags
              1... ....      CPEVIDVL       X'80' CPEVIDVL The UID/GID
                                            information has been filled in.
    0079  121 Bitstring    3 *              Reserved for IBM use
    007C  124 Signed       4 CPEVEUID       Effective UID of the process
                                            issuing the CONNECT.
    0080  128 Signed       4 CPEVEGID       Effective GID of the process
                                            issuing the CONNECT.
    0084  132 Signed       4 CPEVRUID       Real UID of the process issuing
                                            the CONNECT.
    0088  136 Signed       4 CPEVRGID       Real GID of the process issuing
                                            the CONNECT.
    008C  140 Signed       4 CPEVIDLN       Length of the supplementary GID
                                            information (may be in the range
                                            zero to NGMAXMAX*4).
    0090  144 Signed       4 CPEVVARL       Total length of the VM-defined
                                            variable length section of this
                                            block. This section begins after
                                            the FMH5 and is followed by the
                                            communication server area.
              00000094       CPEVVRSL       *-CPED VMA area length including
                                            the variable-length section
                                            length field. This field must be
                                            distinct from CPEVMLEN to allow
                                            future expansion.
    0094  148 Character   16 CPEVCBPL (0)   Partner LUNAME to use in
                                            connecting back to the partner.
    0094  148 Character    8 CPEVCBLQ       LUNAME qualifier to use in
                                            connecting back to the partner.
                                            Contains one of the following:
                                            *USERID if the connection
                                            originated on the same system as
                                            the target. (The value is equal
                                            to that in CPEVPLUQ.)
                                            <gatelu> if the connection
                                            is through AVS or an unknown
                                            comserv. (The value is equal to
                                            that in CPEVPLUQ.) <system
                                            gateway name of originating
                                            system> if the connection is
                                            through ISFC or TSAF. <system
                                            gateway name of the gateway
                                            system> if the connection is
                                            passing from a CS collection to a
                                            TSAF collection or vice versa.
    009C  156 Character    8 CPEVCBTL       Target luname to use in
                                            connecting back to the partner.
                                            This should always be equal to
                                            CPEVPTLU; it's added here for
                                            ease of use.
              000000A4       CPEVMLEN       *-CPED VM AREA LENGTH
          Function Management Header 5
           FMH5 Fixed area

    CPEFMH5 DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CPEFMH5        CONNECTION PENDING EXTENDED DATA (CPED)
    0000    0 Character   10 CPEFBASE (0)   FIXED LENGTH BASE
    0000    0 Bitstring    1 CPEFLEN        FMH5 TOTAL LENGTH
              1111 1111      CPEFMXLN       255 CPEFMXLN Maximum length of
                                            the FMH5
    0001    1 Bitstring    1 CPEFTYPE       FMH TYPE FIELD
              .... .1.1      CPEFTYP5       X'05' CPEFTYP5 FMH TYPE = X'05'
    0002    2 Bitstring    2 CPEFCODE       FMH5 COMMAND CODE
              CPEFCODE       CPEFATT        X'02FF' CPEFATT ATTACH COMMAND
                                            CODE
    0004    4 Bitstring    1 CPEFFLG1       FLAG FIELD
              1... ....      CPEFSECI       X'80' CPEFSECI SECURITY INDICATOR
              .... 1...      CPEFPIP        X'08' CPEFPIP PIP DATA PRESENT
    0005    5 Bitstring    1 CPEFPRML       LENGTH OF FIXED LENGTH PARMS
    0006    6 Bitstring    3 CPEFPARM (0)   FIXED LENGTH PARAMETERS
    0006    6 Bitstring    1 CPEFCONT       CONVERSATION TYPE
              11.1 ....      CPEFBASC       X'D0' CPEFBASC BASIC CONVERSATION
              11.1 ...1      CPEFMAPC       X'D1' CPEFMAPC MAPPED
                                            CONVERSATION
    0007    7 Character    1 *              RESERVED
    0008    8 Bitstring    1 CPEFFLG2       FLAG FIELD
              11.. ....      CPEFSYNM       X'C0' CPEFSYNM SYNCHRONIZATION
                                            LEVEL MASK
              .... ....      CPEFSYNO       X'00' CPEFSYNO NONE
              .1.. ....      CPEFSYCF       X'40' CPEFSYCF CONFIRM
              1... ....      CPEFSYSP       X'80' CPEFSYSP CONFIRM,SYNC
                                            POINT,BACKOUT
              ..1. ....      CPEFSYRC       X'20' CPEFSYRC RECONNECTION
                                            SUPPORT
    0009    9 Bitstring    1 CPEFTPNL       TRANSACTION PROGRAM NAME LENGTH
                                            (NOT INC. THIS BYTE)
           FMH5 Variable area
    000A   10 Bitstring    1 CPEFTPN (0)    TRANS. PROGRAM NAME (TPN)

    CPEFASI DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CPEFASI        CONNECTION PENDING EXTENDED DATA (CPED)
                                           SUBFIELDS
    0000    0 Bitstring    1 CPEFASIL       TOTAL LENGTH OF ALL ASI
                                            SUBFIELDS-NOT INC. THIS FLD
    0001    1 Bitstring    1 CPEFSEC (0)    CONTAINS ALL ASI SUBFIELDS MAPPED
                                            VIA THE CPEFASIS DSECT. EACH ASI
                                            SUBFIELDS MUST BE MAPPED
                                            SEPARATELY BY THE CPEFASIS DSECT.

    CPEFLUW1 DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CPEFLUW1       CONNECTION PENDING EXTENDED DATA (CPED)
                                           FIELD
    0000    0 Bitstring    1 CPEFLUWL       LENGTH OF LUW FIELD (NOT
                                            INCLUDING THIS BYTE)
    0001    1 Bitstring    1 CPEFFQNL       LENGTH OF FULLY QUALIFIED LUNAME
                                            (NOT INC. THIS BYTE)
    0002    2 Bitstring    1 CPEFFQN (0)    NETWORK FULLY QUALIFIED LUNAME

    CPEFLUW2 DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CPEFLUW2       CONNECTION PENDING EXTENDED DATA (CPED)
    0000    0 Bitstring    6 CPEFLUIN       LUW INSTANCE NUMBER
    0006    6 Bitstring    2 CPEFLUSN       LUW SEQUENCE NUMBER

    CPEFCOR DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CPEFCOR        CONNECTION PENDING EXTENDED DATA (CPED)
    0000    0 Bitstring    1 CPEFCORL       LENGTH OF CONVERSATION CORRELATOR
                                            OF SENDER (NOT INCLUDING THIS
                                            BYTE)
    0001    1 Bitstring    1 CPEFCORT (0)   CONVERSATION CORRELATOR OF
                                            SENDING TRANSACTION
          Access Security Information(ASI) subfield
          This DSECT is used to map each ASI SUBFIELD. THESE subfields are
          all contained in the field 'CPEFSEC'. You must determine how many
          subfields are specified and determine the length of each subfield.

    CPEFASIS DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CPEFASIS       CONNECTION PENDING EXTENDED DATA (CPED)
    0000    0 Bitstring    1 CPEFSUBL       SUBFIELD LENGTH (NOT INCLUDING
                                            THIS BYTE)
    0001    1 Bitstring    1 CPEFSUBT       SUBFIELD TYPE
              .... ....      CPEFPROF       X'00' CPEFPROF PROFILE TYPE
              .... ...1      CPEFPASS       X'01' CPEFPASS PASSWORD TYPE
              .... ..1.      CPEFUSER       X'02' CPEFUSER USER ID TYPE
    0002    2 Bitstring    1 CPEFDATA (0)   SUBFIELD DATA
          Beginning of the VM-defined variable-length section.
          This section directly follows the FMH5 and precedes the
          communication server area. It consists of zero or more
          variable-length areas. The sum of the lengths of
          all of the information in this section is defined in
          CPEVVARL.
          Supplementary GID information area
          This section comes immediately after the FMH5 and contains
          the supplementary group IDs (part of the set of POSIX
          access control values). The length of this section is
          in CPEVIDLN in the VMA area; if the length is zero, there
          are no supplementary group IDs. The valid range for the
          length is zero to NGMAXMAX*4; APPC/VM connect
          processing checks to ensure that this area does not grow
          too big for APPC/VM connect processing to handle.
          Each SGID is four bytes long. The first starts at
          displacement zero in this area, the second at displacement
          four, and so on.
          Notes      : in the CONBK, CONSGIDS is defined with a length
          of NGMAXMAX*4. Since the levels of CP and CMS could
          be different and thus the NGROUPS_MAX value as represented
          by NGMAXMAX could be different, the reference to
          NGROUPS_MAX (NGMAXMAX) is omitted here to avoid the risk
          of misunderstanding and misuse.

    CPESGIDV DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CPESGIDV       CONNECTION PENDING EXTENDED DATA (CPED)
    0000    0 Bitstring    1 CPESGIDS (0)   Supplementary GIDs
          End of the VM-defined variable-length section.
            PROGRAM INITIALIZATION PARAMETER (PIP).
                       +-----------------------+-----------------------+
                       | CPEPIPLN              | CPEPIPID              |
                       +-----------------------+-----------------------+
                       | CPEPIPSU                                      |
                       +                                               +
                       |                                         +-----+
                       |                                         | /// |
                       +-----------------------------------------+-----+

    CPEPIP DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CPEPIP         CONNECTION PENDING EXTENDED DATA (CPED)
    0000    0 Bitstring    2 CPEPIPLN       PIP LENGTH (INC. THIS FIELD)
    0002    2 Bitstring    2 CPEPIPID       GDS INDICATOR
              CPEPIPID       CPEPIPVA       X'12F5' CPEPIPVA PIP VARIABLE
    0004    4 Bitstring    1 CPEPIPSU (0)   ZERO OR MORE PIP SUBFIELDS, EACH
                                            OF WHICH HAS THE FOLLOWING FORMAT

    CPEPIPMP DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CPEPIPMP       CONNECTION PENDING EXTENDED DATA (CPED)
    0000    0 Bitstring    2 CPEPIPSL       SUBFIELD LENGTH (INCLUDING THIS
                                            BYTE)
    0002    2 Bitstring    2 CPEPIPSI       GDS INDICATOR
              CPEPIPSI       CPEPIPSF       X'12E2' CPEPIPSF PIP SUBFIELD
    0004    4 Bitstring    1 CPEPIPSD (0)   SUBFIELD DATA
            VM Communication Server Area
                       +-----------+-----------------------+-----------+
                       | CPECOMFL  | CPECOMPL              | RESERVED  |
                       +-----------+-----------------------+-----------+
                       | CPECOMPA                                      |
                       +-----------------------------------------------+

    CPECSRV DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CPECSRV        CONNECTION PENDING EXTENDED DATA (CPED)
    0000    0 Bitstring    8 CPECOMSV (0)
    0000    0 Bitstring    1 CPECOMFL       FLAG BYTE
              .1.. ....      CPECOMBL       X'40' CPECOMBL PIP ADDRESS IS
                                            BUFFER LIST
    0001    1 Bitstring    2 CPECOMPL       LENGTH OF PIP DATA
    0003    3 Bitstring    1 *              RESERVED
    0004    4 Bitstring    4 CPECOMPA       ADDRESS OF PIP DATA
              00000001       CPECOMSZ       (*-CPECOMSV+7)/8 CPECOMSV SIZE IN
                                            DOUBLEWORD

    CPED Storage Layout

    *** CPED - CONNECTION PENDING EXTENDED DATA (CPED)
    *
    *     +-------------+-------------+-------------+-------------+
    *   0 |  CPEVTOTL   |  CPEVFIXL   |/////////////|  CPEVSRVL   |
    *     +------+------+------+------+-------------+-------------+
    *   8 |:VSESL|:VLLUL|:VRLUL|//////////////////////////////////|
    *     +------+------+------+----------------------------------+
    *  10 |                       CPEVMODE                        |
    *     +-------------------------------------------------------+
    *  18 |                       CPEVSESS                        |
    *     +-------------------------------------------------------+
    *  20 |                       CPEVLUQ                         |
    *     +-------------------------------------------------------+
    *  28 |                       CPEVTLU                         |
    *     +-------------------------------------------------------+
    *  30 |                       CPEVPLUQ                        |
    *     +-------------------------------------------------------+
    *  38 |                       CPEVPTLU                        |
    *     +-------------------------------------------------------+
    *  40 |                                                       |
    *     =                       CPEVLLUN                        =
    *     |      +------------------------------------------------+
    *  50 |      |                                                |
    *     +------+                                                |
    *     |                       CPEVRLUN                        |
    *     |             +-----------------------------------------+
    *  60 |             |/////////////////////////////////////////|
    *     +-------------+-----------------------------------------+
    *  68 |                       CPEVALT                         |
    *     +-------------------------------------------------------+
    *  70 |                       CPEVCIT                         |
    *     +------+--------------------+---------------------------+
    *  78 |:VIDFL|////////////////////|         CPEVEUID          |
    *     +------+--------------------+---------------------------+
    *  80 |         CPEVEGID          |         CPEVRUID          |
    *     +---------------------------+---------------------------+
    *  88 |         CPEVRGID          |         CPEVIDLN          |
    *     +---------------------------+---------------------------+
    *  90 |         CPEVVARL          |        CPEVCBLQ-          |
    *     +---------------------------+---------------------------+
    *  98 |          -(094)           |        CPEVCBTL-          |
    *     +---------------------------+---------------------------+
    *  A0 |          -(09C)           | A4
    *     +---------------------------+
    *
    *** CPED - CONNECTION PENDING EXTENDED DATA (CPED)

    *** CPEFMH5 - CONNECTION PENDING EXTENDED DATA (CPED)
    *
    *     +------+------+-------------+------+------+------+------+
    *   0 |:FLEN |:FTYPE|  CPEFCODE   |:FFLG1|:FPRML|:FCONT|//////|
    *     +------+------+-------------+------+------+------+------+
    *   8 |:FFLG2|:FTPNL|
    *     +------+------+
    *
    *** CPEFMH5 - CONNECTION PENDING EXTENDED DATA (CPED)

    *** CPEFASI - CONNECTION PENDING EXTENDED DATA (CPED)
    *
    *     +------+
    *   0 |:FASIL|
    *     +------+
    *
    *** CPEFASI - CONNECTION PENDING EXTENDED DATA (CPED)

    *** CPEFLUW1 - CONNECTION PENDING EXTENDED DATA (CPED)
    *
    *     +------+------+
    *   0 |:FLUWL|:FFQNL|
    *     +------+------+
    *
    *** CPEFLUW1 - CONNECTION PENDING EXTENDED DATA (CPED)

    *** CPEFLUW2 - CONNECTION PENDING EXTENDED DATA (CPED)
    *
    *     +-----------------------------------------+-------------+
    *   0 |                CPEFLUIN                 |  CPEFLUSN   |
    *     +-----------------------------------------+-------------+
    *   8
    *
    *** CPEFLUW2 - CONNECTION PENDING EXTENDED DATA (CPED)

    *** CPEFCOR - CONNECTION PENDING EXTENDED DATA (CPED)
    *
    *     +------+
    *   0 |:FCORL|
    *     +------+
    *
    *** CPEFCOR - CONNECTION PENDING EXTENDED DATA (CPED)

    *** CPEFASIS - CONNECTION PENDING EXTENDED DATA (CPED)
    *
    *     +------+------+
    *   0 |:FSUBL|:FSUBT|
    *     +------+------+
    *
    *** CPEFASIS - CONNECTION PENDING EXTENDED DATA (CPED)

    *** CPESGIDV - CONNECTION PENDING EXTENDED DATA (CPED)
    *
    *
    *** CPESGIDV - CONNECTION PENDING EXTENDED DATA (CPED)

    *** CPEPIP - CONNECTION PENDING EXTENDED DATA (CPED)
    *
    *     +-------------+-------------+
    *   0 |  CPEPIPLN   |  CPEPIPID   |
    *     +-------------+-------------+
    *
    *** CPEPIP - CONNECTION PENDING EXTENDED DATA (CPED)

    *** CPEPIPMP - CONNECTION PENDING EXTENDED DATA (CPED)
    *
    *     +-------------+-------------+
    *   0 |  CPEPIPSL   |  CPEPIPSI   |
    *     +-------------+-------------+
    *
    *** CPEPIPMP - CONNECTION PENDING EXTENDED DATA (CPED)

    *** CPECSRV - CONNECTION PENDING EXTENDED DATA (CPED)
    *
    *     +------+-------------+------+---------------------------+
    *   0 |:COMFL|  CPECOMPL   |//////|         CPECOMPA          |
    *     +------+-------------+------+---------------------------+
    *   8
    *
    *** CPECSRV - CONNECTION PENDING EXTENDED DATA (CPED)

    CPED Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    CPECOMBL       0000 40
    CPECOMFL       0000
    CPECOMPA       0004
    CPECOMPL       0001
    CPECOMSV       0000
    CPECOMSZ       0004 00000001
    CPEFASIL       0000
    CPEFATT        0002 CPEFCODE
    CPEFBASC       0006 D0
    CPEFBASE       0000
    CPEFCODE       0002
    CPEFCONT       0006
    CPEFCORL       0000
    CPEFCORT       0001
    CPEFDATA       0002
    CPEFFLG1       0004
    CPEFFLG2       0008
    CPEFFQN        0002
    CPEFFQNL       0001
    CPEFLEN        0000
    CPEFLUIN       0000
    CPEFLUSN       0006
    CPEFLUWL       0000
    CPEFMAPC       0006 D1
    CPEFMXLN       0000 FF
    CPEFPARM       0006
    CPEFPASS       0001 01
    CPEFPIP        0004 08
    CPEFPRML       0005
    CPEFPROF       0001 00
    CPEFSEC        0001
    CPEFSECI       0004 80
    CPEFSUBL       0000
    CPEFSUBT       0001
    CPEFSYCF       0008 40
    CPEFSYNM       0008 C0
    CPEFSYNO       0008 00
    CPEFSYRC       0008 20
    CPEFSYSP       0008 80
    CPEFTPN        000A
    CPEFTPNL       0009
    CPEFTYPE       0001
    CPEFTYP5       0001 05
    CPEFUSER       0001 02
    CPEPIPID       0002
    CPEPIPLN       0000
    CPEPIPSD       0004
    CPEPIPSF       0002 CPEPIPSI
    CPEPIPSI       0002
    CPEPIPSL       0000
    CPEPIPSU       0004
    CPEPIPVA       0002 CPEPIPID
    CPESGIDS       0000
    CPEVALT        0068
    CPEVCBLQ       0094
    CPEVCBPL       0094
    CPEVCBTL       009C
    CPEVCIT        0070
    CPEVEGID       0080
    CPEVEUID       007C
    CPEVFIXL       0002
    CPEVIDFL       0078
    CPEVIDLN       008C
    CPEVIDVL       0078 80
    CPEVLKL        0020
    CPEVLLUL       0009
    CPEVLLUN       0040
    CPEVLUQ        0020
    CPEVMLEN       009C 000000A4
    CPEVMODE       0010
    CPEVPLKL       0030
    CPEVPLUQ       0030
    CPEVPTLU       0038
    CPEVRGID       0088
    CPEVRLUL       000A
    CPEVRLUN       0051
    CPEVRUID       0084
    CPEVSESL       0008
    CPEVSESS       0018
    CPEVSRVL       0006
    CPEVTLU        0028
    CPEVTOTL       0000
    CPEVVARL       0090
    CPEVVRSL       0090 00000094

    This information is
    based on z/VM V6R1.0.
    Last updated on 18 Feb 2010 at 08:20:43 EDT.

    Copyright IBM Corporation, 1990, 2008