Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### RSAAVNKR

Prolog

Control Block Contents
RSAAVNKR DSECT
RSMANCHR DSECT
RSMBK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### RSAAVNKR Control Block Content

#### RSAAVNKR DSECT

####

####

####

####

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      RSAAVNKR       RSM common area mapping
    0000    0 Address      8 RSAAVFP        Forward pointer
    0008    8 Address      4 * (0)          Force a cross reference
    0008    8 Address      4 * (0)          Force a cross reference
    0008    8 Address      4 * (0)          Force a cross reference
    0008    8 Address      4 * (0)          Force a cross reference
    0008    8 Address      8 RSAAVBP        Backward pointer
    0010   16 Address      4 * (0)          Force a cross reference
    0010   16 Address      4 * (0)          Force a cross reference
    0010   16 Address      4 * (0)          Force a cross reference
    0010   16 Address      4 * (0)          Force a cross reference
    0010   16 Signed       4 RSAAVCT4 (0)   Count (4-byte)
    0010   16 Signed       8 RSAAVCT        Count
    0018   24 Address      4 * (0)          Force a cross reference
    0018   24 Address      4 * (0)          Force a cross reference
    0018   24 Address      4 * (0)          Force a cross reference
    0018   24 Address      4 * (0)          Force a cross reference
         | This section maps the three free frames anchors.         |
         | Use EXTRNs HCPRSMFR/HCPRSMSV/HCPRSMPR to locate them.    |

    RSMANCHR DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      RSMANCHR       RSM common area mapping
    0000    0 Dbl-Word     8 * (0)          HCPRSMFR and HCPRSMSV are list
                                            anchors that contain the address
                                            of the first SXSTE which
                                            represents a free storage page
                                            with available space of the
                                            appropriate type to be examine
                                            when allocating or deallocating
                                            VMDBK (Guestperm), or System
                                            (Sysperm) free storage
                                            respectively. The count of SXSTEs
                                            on the list follows the anchor.
    0000    0 Address      8 RSMFRCHN       Host Logical Address Anchor for
                                            SXSTE chain of free storage
                                            frames with avbl space
    0008    8 Signed       8 RSMFRCNT       Count of FRMTEs on chain

    RSMBK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      RSMBK          RSM common area mapping
         |        Real Storage Management Common Data Area.         |
         |        Located by HCPRSMCM.                              |
    0000    0 Signed       4 RSASAVFR       Non-negative count of frames in
                                            use by the save area manager.
                                            Serialized by save page queue
                                            lock (RCCSFQL)
          System-real space information
    0004    4 Address      4 RSARSAST       Host Logical Address ASTE @ for
                                            the system-real space, which
                                            identity maps all of real storage
                                            (including real storage above 2G)
                                            via an RSD (meaning no DAT tables
                                            are required)
    0008    8 Signed       4 RSAMSARC       Count of machine storage areas
                                            (MSA) below the highest sysgen
                                            frame (RSASTORE)
    000C   12 Signed       4 RSAMSASC       Count of machine storage areas
                                            (MSA) below the highest sysgen
                                            frame (RSASTORE) or addressable
                                            frame (SYSTORS) whichever is
                                            lower
    0010   16 Signed       4 RSAMSARH       Count of machine storage areas
                                            (MSA) above the highest sysgen
                                            frame (RSASTORE)
    0014   20 Signed       4 RSADPACP       Count of DPA frames containing CP
                                            data (includes all frames which
                                            have the FRMCP bit on in FRMCSB0
                                            of their FRMTEs, except for VDISK
                                            frames, which are CP owned, but
                                            contain user data). This is the
                                            count of frames that will be
                                            included in a CP dump, and is
                                            used to allocate additional space
                                            for a CP dump as CP grows.
                                            Compare and Swap logic must be
                                            used to update this field. If
                                            this 32-bit field is treated as
                                            SIGNED, it will overflow when CP
                                            DPA reaches 2G frames, or 8T
                                            bytes. If this 32-bit field is
                                            treated as UNSIGNED, it will
                                            overflow when CP DPA reaches 4G
                                            frames, or 16T bytes.
    0018   24 Signed       4 RSATRSAV       Count of DPA frames in use for
                                            DEFERIO traces. This count is
                                            used to ensure that the number of
                                            DPA frames allocated for DEFERIO
                                            traces does not exceed 75% of the
                                            pageable pages in the DPA. This
                                            count is serialized by TXCDFRIO,
                                            the DEFERIO frames lock.
    001C   28 Signed       4 RSASTORE       Real machine actual storage size
                                            below 2G. Calculated during
                                            system init.
          Storage for 64 alternate processor PFXPGs are allocated
          during initialization from storage following the CP nucleus
          and is identity-mapped into the System Execution Space.
          The CPU address of the processor is used to index into this
          storage when allocating/deallocating prefix pages.
          Prefix pages are allocated below 2G in storage. Since they
          are allocated from identity-mapped storage the addresses
          can be used as host real or host logical (SXS) addresses.
    0020   32 Address      4 RSAPFXAF       First alternate proc PFXPG addr.
                                            Host real = host logical address.
    0024   36 Address      4 RSAPFXND       Address of the end of alternate
                                            processor PFXPG table. Points to
                                            the byte just after the last
                                            PFXPG in the table. Host real =
                                            host logical address.
          This area contains information regarding the use or non-use
          of host storage above the 2G line.
          All fields serialized by >= 2G available list lock-RSA2GLCK
          except where noted otherwise.
    0028   40 Signed       4 RSATASKB (0)   Task active bits. C/S to update.
    0028   40 Bitstring    1 RSATSKB0       RSATASKB task bits 0- 7
    0029   41 Bitstring    1 RSATSKB1       RSATASKB task bits 8-15
    002A   42 Bitstring    1 RSATSKB2       RSATASKB task bits 16-23
    002B   43 Bitstring    1 RSATSKB3       RSATASKB task bits 24-31
              .... ...1      RSAneTSK       X'01' RSAneTSK Phonetically: RSA
                                            "ini" TSK. Indicates low priority
                                            frame initialization task is
                                            active.
              .... ..1.      RSAneCNT       X'02' RSAneCNT Phonetically: RSA
                                            "ini" CNT. Indicates RSAFNOTI
                                            must be re-calculated.
              .... .1..      RSAneCTG       X'04' RSAneCTG Phonetically: RSA
                                            "ini" CTG. Indicates contig list
                                            should be filled
    002C   44 Signed       4 RSADPAAD       Number of frames that are CP
                                            frames in the storage being added
                                            by SET STORAGE
    0030   48 Signed       8 RSAFNOTI       Count of 'not-init' FRMTEs. This
                                            is the number of FRMTEs which
                                            have not yet been checked to see
                                            if they are usable.
    0038   56 Signed       8 RSALGFRM       Count of usable frames >= 2G.
                                            Only pageable or available frames
                                            are considered "usable" since
                                            they can be used to satisfy new
                                            requests. Non-pageable frames
                                            can't be stolen so they aren't
                                            considered usable. Pageable type
                                            frames that are pinned are
                                            considered non-pageable while
                                            pinned.
    0040   64 Signed       8 RSAGOFFL       Count of offline frames >= 2G.
    0048   72 Address      8 RSAGSTOR       Host Real Address Last
                                            addressable byte, including
                                            storage > 2G.
    0050   80 Address      8 RSASTORL       Host Real Address Highest real
                                            host storage addr, including
                                            STANDY and RESERVED. This is
                                            uncapped. Calculated from SCLP
                                            storage data or Diagnose.
    0058   88 Address      8 RSALG1ST       Host Logical Address Address of
                                            first FRMTE for frames >= 2G.
                                            It does not skip 'not-init'
                                            frames.
    0060   96 Address      8 RSALGLST       Host Logical Address Address of
                                            last FRMTE for frames >= 2G.
                                            This address is below any offline
                                            frames at the high end of
                                            storage. It does not skip
                                            'not-init' frames.
    0068  104 Address      8 RSANOTIB       Host Logical Address Address of
                                            FRMTE for the highest frame
                                            marked 'not-init'.
         |  >=2G Uncleared Global Available Lists Data:             |
         |                                                          |
         |  Refer to HCPPTE for a description of the organization   |
         |  of these lists.                                         |
          >2G SINGLE FRAMES available list
    0070  112 Dbl-Word     8 RSA2GAHD (0)   >= 2G available list data area
                                            with forward and backward
                                            pointers to the standard list of
                                            >= 2G available 4k frames, and
                                            the three doubleword area for the
                                            available list spin lock.
    0070  112 Address      8 RSA2GAFP       >=2G available list forward
                                            ptr
    0078  120 Address      8 RSA2GABP       >=2G available list backward
                                            ptr
    0080  128 Signed       8 RSA2GAVL       Count of frames on the >= 2G
                                            available list.
    0088  136 Dbl-Word     8 *              Reserved for IBM use.
    0090  144 Dbl-Word     8 *              Reserved for IBM use.
    0098  152 Signed       4 *              Reserved for IBM use.
    009C  156 Signed       4 RSAAVLHG       >= 2G avbl list high threshold
    00A0  160 Signed       8 RSA2GLCK (6)   >= 2G available list lock.
                                            This lock is obtained & released
                                            via macros HCPLK2GA and HCPUL2GA.
          >2G CONTIGUOUS FRAMES available list
    00D0  208 Dbl-Word     8 RSA2GCHD (0)   >= 2G contig avail list data
                                            area with forward and backward
                                            pointers to the standard list of
                                            >= 2G available 4k frames, and
                                            the three doubleword area for the
                                            available list spin lock.
    00D0  208 Address      8 RSA2GCFP       >=2G available list forward
                                            ptr
    00D8  216 Address      8 RSA2GCBP       >=2G available list backward
                                            ptr
    00E0  224 Signed       8 RSA2GCVL       Count of frames on the >= 2G
                                            available list.
    00E8  232 Dbl-Word     8 *              Reserved for IBM use.
    00F0  240 Dbl-Word     8 *              Reserved for IBM use.
    00F8  248 Signed       4 *              Reserved for IBM use.
    00FC  252 Signed       4 RSAAVCHG       >= 2G contig avbl list high
                                            thresh
    0100  256 Signed       8 RSA2GCLK (6)   >= 2G contig available list lk
                                            This lock is obtained & released
                                            via macros HCPLK2GC and HCPUL2GC.
    0130  304 Dbl-Word     8 RSAPRLK (3)    PTRM address space resolution
                                            lock. This is a formal exclusive
                                            lock, managed by HCPLCK. This
                                            lock serializes RSAASITB during
                                            PTRM address space creation. This
                                            lock must be held to resolve an
                                            "address space fault" when
                                            working with PTRM address spaces.
    0148  328 Dbl-Word     8 RSAASITB (16)  Table of i-ASITs for the PTRM
                                            address spaces. RSAPRLK must be
                                            held to validate an entry in this
                                            table. Each table entry is mapped
                                            by the HCPAMTE control block.
    01C8  456 Address      8 RSADPPFW (0)   Host Real Address
    01C8  456 Address      4 *              Deferred PGMBK paging list ...
    01CC  460 Address      4 *              (DPPL) forward pointer
    01D0  464 Address      8 RSADPPBW (0)   Host Real Address
    01D0  464 Address      4 *              Deferred PGMBK paging list ...
    01D4  468 Address      4 *              (DPPL) backward pointer
    01D8  472 Address      8 RSAPPAFW (0)   Host Real Address
    01D8  472 Address      4 *              Paged PGMBK aging list (PPAL) ...
    01DC  476 Address      4 *              forward ptr. PPAL is actually a
                                            list of PGMBKs and DAT frames.
    01E0  480 Address      8 RSAPPABW (0)   Host Real Address
    01E0  480 Address      4 *              Paged PGMBK aging list ...
    01E4  484 Address      4 *              (PPAL) backward pointer.
    01E8  488 Signed       4 RSAPPAQD       If non-zero, a task has been
                                            queued for deferred processing of
                                            the PPAL (contains the R13
                                            savearea address of the queueing
                                            task). Set with CS, reset with
                                            store of 0s.
    01EC  492 Signed       4 RSAPPTLK       Pageable Page Table Lock This is
                                            an informal spin lock. The lock
                                            must be held when adding FRMTEs
                                            to or removing FRMTEs from the
                                            DPPL or the PPAL. RSAPPTLK is set
                                            to the address obtaining the
                                            lock. When free, its value is
                                            zero. Use Compare-and-Swap to
                                            update. (This lock must also be
                                            held when decrementing a PGMFRMCT
                                            or PGMMIGCT field to zero, and
                                            then seeing if we can put that
                                            PGMBK on the DPPL.) It must be
                                            held while processing the DPPL,
                                            but can be held only while the
                                            PPAL is 'harvested' See HCPHRUPA
                                            prolog for details This lock also
                                            serializes the bit FRMONQUE in a
                                            FRMTE being put on the DPPL or
                                            PPAL. For FRMTEs on the PPAL, the
                                            ONLY procession for them is to an
                                            available list, and FRMONQUE is
                                            then reset.
    01F0  496 Signed       4 RSARESAC       Count of resident PTRM pages
                                            >=2G i.e. count of resident
                                            PGMBK frames >= 2G
    01F4  500 Signed       4 *              reserved for IBM use
    01F8  504 Dbl-Word     8 RSARFRSG       Count of frames allocated for
                                            real free storage requests
                                            >2G. This count is updated
                                            using Compare-and-Swap logic.
    0200  512 Dbl-Word     8 RSAAFRDW       Count of doublewords of aligned
                                            real free storage above 2G. This
                                            count includes the number of
                                            doublewords of active as well as
                                            inactive aligned free storage.
                                            This count will always be a
                                            multiple of 512. This count is
                                            updated using Compare-and-Swap
                                            logic.
    0208  520 Dbl-Word     8 RSAAFRIU       Count of doublewords of in use
                                            aligned real free storage above
                                            2G. This count includes only the
                                            active aligned free storage
                                            blocks This count is updated
                                            using Compare-and-Swap logic.
    0210  528 Signed       4 RSAAFSDW       Count of doublewords of aligned
                                            host logical free storage backed
                                            above 2G. This count includes the
                                            number of doublewords of active
                                            as well as inactive aligned free
                                            storage. This count will always
                                            be a multiple of 512. This count
                                            is updated using Compare-and-Swap
                                            logic.
    0214  532 Signed       4 RSAAFSDB       Count of doublewords of aligned
                                            host logical free storage backed
                                            below 2G. This count includes
                                            active as well as inactive
                                            aligned free storage. This count
                                            will always be a multiple of 512.
                                            This count is updated using
                                            Compare-and-Swap logic.
    0218  536 Signed       4 RSARFRST       Count of frames allocated for
                                            real free storage requests
                                            <2G. This count is updated
                                            using Compare-and-Swap logic.
    021C  540 Signed       4 RSAAFRDB       Count of doublewords of aligned
                                            real free storage below 2G. This
                                            count includes active as well as
                                            inactive aligned free storage.
                                            This count will always be a
                                            multiple of 512. This count is
                                            updated using Compare-and-Swap
                                            logic.
    0220  544 Signed       4 RSAAFSIU       Count of doublewords of in use
                                            aligned host logical free storage
                                            backed above 2G. This count
                                            includes only the active aligned
                                            free storage blocks. This count
                                            is updated using Compare-and-Swap
                                            logic.
    0224  548 Signed       4 RSAAFSIB       Count of doublewords of in use
                                            aligned host logical free storage
                                            backed below 2G. This count
                                            includes only the active aligned
                                            free storage blocks. This count
                                            is updated using Compare-and-Swap
                                            logic.
    0228  552 Signed       4 RSAAFRIB       Count of doublewords of in use
                                            aligned real free storage below
                                            2G. This count includes only the
                                            active aligned free storage
                                            blocks This count is updated
                                            using Compare-and-Swap logic.
    022C  556 Signed       4 RSAVCBDW       Count of doublewords of
                                            verifiable control block free
                                            storage backed above 2G. This
                                            control block free storage. count
                                            includes the number of
                                            doublewords of active as well as
                                            inactive verifiable control block
                                            free storage and will always be a
                                            multiple of 512. This count is
                                            updated using Compare-and-Swap
                                            logic.
    0230  560 Signed       4 RSAVCBDB       Count of doublewords of
                                            verifiable control block free
                                            storage backed below 2G. This
                                            control block free storage. count
                                            includes the number of
                                            doublewords of active as well as
                                            inactive verifiable control block
                                            free storage and will always be a
                                            multiple of 512. This count is
                                            updated using Compare-and-Swap
                                            logic.
    0234  564 Signed       4 RSAVCBIU       Count of doublewords of in use
                                            verifiable control block free
                                            storage backed above 2G. This
                                            count includes only the active
                                            verifiable control block free
                                            storage blocks. This count is
                                            updated using Compare-and-Swap
                                            logic.
    0238  568 Signed       4 RSAVCBIB       Count of doublewords of in use
                                            verifiable control block free
                                            storage backed below 2G. This
                                            count includes only the active
                                            verifiable control block free
                                            storage blocks. This count is
                                            updated using Compare-and-Swap
                                            logic.
    023C  572 Signed       4 RSAVFSDW       Count of doublewords of virtual
                                            free storage. This count includes
                                            active as well as inactive
                                            virtual free storage blocks (Note
                                            that inactive means currently
                                            resident on the virtual SUBBK
                                            FRMTE list).
                                     Note that this count represents
                                     virtual storage, not real.  The
                                     count is the number of doublewords
                                     within the virtual free storage
                                     CP utility address space currently
                                     in use or residing on the virtual
                                     SUBBK FRMTE lists.  This count
                                     will always be a multiple of 2048.
                                     This count is updated using
                                     Compare-and-Swap logic.
    0240  576 Signed       4 RSAVFSIU       Count of doublewords of virtual
                                            free storage in use. This count
                                            includes only active free storage
                                            blocks. Note this count
                                            represents virtual storage, not
                                            real. The count is the number of
                                            doublewords within the virtual
                                            free storage CP utility address
                                            space. This count is updated
                                            using Compare-and-Swap logic.
    0244  580 Signed       4 RSANALD        Host Real Address ALD for "null"
                                            access list
    0248  584 Dbl-Word     8 RSANASIT (0)   i-ASIT for "null" address space.
                                            The ASTE for the null address
                                            space is guaranteed to designate
                                            both a null access list (RSANALD)
                                            and a null authority table, and
                                            the ASTE ASCE is guaranteed to
                                            designate a segment table with
                                            STL of 1, indicating that the
                                            segment table is two segment
                                            table units in length (2 pages =
                                            8K in z/Arch).
    0248  584 Address      4 *              Null ASTE with IASRACC and
                                            IASFPRIV set. The value is
                                            updated during initialization to
                                            address the null ASTE.
    024C  588 Signed       4 *              ASTE sequence number=1.
    0250  592 Address      4 RSANDUCT       Host Real Address Address of
                                            "null" dispatchable- unit control
                                            table (DUCT).
    0254  596 Address      4 RSASHRSP       Host Logical Address Anchor for
                                            chain of shareable address
                                            spaces. Chain is serialized by
                                            RSASHRLK.
    0258  600 Dbl-Word     8 RSAPPTN        STE invalidation timestamp of
                                            most recently decoupled frame
                                            (pair) on the PPAL.
    0260  608 Signed       4 RSAPPTPS       ALB/TLB purges started prior to
                                            entering wait
    0264  612 Signed       4 RSAPPTPF       ALB/TLB purges finished prior to
                                            entering wait
    0268  616 Signed       4 RSAPPTCS       ALB/TLB purges via CSP during
                                            emergency PPAL processing
    026C  620 Signed       4 *              Reserved for IBM use
    0270  624 Dbl-Word     8 RSASHRLK (3)   A shared/exclusive defer lock
                                            serializing the RSASHRSP chain.
    0288  648 Dbl-Word     8 RSASPMLK (3)   A shared/exclusive defer lock
                                            serializing all SPIBK chains
                                            system-wide.
    02A0  672 Dbl-Word     8 RSAALCIN (3)   An exclusive-only defer lock to
                                            serialize tasks changing an ALD
                                            from the "null" ALD to a non-null
                                            ALD.
    02B8  696 Signed       4 RSACTSHR       Global count of shared address
                                            space resident frames
    02BC  700 Signed       4 RSABLKGC       Count of tasks representing frame
                                            requests requesting or deferred
                                            on RSABLKGF lock
    02C0  704 Dbl-Word     8 RSABLKGF (3)   An exclusive-only defer lock to
                                            serialize tasks obtaining frames
                                            to resolve page faults in a group
                                            of blocked pages. Used when there
                                            are no frames on the available
                                            list.
         |        RSM allocation counts:                            |
    02D8  728 Signed       4 RSACPLOK       Integer non-negative exact count
                                            of frames that are locked by the
                                            CP LOCK command (PGSCPLOK) below
                                            2G. This count is updated using
                                            Compare-and-Swap logic.
    02DC  732 Signed       4 RSAOFFLN       Non-negative count of the number
                                            of offline frames. The count of
                                            offline frames may never be
                                            decremented since once a frame is
                                            marked offline, it is never
                                            brought back online. This field
                                            is initialized during system
                                            initialization and should always
                                            be updated with the available
                                            list spin lock held. However,
                                            because this field may be updated
                                            by the extend free storage
                                            replenishment scan which does not
                                            normally function with the
                                            available list lock held, there
                                            is a minute chance that the count
                                            may be off slightly.
    02E0  736 Signed       4 RSASHARE       Non-negative count of frames that
                                            currently are translated as a
                                            shared frame (DCSS/NSS frames
                                            only, shared address space frames
                                            are not included (see RSACTSHR)).
                                            This count is updated using
                                            Compare-and-Swap logic.
    02E4  740 Signed       4 RSANONPG       Count of DPA frames which are
                                            currently non-pageable, including
                                            locked pageable frames, CP owned
                                            or free storage frames, etc. This
                                            field is only updated during
                                            system initialization or using
                                            Compare-and-Swap logic.
    02E8  744 Signed       4 RSAPGABL       Count of usable frames in the DPA
                                            including both pageable and
                                            non-pageable (locked, CP owned,
                                            free storage, etc.) frames. It
                                            does not include offline frames.
                                            This field is only updated during
                                            system initialization or using
                                            Compare-and-Swap logic.
    02EC  748 Signed       4 RSACPLKG       Integer non-negative exact count
                                            of frames that are locked by the
                                            CP LOCK command (PGSCPLOK) above
                                            2G. This count is updated using
                                            Compare-and-Swap logic.
         |  <2G Uncleared Global Available lists data:              |
         |                                                          |
         |  Refer to HCPPTE for a description of the organization   |
         |  of these lists.                                         |
          <2G SINGLE FRAMES available list
    02F0  752 Dbl-Word     8 RSAAVLAN (0)   Available list data area with
                                            forward and backward pointers to
                                            the standard list of available 4K
                                            frames, a backward pointer for
                                            the list of available 16K blocks
                                            (for IFSNT allocation requests)
                                            and the three doubleword area for
                                            the available list spin lock.
                                            This area is initialized during
                                            system initialization and updated
                                            only when the available list lock
                                            is held.
    02F0  752 Address      8 RSAAVLFP       Host Logical Address FRMTE
                                            available list forward ptr
    02F8  760 Address      8 RSAAVLBP       Host Logical Address FRMTE
                                            available list backward ptr
    0300  768 Signed       4 *              Not used, but needed to be
                                            compatible with RSA2GAVL
    0304  772 Signed       4 RSAAVAIL       Non-negative count of frames that
                                            are currently on the < 2G
                                            frames available list. This field
                                            is initialized during system
                                            initialization and updated only
                                            when the available list lock is
                                            held.
    0308  776 Signed       4 *              Reserved for IBM use.
    030C  780 Signed       4 *              Reserved for IBM use.
    0310  784 Signed       4 *              Reserved for IBM use.
    0314  788 Signed       4 RSAAVLHT       < 2G avbl list high threshold
    0318  792 Signed       8 RSAAVLLK (6)   Avbl list spin lock
    0348  840 Bitstring    8 RSA16KBP       Host Logical Address Backward ptr
                                            to FRMTE for the list of
                                            available 16K blocks. They are
                                            chained via the backward pointer
                                            in the FRMTE for the last frame
                                            in each 16K block
          <2G CONTIGUOUS FRAMES available list
    0350  848 Dbl-Word     8 RSAAVCAN (0)   Contig avail list data area with
                                            forward and backward pointers to
                                            the standard list of available 4K
                                            frames, and the six doubleword
                                            area for the available list spin
                                            lock. This area is initialized
                                            during system initialization and
                                            updated only when the available
                                            list lock is held.
    0350  848 Address      8 RSAAVCFP       Host Logical Address FRMTE
                                            available list forward ptr
    0358  856 Address      8 RSAAVCBP       Host Logical Address FRMTE
                                            available list backward ptr
    0360  864 Signed       4 *              Not used, but needed to be
                                            compatible with RSA2GCVL
    0364  868 Signed       4 RSAAVCIL       Non-negative count of frames that
                                            are currently on the < 2G
                                            frames available list. This field
                                            is initialized during system
                                            initialization and updated only
                                            when the available list lock is
                                            held.
    0368  872 Signed       4 *              Reserved for IBM use.
    036C  876 Signed       4 *              Reserved for IBM use.
    0370  880 Signed       4 *              Reserved for IBM use.
    0374  884 Signed       4 RSAAVCHT       <2G contig avbl list high
                                            thresh
    0378  888 Signed       8 RSAAVCLK (6)   Contig available list spin lock
    03A8  936 Dbl-Word     8 RSAFRQAN (0)   Frame request defer anchor
    03A8  936 Address      4 RSAFRQFP       Host Logical Address Forward
                                            pointer to deferred queue of
                                            CPEBKs
    03AC  940 Address      4 RSAFRQBP       Host Logical Address Backward
                                            pointer to deferred queue of
                                            CPEBKs
    03B0  944 Signed       4 RSA2GDCT       Count of deferred frame requests
                                            that are waiting for any
                                            available frame. This plus
                                            RSAFRQWT is the total wait count.
    03B4  948 Signed       4 RSAFRQMW       Count of tasks deferring or
                                            delaying attempting to obtain
                                            multiple frames (for PGMBKs only
                                            at this point). Incrememented
                                            once after initial attempt fails,
                                            decremented only after request is
                                            satisfied, or given up on.
    03B8  952 Signed       4 RSAFRQDF       Count of deferred multiple frame
                                            requests for PGMBKs Incremented
                                            during actual deferment.
    03BC  956 Signed       4 RSAFRQDL       Count of delayed multiple frame
                                            requests for PGMBKs Incremented
                                            during actual delay.
    03C0  960 Dbl-Word     8 RSAFRQDT       Total multiple frame request
                                            delay interval for PGMBKs since
                                            last system timer pop
    03C8  968 Dbl-Word     8 RSAFRQDA       Average multiple frame request
                                            delay interval for PGMBKs between
                                            system timer pop instances
    03D0  976 Signed       4 RSA2GRDA       Count of times HCPPTGRD attempted
                                            to redrive tasks waiting for any
                                            available frame (>= 2G or
                                            <2G)
    03D4  980 Signed       4 RSA2GRDC       Count of individual task redrives
                                            performed by HCPPTGRD for any
                                            available frame (>= 2G or
                                            <2G)
    03D8  984 Signed       4 * (0)          These fields are grouped together
    03D8  984 Signed       4 RSAFRQWT       Non-negative count of deferred
                                            requests for real frames which
                                            have not yet been satisfied since
                                            there are no frames available.
                                            Requests are for frames < 2G.
                                            Also see RSA2GDCT. Update by
                                            holding the available list spin
                                            lock.
    03DC  988 Signed       4 RSAFRRDA       Count of HCPPTGRD attempts to
                                            redrive tasks waiting for frames
                                            below 2G. Update by holding the
                                            available list spin lock.
    03E0  992 Signed       4 RSAFRRDC       Count of individual task redrives
                                            performed by HCPPTGRD for frames
                                            below 2G. Update by holding the
                                            available list spin lock.
    03E4  996 Signed       4 RSARESBC       Count of resident PTRM pages
                                            <2G i.e. count of resident
                                            PGMBK frames <2G
         |        Available list replenishment (steal) data:        |
    03E8 1000 Dbl-Word     8 * (0)
    03E8 1000 Signed       4 RSADSLOK (0)   Demand Scan (Steal) lock. When
                                            held, this lock indicates the
                                            Demand Scan is replenishing the
                                            available list of frames. This
                                            lock is normally obtained via TS.
                                            However CS may be used if
                                            RSARFLOK is set to X'FF' as TS
                                            would and RSADSCPU is set at the
                                            same time.
    03E8 1000 Bitstring    1 RSARFLOK       TS lock to prevent triggering of
                                            multiple concurrent steal tasks
    03E9 1001 Bitstring    3 RSADSCPU       When non-zero, indicates a CPU is
                                            running the Steal task
    03EC 1004 Bitstring    1 RSATRQLK       Delayed Demand Scan TRQBK lock.
                                            This TS lock is used to prevent
                                            stacking multiple TRQBK's when
                                            Demand Scan determines it may
                                            need to reinvoke itself.
    03ED 1005 Bitstring    3 *              Reserved for IBM use
    03F0 1008 Dbl-Word     8 * (0)
    03F0 1008 Dbl-Word     8 RSADSTSA       Timestamp of when entered
                                            emergency pass in demand scan for
                                            >=2G frames
    03F8 1016 Dbl-Word     8 RSADSTSB       Timestamp of when entered
                                            emergency pass in demand scan for
                                            <2G frames
    0400 1024 Dbl-Word     8 * (0)          Available list high thresholds
                                            which indicates how many frames
                                            should be taken by the available
                                            list replenishment functions to
                                            satisfy the current user and
                                            system needs for frames. These
                                            fields are updated with
                                            Compare-and-Swap logic.
    0400 1024 Signed       4 RSASWPWT       Count of available list
                                            replenishment page writes (steal
                                            writes) for < 2G PGMBKs in
                                            frames This count is updated
                                            using Compare-and-Swap logic.
    0404 1028 Signed       4 RSASWP2G       Count of available list
                                            replenishment page writes (steal
                                            writes) for >= 2G PGMBKs in
                                            frames
    0408 1032 Dbl-Word     8 * (0)          Available list low thresholds
                                            (which indicates when the demand
                                            scan should be invoked providing
                                            a buffer for the system until
                                            more frames become available),
                                            the decrement count (which says
                                            how many times the demand scan
                                            has run since the low threshold
                                            was last checked for
                                            decrementing; it wasn't
                                            decremented if it was recently
                                            incremented), and the decrement
                                            flag (which is on when the
                                            threshold was not incremented
                                            recently and may be decremented).
                                            These fields are updated with
                                            Compare-and-Swap logic except at
                                            initialization time. The count
                                            and flag fields are used to
                                            determine whether or not to
                                            decrement the low threshold in
                                            this run of the demand scan.
    0408 1032 Signed       4 RSAAVLLT       Available list low threshold for
                                            frames < 2G
    040C 1036 Signed       4 RSADECCT       Decrement low threshold count for
                                            frames < 2G
    0410 1040 Signed       4 RSAAVCLT       Cont avail list low threshold for
                                            frames < 2G
    0414 1044 Signed       4 RSADECCC       Decrement low threshold count for
                                            cont frames < 2G
    0418 1048 Signed       4 RSADECCS (0)   DECREMENT FLAG COMP. & SWAP WORD
    0418 1048 Bitstring    2 *              Reserved for IBM use
    041A 1050 Bitstring    1 RSADECFG       Decrement low threshold flag for
                                            frames >= 2G
              .... ...1      RSADECRG       X'01' RSADECRG The >=2G low
                                            threshold may be decremented when
                                            on (if off, the low threshold was
                                            recently incremented and should
                                            not be decremented)
              .... ..1.      RSAINCRG       X'02' RSAINCRG The >=2G low
                                            threshold has been incremented
                                            already this cycle (controls the
                                            increment amount)
              .... .1..      RSADCCGC       X'04' RSADCCGC The >=2G contig
                                            low threshold may be decremented
                                            when on (if off, the low
                                            threshold was recently
                                            incremented and should not be
                                            decremented)
              .... 1...      RSAINCGC       X'08' RSAINCGC The >=2G contig
                                            low threshold has been
                                            incremented already this cycle
                                            (controls the increment amount)
    041B 1051 Bitstring    1 RSADECFL       Decrement low threshold flag for
                                            frames < 2G
              .... ...1      RSADECRB       X'01' RSADECRB The <2G low
                                            threshold may be decremented when
                                            on (if off, the low threshold was
                                            recently incremented and should
                                            not be decremented)
              .... ..1.      RSAINCRB       X'02' RSAINCRB The <2G low
                                            threshold has been incremented
                                            already this cycle (controls the
                                            increment amount)
              .... .1..      RSADECRC       X'04' RSADECRC The <2G contig
                                            low threshold may be decremented
                                            when on (if off, the low
                                            threshold was recently
                                            incremented and should not be
                                            decremented)
              .... 1...      RSAINCRC       X'08' RSAINCRC The <2G contig
                                            low threshold has been
                                            incremented already this cycle
                                            (controls the increment amount)
    041C 1052 Signed       4 RSAAVLLG       >=2G available list low
                                            threshold
    0420 1056 Signed       4 RSADECCG       Decrement >=2G low threshold
                                            count
    0424 1060 Signed       4 RSAAVCLG       >=2G cont avail list low
                                            threshold
    0428 1064 Signed       4 RSADECGC       Decrement contig >=2G low
                                            threshold count
    042C 1068 Signed       4 RSACFPCT       Count of contiguous frames for
                                            PGMBKs since last demand scan
    0430 1072 Signed       4 RSACFPAV       Average count of contiguous frame
                                            requests for PGMBKs between
                                            demand scan instances
    0434 1076 Signed       4 RSAALFMF       Total count of contiguous frames
                                            being scanned for by active
                                            HCPALFMF FREXSCAN tasks
    0438 1080 Signed       4 RSAAVLEP       Low threshold adjustment to
                                            account for dynamic free storage
                                            requests made for emulated paging
                                            devices during demand scan
    043C 1084 Signed       4 *              Reserved for IBM use
    0440 1088 Dbl-Word     8 * (0)
    0440 1088 Signed       4 RSASTLWT       Count of available list
                                            replenishment page writes (steal
                                            writes) for < 2G frames. This
                                            count is updated using
                                            Compare-and-Swap logic.
    0444 1092 Signed       4 RSASWG2G       Count of available list
                                            replenishment page writes (steal
                                            writes) for >= 2G frames
    0448 1096 Signed       8 RSACNOTI       Quota for contig list use of NOTI
    0450 1104 Dbl-Word     8 * (0)          Frame table scan extent block
                                            ptrs
    0450 1104 Address      4 RSAFTXFL       Host Logical Address Address of
                                            first FTXBK for frames < 2G
    0454 1108 Address      4 *              Reserved for IBM use
    0458 1112 Address      4 RSAFTXFG       Host Logical Address Address of
                                            first FTXBK for frames >= 2G
    045C 1116 Address      4 *              Reserved for IBM use
    0460 1120 Signed       4 * (4)          Reserved for IBM use
         |        Reset interval data area:                         |
    0470 1136 Dbl-Word     8 RSARINTA (8)   Reset interval data and work area
         |        Free storage data:                                |
    04B0 1200 Signed       4 RSAFSA2G       Non-negative count of doublewords
                                            of system free storage backed
                                            above 2G. Count includes the
                                            number of doublewords of free
                                            storage available. This count is
                                            updated only by HCPFRFDX (free
                                            storage garbage collection) which
                                            runs on the master processor
                                            only.
    04B4 1204 Signed       4 RSAFSB2G       Non-negative count of doublewords
                                            of system free storage backed
                                            below 2G. Count includes the
                                            number of doublewords of free
                                            storage available. This count is
                                            updated only by HCPFRFDX (free
                                            storage garbage collection) which
                                            runs on the master processor
                                            only.
    04B8 1208 Signed       4 RSAFSYUA       Non-negative count of doublewords
                                            of in use system free storage
                                            backed above 2G. This count is
                                            updated only by HCPFRFDX (free
                                            storage garbage collection) which
                                            runs on the master processor
                                            only.
    04BC 1212 Signed       4 RSAFSYUB       Non-negative count of doublewords
                                            of in use system free storage
                                            backed below 2G. This count is
                                            updated only by HCPFRFDX (free
                                            storage garbage collection) which
                                            runs on the master processor
                                            only.
    04C0 1216 Signed       4 RSAFVMUD       Count of doublewords of VMDBK
                                            free storage in use above 2G.
                                            Allocated from VMDBKs, VMDBK free
                                            storage pages, and system free
                                            storage pages. This count does
                                            not include the storage allocated
                                            from the free storage subpools.
                                            This count is updated only when
                                            holding FSDVMLK formal spin lock.
    04C4 1220 Signed       4 RSAFVMUB       Count of doublewords of VMDBK
                                            free storage in use below 2G.
                                            Allocated from VMDBKs, VMDBK free
                                            storage pages, and system free
                                            storage pages. This count does
                                            not include the storage allocated
                                            from the free storage subpools.
                                            This count is updated only when
                                            holding FSDVMLK formal spin lock.
    04C8 1224 Signed       4 RSAVMXFR       Count of pages in use for VMDBK
                                            free storage above 2G, i.e., user
                                            free pages allocated. This count
                                            does not include the VMDBKs
                                            themselves. This count is updated
                                            only when holding FSDVMLK formal
                                            spin lock.
    04CC 1228 Signed       4 RSAVMXFB       Count of pages in use for VMDBK
                                            free storage above 2G, i.e., user
                                            free pages allocated. This count
                                            does not include the VMDBKs
                                            themselves. This count is updated
                                            only when holding FSDVMLK formal
                                            spin lock.
    04D0 1232 Signed       4 RSAVMXUD       Count of in use user free storage
                                            doublewords (allocated from VMDBK
                                            free storage pages) backed above
                                            2G. This count does not include
                                            storage in the VMDBKs themselves.
                                            This count is updated only when
                                            holding FSDVMLK formal spin lock.
    04D4 1236 Signed       4 RSAVMXUB       Count of in use user free storage
                                            doublewords (allocated from VMDBK
                                            free storage pages) backed below
                                            2G. This count does not include
                                            storage in the VMDBKs themselves.
                                            This count is updated only when
                                            holding FSDVMLK formal spin lock.
    04D8 1240 Signed       4 RSASYSFR       Count of pages in use for system
                                            free storage above 2G. This count
                                            is updated only when holding
                                            FSDVMLK formal spin lock.
    04DC 1244 Signed       4 RSASYSFB       Count of pages in use for system
                                            free storage below 2G. This count
                                            is updated only when holding
                                            FSDVMLK formal spin lock.
    04E0 1248 Signed       4 RSASYSUD       Count of system free storage
                                            doublewords above 2G in use
                                            allocated from system free
                                            storage chain. This count is
                                            updated when holding FSDVMLK
                                            formal spin lock.
    04E4 1252 Signed       4 RSASYSUB       Count of system free storage
                                            doublewords below 2G in use
                                            allocated from system free
                                            storage chain. This count is
                                            updated when holding FSDVMLK
                                            formal spin lock.
    04E8 1256 Signed       4 *              Reserved for IBM use
    04EC 1260 Signed       4 *              Reserved for IBM use
         | Data for free storage limit detection. The 3 thresholds  |
         | will determine when to issue a warning message, put a    |
         | user into a stopped state and when to logoff a user who  |
         | is abusing free storage. These fields are updated with   |
         | Compare-and-Swap logic.                                  |
         | The flag field is used to determine whether free storage |
         | limit detection is on or off for the system.             |
    04F0 1264 Dbl-Word     8 * (0)          5 word long area on dword bdy
    04F0 1264 Signed       4 RSALIM1        Free storage threshold 1 (WRNG)
    04F4 1268 Signed       4 RSALIM2        Free storage threshold 2 (STOP)
    04F8 1272 Signed       4 RSALIM3        Free storage threshold 3 (FORCE)
          RSALMFUZ is calculated to be .5% DPA and will be used as the
          fuzz around the thresholds to prevent multiple messages from
          being issued if the limit oscillates about the threshold.
    04FC 1276 Signed       4 RSALMFUZ       Free storage threshold fuzz
    0500 1280 Signed       4 RSALIMCS (0)   Free storage limits Compare-and-
                                            Swap word
    0500 1280 Bitstring    3 *              Reserved for IBM use
    0503 1283 Bitstring    1 RSALIMCK       Free storage limit detection flag
              00000000       RSALIMOF       X'00' RSALIMOF Free storage limit
                                            detection off
              00000001       RSALIMON       X'01' RSALIMON Free storage limit
                                            detection on
         |       Free storage emergency mode counts/timestamps.     |
         |       The RSAFSELK lock must be held to inspect/change   |
         |       these fields.  RSAFSELK is obtained via CS logic.  |
    0504 1284 Signed       4 RSAFSELK       Free storage emergency mode data
                                            area lock word
    0508 1288 Signed       4 RSAPLPCT       Count of processors looping in
                                            HCPFRFGP/GB trying to get an SXS
                                            page backed any for free storage
    050C 1292 Signed       4 RSAPLPCB       Count of processors looping in
                                            HCPFRFGP/GB trying to get an SXS
                                            page backed below 2G for free stg
    0510 1296 Signed       4 RSANPGCT       Count of consecutive failure
                                            returns from SXPFS where no pages
                                            were available for free storage
    0514 1300 Signed       4 *              Reserved to maintain alignment
    0518 1304 Dbl-Word     8 RSAEMTSA       Timestamp of when entered
                                            emergency mode looking for a free
                                            storage page backed any
    0520 1312 Dbl-Word     8 RSAEMTSB       Timestamp of when entered
                                            emergency mode looking for a free
                                            storage page backed below
    0528 1320 Signed       4 RSANPGMX       Maximum cap on number of times we
                                            will allow a consecutive failure
                                            from HCPSXPFS when trying to get
                                            a page for free storage
    052C 1324 Signed       4 RSANPGHI       High water mark for number of
                                            consecutive failures from
                                            HCPSXPFS when trying to get a
                                            page for free storage (all
                                            processors)
         |       Free storage reserved pages data area:             |
    0530 1328 Dbl-Word     8 * (0)          This is the free storage reserved
                                            pages data area consisting of a
                                            count of unique extend requests
                                            that have not been satisfied yet,
                                            the free storage reserved pages
                                            anchor, the free storage reserved
                                            pages data area lock word, the
                                            count of free storage reserved
                                            pages required by the system, and
                                            the number of free storage
                                            reserved pages per processor.
                                            Note: The number of free storage
                                            reserved pages per processor must
                                            be positive. Update while holding
                                            the free storage reserved pages
                                            data area Compare-and-Swap lock
                                            word or during system
                                            initialization.
    0530 1328 Signed       4 RSAXTEND       Count of pages missing from the
                                            free storage reserved pages list
                                            i.e., count of unique extend
                                            conditions not yet satisfied.
    0534 1332 Address      4 RSARESAN       Reserved pages queue anchor
                                            forward pointer
    0538 1336 Address      4 RSARSVLK       Free storage reserved pages data
                                            area Compare-and-Swap lock word
    053C 1340 Signed       4 RSARSVSY       Total number of free storage
                                            reserved pages required to be on
                                            the reserved pages list Includes
                                            RSAMAXPP frames per online
                                            processor, plus additional frames
                                            per emulated CP owned device
                                            containing page or spool space
                                            (the number of frames is based on
                                            emulated device specific
                                            information provided in the
                                            EDEV).
    0540 1344 Signed       4 RSAMAXPP       Number of free storage reserved
                                            pages required per processor.
                                            Note: Field must be positive.
    0544 1348 Signed       4 *              Reserved for IBM use
         |        Segment translation data:                         |
    0548 1352 Dbl-Word     8 * (0)          This is the deferred segment
                                            translation queue data area. It
                                            consists of the queue anchor and
                                            the Compare-and-Swap lock.
    0548 1352 Address      4 RSADEFAN       Host Logical Address Pointer to
                                            first CPEBK of the deferred
                                            segment translation queue
    054C 1356 Address      4 RSADEFLK       Compare-and-Swap lock. Zero means
                                            the lock is not held.
    0550 1360 Signed       4 RSAPRQWT       Non-negative count of tasks
                                            waiting for a page translation
                                            request. This count also includes
                                            tasks waiting for a segment
                                            translation. This count is
                                            updated with Compare-and-Swap
                                            logic.
    0554 1364 Signed       4 *              Reserved for IBM use
         |        Fixed storage management data:                    |
           This area contains the fixed storage management block.
           It contains information regarding the allocation of
           contiguous host real storage from the V=F area.
           Additionally, information for the dedicated region
           facility is kept here to keep track of zone numbers
           available for assigning to MHPG users or to CP.
           The allocation of storage from the V=F area is
           maintained in the fixed storage assignment block
           anchored in HCPWRK.
           All changes to fields in the fixed storage management
           block and in the fixed storage assignment table are
           either made during system initialization or are under
           the control of the fixed storage management lock.
    0558 1368 Dbl-Word     8 RSAFSTBK (0)   Fixed storage management block
    0558 1368 Dbl-Word     8 RSAFSLCK (3)   Fixed storage mgmt lock (defer)
    0570 1392 Bitstring    2 RSASA1ST       Offset of entry in the fixed
                                            storage assignment table
                                            containing the lowest main
                                            storage origin
    0572 1394 Bitstring    2 RSASALST       Offset of entry in the fixed
                                            storage assignment table
                                            containing the highest main
                                            storage origin
    0574 1396 Signed       4 RSASTRNG (0)   The entire storage range for the
                                            V=F area. (Never changes)
    0574 1396 Signed       2 RSAMSO         Bits 5-15 specify a 1 meg main
                                            storage origin of the V=F area.
                                            Main storage origin is the
                                            address of the first byte, on a
                                            megabyte boundary, of the V=F
                                            area, shifted right 20 bits.
    0576 1398 Signed       2 RSAMSL         Bits 5-15 specify a 1 meg main
                                            storage limit of the V=F area.
                                            Main storage limit is the address
                                            of the last byte of the V=F area,
                                            shifted right 20 bits.
    0578 1400 Bitstring    1 RSAAZNCT       Count of zones available for
                                            guest use, including zones in use
                                            (never changes)
    0579 1401 Bitstring    1 RSAZPOOL       Pool of available zones, not
                                            including those in use
    057A 1402 Bitstring    2 *              Reserved for IBM use
    057C 1404 Signed       4 *              Reserved for IBM use
              00000028       RSAFSTLN       *-RSAFSTBK Length of FSTBK
              00000005       RSAFSTSZ       (*-RSAFSTBK+7)/8 Size of FSTBK
         |        Virtual storage management data:                  |
    0580 1408 Dbl-Word     8 RSAVVBLK (0)   Virtual Storage Management Block.
                                            This area contains information
                                            needed to manage the System
                                            Virtual Address Space.
    0580 1408 Bitstring    4 *              Reserved for IBM use
    0584 1412 Address      4 RSAVSLOW       Lowest available virtual page.
                                            Initialized by HCPIST at IPL.
                                            Serialized by Compare-and-Swap
           Allocation of System Virtual Addresses above RSAVHSAD
             is serialized by the High Storage Lock (RSAVHSLK).
    0588 1416 Dbl-Word     8 RSAVHSLK (3)   High storage lock
    05A0 1440 Bitstring    4 *              Reserved
    05A4 1444 Address      4 RSAVHSAD       High storage starting addr.
                                            Initialized with constant 1G (the
                                            upper half of the addr space).
                                            Must be on a segment boundary
                                            (right most 20 bits must be
                                            zero).
         |  No-owned resources data area                            |
         |                                                          |
         |  No-owned resources are pagable address space structures |
         |  that no longer belong to any pagable address space but  |
         |  cannot be reclaimed by CP because someone else has      |
         |  rights to the structure, or the structure is locked or  |
         |  last translated.                                        |
    05A8 1448 Signed       8 RSANOQLK (6)   No-owned resources queue lock.
                                            Lock serializes the no-owned
                                            queues, RSANOQSX, RSANOQFR, and
                                            RSANOQPG. Lock is obtained and
                                            released via macros HCPLKNOR and
                                            HCPULNOR.
                                     Reclaimable no-owned SXSTE queue
    05D8 1496 Address      8 RSANOXFP (0)   SXSTE forward pointer
    05D8 1496 Address      4 *              is initialized to
    05DC 1500 Address      4 *              queue origen
    05E0 1504 Address      8 RSANOXBP (0)   SXSTE backward pointer
    05E0 1504 Address      4 *              is initialized to
    05E4 1508 Address      4 *              queue origen
    05E8 1512 Bitstring    8 RSANOQFR       Reclaimable no-owned FRMTE queue
                                            header
    05F0 1520 Dbl-Word     8 RSANOQPG       No-owned PGMBK queue header
    05F8 1528 Signed       4 *              Reserved for IBM use
    05FC 1532 Signed       4 RSANOLKL       Count of no-owned locked pages in
                                            host logical storage
    0600 1536 Dbl-Word     8 RSANOLKA       Count of no-owned locked pages in
                                            absolute storage
    0608 1544 Signed       4 RSANOLOK       Word used to ensure the no own
                                            resource reclaim routine is only
                                            invoked by the dispatcher on one
                                            processor at a time. This ensures
                                            only one of the background or
                                            foreground replenishment tasks
                                            are running at a time. This word
                                            can be in any of the following
                                            states as defined in HCPEQUAT:
                                            DSPNOBFW - no work to do DSPFSCHD
                                            - foreground scheduled DSPFACTV -
                                            foreground active DSPBSCHD -
                                            background scheduled DSPBACTV -
                                            background active Serialized by
                                            compare-and-swap
    060C 1548 Signed       4 *              Reserved for IBM use.
         |  Delta-Pinned-Page-Count Array (DPPCA) for page class 1  |
         |                                                          |
         | Used by both hardware and software to maintain pinned    |
         | page counts for page class 1 pages.  Page class 1 is     |
         | used for NSS/DCSS imbedded shared pages.  This array is  |
         | pointed to by the class 1 Delta-Pinned-Page-Count-Array  |
         | Origin in the prefix area, PFXDPPCAO. The page class     |
         | 0 array is used for base address space pages owned by    |
         | the user and resides in the virtual configuration's base |
         | ASCBK.                                                   |
    0610 1552 Dbl-Word     8 RSADPPCA (0)   Delta-pinned-page count array
    0610 1552 Signed       4 RSADPPB        Delta-pinned-page count for all
                                            class 1 pages pinned below 2G
    0614 1556 Signed       4 RSADPPA        Delta-pinned-page count for all
                                            class 1 pages pinned at or above
                                            2G
         |  System Execution Space Page Manager (SXSPM) data area   |
         |                                                          |
         | These fields are serialized by SXSPM queue lock unless   |
         | otherwise noted for the individual fields.               |
         | Use HCPLKSXQ/HCPULSXQ to obtain/release the lock.        |
    0618 1560 Signed       8 RSASXQLK (6)   SXSPM queue lock. This lock is
                                            obtained & released via macros
                                            HCPLKSXQ and HCPULSXQ.
          SXS pages may or may not be on one of the queues that the
          SXS page manager maintains.
                            |     SXSTE state indicators:         |
           where queued:    | SXSAVAIL  |  SXSBACKD  |  an alias  |
                            |-----------|------------|------------|
          Avail, backed <2G |     1     |     1      |     no     |
          Avail, backed >2G |     1     |     1      |     no     |
          Avail, unbacked   |     1     |     0      |     no     |
          Potentially Steal.|     0     |     1      |    yes     |
          not in SXS queue  |     0     |     1      |    yes     |
          not in SXS queue  |     0     |     1      |     no     |
          (invalid state)   |     0     |     0      |    N/A     |
          (invalid state)   |    N/A    |     0      |    yes     |
          (invalid state)   |     1     |    N/A     |    yes     |
                            |******************************-------|
          An alias is an SXS page associated with a "pageable FRMTE".
          All available SXS pages must be on one of the queues. If
          the page is not backed it is on the Available, Unbacked SXS
          Page Queue. If it is backed it is on one of the Available,
          Backed SXS Page Queues (backed >2G or backed <2G). The one
          exception to this rule is for SXSTEs in the Transitory
          which are in transition between states. See HCPSXSTE COPY
          for details regarding SXSTE states and serialization rules.
          All in use SXS pages not associated with a "pageable FRMTE"
          will be dequeued; i.e. not on any SXS page mgr queue.
          All SXS pages which are associated with "pageable FRMTEs"
          but are not locked will be kept on the SXS Potentially
          Stealable Page Queue.
          All SXS pages which are associated with "pageable FRMTEs"
          and are locked may or may not be on the SXS Potentially
          Stealable Page Queue. They are initially left on the queue
          but are dequeued if the SXS page manager comes across them
          when looking for an available page on the Potentially
          Stealable Page Queue.
          If SXSBACKD is not on, then SXSAVAIL must be on. If an
          SXS page is in use as an alias, SXSBACKD must be set.
                     SXS Available, Unbacked Page Queue
                            a.k.a SXS Page Queue
    0648 1608 Dbl-Word     8 RSASXQAN (0)   SXS Available, Unbacked Page
                                            Queue Anchor. It consists of
                                            forward and backward pointers to
                                            the list of SXSTEs for SXS pages
                                            that are available and not
                                            backed. This area is initialized
                                            during system initialization and
                                            updated only when the SXSPM queue
                                            lock is held.
    0648 1608 Address      8 RSASXQFP       SXS page queue forward pointer.
                                            Points to a SXSTE. This is a host
                                            logical address > 2G unless
                                            the queue is empty.
    0650 1616 Address      8 RSASXQBP       SXS page queue backward pointer.
                                            Points to a SXSTE. This is a host
                                            logical address > 2G unless
                                            the queue is empty.
    0658 1624 Signed       4 RSASXQCT       Count of SXS pages on the SXS
                                            page queue. This represents the
                                            total number of SXS pages that
                                            are available and not backed.
    065C 1628 Signed       4 RSASXQMN       Minimum number of pages on the
                                            available, unbacked page queue
                                            before triggering replenishment.
                     SXS Potentially Stealable Page Queue
    0660 1632 Dbl-Word     8 RSASXPAN (0)   SXS Potentially Stealable Page
                                            Queue Anchor. It consists of
                                            forward and backward pointers to
                                            the list of SXSTEs for SXS pages
                                            that are in use as aliases and
                                            are potentially stealable. This
                                            queue is initially empty and
                                            SXSTEs are added to it during
                                            Create Alias processing. This
                                            queue is only updated when the
                                            SXSPM queue lock is held.
    0660 1632 Address      8 RSASXPFP       SXS Potentially Stealable Page
                                            Queue forward pointer which
                                            points to a SXSTE. This is a host
                                            logical address > 2G unless
                                            the queue is empty.
    0668 1640 Address      8 RSASXPBP       SXS Potentially Stealable Page
                                            Queue backward pointer which
                                            points to a SXSTE. This is a host
                                            logical address > 2G unless
                                            the queue is empty.
    0670 1648 Signed       4 RSASXPCT       Count of SXS pages on the SXS
                                            Potentially Stealable Page Queue.
    0674 1652 Signed       4 *              Reserved for IBM use.
              Queues of Available SXS Pages With Backing Frames
          Only SXSTEs with SXSAVAIL=1, SXSBACKD=1 which are not in
          use are on these queues and all available, backed SXSTEs
          must be on one of the queues unless it is in transition
          to or from another state. If they are in the Transitory
          state then SXSONQUE will be off.
          Which of the queues the SXSTE is on depends on whether the
          backing frame resides above or below 2G in real storage.
    0678 1656 Dbl-Word     8 RSASXAAN (0)   Anchor for queue of available SXS
                                            pages backed Above 2G.
    0678 1656 Address      8 RSASXAFP       Forward pointer for available SXS
                                            pages backed Above 2G. This is a
                                            host logical address >2G
                                            unless the queue is empty.
    0680 1664 Address      8 RSASXABP       Backward pointer for available
                                            SXS pages backed Above 2G. This
                                            is a host logical address >2G
                                            unless the queue is empty.
    0688 1672 Signed       4 RSASXACT       Count of SXS pages on the queue
                                            of SXS pages backed Above 2G.
    068C 1676 Signed       4 RSASXAMX       Maximum number of pages on the
                                            backed Above 2G queue. Note:
                                            Field must be positive.
    0690 1680 Dbl-Word     8 RSASXBAN (0)   Anchor for queue of available SXS
                                            pages backed Below 2G.
    0690 1680 Address      8 RSASXBFP       Forward pointer for available SXS
                                            pages backed Below 2G. This is a
                                            host logical address >2G
                                            unless the queue is empty.
    0698 1688 Address      8 RSASXBBP       Backward pointer for available
                                            SXS pages backed Below 2G. This
                                            is a host logical address >2G
                                            unless the queue is empty.
    06A0 1696 Signed       4 RSASXBCT       Count of SXS pages on the queue
                                            of SXS pages backed Below 2G.
    06A4 1700 Signed       4 RSASXBMX       Maximum number of pages on the
                                            backed Below 2G queue. Note:
                                            Field must be positive.
                    SXS Page Request Defer Queue data
    06A8 1704 Dbl-Word     8 RSASXDAN (0)   SXS page request defer anchor.
    06A8 1704 Address      4 RSASXDFP       Defer queue forward pointer. It
                                            is a host logical CPEBK address
                                            unless the queue is empty.
    06AC 1708 Address      4 RSASXDBP       Defer queue backward pointer. It
                                            is a host logical CPEBK address
                                            unless the queue is empty.
    06B0 1712 Signed       4 RSASXDCT       Count deferred SXS page requests
                                            that are waiting for an available
                                            SXS page. This is the sum
                                            RSASXDCA+RSASXDPB+RSASXDPA.
    06B4 1716 Signed       4 RSASXDCA       Count deferred SXS page requests
                                            that are waiting for an available
                                            SXS page for an alias. This is a
                                            subset of RSASXDCT.
    06B8 1720 Signed       4 RSASXDPB       Count deferred SXS page requests
                                            that are waiting for an SXS page
                                            to satisfy a request for a page
                                            backed <2G. This is a subset
                                            of RSASXDCT.
    06BC 1724 Signed       4 RSASXDPA       Count deferred SXS page requests
                                            that are waiting for an SXS page
                                            to satisfy a request for a page
                                            with backing=ANY. This is a
                                            subset of RSASXDCT.
    06C0 1728 Signed       4 RSASXRDA       Count of times an attempt was
                                            made to redrive tasks waiting for
                                            an available SXS page.
    06C4 1732 Signed       4 RSASXRDC       Count of individual task redrives
                                            for tasks waiting for a page.
                             SXS Page Counts
          These counts only include SXS pages managed by the page
          manager using the SXS page management table (SXSTEs). This
          does not include the SXS pages used for the frame table or
          the SXS page management table itself. The total managed
          SXS pages is SYSSXSSZ/x'1000' and set at initialization or
          by the dynamic storage reconfiguration function.
          All managed SXS pages are:
          - backed or not backed
          - available or in use, unless in the Transitory state.
          All backed SXS pages are:
          - backed below 2G or backed above 2G. Backed pages may be
            in use or available. Available backed pages will be on
            one of the available SXS page queues. In use SXS pages
            may or may not be on the SXS Potentially Stealable Queue.
            Backed pages may be in the Transitory state temporarily
            while being converted between the in-use and available
            states.
          All available SXS pages are:
          - not backed, backed <2G, or backed >2G. Each of these
            types of available pages are on different queues.
          All in use SXS pages:
          - must be backed
          - are aliases or CP type SXS pages (eg. HCPGETST PAGES=)
          All in use CP type SXS pages are:
          - permanently allocated at initialization, by the dynamic
            storage reconfiguration function, or allocated
            later using HCPGETST PAGES= or for free storage using
            HCPSXPFS.
          Some pages considered in use may be made available by
          stealing. This applies to SXS alias pages for translated
          pageable frames if the page is not last translated or
          locked. All pages in the stealable state will be on the
          Potentially Stealable Queue, but not all pages on the
          Potentially Stealable Queue will be stealable. See HCPSXSTE
          COPY for a discussion of rules for stealing Aliases.
    06C8 1736 Signed       4 RSASXAVL       Count of available SXS pages
                                            including those with backing
                                            frames. The number of available
                                            SXS pages without backing frames
                                            is RSASXAVL-(RSASXACT+RSASXBCT)
                                            which is also RSASXQCT. Does not
                                            include Transitory state SXSTEs.
    06CC 1740 Signed       4 RSASXUSD       Count of SXS pages in use as CP
                                            pages or aliases including
                                            no-owned aliases and SXS pages
                                            assigned to tasks deferred on
                                            frames in the real frame manager.
                                            This value should match
                                            ((SYSSXSZ/x'1000')-RSASXAVL).
    06D0 1744 Signed       4 RSASXUCP       Count of SXS pages in use as CP
                                            pages. This includes free
                                            storage, HCPGETST PAGES=, and
                                            permanently allocated at
                                            initialization.
    06D4 1748 Signed       4 RSASXUID       Count of all ID-mapped SXS pages
                                            (host logical = host real addr)
                                            primarily CP nucleus and PFXPGS.
    06D8 1752 Signed       4 RSASXUFS       Count of SXS pages in use as free
                                            storage pages with backing frames
                                            below 2G. These are SXSTEs with
                                            SXSCSB0=x'61'.
    06DC 1756 Signed       4 RSASXUFG       Count of SXS pages in use as free
                                            storage pages with backing frames
                                            above 2G. These are SXSTEs with
                                            SXSCSB0=x'61'.
    06E0 1760 Signed       4 RSASXUOT       Count of pages of other CP types:
                                            (RSASXUCP-(RSASXUID+RSASXUFS
                                            +RSASXUFG).
    06E4 1764 Signed       4 RSASXBKA       Count of SXS pages backed above
                                            2G. This includes RSASXACT as
                                            well as in use SXS pages and
                                            Transitory SXSTEs backed>2G.
    06E8 1768 Signed       4 RSASXBKB       Count of SXS pages backed below
                                            2G. This includes RSASXBCT as
                                            well as in use SXS pages and
                                            Transitory SXSTEs backed<2G.
    06EC 1772 Signed       4 RSASXALI       Count of SXS alias pages
                                            associated with "pageable FRMTEs"
                                            and may be stealable if not last
                                            translated or locked. Also
                                            includes count of no-owned
                                            SXSTEs.
    06F0 1776 Signed       4 RSASXNOP       Count of no-owned SXS aliases.
    06F4 1780 Signed       4 RSASXCTG       Count of SXS pages in use as part
                                            of a contiguous page request from
                                            HCPGETST with PAGES>1. This
                                            count does not include the pages
                                            that were pre-allocated as part
                                            of storage initialization.
          The following fields are not serialized by RSASXQLK.
    06F8 1784 Signed       4 RSASXDFA       Count of SXS page requests
                                            deferred in the real frame
                                            manager for ANY backing frame.
                                            Since only requests for single
                                            pages can defer, this is also the
                                            count of pages associated with
                                            those deferred tasks. It is also
                                            the count of frames needed. A
                                            Transitory SXSTE exists for each
                                            deferred frame request. This
                                            count is serialized by CS.
    06FC 1788 Signed       4 RSASXDFB       Count of SXS pages requests
                                            deferred in the real frame
                                            manager for a frame below 2G.
                                            Since only requests for single
                                            pages can defer, this is also the
                                            count of pages associated with
                                            those deferred tasks. It is also
                                            the count of frames needed. A
                                            Transitory SXSTE exists for each
                                            deferred frame request. This
                                            count is serialized by CS.
    0700 1792 Signed       4 RSASXCLA       Count of locked SXS alias pages
                                            locked by HCPTRANS or command.
                                            Updated in HCPTRANS processor,
                                            not updated by SXS page mgr.
                                            Serialized by Compare-and-Swap.
    0704 1796 Signed       4 RSASXCPL       Count of SXS alias pages locked
                                            by the CP LOCK command. Updated
                                            in the LOCK command processor,
                                            not updated by SXS page mgr. This
                                            is a subset of RSASXCLA.
                                            Serialized by Compare-and-Swap.
    0708 1800 Signed       4 *              Reserved for IBM use.
               Miscellaneous SXS Page Manager Fields.
    070C 1804 Signed       4 RSASXLOK       SXSPM redrive process lockword.
                                            Word used to ensure the SXSPM
                                            request redrive routine is only
                                            invoked by the dispatcher on one
                                            processor at a time. This word
                                            can be in any of the following
                                            states as defined in HCPEQUAT:
                                            DSPNOBFW - no work to do DSPFSCHD
                                            - foreground scheduled DSPFACTV -
                                            foreground active DSPBSCHD -
                                            background scheduled DSPBACTV -
                                            background active Serialized by
                                            compare-and-swap
    0710 1808 Dbl-Word     8 RSASXFLGS      SXS status flag bits
    0718 1816 Address      8 RSASXSTO       SXS Segment Table Origin for the
                                            segment table that maps the SXS
                                            storage from 0 to SYSSXSSZ. This
                                            is the only section of the SXS
                                            that has PTEs that are updated
                                            after initialization. Because the
                                            entire address range from 0 to
                                            SYSSXSSZ can currently be mapped
                                            by a single segment table, this
                                            STO is used in HCPSXA and HCPSXP
                                            instead of starting at the ASCE
                                            to walk the DAT tables. Starting
                                            at the segment table also depends
                                            on the fact that the segment
                                            table is permanently allocated
                                            during initialization. This field
                                            is set at initialization and
                                            never changes.
    0720 1824 Signed       4 RSASXQRA       Replenishment Amount - number of
                                            SXS pages to add to available,
                                            unbacked SXS page queue each time
                                            it is replenished. Must be a
                                            multiple of RSASXQBS.
    0724 1828 Signed       4 RSASXRPM       The minimum number of pages on
                                            the available, unbacked SXS page
                                            queue at the completion of the
                                            replenishment routine since the
                                            system was IPLed.
    0728 1832 Signed       4 RSASXRFC       Redrive Failure Count. The number
                                            of consecutive times HCPSXARR ran
                                            and the reserved page list was
                                            depleted or there were deferred
                                            requests but HCPSXARR could not
                                            satisfy any of them. This count
                                            is used by HCPSXARR to determine
                                            when to give up (SXA004 abend).
    072C 1836 Signed       4 *              Reserved for IBM use.
                  End of SXS page manager data area
    0730 1840 Signed       4 RSAFOBCT       Count of FCP Operation Blocks
                                            (FOBs) that are currently in the
                                            system. This includes all FOBs
                                            that are on processor local
                                            Available lists as well as those
                                            that are currently in use.
    0734 1844 Signed       4 *              RESERVED FOR IBM USE
         |        Cleared Available List Data:                      |
    0738 1848 Dbl-Word     8 RSACALAN (0)
    0738 1848 Signed       8 RSACALFP       Forward Pointer: Host Logical
                                            Address of the first FRMTE on the
                                            Cleared Available List.
    0740 1856 Signed       8 RSACALBP       Backward Pointer: Host Logical
                                            Address of the last FRMTE on the
                                            Cleared Available List.
    0748 1864 Signed       8 RSACALCT       Non-negative count of the total
                                            number of FRMTEs on the Cleared
                                            Available List.
    0750 1872 Address      8 RSACALUT       Upper Threshold: Non-negative
                                            target number of FRMTEs for the
                                            background replenishment task to
                                            have on the Cleared Available
                                            List. Note: As currently
                                            implemented, this field can
                                            really only be a value that can
                                            be represented with 31 bits.
              00000020       RSAINITU       32 Initial, increment, and
                                            decrement value for RSACALUT.
    0758 1880 Address      8 RSACALMT       Middle Threshold: Non-negative
                                            target number of FRMTEs for the
                                            foreground replenishment task to
                                            have on the Cleared Available
                                            List. Note that we do not want to
                                            fill to the Upper Threshold in
                                            the foreground because this might
                                            take too long and we'd rather
                                            have the replenishment done in
                                            the background if possible. Note:
                                            As currently implemented, this
                                            field can really only be a value
                                            that can be represented with 31
                                            bits.
              00000008       RSAINITM       8 Initial, increment, and
                                            decrement value for RSACALMT.
    0760 1888 Address      8 RSACALLT       Lower Threshold: Non-negative
                                            number of FRMTEs on the Cleared
                                            Available List below which the
                                            Dispatcher must call a foreground
                                            replenishment task since the
                                            background task is not being
                                            called frequently enough to keep
                                            the list at a sufficient level.
                                            Note: As currently implemented,
                                            this field can really only be a
                                            value that can be represented
                                            with 31 bits.
              00000004       RSAINITL       4 Initial, increment, and
                                            decrement value for RSACALLT.
    0768 1896 Signed       8 RSACALLK (6)   Spin-lock word to control access
                                            to the Cleared Available List.
    0798 1944 Signed       4 RSARCLOK       Word used to ensure the list
                                            replenishment routine is only
                                            invoked by the dispatcher on one
                                            processor at a time. This ensures
                                            only one of the background or
                                            foreground replenishment tasks
                                            are running at a time. This word
                                            can be in any of the following
                                            states as defined in HCPEQUAT:
                                            DSPNOBFW - no work to do DSPFSCHD
                                            - foreground scheduled DSPFACTV -
                                            foreground active DSPBSCHD -
                                            background scheduled DSPBACTV -
                                            background active Serialized by
                                            compare-and-swap
    079C 1948 Signed       4 *              Reserved for IBM use
           End of Cleared Available List Data Area
         |  Anti-Aliasing data area                                 |
          NOTES      : When HCPISGTP decides that the storage configuration
                supports anti-aliasing it will turn on RSAAAON,
                initialize RSAAAPFX to be the top half megabyte of
                lowest online range of storage, and set RSAAASXS to
                the value to use for SYSSXSSZ. When RSAAAON is set
                frame table and SXSTB initialization will use the
                alternate origins specified in RSAAAFTO and RSAAASTO,
                respectively.
    07A0 1952 Signed       4 RSAAAFLG (0)   Anti-aliasing status flags
    07A0 1952 Bitstring    3 *              RESERVED
    07A3 1955 Bitstring    1 RSAAASTA       Anti-Aliasing status
              1... ....      RSAAAON        X'80' RSAAAON ON = Anti-aliasing
                                            is active
    07A4 1956 Signed       4 RSAAAPFX       Alternate processor PFXPG table
                                            origin when using anti-aliasing.
    07A8 1960 Dbl-Word     8 RSAAASXS (0)   Anti-aliasing SYSSXSSZ value.
    07A8 1960 Bitstring    8 *              DEFAULT VALUE TO USE WHEN
                                            ANTI-ALIASING IS ON, AND
                                            SYSGTORS=8G-1 OR SYSGTORS=2G-1,
                                            AND SYSSXSSZ WAS NOT REDUCED BY
                                            USE OF A REGULATOR RANGE.
    07B0 1968 Dbl-Word     8 RSAAAFTO (0)   Frame Table Origin when using
    07B0 1968 Bitstring    8 *              ANTI-ALIASING. (5G-112M)
    07B8 1976 Dbl-Word     8 RSAAASTO (0)   SXSTB Origin when using
    07B8 1976 Bitstring    8 *              ANTI-ALIASING. (2T+1G-32M)
         |  Emergency PGMBK allocation section                      |
          NOTES      :
                If HCPPPIGF attempts to obtain a PGMBK but fails
                too many times, an emergency PGMBK will be allocated
                from this queue.
    07C0 1984 Dbl-Word     8 * (0)          Alignment
    07C0 1984 Bitstring    1 RSAemTS        Test-and-Set controls access to
                                            these next fields
    07C1 1985 Bitstring    1 RSAemFL        Emergency PGMBK pool flags
              .... 1...      RSAemRP        X'08' RSAemRP Replenishment
                                            required
    07C2 1986 Bitstring    1 * (2)          Reserved for IBM use
    07C4 1988 Signed       4 RSAemERG       Count of all attempts to get an
                                            emergency PGMBK, including when
                                            the pool was empty. May wrap.
    07C8 1992 Address      8 RSAemFMT       A(FRMTE that starts the queue)
    07D0 2000 Signed       4 RSAemCPc       Count of emergency PGMBKs. Number
                                            of frames is equal to RSAemCPc *
                                            2
    07D4 2004 Signed       4 RSAemDFR       Count of deferrals of guests. May
                                            wrap.
    07D8 2008 Signed       4 RSAemBLO       Count of times when the pool
                                            dipped below RSAemLO. May wrap.
    07DC 2012 Signed       4 RSAemPTY       Count of times the pool was
                                            empty. May wrap.
    07E0 2016 Address      4 RSAemCPq       A(deferred CPEBK queue)
    07E4 2020 Address      4 RSAemRPT       A(replenishment task CPEBK)
          End of fields controlled by RSAemTS.
    07E8 2024 Signed       4 RSAemLO        Lo threshold. Updated only under
                                            the VARY PROCESSOR lock. Computed
                                            value is PGMBKperPROC * #online
                                            processors
    07EC 2028 Signed       4 RSAemHI        Hi threshold. Updated only under
                                            the VARY PROCESSOR lock.
         |        Demand Scan Steal Counts:                         |
          NOTES      : These fields are arranged in blocks of four related
                fields corresponding to the PLSBK fields.
                For example, given the PLSBK field PLSLTDP1 there
                are four fields here that contain the counts of
                singles <2G, singles >2G, contigs <2G, and contigs
                >2G. The order of the fields in each set of four
                is important because the code that updates them
                assumes they are in sequential words in storage.
          Updates to these fields are serialized by RSADSLOK.
    07F0 2032 Signed       4 RSALTDB1       Stolen B2G LT Dorm P1
    07F4 2036 Signed       4 RSALTDA1       Stolen A2G LT Dorm P1
    07F8 2040 Signed       4 RSALTDD1       Stolen contig B2G LT Dorm P1
    07FC 2044 Signed       4 RSALTDC1       Stolen contig A2G LT Dorm P1
    0800 2048 Signed       4 RSALTDB2       Stolen B2G LT Dorm P2
    0804 2052 Signed       4 RSALTDA2       Stolen A2G LT Dorm P2
    0808 2056 Signed       4 RSALTDD2       Stolen contig B2G LT Dorm P2
    080C 2060 Signed       4 RSALTDC2       Stolen contig A2G LT Dorm P2
    0810 2064 Signed       4 RSALTDBE       Stolen B2G LT Dorm EP
    0814 2068 Signed       4 RSALTDAE       Stolen A2G LT Dorm EP
    0818 2072 Signed       4 RSALTDDE       Stolen contig B2G LT Dorm EP
    081C 2076 Signed       4 RSALTDCE       Stolen contig A2G LT Dorm EP
    0820 2080 Signed       4 RSADRMB1       Stolen B2G Dorm P1
    0824 2084 Signed       4 RSADRMA1       Stolen A2G Dorm P1
    0828 2088 Signed       4 RSADRMD1       Stolen contig B2G Dorm P1
    082C 2092 Signed       4 RSADRMC1       Stolen contig A2G Dorm P1
    0830 2096 Signed       4 RSADRMB2       Stolen B2G Dorm P2
    0834 2100 Signed       4 RSADRMA2       Stolen A2G Dorm P2
    0838 2104 Signed       4 RSADRMD2       Stolen contig B2G Dorm P2
    083C 2108 Signed       4 RSADRMC2       Stolen contig A2G Dorm P2
    0840 2112 Signed       4 RSADRMBE       Stolen B2G Dorm EP
    0844 2116 Signed       4 RSADRMAE       Stolen A2G Dorm EP
    0848 2120 Signed       4 RSADRMDE       Stolen contig B2G Dorm EP
    084C 2124 Signed       4 RSADRMCE       Stolen contig A2G Dorm EP
    0850 2128 Signed       4 RSAELGB1       Stolen B2G Elig P1
    0854 2132 Signed       4 RSAELGA1       Stolen A2G Elig P1
    0858 2136 Signed       4 RSAELGD1       Stolen contig B2G Elig P1
    085C 2140 Signed       4 RSAELGC1       Stolen contig A2G Elig P1
    0860 2144 Signed       4 RSAELGB2       Stolen B2G Elig P2
    0864 2148 Signed       4 RSAELGA2       Stolen A2G Elig P2
    0868 2152 Signed       4 RSAELGD2       Stolen contig B2G Elig P2
    086C 2156 Signed       4 RSAELGC2       Stolen contig A2G Elig P2
    0870 2160 Signed       4 RSAELGBE       Stolen B2G Elig EP
    0874 2164 Signed       4 RSAELGAE       Stolen A2G Elig EP
    0878 2168 Signed       4 RSAELGDE       Stolen contig B2G Elig EP
    087C 2172 Signed       4 RSAELGCE       Stolen contig A2G Elig EP
    0880 2176 Signed       4 RSADSPB1       Stolen B2G Disp P1
    0884 2180 Signed       4 RSADSPA1       Stolen A2G Disp P1
    0888 2184 Signed       4 RSADSPD1       Stolen contig B2G Disp P1
    088C 2188 Signed       4 RSADSPC1       Stolen contig A2G Disp P1
    0890 2192 Signed       4 RSADSPB2       Stolen B2G Disp P2
    0894 2196 Signed       4 RSADSPA2       Stolen A2G Disp P2
    0898 2200 Signed       4 RSADSPD2       Stolen contig B2G Disp P2
    089C 2204 Signed       4 RSADSPC2       Stolen contig A2G Disp P2
    08A0 2208 Signed       4 RSADSPBE       Stolen B2G Disp EP
    08A4 2212 Signed       4 RSADSPAE       Stolen A2G Disp EP
    08A8 2216 Signed       4 RSADSPDE       Stolen contig B2G Disp EP
    08AC 2220 Signed       4 RSADSPCE       Stolen contig A2G Disp EP
    08B0 2224 Signed       4 RSASHRB1       Stolen B2G Shared P1
    08B4 2228 Signed       4 RSASHRA1       Stolen A2G Shared P1
    08B8 2232 Signed       4 RSASHRD1       Stolen contig B2G Shared P1
    08BC 2236 Signed       4 RSASHRC1       Stolen contig A2G Shared P1
    08C0 2240 Signed       4 RSASHRB2       Stolen B2G Shared P2
    08C4 2244 Signed       4 RSASHRA2       Stolen A2G Shared P2
    08C8 2248 Signed       4 RSASHRD2       Stolen contig B2G Shared P2
    08CC 2252 Signed       4 RSASHRC2       Stolen contig A2G Shared P2
    08D0 2256 Signed       4 RSASHRBE       Stolen B2G Shared EP
    08D4 2260 Signed       4 RSASHRAE       Stolen A2G Shared EP
    08D8 2264 Signed       4 RSASHRDE       Stolen contig B2G Shared EP
    08DC 2268 Signed       4 RSASHRCE       Stolen contig A2G Shared EP
         |        Available List Floor Constants                    |
    08E0 2272 Signed       4 RSAAVLFT       <2G Singles list Floor
    08E4 2276 Signed       4 RSAAVCFT       <2G Contigs list Floor
    08E8 2280 Signed       4 RSAAVLFG       >2G Singles list Floor
    08EC 2284 Signed       4 RSAAVCFG       >2G Contigs list Floor
         |        Demand Scan 'unsatisfied' counts                  |
    08F0 2288 Signed       4 RSADSCD0       <2G Singles unsatisfied count
    08F4 2292 Signed       4 RSADSCDG       >2G Singles unsatisfied count
    08F8 2296 Signed       4 RSADSCC0       <2G Contigs unsatisfied count
    08FC 2300 Signed       4 RSADSCCG       >2G Contigs unsatisfied count
    0900 2304 Signed       4 RSAPGMQ1       Count of times Demand Scan PGBMK
                                            steal had to quit early because
                                            paging capacity overrun during
                                            Pass 1
    0904 2308 Signed       4 RSAPGMQ2       Count of times Demand Scan PGBMK
                                            steal had to quit early because
                                            paging capacity overrun during
                                            Pass 2
    0908 2312 Signed       4 RSAPGMQE       Count of times Demand Scan PGBMK
                                            steal had to quit early because
                                            paging capacity overrun during
                                            Emergency Pass
    090C 2316 Signed       4 *              Reserved for IBM
         |        Turnover Rate Balancing Multipliers               |
         |                                                          |
         | Notes      :                                                   |
         |  - RSATURN0 = ROUND(RSATURBS*uB2G/(uB2G+uA2G))           |
         |    where uB2G is the count of usable frames <2G and      |
         |    and uA2B is the count of usable frames >2G.           |
         |  - RSATURNG is calculated as 4096-RSATURN0.              |
         |  - A 10G system might have values of RSATURN0=820 and    |
         |    RSATURNG=3276 while a 512G system might have values   |
         |    of RSATURN0=16 and RSATURNG=4080.                     |
         |  - The memory size is very significant in calculating    |
         |    the multipliers, but the actual values will differ    |
         |    depending on the relative proportion of memory in     |
         |    each pool which is usable.                            |
         |  - the equates below are added to simplify experiments.  |
         |    For example:                                          |
         |    - to test with the Turnover Rate Balancing Algorithm  |
         |      disabled, set RSATURBS=4096 and RSATURMN=2048.      |
         |    - to test with the Turnover Rate Balancing Algorithm  |
         |      cap removed instead of being softened as was done   |
         |      by VM64349, set RSATURBS=100 and RSATURMN=0.        |
         |                                                          |
         | RSATURN0 and RSATURNG should be considered a unit.       |
         | They should be changed by a single block concurrent      |
         | instruction, and should be fetched similarly.            |
    0910 2320 Dbl-Word     8 * (0)          RSATURN0 & RSATURNG in this Dword
    0910 2320 Signed       4 RSATURN0       <2G Turnover Rate Multiplier
    0914 2324 Signed       4 RSATURNG       >2G Turnover Rate Multiplier
              RSATURNG       RSATURBS       4096 RSATURBS Basis for
                                            proportion used for the Turnover
                                            Rate Balancing Multiplier
                                            calculations.
              .... ...1      RSATURMN       1 RSATURMN Minimum RSATURNx value
              RSATURNG       RSATURMX       RSATURBS-RSATURMN RSATURMX
                                            Maximum RSATURNx value
              .... ..11      RSATURHD       3 RSATURHD Minimum HT-LT distance
                                            used when applying turnover rate
                                            balancing.
         |        PGMBK Steal Performance Indicators                |
          Updates to these fields are serialized by RSADSLOK.
    0918 2328 Dbl-Word     8 RSAVGPST       Average time spent (in TOD units)
                                            in PGMBK Steal per PGMBK
         |        Reset interval data area:                         |
    0470 1136 Address      4 RSARESLK       Reset interval data area lock
                                            This field is updated using
                                            Compare-and-Swap logic.
    0474 1140 Signed       4 *              Reserved for IBM use
    0478 1144 Signed       4 RSAALLTA       Total number of frames taken by
                                            the available list replenishment
                                            functions since System IPL. This
                                            count is updated using
                                            Compare-and-Swap logic.
    047C 1148 Signed       4 RSAAVGDU       Average number of users in the
                                            dispatch list (samples taken by
                                            HCPALURS). This count is updated
                                            only when the reset interval data
                                            area lock (RSARESLK) is held.
    0480 1152 Signed       4 RSAAVGRT       Average number of frames taken by
                                            the available list replenishment
                                            functions per second. This count
                                            is updated only when the reset
                                            interval data area lock
                                            (RSARESLK) is held.
    0484 1156 Signed       4 RSAOLDTA       Total number of frames taken by
                                            the available list replenishment
                                            functions at the time of the last
                                            reset interval calculation. This
                                            count is updated only when the
                                            reset interval data area lock
                                            (RSARESLK) is held.
    0488 1160 Dbl-Word     8 * (0)
    0488 1160 Signed       8 RSAOLDTD       TOD at the time of the last reset
                                            interval calculation. This count
                                            is updated only when the reset
                                            interval data area lock
                                            (RSARESLK) is held.
    0490 1168 Dbl-Word     8 * (0)
    0490 1168 Signed       8 RSARESSA       Reset interval for shared address
                                            spaces in TOD units This count is
                                            updated only when the reset
                                            interval data area lock
                                            (RSARESLK) is held or at
                                            initialization time.
         |                   SXS status flag bits                   |
    0710 1808 Bitstring    5 *              Reserved
    0715 1813 Bitstring    1 RSASXINI       SXSPM initialization flags.
              1... ....      RSASXIMX       X'80' RSASXIMX When set indicates
                                            the maximum available, backed
                                            page queue size values are set to
                                            values used during
                                            initialization. The values get
                                            reset after seeing SYSSINIT is
                                            off.
    0716 1814 Bitstring    1 RSASXREP       SXSPM queue replenishment flags
              1... ....      RSASXRPF       X'80' RSASXRPF Replenishment
                                            failed to steal any aliases the
                                            last time it ran.
              .1.. ....      RSASXRPL       X'40' RSASXRPL Replenishment
                                            stole less aliases than
                                            replenishment amt (RSASXQRA)
    0717 1815 Bitstring    1 RSASXPQS       Potentially stealable queue
                                            status bits
              1... ....      RSASXNST       X'80' ON = SX Page Mgr is
                                            prohibited from using the
                                            stealable queue (RSASXPAN) for
                                            anything other than free storage.
                                            Turned on by HCPSXPFS only
         |        Frame Table Extent Block data:                    |
              00000020       FTXSIZED       4*8 FTXBK is 4 dwords
          The following two pre-allocated FTXBKs are mapped by the
          FTXBK DSECT in HCPFTXBK COPY and must be kept consistent if
          changes are made to either HCPRSMBK or HCPFTXBK.
          All fields are serialized by the FTXBK spin lock (RSAFTXLK)
          <2G Frame Table Extent Block
    0920 2336 Dbl-Word     8 RSAFTXBL (0)
    0920 2336 Dbl-Word     8 * (32)
    0920 2336 Address      4 *              Next FTXBK address
    0924 2340 Address      4 *              Previous FTXBK address
    0928 2344 Address      8 RSAFTSSL       Host Logical Address of FRMTE at
                                            which to start frame table scan
                                            for frames < 2G FTXSTART=0
                                            means FTXBK not in use
    0930 2352 Address      8 RSAFTSEL       Host Logical Address of FRMTE at
                                            which to end frame table scan for
                                            frames < 2G
          >2G Frame Table Extent Block
    0A20 2592 Dbl-Word     8 RSAFTXBG (0)
    0A20 2592 Dbl-Word     8 * (32)
    0A20 2592 Address      4 *              Next FTXBK address
    0A24 2596 Address      4 *              Previous FTXBK address
    0A28 2600 Address      8 RSAFTSSG       Host Logical Address of FRMTE at
                                            which to start frame table scan
                                            for frames >= 2G FTXSTART=0
                                            means FTXBK not in use
    0A30 2608 Address      8 RSAFTSEG       Host Logical Address of FRMTE at
                                            which to end frame table scan for
                                            frames >= 2G
    0B20 2848 Signed       8 RSAFTXLK (6)   FTXBK chain spin lock
                  End of Frame Table Extent Block data
                  End of RSM common area
                  Start of RSM Dynamic Memory Upgrade work area
           This area will be used to accumulate the changes to be
           applied once all the new frames, lists, counts, and
           whatever else is affected by the SET STORAGE command
           have been prepared.
          Definitions for fields that are not part of the
          real RSMBK common area
    0B50 2896 Signed       8 rsaPFXFTLEN    Length of frame table
    0B58 2904 Signed       8 rsaPFXSTLEN    SXSTB size
    0B60 2912 Bitstring    1 rsaPFXGPFLG    General purpose flag PFX2GU -
                                            usable storage exists >2G
                                            (flag)
    0B61 2913 Bitstring    1 rsaVMDLOWW0    work bit VMDINI2G - >2G frame
                                            initialization required
    0B68 2920 Signed       8 rsaSYSGTORS    - new SYSGTORS
    0B70 2928 Signed       8 rsaSYSSXSSZ    - new SYSSXSSZ
    0B78 2936 Signed       8 *              - Reserved for IBM use.
    0B80 2944 Signed       4 rsaSYSTORS     - new SYSTORS
                  End of RSM Dynamic Memory Upgrade work area
                  Size of work RSM for Dynamic Memory Upgrade
              00000171       RSASZD         (*-RSMBK+7)/8 Size in D-words

    RSAAVNKR Storage Layout

    *** RSAAVNKR - RSM common area mapping
    *
    *     +-------------------------------------------------------+
    *   0 |                       RSAAVFP                         |
    *     +-------------------------------------------------------+
    *   8 |                       RSAAVBP                         |
    *     +-------------------------------------------------------+
    *  10 |                       RSAAVCT                         |
    *     +-------------------------------------------------------+
    *  18
    *
    *** RSAAVNKR - RSM common area mapping

    *** RSMANCHR - RSM common area mapping
    *
    *     +-------------------------------------------------------+
    *   0 |                       RSMFRCHN                        |
    *     +-------------------------------------------------------+
    *   8 |                       RSMFRCNT                        |
    *     +-------------------------------------------------------+
    *  10
    *
    *** RSMANCHR - RSM common area mapping

    *** RSMBK - RSM common area mapping
    *
    *     +---------------------------+---------------------------+
    *   0 |         RSASAVFR          |         RSARSAST          |
    *     +---------------------------+---------------------------+
    *   8 |         RSAMSARC          |         RSAMSASC          |
    *     +---------------------------+---------------------------+
    *  10 |         RSAMSARH          |         RSADPACP          |
    *     +---------------------------+---------------------------+
    *  18 |         RSATRSAV          |         RSASTORE          |
    *     +---------------------------+---------------------------+
    *  20 |         RSAPFXAF          |         RSAPFXND          |
    *     +------+------+------+------+---------------------------+
    *  28 |:TSKB0|:TSKB1|:TSKB2|:TSKB3|         RSADPAAD          |
    *     +------+------+------+------+---------------------------+
    *  30 |                       RSAFNOTI                        |
    *     +-------------------------------------------------------+
    *  38 |                       RSALGFRM                        |
    *     +-------------------------------------------------------+
    *  40 |                       RSAGOFFL                        |
    *     +-------------------------------------------------------+
    *  48 |                       RSAGSTOR                        |
    *     +-------------------------------------------------------+
    *  50 |                       RSASTORL                        |
    *     +-------------------------------------------------------+
    *  58 |                       RSALG1ST                        |
    *     +-------------------------------------------------------+
    *  60 |                       RSALGLST                        |
    *     +-------------------------------------------------------+
    *  68 |                       RSANOTIB                        |
    *     +-------------------------------------------------------+
    *  70 |                       RSA2GAFP                        |
    *     +-------------------------------------------------------+
    *  78 |                       RSA2GABP                        |
    *     +-------------------------------------------------------+
    *  80 |                       RSA2GAVL                        |
    *     +-------------------------------------------------------+
    *  88 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  90 |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    *  98 |///////////////////////////|         RSAAVLHG          |
    *     +---------------------------+---------------------------+
    *  A0 |                                                       |
    *     =                       RSA2GLCK                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  D0 |                       RSA2GCFP                        |
    *     +-------------------------------------------------------+
    *  D8 |                       RSA2GCBP                        |
    *     +-------------------------------------------------------+
    *  E0 |                       RSA2GCVL                        |
    *     +-------------------------------------------------------+
    *  E8 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  F0 |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    *  F8 |///////////////////////////|         RSAAVCHG          |
    *     +---------------------------+---------------------------+
    * 100 |                                                       |
    *     =                       RSA2GCLK                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 130 |                                                       |
    *     =                       RSAPRLK                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 148 |                                                       |
    *     =                       RSAASITB                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 1C8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 1D0 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 1D8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 1E0 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 1E8 |         RSAPPAQD          |         RSAPPTLK          |
    *     +---------------------------+---------------------------+
    * 1F0 |         RSARESAC          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 1F8 |                       RSARFRSG                        |
    *     +-------------------------------------------------------+
    * 200 |                       RSAAFRDW                        |
    *     +-------------------------------------------------------+
    * 208 |                       RSAAFRIU                        |
    *     +---------------------------+---------------------------+
    * 210 |         RSAAFSDW          |         RSAAFSDB          |
    *     +---------------------------+---------------------------+
    * 218 |         RSARFRST          |         RSAAFRDB          |
    *     +---------------------------+---------------------------+
    * 220 |         RSAAFSIU          |         RSAAFSIB          |
    *     +---------------------------+---------------------------+
    * 228 |         RSAAFRIB          |         RSAVCBDW          |
    *     +---------------------------+---------------------------+
    * 230 |         RSAVCBDB          |         RSAVCBIU          |
    *     +---------------------------+---------------------------+
    * 238 |         RSAVCBIB          |         RSAVFSDW          |
    *     +---------------------------+---------------------------+
    * 240 |         RSAVFSIU          |         RSANALD           |
    *     +---------------------------+---------------------------+
    * 248 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 250 |         RSANDUCT          |         RSASHRSP          |
    *     +---------------------------+---------------------------+
    * 258 |                       RSAPPTN                         |
    *     +---------------------------+---------------------------+
    * 260 |         RSAPPTPS          |         RSAPPTPF          |
    *     +---------------------------+---------------------------+
    * 268 |         RSAPPTCS          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 270 |                                                       |
    *     =                       RSASHRLK                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 288 |                                                       |
    *     =                       RSASPMLK                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 2A0 |                                                       |
    *     =                       RSAALCIN                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 2B8 |         RSACTSHR          |         RSABLKGC          |
    *     +---------------------------+---------------------------+
    * 2C0 |                                                       |
    *     =                       RSABLKGF                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 2D8 |         RSACPLOK          |         RSAOFFLN          |
    *     +---------------------------+---------------------------+
    * 2E0 |         RSASHARE          |         RSANONPG          |
    *     +---------------------------+---------------------------+
    * 2E8 |         RSAPGABL          |         RSACPLKG          |
    *     +---------------------------+---------------------------+
    * 2F0 |                       RSAAVLFP                        |
    *     +-------------------------------------------------------+
    * 2F8 |                       RSAAVLBP                        |
    *     +---------------------------+---------------------------+
    * 300 |///////////////////////////|         RSAAVAIL          |
    *     +---------------------------+---------------------------+
    * 308 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 310 |///////////////////////////|         RSAAVLHT          |
    *     +---------------------------+---------------------------+
    * 318 |                                                       |
    *     =                       RSAAVLLK                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 348 |                       RSA16KBP                        |
    *     +-------------------------------------------------------+
    * 350 |                       RSAAVCFP                        |
    *     +-------------------------------------------------------+
    * 358 |                       RSAAVCBP                        |
    *     +---------------------------+---------------------------+
    * 360 |///////////////////////////|         RSAAVCIL          |
    *     +---------------------------+---------------------------+
    * 368 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 370 |///////////////////////////|         RSAAVCHT          |
    *     +---------------------------+---------------------------+
    * 378 |                                                       |
    *     =                       RSAAVCLK                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 3A8 |         RSAFRQFP          |         RSAFRQBP          |
    *     +---------------------------+---------------------------+
    * 3B0 |         RSA2GDCT          |         RSAFRQMW          |
    *     +---------------------------+---------------------------+
    * 3B8 |         RSAFRQDF          |         RSAFRQDL          |
    *     +---------------------------+---------------------------+
    * 3C0 |                       RSAFRQDT                        |
    *     +-------------------------------------------------------+
    * 3C8 |                       RSAFRQDA                        |
    *     +---------------------------+---------------------------+
    * 3D0 |         RSA2GRDA          |         RSA2GRDC          |
    *     +---------------------------+---------------------------+
    * 3D8 |         RSAFRQWT          |         RSAFRRDA          |
    *     +---------------------------+---------------------------+
    * 3E0 |         RSAFRRDC          |         RSARESBC          |
    *     +------+--------------------+------+--------------------+
    * 3E8 |:RFLOK|     RSADSCPU       |:TRQLK|////////////////////|
    *     +------+--------------------+------+--------------------+
    * 3F0 |                       RSADSTSA                        |
    *     +-------------------------------------------------------+
    * 3F8 |                       RSADSTSB                        |
    *     +---------------------------+---------------------------+
    * 400 |         RSASWPWT          |         RSASWP2G          |
    *     +---------------------------+---------------------------+
    * 408 |         RSAAVLLT          |         RSADECCT          |
    *     +---------------------------+---------------------------+
    * 410 |         RSAAVCLT          |         RSADECCC          |
    *     +-------------+------+------+---------------------------+
    * 418 |/////////////|:DECFG|:DECFL|         RSAAVLLG          |
    *     +-------------+------+------+---------------------------+
    * 420 |         RSADECCG          |         RSAAVCLG          |
    *     +---------------------------+---------------------------+
    * 428 |         RSADECGC          |         RSACFPCT          |
    *     +---------------------------+---------------------------+
    * 430 |         RSACFPAV          |         RSAALFMF          |
    *     +---------------------------+---------------------------+
    * 438 |         RSAAVLEP          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 440 |         RSASTLWT          |         RSASWG2G          |
    *     +---------------------------+---------------------------+
    * 448 |                       RSACNOTI                        |
    *     +---------------------------+---------------------------+
    * 450 |         RSAFTXFL          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 458 |         RSAFTXFG          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 460 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 470 |                                                       |
    *     =                       RSARINTA                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 4B0 |         RSAFSA2G          |         RSAFSB2G          |
    *     +---------------------------+---------------------------+
    * 4B8 |         RSAFSYUA          |         RSAFSYUB          |
    *     +---------------------------+---------------------------+
    * 4C0 |         RSAFVMUD          |         RSAFVMUB          |
    *     +---------------------------+---------------------------+
    * 4C8 |         RSAVMXFR          |         RSAVMXFB          |
    *     +---------------------------+---------------------------+
    * 4D0 |         RSAVMXUD          |         RSAVMXUB          |
    *     +---------------------------+---------------------------+
    * 4D8 |         RSASYSFR          |         RSASYSFB          |
    *     +---------------------------+---------------------------+
    * 4E0 |         RSASYSUD          |         RSASYSUB          |
    *     +---------------------------+---------------------------+
    * 4E8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 4F0 |         RSALIM1           |         RSALIM2           |
    *     +---------------------------+---------------------------+
    * 4F8 |         RSALIM3           |         RSALMFUZ          |
    *     +--------------------+------+---------------------------+
    * 500 |////////////////////|:LIMCK|         RSAFSELK          |
    *     +--------------------+------+---------------------------+
    * 508 |         RSAPLPCT          |         RSAPLPCB          |
    *     +---------------------------+---------------------------+
    * 510 |         RSANPGCT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 518 |                       RSAEMTSA                        |
    *     +-------------------------------------------------------+
    * 520 |                       RSAEMTSB                        |
    *     +---------------------------+---------------------------+
    * 528 |         RSANPGMX          |         RSANPGHI          |
    *     +---------------------------+---------------------------+
    * 530 |         RSAXTEND          |         RSARESAN          |
    *     +---------------------------+---------------------------+
    * 538 |         RSARSVLK          |         RSARSVSY          |
    *     +---------------------------+---------------------------+
    * 540 |         RSAMAXPP          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 548 |         RSADEFAN          |         RSADEFLK          |
    *     +---------------------------+---------------------------+
    * 550 |         RSAPRQWT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 558 |                                                       |
    *     =                       RSAFSLCK                        =
    *     |                                                       |
    *     +-------------+-------------+-------------+-------------+
    * 570 |  RSASA1ST   |  RSASALST   |   RSAMSO    |   RSAMSL    |
    *     +------+------+-------------+-------------+-------------+
    * 578 |:AZNCT|:ZPOOL|/////////////|///////////////////////////|
    *     +------+------+-------------+---------------------------+
    * 580 |///////////////////////////|         RSAVSLOW          |
    *     +---------------------------+---------------------------+
    * 588 |                                                       |
    *     =                       RSAVHSLK                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 5A0 |///////////////////////////|         RSAVHSAD          |
    *     +---------------------------+---------------------------+
    * 5A8 |                                                       |
    *     =                       RSANOQLK                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 5D8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 5E0 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 5E8 |                       RSANOQFR                        |
    *     +-------------------------------------------------------+
    * 5F0 |                       RSANOQPG                        |
    *     +---------------------------+---------------------------+
    * 5F8 |///////////////////////////|         RSANOLKL          |
    *     +---------------------------+---------------------------+
    * 600 |                       RSANOLKA                        |
    *     +---------------------------+---------------------------+
    * 608 |         RSANOLOK          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 610 |         RSADPPB           |         RSADPPA           |
    *     +---------------------------+---------------------------+
    * 618 |                                                       |
    *     =                       RSASXQLK                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 648 |                       RSASXQFP                        |
    *     +-------------------------------------------------------+
    * 650 |                       RSASXQBP                        |
    *     +---------------------------+---------------------------+
    * 658 |         RSASXQCT          |         RSASXQMN          |
    *     +---------------------------+---------------------------+
    * 660 |                       RSASXPFP                        |
    *     +-------------------------------------------------------+
    * 668 |                       RSASXPBP                        |
    *     +---------------------------+---------------------------+
    * 670 |         RSASXPCT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 678 |                       RSASXAFP                        |
    *     +-------------------------------------------------------+
    * 680 |                       RSASXABP                        |
    *     +---------------------------+---------------------------+
    * 688 |         RSASXACT          |         RSASXAMX          |
    *     +---------------------------+---------------------------+
    * 690 |                       RSASXBFP                        |
    *     +-------------------------------------------------------+
    * 698 |                       RSASXBBP                        |
    *     +---------------------------+---------------------------+
    * 6A0 |         RSASXBCT          |         RSASXBMX          |
    *     +---------------------------+---------------------------+
    * 6A8 |         RSASXDFP          |         RSASXDBP          |
    *     +---------------------------+---------------------------+
    * 6B0 |         RSASXDCT          |         RSASXDCA          |
    *     +---------------------------+---------------------------+
    * 6B8 |         RSASXDPB          |         RSASXDPA          |
    *     +---------------------------+---------------------------+
    * 6C0 |         RSASXRDA          |         RSASXRDC          |
    *     +---------------------------+---------------------------+
    * 6C8 |         RSASXAVL          |         RSASXUSD          |
    *     +---------------------------+---------------------------+
    * 6D0 |         RSASXUCP          |         RSASXUID          |
    *     +---------------------------+---------------------------+
    * 6D8 |         RSASXUFS          |         RSASXUFG          |
    *     +---------------------------+---------------------------+
    * 6E0 |         RSASXUOT          |         RSASXBKA          |
    *     +---------------------------+---------------------------+
    * 6E8 |         RSASXBKB          |         RSASXALI          |
    *     +---------------------------+---------------------------+
    * 6F0 |         RSASXNOP          |         RSASXCTG          |
    *     +---------------------------+---------------------------+
    * 6F8 |         RSASXDFA          |         RSASXDFB          |
    *     +---------------------------+---------------------------+
    * 700 |         RSASXCLA          |         RSASXCPL          |
    *     +---------------------------+---------------------------+
    * 708 |///////////////////////////|         RSASXLOK          |
    *     +---------------------------+---------------------------+
    * 710 |                      RSASXFLGS                        |
    *     +-------------------------------------------------------+
    * 718 |                       RSASXSTO                        |
    *     +---------------------------+---------------------------+
    * 720 |         RSASXQRA          |         RSASXRPM          |
    *     +---------------------------+---------------------------+
    * 728 |         RSASXRFC          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 730 |         RSAFOBCT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 738 |                       RSACALFP                        |
    *     +-------------------------------------------------------+
    * 740 |                       RSACALBP                        |
    *     +-------------------------------------------------------+
    * 748 |                       RSACALCT                        |
    *     +-------------------------------------------------------+
    * 750 |                       RSACALUT                        |
    *     +-------------------------------------------------------+
    * 758 |                       RSACALMT                        |
    *     +-------------------------------------------------------+
    * 760 |                       RSACALLT                        |
    *     +-------------------------------------------------------+
    * 768 |                                                       |
    *     =                       RSACALLK                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 798 |         RSARCLOK          |///////////////////////////|
    *     +--------------------+------+---------------------------+
    * 7A0 |////////////////////|:AASTA|         RSAAAPFX          |
    *     +--------------------+------+---------------------------+
    * 7A8 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 7B0 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 7B8 |///////////////////////////////////////////////////////|
    *     +------+------+-------------+---------------------------+
    * 7C0 |:EMTS |:EMFL |/////////////|         RSAEMERG          |
    *     +------+------+-------------+---------------------------+
    * 7C8 |                       RSAEMFMT                        |
    *     +---------------------------+---------------------------+
    * 7D0 |         RSAEMCPC          |         RSAEMDFR          |
    *     +---------------------------+---------------------------+
    * 7D8 |         RSAEMBLO          |         RSAEMPTY          |
    *     +---------------------------+---------------------------+
    * 7E0 |         RSAEMCPQ          |         RSAEMRPT          |
    *     +---------------------------+---------------------------+
    * 7E8 |         RSAEMLO           |         RSAEMHI           |
    *     +---------------------------+---------------------------+
    * 7F0 |         RSALTDB1          |         RSALTDA1          |
    *     +---------------------------+---------------------------+
    * 7F8 |         RSALTDD1          |         RSALTDC1          |
    *     +---------------------------+---------------------------+
    * 800 |         RSALTDB2          |         RSALTDA2          |
    *     +---------------------------+---------------------------+
    * 808 |         RSALTDD2          |         RSALTDC2          |
    *     +---------------------------+---------------------------+
    * 810 |         RSALTDBE          |         RSALTDAE          |
    *     +---------------------------+---------------------------+
    * 818 |         RSALTDDE          |         RSALTDCE          |
    *     +---------------------------+---------------------------+
    * 820 |         RSADRMB1          |         RSADRMA1          |
    *     +---------------------------+---------------------------+
    * 828 |         RSADRMD1          |         RSADRMC1          |
    *     +---------------------------+---------------------------+
    * 830 |         RSADRMB2          |         RSADRMA2          |
    *     +---------------------------+---------------------------+
    * 838 |         RSADRMD2          |         RSADRMC2          |
    *     +---------------------------+---------------------------+
    * 840 |         RSADRMBE          |         RSADRMAE          |
    *     +---------------------------+---------------------------+
    * 848 |         RSADRMDE          |         RSADRMCE          |
    *     +---------------------------+---------------------------+
    * 850 |         RSAELGB1          |         RSAELGA1          |
    *     +---------------------------+---------------------------+
    * 858 |         RSAELGD1          |         RSAELGC1          |
    *     +---------------------------+---------------------------+
    * 860 |         RSAELGB2          |         RSAELGA2          |
    *     +---------------------------+---------------------------+
    * 868 |         RSAELGD2          |         RSAELGC2          |
    *     +---------------------------+---------------------------+
    * 870 |         RSAELGBE          |         RSAELGAE          |
    *     +---------------------------+---------------------------+
    * 878 |         RSAELGDE          |         RSAELGCE          |
    *     +---------------------------+---------------------------+
    * 880 |         RSADSPB1          |         RSADSPA1          |
    *     +---------------------------+---------------------------+
    * 888 |         RSADSPD1          |         RSADSPC1          |
    *     +---------------------------+---------------------------+
    * 890 |         RSADSPB2          |         RSADSPA2          |
    *     +---------------------------+---------------------------+
    * 898 |         RSADSPD2          |         RSADSPC2          |
    *     +---------------------------+---------------------------+
    * 8A0 |         RSADSPBE          |         RSADSPAE          |
    *     +---------------------------+---------------------------+
    * 8A8 |         RSADSPDE          |         RSADSPCE          |
    *     +---------------------------+---------------------------+
    * 8B0 |         RSASHRB1          |         RSASHRA1          |
    *     +---------------------------+---------------------------+
    * 8B8 |         RSASHRD1          |         RSASHRC1          |
    *     +---------------------------+---------------------------+
    * 8C0 |         RSASHRB2          |         RSASHRA2          |
    *     +---------------------------+---------------------------+
    * 8C8 |         RSASHRD2          |         RSASHRC2          |
    *     +---------------------------+---------------------------+
    * 8D0 |         RSASHRBE          |         RSASHRAE          |
    *     +---------------------------+---------------------------+
    * 8D8 |         RSASHRDE          |         RSASHRCE          |
    *     +---------------------------+---------------------------+
    * 8E0 |         RSAAVLFT          |         RSAAVCFT          |
    *     +---------------------------+---------------------------+
    * 8E8 |         RSAAVLFG          |         RSAAVCFG          |
    *     +---------------------------+---------------------------+
    * 8F0 |         RSADSCD0          |         RSADSCDG          |
    *     +---------------------------+---------------------------+
    * 8F8 |         RSADSCC0          |         RSADSCCG          |
    *     +---------------------------+---------------------------+
    * 900 |         RSAPGMQ1          |         RSAPGMQ2          |
    *     +---------------------------+---------------------------+
    * 908 |         RSAPGMQE          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 910 |         RSATURN0          |         RSATURNG          |
    *     +---------------------------+---------------------------+
    * 918 |                       RSAVGPST                        |
    *     +-------------------------------------------------------+
    * 920 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * A20 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * B20 |                                                       |
    *     =                       RSAFTXLK                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * B50 |                     RSAPFXFTLEN                       |
    *     +-------------------------------------------------------+
    * B58 |                     RSAPFXSTLEN                       |
    *     +------+------+-----------------------------------------+
    * B60 |(B60) |(B61) |/////////////////////////////////////////|
    *     +------+------+-----------------------------------------+
    * B68 |                     RSASYSGTORS                       |
    *     +-------------------------------------------------------+
    * B70 |                     RSASYSSXSSZ                       |
    *     +-------------------------------------------------------+
    * B78 |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * B80 |        RSASYSTORS         | B84
    *     +---------------------------+
    *
    *** RSMBK - RSM common area mapping

    *** Overlay for RSARINTA in RSMBK
    *
    *     +---------------------------+---------------------------+
    * 470 |         RSARESLK          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 478 |         RSAALLTA          |         RSAAVGDU          |
    *     +---------------------------+---------------------------+
    * 480 |         RSAAVGRT          |         RSAOLDTA          |
    *     +---------------------------+---------------------------+
    * 488 |                       RSAOLDTD                        |
    *     +-------------------------------------------------------+
    * 490 |                       RSARESSA                        |
    *     +-------------------------------------------------------+
    * 498
    *
    *** Overlay for RSARINTA in RSMBK

    *** Overlay for RSASXFLGS in RSMBK
    *
    *     +----------------------------------+------+------+------+
    * 710 |//////////////////////////////////|:SXINI|:SXREP|:SXPQS|
    *     +----------------------------------+------+------+------+
    * 718
    *
    *** Overlay for RSASXFLGS in RSMBK

    *** Overlay for RSAFTXBL in RSMBK
    *
    *     +---------------------------+---------------------------+
    * 920 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 928 |                       RSAFTSSL                        |
    *     +-------------------------------------------------------+
    * 930 |                       RSAFTSEL                        |
    *     +-------------------------------------------------------+
    * 938
    *
    *** Overlay for RSAFTXBL in RSMBK

    *** Overlay for RSAFTXBG in RSMBK
    *
    *     +---------------------------+---------------------------+
    * A20 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * A28 |                       RSAFTSSG                        |
    *     +-------------------------------------------------------+
    * A30 |                       RSAFTSEG                        |
    *     +-------------------------------------------------------+
    * A38
    *
    *** Overlay for RSAFTXBG in RSMBK

    RSAAVNKR Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    rsaPFXFTLEN    0B50
    rsaPFXGPFLG    0B60
    rsaPFXSTLEN    0B58
    rsaSYSGTORS    0B68
    rsaSYSSXSSZ    0B70
    rsaSYSTORS     0B80
    rsaVMDLOWW0    0B61
    FTXSIZED       0717 00000020
    RSAemBLO       07D8
    RSAemCPc       07D0
    RSAemCPq       07E0
    RSAemDFR       07D4
    RSAemERG       07C4
    RSAemFL        07C1
    RSAemFMT       07C8
    RSAemHI        07EC
    RSAemLO        07E8
    RSAemPTY       07DC
    RSAemRP        07C1 08
    RSAemRPT       07E4
    RSAemTS        07C0
    RSAneCNT       002B 02
    RSAneCTG       002B 04
    RSAneTSK       002B 01
    RSAAAFLG       07A0
    RSAAAFTO       07B0
    RSAAAON        07A3 80
    RSAAAPFX       07A4
    RSAAASTA       07A3
    RSAAASTO       07B8
    RSAAASXS       07A8
    RSAAFRDB       021C
    RSAAFRDW       0200
    RSAAFRIB       0228
    RSAAFRIU       0208
    RSAAFSDB       0214
    RSAAFSDW       0210
    RSAAFSIB       0224
    RSAAFSIU       0220
    RSAALCIN       02A0
    RSAALFMF       0434
    RSAALLTA       0478
    RSAASITB       0148
    RSAAVAIL       0304
    RSAAVBP        0008
    RSAAVCAN       0350
    RSAAVCBP       0358
    RSAAVCFG       08EC
    RSAAVCFP       0350
    RSAAVCFT       08E4
    RSAAVCHG       00FC
    RSAAVCHT       0374
    RSAAVCIL       0364
    RSAAVCLG       0424
    RSAAVCLK       0378
    RSAAVCLT       0410
    RSAAVCT        0010
    RSAAVCT4       0010
    RSAAVFP        0000
    RSAAVGDU       047C
    RSAAVGRT       0480
    RSAAVLAN       02F0
    RSAAVLBP       02F8
    RSAAVLEP       0438
    RSAAVLFG       08E8
    RSAAVLFP       02F0
    RSAAVLFT       08E0
    RSAAVLHG       009C
    RSAAVLHT       0314
    RSAAVLLG       041C
    RSAAVLLK       0318
    RSAAVLLT       0408
    RSAAZNCT       0578
    RSABLKGC       02BC
    RSABLKGF       02C0
    RSACALAN       0738
    RSACALBP       0740
    RSACALCT       0748
    RSACALFP       0738
    RSACALLK       0768
    RSACALLT       0760
    RSACALMT       0758
    RSACALUT       0750
    RSACFPAV       0430
    RSACFPCT       042C
    RSACNOTI       0448
    RSACPLKG       02EC
    RSACPLOK       02D8
    RSACTSHR       02B8
    RSADCCGC       041A 04
    RSADECCC       0414
    RSADECCG       0420
    RSADECCS       0418
    RSADECCT       040C
    RSADECFG       041A
    RSADECFL       041B
    RSADECGC       0428
    RSADECRB       041B 01
    RSADECRC       041B 04
    RSADECRG       041A 01
    RSADEFAN       0548
    RSADEFLK       054C
    RSADPAAD       002C
    RSADPACP       0014
    RSADPPA        0614
    RSADPPB        0610
    RSADPPBW       01D0
    RSADPPCA       0610
    RSADPPFW       01C8
    RSADRMAE       0844
    RSADRMA1       0824
    RSADRMA2       0834
    RSADRMBE       0840
    RSADRMB1       0820
    RSADRMB2       0830
    RSADRMCE       084C
    RSADRMC1       082C
    RSADRMC2       083C
    RSADRMDE       0848
    RSADRMD1       0828
    RSADRMD2       0838
    RSADSCCG       08FC
    RSADSCC0       08F8
    RSADSCDG       08F4
    RSADSCD0       08F0
    RSADSCPU       03E9
    RSADSLOK       03E8
    RSADSPAE       08A4
    RSADSPA1       0884
    RSADSPA2       0894
    RSADSPBE       08A0
    RSADSPB1       0880
    RSADSPB2       0890
    RSADSPCE       08AC
    RSADSPC1       088C
    RSADSPC2       089C
    RSADSPDE       08A8
    RSADSPD1       0888
    RSADSPD2       0898
    RSADSTSA       03F0
    RSADSTSB       03F8
    RSAELGAE       0874
    RSAELGA1       0854
    RSAELGA2       0864
    RSAELGBE       0870
    RSAELGB1       0850
    RSAELGB2       0860
    RSAELGCE       087C
    RSAELGC1       085C
    RSAELGC2       086C
    RSAELGDE       0878
    RSAELGD1       0858
    RSAELGD2       0868
    RSAEMTSA       0518
    RSAEMTSB       0520
    RSAFNOTI       0030
    RSAFOBCT       0730
    RSAFRQAN       03A8
    RSAFRQBP       03AC
    RSAFRQDA       03C8
    RSAFRQDF       03B8
    RSAFRQDL       03BC
    RSAFRQDT       03C0
    RSAFRQFP       03A8
    RSAFRQMW       03B4
    RSAFRQWT       03D8
    RSAFRRDA       03DC
    RSAFRRDC       03E0
    RSAFSA2G       04B0
    RSAFSB2G       04B4
    RSAFSELK       0504
    RSAFSLCK       0558
    RSAFSTBK       0558
    RSAFSTLN       057C 00000028
    RSAFSTSZ       057C 00000005
    RSAFSYUA       04B8
    RSAFSYUB       04BC
    RSAFTSEG       0A30
    RSAFTSEL       0930
    RSAFTSSG       0A28
    RSAFTSSL       0928
    RSAFTXBG       0A20
    RSAFTXBL       0920
    RSAFTXFG       0458
    RSAFTXFL       0450
    RSAFTXLK       0B20
    RSAFVMUB       04C4
    RSAFVMUD       04C0
    RSAGOFFL       0040
    RSAGSTOR       0048
    RSAINCGC       041A 08
    RSAINCRB       041B 02
    RSAINCRC       041B 08
    RSAINCRG       041A 02
    RSAINITL       0760 00000004
    RSAINITM       0758 00000008
    RSAINITU       0750 00000020
    RSALGFRM       0038
    RSALGLST       0060
    RSALG1ST       0058
    RSALIMCK       0503
    RSALIMCS       0500
    RSALIMOF       0503 00000000
    RSALIMON       0503 00000001
    RSALIM1        04F0
    RSALIM2        04F4
    RSALIM3        04F8
    RSALMFUZ       04FC
    RSALTDAE       0814
    RSALTDA1       07F4
    RSALTDA2       0804
    RSALTDBE       0810
    RSALTDB1       07F0
    RSALTDB2       0800
    RSALTDCE       081C
    RSALTDC1       07FC
    RSALTDC2       080C
    RSALTDDE       0818
    RSALTDD1       07F8
    RSALTDD2       0808
    RSAMAXPP       0540
    RSAMSARC       0008
    RSAMSARH       0010
    RSAMSASC       000C
    RSAMSL         0576
    RSAMSO         0574
    RSANALD        0244
    RSANASIT       0248
    RSANDUCT       0250
    RSANOLKA       0600
    RSANOLKL       05FC
    RSANOLOK       0608
    RSANONPG       02E4
    RSANOQFR       05E8
    RSANOQLK       05A8
    RSANOQPG       05F0
    RSANOTIB       0068
    RSANOXBP       05E0
    RSANOXFP       05D8
    RSANPGCT       0510
    RSANPGHI       052C
    RSANPGMX       0528
    RSAOFFLN       02DC
    RSAOLDTA       0484
    RSAOLDTD       0488
    RSAPFXAF       0020
    RSAPFXND       0024
    RSAPGABL       02E8
    RSAPGMQE       0908
    RSAPGMQ1       0900
    RSAPGMQ2       0904
    RSAPLPCB       050C
    RSAPLPCT       0508
    RSAPPABW       01E0
    RSAPPAFW       01D8
    RSAPPAQD       01E8
    RSAPPTCS       0268
    RSAPPTLK       01EC
    RSAPPTN        0258
    RSAPPTPF       0264
    RSAPPTPS       0260
    RSAPRLK        0130
    RSAPRQWT       0550
    RSARCLOK       0798
    RSARESAC       01F0
    RSARESAN       0534
    RSARESBC       03E4
    RSARESLK       0470
    RSARESSA       0490
    RSARFLOK       03E8
    RSARFRSG       01F8
    RSARFRST       0218
    RSARINTA       0470
    RSARSAST       0004
    RSARSVLK       0538
    RSARSVSY       053C
    RSASALST       0572
    RSASAVFR       0000
    RSASA1ST       0570
    RSASHARE       02E0
    RSASHRAE       08D4
    RSASHRA1       08B4
    RSASHRA2       08C4
    RSASHRBE       08D0
    RSASHRB1       08B0
    RSASHRB2       08C0
    RSASHRCE       08DC
    RSASHRC1       08BC
    RSASHRC2       08CC
    RSASHRDE       08D8
    RSASHRD1       08B8
    RSASHRD2       08C8
    RSASHRLK       0270
    RSASHRSP       0254
    RSASPMLK       0288
    RSASTLWT       0440
    RSASTORE       001C
    RSASTORL       0050
    RSASTRNG       0574
    RSASWG2G       0444
    RSASWPWT       0400
    RSASWP2G       0404
    RSASXAAN       0678
    RSASXABP       0680
    RSASXACT       0688
    RSASXAFP       0678
    RSASXALI       06EC
    RSASXAMX       068C
    RSASXAVL       06C8
    RSASXBAN       0690
    RSASXBBP       0698
    RSASXBCT       06A0
    RSASXBFP       0690
    RSASXBKA       06E4
    RSASXBKB       06E8
    RSASXBMX       06A4
    RSASXCLA       0700
    RSASXCPL       0704
    RSASXCTG       06F4
    RSASXDAN       06A8
    RSASXDBP       06AC
    RSASXDCA       06B4
    RSASXDCT       06B0
    RSASXDFA       06F8
    RSASXDFB       06FC
    RSASXDFP       06A8
    RSASXDPA       06BC
    RSASXDPB       06B8
    RSASXFLGS      0710
    RSASXIMX       0715 80
    RSASXINI       0715
    RSASXLOK       070C
    RSASXNOP       06F0
    RSASXNST       0717 80
    RSASXPAN       0660
    RSASXPBP       0668
    RSASXPCT       0670
    RSASXPFP       0660
    RSASXPQS       0717
    RSASXQAN       0648
    RSASXQBP       0650
    RSASXQCT       0658
    RSASXQFP       0648
    RSASXQLK       0618
    RSASXQMN       065C
    RSASXQRA       0720
    RSASXRDA       06C0
    RSASXRDC       06C4
    RSASXREP       0716
    RSASXRFC       0728
    RSASXRPF       0716 80
    RSASXRPL       0716 40
    RSASXRPM       0724
    RSASXSTO       0718
    RSASXUCP       06D0
    RSASXUFG       06DC
    RSASXUFS       06D8
    RSASXUID       06D4
    RSASXUOT       06E0
    RSASXUSD       06CC
    RSASYSFB       04DC
    RSASYSFR       04D8
    RSASYSUB       04E4
    RSASYSUD       04E0
    RSASZD         0B80 00000171
    RSATASKB       0028
    RSATRQLK       03EC
    RSATRSAV       0018
    RSATSKB0       0028
    RSATSKB1       0029
    RSATSKB2       002A
    RSATSKB3       002B
    RSATURBS       0914 RSATURNG
    RSATURHD       0914 03
    RSATURMN       0914 01
    RSATURMX       0914 RSATURNG
    RSATURNG       0914
    RSATURN0       0910
    RSAVCBDB       0230
    RSAVCBDW       022C
    RSAVCBIB       0238
    RSAVCBIU       0234
    RSAVFSDW       023C
    RSAVFSIU       0240
    RSAVGPST       0918
    RSAVHSAD       05A4
    RSAVHSLK       0588
    RSAVMXFB       04CC
    RSAVMXFR       04C8
    RSAVMXUB       04D4
    RSAVMXUD       04D0
    RSAVSLOW       0584
    RSAVVBLK       0580
    RSAXTEND       0530
    RSAZPOOL       0579
    RSA16KBP       0348
    RSA2GABP       0078
    RSA2GAFP       0070
    RSA2GAHD       0070
    RSA2GAVL       0080
    RSA2GCBP       00D8
    RSA2GCFP       00D0
    RSA2GCHD       00D0
    RSA2GCLK       0100
    RSA2GCVL       00E0
    RSA2GDCT       03B0
    RSA2GLCK       00A0
    RSA2GRDA       03D0
    RSA2GRDC       03D4
    RSMFRCHN       0000
    RSMFRCNT       0008

    This information is
    based on z/VM V6R1.0.
    Last updated on 18 Feb 2010 at 09:01:48 EDT.

    Copyright IBM Corporation, 1990, 2008