Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRUSELOF

Prolog
Control Block Contents
Cross Reference

#### MRUSELOF Prolog

####

####

     DSECT NAME - USELOF
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRUSELOF
     DESCRIPTIVE NAME - Monitor Event Record
                        Domain 4 - User Domain
                        Record 2 - User Logoff Data
     DESCRIPTION - Records a user that has logged off.  A record
                   is created for the base VMDBK and each virtual@SQ534PQ
                   CPU that is active at LOGOFF.
     NOTE - Alternate VMDBKs of the user that has logged off are
            recorded in MRUSEDTC (Domain 4, Record 6).
          - Fields which are valid only for the base VMDBK are
            indicated in the comments for the fields.

    MRUSELOF Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure  444  USELOF                 Start of monitor record
      0   0  Character    0  USELOF_MRHDR           record header
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN               record length in bytes
      2   2  Unsigned     2  MRHDRZER               field of zeros
      4   4  Unsigned     1  MRHDRDM                domain identifier
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC                record identifier
      8   8  Character    8  MRHDRTOD               Time at which this record was
                                                    built. In time-of-day (TOD)
                                                    clock format. See IBM System
                                                    370 XA Principle of Operation
                                                    for explanation of format.
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END              End of header
     20  14  Character    8  USELOF_VMDUSER         USERID
     28  1C  Unsigned     2  USELOF_VMDCPUAD        Processor ID
     30  1E  Bitstring    1  USELOF_VMDMODE         Guest machine mode. This is
                                                    as set for internal use by CP.
                                                    See USELOF_CALMODE for the mode
                                                    'calculated' at.
     31  1F  Bitstring    1  USELOF_CALMODE         Architectural mode of the
                                                    virtual machine
              1... ....      *
              .1.. ....      USELOF_CALMESA         ESA architecture
              ..1. ....      USELOF_CALMXA          XA architecture
              ...1 ....      USELOF_CALM370         370 architecture
              .... 1...      USELOF_CALMXC          XC architecture
              .... .1..      USELOF_CALMESAM        ESA mode machine has entered
                                                    z/Arch mode.
              .... ..1.      *
              .... ...1      *
     32  20  Bitstring    1  USELOF_VMDSLIST        Scheduling list that the user
                                                    is in: X'37' = Dispatch List.
                                                    X'21' = Eligible List. X'0B' =
                                                    Dormant List. X'00' = user is
                                                    not in any list.
     33  21  Unsigned     1  USELOF_VMDELIST        Class number (0,1,2,or 3) of
                                                    the scheduling list the user is
                                                    in
     34  22  Bitstring    1  USELOF_CALFLAG1        Flag byte
              1... ....      *
              .1.. ....      USELOF_VMDQDSPU        This user has the QUICKDSP
                                                    designation, as set or
                                                    defaulted by the SET QUICKDSP
                                                    command. When the user has work
                                                    to do, it will be added to the
                                                    dispatch list immediately
                                                    without waiting in the eligible
                                                    list.
              ..1. ....      USELOF_CALDIAL         This user is a dialed user
              ...1 ....      USELOF_CALSNA          This user is connected
                                                    through System Network
                                                    Architecture (SNA)
              .... 1...      USELOF_VMDNOINS        User is prevented from
                                                    inserting any tracks into the
                                                    minidisk cache. (set when SET
                                                    MDC INS OFF command is issued)
              .... .1..      USELOF_VMDNOFSL        No MDC fair share limit
                                                    applies. Set at LOGON if the
                                                    NOMDCFS option is specified on
                                                    the OPTIONS statement in the
                                                    user's directory.
              .... ..1.      USELOF_VMDMASST        Collaborative Memory
                                                    Management assist enabled.
              .... ...1      USELOF_VMDMAACT        Collaborative Memory
                                                    Management assist is active,
                                                    i.e. in use by this virtual
                                                    machine. Note: This guest may
                                                    be in a pending off state if
                                                    either a global or per-user SET
                                                    MEMASSIST OFF has been issued
                                                    (SYSMASST or VMDMASST is off).
                                                    This indicates that the system
                                                    or user setting was turned off
                                                    after the guest started using
                                                    the assist. The assist will
                                                    remain active
                                                    (USELOF_VMDMAACT=1) and
                                                    available to this guest until
                                                    the next virtual machine reset
                                                    or IPL.
     35  23  Bitstring    1  USELOF_VMDSTYPE        Storage type this virtual
                                                    machine resides in. X'00' =>
                                                    V=V. X'80' => Reserved and no
                                                    longer available. X'40' => V=F.
     36  24  Character    8  USELOF_VMDTTIME        Total time which has been
                                                    expended on this VMDBK. This
                                                    includes time which the VMDBK
                                                    spent doing its own work and
                                                    also time which CP spent doing
                                                    work on behalf of the VMDBK. It
                                                    is in CPU timer format. The
                                                    complement of this field is the
                                                    elapsed time in TOD clock
                                                    units.
     44  2C  Character    8  USELOF_VMDVTIME        Total time that this user was
                                                    running and doing productive
                                                    work. It does NOT include any
                                                    time that CP spends on behalf
                                                    of that user doing such things
                                                    as instruction simulation or
                                                    page translation. This is in
                                                    CPU timer format. The
                                                    complement of this field is the
                                                    elapsed time in TOD clock
                                                    units.
     52  34  Character    8  *                      Reserved for IBM use.
                                                    Previous field is no longer
                                                    meaningful. (USELOF_VMDVFVTM)
     60  3C  Character    8  *                      Reserved for IBM use.
                                                    Previous field is no longer
                                                    meaningful. (USELOF_VMDVFOTM)
     68  44  Unsigned     4  USELOF_VMDCTPVR        Cardinal count of private
                                                    resident pages in the virtual
                                                    machine. This monitor field is
                                                    actually the sum of VMDCTPVR +
                                                    VMDCTPVG, which includes pages
                                                    above and below the 2GB line.
                                                    To get the count of the
                                                    resident pages below the 2GB
                                                    line, subtract USELOF_VMDCTPVG
                                                    from USELOF_VMDCTPVR. Valid
                                                    only on base VMDBK.
     72  48  Unsigned     4  USELOF_VMDCTPVL        Cardinal count of locked
                                                    pages in private address spaces
                                                    <2G belonging to this user. See
                                                    USELOF_VMDCTPVLA for the >2G
                                                    value. Valid only on base
                                                    VMDBK.
     76  4C  Unsigned     4  USELOF_VMDWSSPR        This user's projected working
                                                    set size. This is the
                                                    scheduler's estimate of the
                                                    amount of storage this user
                                                    will require to be resident as
                                                    it runs during its next stay in
                                                    the dispatch list. It is based
                                                    upon the user's past behavior
                                                    and in some cases, on the
                                                    behavior of similar types of
                                                    users. Valid only on base
                                                    VMDBK.
     80  50  Unsigned     4  USELOF_VMDCTXBK        Number of expanded storage
                                                    blocks allocated to a virtual
                                                    machine by CP for paging. Valid
                                                    only on base VMDBK.
     84  54  Unsigned     4  USELOF_CALXSTOR        Size, in megabytes, of
                                                    expanded storage attached to
                                                    the user. If zero, no expanded
                                                    storage is attached. VMDXSTOR
     88  58  Unsigned     4  USELOF_VMDCTFLT        Count of host segment and
                                                    page faults on guest pages
                                                    which occurred while running
                                                    this virtual CPU. It does not
                                                    include faults on RCP pages.
     92  5C  Unsigned     4  *                      Reserved for IBM use.
                                                    Previous field is no longer
                                                    meaningful. (USELOF_VMDCTVFL)
     96  60  Unsigned     4  USELOF_VMDFLREO        Total number of frame list
                                                    reorders for this virtual
                                                    system's private address spaces
    100  64  Unsigned     4  USELOF_VMDCTORF        Total number of referenced
                                                    frames resident when reset was
                                                    done for this virtual system's
                                                    private address spaces
    104  68  Unsigned     4  USELOF_CALCTPGS        Cardinal count of
                                                    non-preferred paging slots for
                                                    private address spaces
                                                    belonging to this user. Valid
                                                    only on base VMDBK.
    108  6C  Unsigned     4  USELOF_VMDCTPWT        Count of outstanding paging
                                                    and spooling I/O's for this
                                                    user
    112  70  Unsigned     4  USELOF_CALCPPGR        Cumulative count of pages
                                                    read from DASD to main storage
                                                    for this user's address spaces
                                                    while they were private. Valid
                                                    only on base VMDBK.
    116  74  Unsigned     4  USELOF_CALCPPGW        Cumulative count of pages
                                                    written from main storage to
                                                    DASD for this user's address
                                                    spaces while they were private.
                                                    Valid only on base VMDBK.
    120  78  Unsigned     4  USELOF_VMDCTSPR        Number of times I/O was
                                                    issued for a spool read request
                                                    Valid only on base VMDBK.
    124  7C  Unsigned     4  USELOF_VMDCTSPW        Number of times I/O was
                                                    issued for a spool write
                                                    request Valid only on base
                                                    VMDBK.
    128  80  Unsigned     4  USELOF_VMDPGSPL        Number of pages spooled for
                                                    this user. This includes the
                                                    pages spooled for the virtual
                                                    reader, printer, punch,
                                                    console, dump, and trace files.
    132  84  Unsigned     4  USELOF_VMDVCSCT        Count of start requests to
                                                    the virtual machine console
    136  88  Unsigned     4  USELOF_VMDVDSCT        Cumulative count of virtual
                                                    I/O requests the virtual
                                                    machine has issued to DASD
                                                    devices
    140  8C  Unsigned     4  USELOF_VMDVUSCT        Count of Start requests to
                                                    virtual Unit Record devices
    144  90  Unsigned     4  USELOF_VMDVTSCT        Count of Start requests to
                                                    virtual channel-to-channel
                                                    adapters
    148  94  Unsigned     4  USELOF_VMDVOSCT        Count of Start requests to
                                                    devices other than console,
                                                    DASDs, CTCAs, and unit records.
                                                    (see USELOF_VMDVCSCT,
                                                    USELOF_VMDVDSCT,
                                                    USELOF_VMDVUSCT, and
                                                    USELOF_VMDVTSCT)
    152  98  Unsigned     4  USELOF_CALCPPST        Cumulative count of pages
                                                    stolen from this user's address
                                                    spaces while they were private.
                                                    Valid only on base VMDBK.
    156  9C  Unsigned     4  USELOF_VMDISEVM        Number of times IUCV data was
                                                    successfully transferred by
                                                    this virtual machine. (SENDs
                                                    and REPLYs with RC=0 when this
                                                    virtual machine is the source).
                                                    Valid only in base VMDBK.
    160  A0  Unsigned     4  USELOF_VMDISTVM        Number of times IUCV data was
                                                    successfully transferred to
                                                    this virtual machine. (SENDs
                                                    and REPLYs with RC=0 when this
                                                    virtual machine is the target).
                                                    Valid only in base VMDBK.
    164  A4  Unsigned     4  USELOF_VMDISUVM        Number of times IUCV data was
                                                    NOT successfully transferred by
                                                    this virtual machine. (SENDs
                                                    and REPLYs with RC^=0 when this
                                                    virtual machine is the source).
                                                    Valid only in the base VMDBK.
    168  A8  Unsigned     4  USELOF_VMDVSEVM        Number of times VMCF data was
                                                    successfully transferred by
                                                    this virtual machine. (SENDs
                                                    SENDXs, SEND/RECEIVEs, and
                                                    REPLYs with RC=0 and this
                                                    virtual machine is source.)
                                                    Valid only on base VMDBK.
    172  AC  Unsigned     4  USELOF_VMDVSTVM        Number of times VMCF data was
                                                    successfully transferred to
                                                    this virtual machine. (SENDs
                                                    SENDXs, SEND/RECEIVEs, and
                                                    REPLYs with RC=0 and this
                                                    virtual machine is target.)
                                                    Valid only on base VMDBK.
    176  B0  Unsigned     4  USELOF_VMDVSUVM        Number of times VMCF data was
                                                    NOT successfully transferred by
                                                    this virtual machine. (SENDs
                                                    SENDXs, SEND/RECEIVEs, and
                                                    REPLYs with RC^=0 and this
                                                    virtual machine is source.)
                                                    Valid only on base VMDBK.
    180  B4  Unsigned     4  USELOF_VMDX98CT        Cumulative number of times
                                                    Diagnose X'98' was issued by
                                                    this virtual machine
    184  B8  Unsigned     4  USELOF_CALCPMIG        Cumulative count of pages
                                                    migrated by CP from expanded
                                                    storage to DASD for this user's
                                                    address spaces while they were
                                                    private. Valid only on base
                                                    VMDBK.
    188  BC  Unsigned     4  USELOF_CALCPXWT        Cumulative count of pages
                                                    written from main storage to
                                                    expanded storage for this
                                                    user's address spaces while
                                                    they were private. Valid only
                                                    on base VMDBK.
    192  C0  Unsigned     4  USELOF_CALCPXRD        Cumulative count of pages
                                                    read from expanded storage to
                                                    main storage for this user's
                                                    address spaces while they were
                                                    private. Valid only on base
                                                    VMDBK.
    196  C4  Unsigned     2  USELOF_VMDASMCT        Cardinal number of non-base
                                                    address spaces owned by this
                                                    user.
    198  C6  Bitstring    1  USELOF_CALSHARF        Set Share flags
              1... ....      USELOF_VMDMXSHA        Max share for this CPU is
                                                    ABSOLUTE if on. Max share for
                                                    this CPU is RELATIVE if off.
              .1.. ....      *
              ..1. ....      *
              ...1 ....      *
              .... 1...      *
              .... .1..      *
              .... ..1.      USELOF_VMDLIMTH        Max share for this CPU is
                                                    LIMITHARD if on. Max share for
                                                    this CPU is LIMITSOFT if off.
              .... ...1      *
    199  C7  Bitstring    1  USELOF_CALOSTAT        Virtual machine operating
                                                    status
              1... ....      USELOF_VMDSYSOP        User is primary system
                                                    operator
              .1.. ....      USELOF_VMDUSRCT        User is counted as being
                                                    logged on
              ..1. ....      *
              ...1 ....      USELOF_VMDFORCE        User is to be logged off.
                                                    This may be requested by CP, a
                                                    forced logoff, or user's logoff
                                                    command.
              .... 1...      USELOF_VMDUFORC        User is forced to logoff the
                                                    system
              .... .1..      USELOF_VMDDISC         User is running disconnected
              .... ..1.      USELOF_VMDAUTOL        AUTOLOG/XAUTOLOG in progress.
                                                    User has been automatically
                                                    logged on. This bit is set off
                                                    when the user's IPL statement
                                                    is processed, or (if there is
                                                    no IPL to process) when the
                                                    user enters a LOGON command
                                                    from a terminal to RECONNECT.
              .... ...1      USELOF_VMDXAUTO        The original command was
                                                    XAUTOLOG. Valid for the base
                                                    VMDBK only (see
                                                    USEINT_CALBASE).
    200  C8  Unsigned     4  USELOF_VMDBLKCT        Count of SSCH's issued by
                                                    BLOCKIO system service
                                                    (includes both read and write
                                                    requests)
    204  CC  Unsigned     4  USELOF_VMDMDCIA        Count of SSCH's avoided due
                                                    to Minidisk Cache read hit
    208  D0  Unsigned     4  USELOF_VMDCOPCT        Number of times this virtual
                                                    CPU had to be redispatched due
                                                    to a crypto operation exception
    212  D4  Unsigned     4  USELOF_VMDCTISO        Number of times ISOLATE
                                                    occurred for spaces owned by
                                                    this virtual system. Valid only
                                                    in base VMDBK
    216  D8  Unsigned     4  USELOF_VMDRELSH        This virtual CPU's RELATIVE
                                                    share of the system, as set in
                                                    the user's directory or via the
                                                    SET SHARE command. Set to zero
                                                    when this VMDBK has an ABSOLUTE
                                                    share value, or has a virtual
                                                    processor dedicated to it, or
                                                    is in the process of being
                                                    logged off.
    220  DC  Unsigned     4  USELOF_VMDABSSH        This virtual CPU's ABSOLUTE
                                                    share of the system, as set in
                                                    the user's directory or via the
                                                    SET SHARE command. Unit of
                                                    value is a hexadecimal factor
                                                    scaled 16 bits. For example,
                                                    X'00010000' = 1.00(100%),
                                                    X'0000C000' = 0.75(75%),
                                                    X'00008000' = 0.50(50%), etc.
                                                    Set to zero when this VMDBK has
                                                    a RELATIVE share value.
    224  E0  Unsigned     4  USELOF_VMDSSIZE        Virtual machine size, in
                                                    bytes. This field is kept for
                                                    compatability reasons, but may
                                                    not be accurate for z/Arch
                                                    systems where larger virtual
                                                    machines are valid. The
                                                    preferred field is
                                                    USELOF_ASCDEFSZ
    228  E4  Unsigned     4  USELOF_VMDMXRVP        Number of pages reserved for
                                                    the user
    232  E8  Character    8  USELOF_VMDACTNO        User accounting number
    240  F0  Character    8  USELOF_VMDGRPN         RACF ACI group name
    248  F8  Character    8  USELOF_CALTODON        Time at which the user logged
                                                    on for this session. In
                                                    time-of-day (TOD) clock format.
                                                    To get the user's connect time,
                                                    subtract this time value from
                                                    the time stamp in the record
                                                    header's MRHDRTOD. If virtual
                                                    CPUs are active at LOGOFF the
                                                    value in this field represents
                                                    the time-of-day when the
                                                    virtual CPU was defined.
    256 100  Unsigned     4  USELOF_VMDVDISK        Count of virtual I/Os to a
                                                    virtual disk in storage.
    260 104  Unsigned     4  USELOF_VMDMXSHR        This virtual CPU's Max share
                                                    of the system, as set in the
                                                    user's directory or via the SET
                                                    SHARE command. This value is
                                                    set to zero if no Max share
                                                    exists. If the Max share is
                                                    Absolute, then the unit of the
                                                    value is a hexadecimal factor
                                                    scaled 16 bits. For example,
                                                    X'00010000' = 1.00(100%),
                                                    X'0000C000' = 0.75(75%),
                                                    X'00008000' = 0.50(50%), etc.
                                                    Check USELOF_VMDMXSHA to
                                                    determine if Max share is
                                                    absolute or relative.
    264 108  Unsigned     4  USELOF_VMDTHRCT        Total number of times this
                                                    user was delayed doing I/O to a
                                                    throttled device
    268 10C  Character    8  USELOF_ASCDEFSZ        Defined storage size in
                                                    addressable bytes, minus one.
                                                    If DEF STOR CONFIG was used to
                                                    define multiple discontiguous
                                                    extents of addressable defined
                                                    storage, this field contains
                                                    the sum of the sizes in bytes
                                                    of all of the individual
                                                    extents (minus one). The minus
                                                    one notation is used so that a
                                                    total size of 16 Exabytes may
                                                    be represented without
                                                    ambiguity (as
                                                    x'FFFFFFFF_FFFFFFFF'). Valid
                                                    only on base VMDBK.
    268 10C  Character    4  USELOF_CALDEFHI        high four bytes
    272 110  Character    4  USELOF_CALDEFLO        low four bytes
    276 114  Unsigned     4  USELOF_VMDCTPVG        Count of private address
                                                    space resident pages in DPA
                                                    owned by this virtual machine
                                                    which are >= 2G. Valid only in
                                                    base VMDBK.
    280 118  Unsigned     4  USELOF_VMDMVB2G        Number of times page
                                                    translation moved a page on
                                                    behalf of this us user from a
                                                    frame with address >= 2GB to
                                                    one < 2GB. This field is only
                                                    valid in the base VMDBK.
    284 11C  Unsigned     4  USELOF_VEBALERT        Number of alert interruptions
                                                    Collected only for base VMDBK.
    288 120  Unsigned     4  USELOF_VEBTVSCT        Number of interceptions for
                                                    guest TVS instructions
                                                    Collected only for base VMDBK.
    292 124  Unsigned     4  USELOF_VEBSVSCT        Number of interceptions for
                                                    guest SVS instructions
                                                    Collected only for base VMDBK.
    296 128  Unsigned     4  USELOF_VEBTPIAI        Number of adapter
                                                    interruptions delivered via
                                                    guest TPI Collected only for
                                                    base VMDBK.
    300 12C  Unsigned     4  USELOF_VEBVIRAI        Number of adapter
                                                    interruptions stacked for guest
                                                    by CP Collected only for base
                                                    VMDBK.
    304 130  Unsigned     4  USELOF_VEBHDWAI        Number of adapter
                                                    interruptions delivered to
                                                    guest inside SIE Collected only
                                                    for base VMDBK.
    308 134  Character    8  USELOF_VMDCTPVLA       Cardinal count of locked
                                                    pages in private address spaces
                                                    >2G belonging to this user. See
                                                    USELOF_VMDCTPVL for the <2G
                                                    value. Valid only on base
                                                    VMDBK.
    316 13C  Unsigned     4  USELOF_VMDCTSHL        Count of shared address space
                                                    resident pages <2G. Valid only
                                                    in the SYSTEM VMDBK.
    320 140  Character    8  USELOF_VMDCTSHLA       Count of shared address space
                                                    resident pages >2G. Valid only
                                                    in the SYSTEM VMDBK.
    328 148  Unsigned     1  USELOF_VMDPUTYP        CPU Type. Valid values: X'00'
                                                    - General Purpose (CP) X'02' -
                                                    zSeries Application Assist
                                                    (zAAP) X'03' - Integrated
                                                    Facility for Linux (IFL) X'04'
                                                    - Internal Coupling Facility
                                                    (ICF) X'05' - zSeries
                                                    Integrated Information (zIIP)
    329 149  Character    3  *                      Reserved for IBM use
    332 14C  Character    8  USELOF_VMDVTMP         Total virtual time for user
                                                    on primary processor
    340 154  Character    8  USELOF_VMDTTMP         Total virtual and simulation
                                                    time for the user on primary
                                                    processor
    348 15C  Character    8  USELOF_VMDVTMS         Total virtual time for user
                                                    on secondary processor
    356 164  Character    8  USELOF_VMDTTMS         Total virtual and simulation
                                                    time for the user on secondary
                                                    processor
    364 16C  Unsigned     4  USELOF_CP_SSHRELSH     This user's RELATIVE share
                                                    setting for CPUs of type CP.
    368 170  Unsigned     4  USELOF_CP_SSHABSSH     This user's ABSOLUTE share
                                                    setting for CPUs of type CP.
    372 174  Unsigned     4  USELOF_CP_SSHMXSHR     This user's Max share setting
                                                    for CPUs of type CP.
    376 178  Bitstring    1  USELOF_CP_SSHFLG1      This user's share flags for
                                                    CPUs of type CP.
              1... ....      *
              .1.. ....      USELOF_CP_SSHLIMH      Max share for type CP is
                                                    LIMITHARD if on. Max share for
                                                    type CP is LIMITSOFT if off.
              ..1. ....      USELOF_CP_SSHNMSHA     Normal share for type CP is
                                                    ABSOLUTE if on. Normal share
                                                    for type CP is RELATIVE if off.
              ...1 ....      USELOF_CP_SSHMXSHA     Max share for type CP is
                                                    ABSOLUTE if on. Max share for
                                                    type CP is RELATIVE if off.
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
    377 179  Bitstring    3  *                      Reserved and available for
                                                    IBM use.
    380 17C  Unsigned     4  USELOF_ZAP_SSHRELSH    This user's RELATIVE share
                                                    setting for CPUs of type zAAP.
    384 180  Unsigned     4  USELOF_ZAP_SSHABSSH    This user's ABSOLUTE share
                                                    setting for CPUs of type zAAP.
    388 184  Unsigned     4  USELOF_ZAP_SSHMXSHR    This user's Max share setting
                                                    for CPUs of type zAAP.
    392 188  Bitstring    1  USELOF_ZAP_SSHFLG1     This user's share flags for
                                                    CPUs of type zAAP.
              1... ....      *
              .1.. ....      USELOF_ZAP_SSHLIMH     Max share for type zAAP is
                                                    LIMITHARD if on. Max share for
                                                    type zAAP is LIMITSOFT if off.
              ..1. ....      USELOF_ZAP_SSHNMSHA    Normal share for type zAAP is
                                                    ABSOLUTE if on. Normal share
                                                    for type zAAP is RELATIVE if
                                                    off.
              ...1 ....      USELOF_ZAP_SSHMXSHA    Max share for type zAAP is
                                                    ABSOLUTE if on. Max share for
                                                    type zAAP is RELATIVE if off.
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
    393 189  Bitstring    3  *                      Reserved and available for
                                                    IBM use.
    396 18C  Unsigned     4  USELOF_IFL_SSHRELSH    This user's RELATIVE share
                                                    setting for CPUs of type IFL.
    400 190  Unsigned     4  USELOF_IFL_SSHABSSH    This user's ABSOLUTE share
                                                    setting for CPUs of type IFL.
    404 194  Unsigned     4  USELOF_IFL_SSHMXSHR    This user's Max share setting
                                                    for CPUs of type IFL.
    408 198  Bitstring    1  USELOF_IFL_SSHFLG1     This user's share flags for
                                                    CPUs of type IFL.
              1... ....      *
              .1.. ....      USELOF_IFL_SSHLIMH     Max share for type IFL is
                                                    LIMITHARD if on. Max share for
                                                    type IFL is LIMITSOFT if off.
              ..1. ....      USELOF_IFL_SSHNMSHA    Normal share for type IFL is
                                                    ABSOLUTE if on. Normal share
                                                    for type IFL is RELATIVE if
                                                    off.
              ...1 ....      USELOF_IFL_SSHMXSHA    Max share for type IFL is
                                                    ABSOLUTE if on. Max share for
                                                    type IFL is RELATIVE if off.
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
    409 199  Bitstring    3  *                      Reserved and available for
                                                    IBM use.
    412 19C  Unsigned     4  USELOF_ICF_SSHRELSH    This user's RELATIVE share
                                                    setting for CPUs of type ICF.
    416 1A0  Unsigned     4  USELOF_ICF_SSHABSSH    This user's ABSOLUTE share
                                                    setting for CPUs of type ICF.
    420 1A4  Unsigned     4  USELOF_ICF_SSHMXSHR    This user's Max share setting
                                                    for CPUs of type ICF.
    424 1A8  Bitstring    1  USELOF_ICF_SSHFLG1     This user's share flags for
                                                    CPUs of type ICF.
              1... ....      *
              .1.. ....      USELOF_ICF_SSHLIMH     Max share for type ICF is
                                                    LIMITHARD if on. Max share for
                                                    type ICF is LIMITSOFT if off.
              ..1. ....      USELOF_ICF_SSHNMSHA    Normal share for type ICF is
                                                    ABSOLUTE if on. Normal share
                                                    for type ICF is RELATIVE if
                                                    off.
              ...1 ....      USELOF_ICF_SSHMXSHA    Max share for type ICF is
                                                    ABSOLUTE if on. Max share for
                                                    type ICF is RELATIVE if off.
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
    425 1A9  Bitstring    3  *                      Reserved and available for
                                                    IBM use.
    428 1AC  Unsigned     4  USELOF_ZIP_SSHRELSH    This user's RELATIVE share
                                                    setting for CPUs of type zIIP.
    432 1B0  Unsigned     4  USELOF_ZIP_SSHABSSH    This user's ABSOLUTE share
                                                    setting for CPUs of type zIIP.
    436 1B4  Unsigned     4  USELOF_ZIP_SSHMXSHR    This user's Max share setting
                                                    for CPUs of type zIIP.
    440 1B8  Bitstring    1  USELOF_ZIP_SSHFLG1     This user's share flags for
                                                    CPUs of type zIIP.
              1... ....      *
              .1.. ....      USELOF_ZIP_SSHLIMH     Max share for type zIIP is
                                                    LIMITHARD if on. Max share for
                                                    type zIIP is LIMITSOFT if off.
              ..1. ....      USELOF_ZIP_SSHNMSHA    Normal share for type zIIP is
                                                    ABSOLUTE if on. Normal share
                                                    for type zIIP is RELATIVE if
                                                    off.
              ...1 ....      USELOF_ZIP_SSHMXSHA    Max share for type zIIP is
                                                    ABSOLUTE if on. Max share for
                                                    type zIIP is RELATIVE if off.
              .... 1...      *
              .... .1..      *
              .... ..1.      *
              .... ...1      *
    441 1B9  Bitstring    3  *                      Reserved and available for
                                                    IBM use.
    444 1BC  Character    0  USELOF_END

    MRUSELOF Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    USELOF                     0    444
    USELOF_ASCDEFSZ          10C      8
    USELOF_CALCPMIG           B8      4
    USELOF_CALCPPGR           70      4
    USELOF_CALCPPGW           74      4
    USELOF_CALCPPST           98      4
    USELOF_CALCPXRD           C0      4
    USELOF_CALCPXWT           BC      4
    USELOF_CALCTPGS           68      4
    USELOF_CALDEFHI          10C      4
    USELOF_CALDEFLO          110      4
    USELOF_CALDIAL            22           20
    USELOF_CALFLAG1           22      1
    USELOF_CALMESA            1F           40
    USELOF_CALMESAM           1F           04
    USELOF_CALMODE            1F      1
    USELOF_CALMXA             1F           20
    USELOF_CALMXC             1F           08
    USELOF_CALM370            1F           10
    USELOF_CALOSTAT           C7      1
    USELOF_CALSHARF           C6      1
    USELOF_CALSNA             22           10
    USELOF_CALTODON           F8      8
    USELOF_CALXSTOR           54      4
    USELOF_CP_SSHABSSH       170      4
    USELOF_CP_SSHFLG1        178      1
    USELOF_CP_SSHLIMH        178           40
    USELOF_CP_SSHMXSHA       178           10
    USELOF_CP_SSHMXSHR       174      4
    USELOF_CP_SSHNMSHA       178           20
    USELOF_CP_SSHRELSH       16C      4
    USELOF_END               1BC      0
    USELOF_ICF_SSHABSSH      1A0      4
    USELOF_ICF_SSHFLG1       1A8      1
    USELOF_ICF_SSHLIMH       1A8           40
    USELOF_ICF_SSHMXSHA      1A8           10
    USELOF_ICF_SSHMXSHR      1A4      4
    USELOF_ICF_SSHNMSHA      1A8           20
    USELOF_ICF_SSHRELSH      19C      4
    USELOF_IFL_SSHABSSH      190      4
    USELOF_IFL_SSHFLG1       198      1
    USELOF_IFL_SSHLIMH       198           40
    USELOF_IFL_SSHMXSHA      198           10
    USELOF_IFL_SSHMXSHR      194      4
    USELOF_IFL_SSHNMSHA      198           20
    USELOF_IFL_SSHRELSH      18C      4
    USELOF_MRHDR               0      0
    USELOF_VEBALERT          11C      4
    USELOF_VEBHDWAI          130      4
    USELOF_VEBSVSCT          124      4
    USELOF_VEBTPIAI          128      4
    USELOF_VEBTVSCT          120      4
    USELOF_VEBVIRAI          12C      4
    USELOF_VMDABSSH           DC      4
    USELOF_VMDACTNO           E8      8
    USELOF_VMDASMCT           C4      2
    USELOF_VMDAUTOL           C7           02
    USELOF_VMDBLKCT           C8      4
    USELOF_VMDCOPCT           D0      4
    USELOF_VMDCPUAD           1C      2
    USELOF_VMDCTFLT           58      4
    USELOF_VMDCTISO           D4      4
    USELOF_VMDCTORF           64      4
    USELOF_VMDCTPVG          114      4
    USELOF_VMDCTPVL           48      4
    USELOF_VMDCTPVLA         134      8
    USELOF_VMDCTPVR           44      4
    USELOF_VMDCTPWT           6C      4
    USELOF_VMDCTSHL          13C      4
    USELOF_VMDCTSHLA         140      8
    USELOF_VMDCTSPR           78      4
    USELOF_VMDCTSPW           7C      4
    USELOF_VMDCTXBK           50      4
    USELOF_VMDDISC            C7           04
    USELOF_VMDELIST           21      1
    USELOF_VMDFLREO           60      4
    USELOF_VMDFORCE           C7           10
    USELOF_VMDGRPN            F0      8
    USELOF_VMDISEVM           9C      4
    USELOF_VMDISTVM           A0      4
    USELOF_VMDISUVM           A4      4
    USELOF_VMDLIMTH           C6           02
    USELOF_VMDMAACT           22           01
    USELOF_VMDMASST           22           02
    USELOF_VMDMDCIA           CC      4
    USELOF_VMDMODE            1E      1
    USELOF_VMDMVB2G          118      4
    USELOF_VMDMXRVP           E4      4
    USELOF_VMDMXSHA           C6           80
    USELOF_VMDMXSHR          104      4
    USELOF_VMDNOFSL           22           04
    USELOF_VMDNOINS           22           08
    USELOF_VMDPGSPL           80      4
    USELOF_VMDPUTYP          148      1
    USELOF_VMDQDSPU           22           40
    USELOF_VMDRELSH           D8      4
    USELOF_VMDSLIST           20      1
    USELOF_VMDSSIZE           E0      4
    USELOF_VMDSTYPE           23      1
    USELOF_VMDSYSOP           C7           80
    USELOF_VMDTHRCT          108      4
    USELOF_VMDTTIME           24      8
    USELOF_VMDTTMP           154      8
    USELOF_VMDTTMS           164      8
    USELOF_VMDUFORC           C7           08
    USELOF_VMDUSER            14      8
    USELOF_VMDUSRCT           C7           40
    USELOF_VMDVCSCT           84      4
    USELOF_VMDVDISK          100      4
    USELOF_VMDVDSCT           88      4
    USELOF_VMDVOSCT           94      4
    USELOF_VMDVSEVM           A8      4
    USELOF_VMDVSTVM           AC      4
    USELOF_VMDVSUVM           B0      4
    USELOF_VMDVTIME           2C      8
    USELOF_VMDVTMP           14C      8
    USELOF_VMDVTMS           15C      8
    USELOF_VMDVTSCT           90      4
    USELOF_VMDVUSCT           8C      4
    USELOF_VMDWSSPR           4C      4
    USELOF_VMDXAUTO           C7           01
    USELOF_VMDX98CT           B4      4
    USELOF_ZAP_SSHABSSH      180      4
    USELOF_ZAP_SSHFLG1       188      1
    USELOF_ZAP_SSHLIMH       188           40
    USELOF_ZAP_SSHMXSHA      188           10
    USELOF_ZAP_SSHMXSHR      184      4
    USELOF_ZAP_SSHNMSHA      188           20
    USELOF_ZAP_SSHRELSH      17C      4
    USELOF_ZIP_SSHABSSH      1B0      4
    USELOF_ZIP_SSHFLG1       1B8      1
    USELOF_ZIP_SSHLIMH       1B8           40
    USELOF_ZIP_SSHMXSHA      1B8           10
    USELOF_ZIP_SSHMXSHR      1B4      4
    USELOF_ZIP_SSHNMSHA      1B8           20
    USELOF_ZIP_SSHRELSH      1AC      4

    This information is
    based on z/VM V6R1.0.

    Last updated on 8 Oct 2009 at 21:08:13.

    Copyright IBM Corporation, 1990, 2009