DG5BK | Back to Index page

| Prolog Control Block Contents DG5BK DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

DG5BK Control Block Content | Top of page

     DG5BK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      DG5BK          NETWORK DIAGNOSE x'2A8' Request Blocks
                 Code defined in DG5FUNC
    0000    0 Bitstring    1 DG5FUNC        Function to Perform
              .... ....      DG5QUERY       0 DG5QUERY Query Device Options
              .... ...1      DG5PRMON       1 DG5PRMON Turn on Promiscuous
                                            Mode
              .... ..1.      DG5PRMOF       2 DG5PRMOF Turn off Promiscuous
                                            Mode
    0001    1 Bitstring    7 *              Reserved for future IBM Use
    0008    8 Dbl-Word     8 * (3)          Reserved for Future IBM Use
    0020   32 Bitstring   32 DG5RESP (0)    Response Area
    0020   32 Signed       4 DG5OPTS (0)    Network Device Options
                 Code defined in DG5FOPT0
    0020   32 Bitstring    1 DG5FOPT0       Device Options Byte 0
              1... ....      DG5PAUTH       X'80' DG5PAUTH Promiscuous Mode
                                            Authorized
              .1.. ....      DG5PROM        X'40' DG5PROM Promiscuous Mode ON
                 Code defined in DG5FOPT1
    0021   33 Bitstring    1 DG5FOPT1       Device Options Byte 1
                 Code defined in DG5FOPT2
    0022   34 Bitstring    1 DG5FOPT2       Device Options Byte 2
                 Code defined in DG5FOPT3
    0023   35 Bitstring    1 DG5FOPT3       Device Options Byte 3
    0024   36 Signed       4 *              Reserved for future IBM Use
    0028   40 Dbl-Word     8 * (3)          Reserved for Future IBM Use
    0040   64 Bitstring    1 DG5$END (0)    The end

DG5BK Storage Layout | Top of page

    *** DG5BK - NETWORK DIAGNOSE x'2A8' Request Blocks
    *
    *     +------+------------------------------------------------+
    *   0 |:FUNC |////////////////////////////////////////////////|
    *     +------+------------------------------------------------+
    *   8 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +------+------+------+------+---------------------------+
    *  20 |:FOPT0|:FOPT1|:FOPT2|:FOPT3|///////////////////////////|
    *     +------+------+------+------+---------------------------+
    *  28 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *
    *** DG5BK - NETWORK DIAGNOSE x'2A8' Request Blocks

DG5BK Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    DG5$END        0040
    DG5FOPT0       0020
    DG5FOPT1       0021
    DG5FOPT2       0022
    DG5FOPT3       0023
    DG5FUNC        0000
    DG5OPTS        0020
    DG5PAUTH       0020 80
    DG5PRMOF       0000 02
    DG5PRMON       0000 01
    DG5PROM        0020 40
    DG5QUERY       0000 00
    DG5RESP        0020

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:27:42 EDT.
Copyright IBM Corporation, 1990, 2020